<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="9.6.2">
<drawing>
<library>
<packages>
<package name="GP_01M">
</package>
<package name="GP_02M">
</package>
<package name="GP_03M">
</package>
<package name="MICROSD">
</package>
<package name="GP_04M">
</package>
<package name="JST-PH-B3">
</package>
<package name="JST-PH-B4">
</package>
<package name="JST-PH-B5">
</package>
<package name="JST-PH-B2">
</package>
<package name="WS-06S">
</package>
<package name="JST-PH-B6">
</package>
<package name="GP_40M">
</package>
<package name="FPC_30_05MM">
</package>
<package name="FPC_30_05_STRIP">
</package>
<package name="GP_02_06M">
</package>
<package name="GP_03_04M">
</package>
<package name="FPC_06_05MM">
</package>
<package name="MICROSIM">
</package>
<package name="KEYS940">
</package>
<package name="U.FL_ADAM_TECH">
</package>
<package name="RAW_3">
</package>
<package name="RAW_5">
</package>
<package name="SMD_CERAMIC_ANT">
</package>
<package name="NANOSIM">
</package>
<package name="S5B-SM4A">
</package>
<package name="RAW_2">
</package>
<package name="KEYS940_F">
</package>
<package name="PCB_USB">
</package>
<package name="GP_05M">
</package>
<package name="SMA_THT_ADAM_TECH">
</package>
<package name="MX-105017-0001">
</package>
<package name="RAW_4">
</package>
<package name="RAW_6">
</package>
<package name="GP_06M">
</package>
<package name="GP_10M">
</package>
<package name="GP_07M">
</package>
<package name="RAW_MINI_2">
</package>
<package name="RAW_MINI_5">
</package>
<package name="USBA-LP-SMD">
</package>
<package name="MX-502570-0893">
</package>
<package name="XT30PW-M">
</package>
<package name="XT30PW-F">
</package>
<package name="XT60PW-M">
</package>
<package name="JST-ZH-S6">
</package>
<package name="JST-ZH-S5">
</package>
<package name="JST-ZH-S2">
</package>
<package name="JST-ZH-S8">
</package>
<package name="JST-ZH-S7">
</package>
<package name="JST-SR-S2">
</package>
<package name="JST-SR-S3">
</package>
<package name="JST-SR-S4">
</package>
<package name="JST-SR-S5">
</package>
<package name="JST-SR-S6">
</package>
<package name="JST-SR-S7">
</package>
<package name="JST-SR-S8">
</package>
<package name="HIGH_AMP">
</package>
<package name="VERY_HIGH_AMP">
</package>
</packages>
<symbols>
<symbol name="MICROSD">
<pin name="D0/MISO"/>
<pin name="D1"/>
<pin name="D2"/>
<pin name="D3/CS"/>
<pin name="CK/SCK"/>
<pin name="CMD/MOSI"/>
<pin name="GND"/>
<pin name="VCC"/>
<pin name="SENSE"/>
</symbol>
<symbol name="USB_OTG">
<pin name="D+"/>
<pin name="D-"/>
<pin name="OTG"/>
<pin name="GND"/>
<pin name="VCC"/>
</symbol>
<symbol name="CONN_03">
<pin name="P1"/>
<pin name="P2"/>
<pin name="P3"/>
</symbol>
<symbol name="CONN_02">
<pin name="P1"/>
<pin name="P2"/>
</symbol>
<symbol name="CONN_04">
<pin name="P2"/>
<pin name="P3"/>
<pin name="P1"/>
<pin name="P4"/>
</symbol>
<symbol name="RPI_ZERO">
<pin name="P0"/>
<pin name="P1"/>
<pin name="P2"/>
<pin name="3V3"/>
<pin name="P4"/>
<pin name="P3"/>
<pin name="P6"/>
<pin name="P5"/>
<pin name="P7"/>
<pin name="5V"/>
<pin name="GND"/>
<pin name="P14"/>
<pin name="P15"/>
<pin name="P16"/>
<pin name="P17"/>
<pin name="P18"/>
<pin name="P19"/>
<pin name="P20"/>
<pin name="P21"/>
<pin name="P22"/>
<pin name="P23"/>
<pin name="P24"/>
<pin name="P25"/>
<pin name="P27"/>
<pin name="P26"/>
<pin name="P13"/>
<pin name="P12"/>
<pin name="P11"/>
<pin name="P10"/>
<pin name="P9"/>
<pin name="P8"/>
</symbol>
<symbol name="CONN_30">
<pin name="P23"/>
<pin name="P22"/>
<pin name="P21"/>
<pin name="P24"/>
<pin name="P25"/>
<pin name="P26"/>
<pin name="P20"/>
<pin name="P27"/>
<pin name="P28"/>
<pin name="P29"/>
<pin name="P19"/>
<pin name="P18"/>
<pin name="P17"/>
<pin name="P16"/>
<pin name="P1"/>
<pin name="P2"/>
<pin name="P3"/>
<pin name="P4"/>
<pin name="P5"/>
<pin name="P6"/>
<pin name="P7"/>
<pin name="P8"/>
<pin name="P9"/>
<pin name="P10"/>
<pin name="P11"/>
<pin name="P12"/>
<pin name="P13"/>
<pin name="P14"/>
<pin name="P15"/>
<pin name="P30"/>
</symbol>
<symbol name="CONN_SERVO">
<pin name="GND"/>
<pin name="VCC"/>
<pin name="SIG"/>
</symbol>
<symbol name="CONN_02_06">
<pin name="P3"/>
<pin name="P4"/>
<pin name="P5"/>
<pin name="P6"/>
<pin name="P2"/>
<pin name="P1"/>
<pin name="P7"/>
<pin name="P8"/>
<pin name="P9"/>
<pin name="P10"/>
<pin name="P11"/>
<pin name="P12"/>
</symbol>
<symbol name="CONN_03_04">
<pin name="P3"/>
<pin name="P2"/>
<pin name="P1"/>
<pin name="P4"/>
<pin name="P5"/>
<pin name="P6"/>
<pin name="P12"/>
<pin name="P11"/>
<pin name="P10"/>
<pin name="P9"/>
<pin name="P8"/>
<pin name="P7"/>
</symbol>
<symbol name="CONN_06">
<pin name="P2"/>
<pin name="P3"/>
<pin name="P1"/>
<pin name="P4"/>
<pin name="P5"/>
<pin name="P6"/>
</symbol>
<symbol name="CONN_07">
<pin name="P2"/>
<pin name="P3"/>
<pin name="P1"/>
<pin name="P4"/>
<pin name="P5"/>
<pin name="P6"/>
<pin name="P7"/>
</symbol>
<symbol name="FPC_06">
<pin name="P2"/>
<pin name="P3"/>
<pin name="P1"/>
<pin name="P4"/>
<pin name="P5"/>
<pin name="P6"/>
<pin name="PAD"/>
</symbol>
<symbol name="MICROSIM">
<pin name="IO"/>
<pin name="CLK"/>
<pin name="GND"/>
<pin name="RST"/>
<pin name="VCC"/>
<pin name="CPP"/>
<pin name="PAD"/>
</symbol>
<symbol name="ANTENN">
<pin name="SIG"/>
<pin name="GROUND"/>
</symbol>
<symbol name="CONN_05">
<pin name="P2"/>
<pin name="P3"/>
<pin name="P1"/>
<pin name="P4"/>
<pin name="P5"/>
</symbol>
<symbol name="CONN_05_P">
<pin name="P2"/>
<pin name="P3"/>
<pin name="P1"/>
<pin name="P4"/>
<pin name="P5"/>
<pin name="PAD"/>
</symbol>
<symbol name="USB">
<pin name="D+"/>
<pin name="D-"/>
<pin name="GND"/>
<pin name="VCC"/>
</symbol>
<symbol name="CONN_34">
<pin name="P1"/>
<pin name="P4"/>
<pin name="P6"/>
<pin name="P5"/>
<pin name="P7"/>
<pin name="P15"/>
<pin name="P16"/>
<pin name="P17"/>
<pin name="P18"/>
<pin name="P19"/>
<pin name="P20"/>
<pin name="P21"/>
<pin name="P22"/>
<pin name="P23"/>
<pin name="P24"/>
<pin name="P25"/>
<pin name="P27"/>
<pin name="P26"/>
<pin name="P11"/>
<pin name="P10"/>
<pin name="P9"/>
<pin name="P8"/>
</symbol>
<symbol name="CONN_01">
<pin name="P1"/>
</symbol>
<symbol name="CONN_10">
<pin name="P2"/>
<pin name="P3"/>
<pin name="P1"/>
<pin name="P4"/>
<pin name="P5"/>
<pin name="P6"/>
<pin name="P7"/>
<pin name="P8"/>
<pin name="P9"/>
<pin name="P10"/>
</symbol>
<symbol name="RPI_BPLUS">
<pin name="5V"/>
<pin name="3V3"/>
<pin name="GND"/>
<pin name="GPIO27"/>
<pin name="GPIO26"/>
<pin name="GPIO25"/>
<pin name="GPIO24"/>
<pin name="GPIO10"/>
<pin name="GPIO11"/>
<pin name="GPIO12"/>
<pin name="GPIO13"/>
<pin name="GPIO14"/>
<pin name="GPIO15"/>
<pin name="GPIO23"/>
<pin name="GPIO22"/>
<pin name="GPIO21"/>
<pin name="GPIO20"/>
<pin name="GPIO19"/>
<pin name="GPIO9"/>
<pin name="GPIO8"/>
<pin name="GPIO7"/>
<pin name="GPIO6"/>
<pin name="GPIO5"/>
<pin name="GPIO4"/>
<pin name="GPIO3"/>
<pin name="GPIO2"/>
<pin name="GPIO18"/>
<pin name="GPIO17"/>
<pin name="GPIO16"/>
<pin name="ID_SD"/>
<pin name="ID_SC"/>
</symbol>
<symbol name="RPI_4B">
<pin name="5V"/>
<pin name="3V3"/>
<pin name="GND"/>
<pin name="GPIO17"/>
<pin name="GPIO26"/>
<pin name="GPIO25"/>
<pin name="GPIO24"/>
<pin name="GPIO6"/>
<pin name="GPIO7(CE1)"/>
<pin name="GPIO8(CE0)"/>
<pin name="GPIO13(PWM1)"/>
<pin name="GPIO14(TXD)"/>
<pin name="GPIO12(PWM0)"/>
<pin name="GPIO23"/>
<pin name="GPIO22"/>
<pin name="(PCM_DOUT)GPIO21"/>
<pin name="(PCM_DIN)GPIO20"/>
<pin name="(PCM_FS)GPIO19"/>
<pin name="GPIO5"/>
<pin name="GPIO11(SCLK)"/>
<pin name="GPIO9(MISO)"/>
<pin name="GPIO10(MOSI)"/>
<pin name="GPIO0(ID_SD)"/>
<pin name="GPIO4(GPCLK0)"/>
<pin name="GPIO3(SCL)"/>
<pin name="GPIO2(SDA)"/>
<pin name="(PCM_CLK)GPIO18"/>
<pin name="GPIO16"/>
<pin name="GPIO15(RXD)"/>
<pin name="(ID_SC)GPIO1"/>
<pin name="GPIO27"/>
</symbol>
<symbol name="CONN_08">
<pin name="P2"/>
<pin name="P3"/>
<pin name="P1"/>
<pin name="P4"/>
<pin name="P5"/>
<pin name="P6"/>
<pin name="P7"/>
<pin name="P8"/>
</symbol>
</symbols>
<devicesets>
<deviceset name="SD_CARD">
<description>Micro SD Card socket</description>
<gates>
<gate name="G$1" symbol="MICROSD"/>
</gates>
<devices>
<device name="" package="MICROSD">
<connects>
<connect gate="G$1" pin="CK/SCK" pad="5"/>
<connect gate="G$1" pin="CMD/MOSI" pad="3"/>
<connect gate="G$1" pin="D0/MISO" pad="7"/>
<connect gate="G$1" pin="D1" pad="8"/>
<connect gate="G$1" pin="D2" pad="1"/>
<connect gate="G$1" pin="D3/CS" pad="2"/>
<connect gate="G$1" pin="GND" pad="6 11 12"/>
<connect gate="G$1" pin="SENSE" pad="9 10"/>
<connect gate="G$1" pin="VCC" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="MOLEX" package="MX-502570-0893">
<connects>
<connect gate="G$1" pin="CK/SCK" pad="P5"/>
<connect gate="G$1" pin="CMD/MOSI" pad="P3"/>
<connect gate="G$1" pin="D0/MISO" pad="P7"/>
<connect gate="G$1" pin="D1" pad="P8"/>
<connect gate="G$1" pin="D2" pad="P1"/>
<connect gate="G$1" pin="D3/CS" pad="P2"/>
<connect gate="G$1" pin="GND" pad="P6 P9 P10 P11 P12 P14"/>
<connect gate="G$1" pin="SENSE" pad="P13"/>
<connect gate="G$1" pin="VCC" pad="P4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="CONN_02" uservalue="yes">
<description>1x2 connector</description>
<gates>
<gate name="G$1" symbol="CONN_02"/>
</gates>
<devices>
<device name="GOLDPIN" package="GP_02M">
<connects>
<connect gate="G$1" pin="P1" pad="1"/>
<connect gate="G$1" pin="P2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="JST-PH" package="JST-PH-B2">
<connects>
<connect gate="G$1" pin="P1" pad="P$1"/>
<connect gate="G$1" pin="P2" pad="P$2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="RAW" package="RAW_2">
<connects>
<connect gate="G$1" pin="P1" pad="P1"/>
<connect gate="G$1" pin="P2" pad="P2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="RAW_MINI" package="RAW_MINI_2">
<connects>
<connect gate="G$1" pin="P1" pad="P1"/>
<connect gate="G$1" pin="P2" pad="P2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="XT30PW-M" package="XT30PW-M">
<connects>
<connect gate="G$1" pin="P1" pad="V+"/>
<connect gate="G$1" pin="P2" pad="MNT1 MNT2 V-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="XT30PW-F" package="XT30PW-F">
<connects>
<connect gate="G$1" pin="P1" pad="V+"/>
<connect gate="G$1" pin="P2" pad="MNT1 MNT2 V-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="XT60PW-M" package="XT60PW-M">
<connects>
<connect gate="G$1" pin="P1" pad="V+"/>
<connect gate="G$1" pin="P2" pad="V-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="JST-ZH" package="JST-ZH-S2">
<connects>
<connect gate="G$1" pin="P1" pad="P1"/>
<connect gate="G$1" pin="P2" pad="P2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="JST-SR" package="JST-SR-S2">
<connects>
<connect gate="G$1" pin="P1" pad="P1"/>
<connect gate="G$1" pin="P2" pad="P2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="HIGH_AMP" package="HIGH_AMP">
<connects>
<connect gate="G$1" pin="P1" pad="P1"/>
<connect gate="G$1" pin="P2" pad="P2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="CONN_03">
<description>1x3 connector</description>
<gates>
<gate name="G$1" symbol="CONN_03"/>
</gates>
<devices>
<device name="GOLDPIN" package="GP_03M">
<connects>
<connect gate="G$1" pin="P1" pad="1"/>
<connect gate="G$1" pin="P2" pad="2"/>
<connect gate="G$1" pin="P3" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="RAW" package="RAW_3">
<connects>
<connect gate="G$1" pin="P1" pad="P1"/>
<connect gate="G$1" pin="P2" pad="P2"/>
<connect gate="G$1" pin="P3" pad="P3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="WS" package="JST-PH-B3">
<connects>
<connect gate="G$1" pin="P1" pad="P$1"/>
<connect gate="G$1" pin="P2" pad="P$2"/>
<connect gate="G$1" pin="P3" pad="P$3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="JST-SR" package="JST-SR-S3">
<connects>
<connect gate="G$1" pin="P1" pad="P1"/>
<connect gate="G$1" pin="P2" pad="P2"/>
<connect gate="G$1" pin="P3" pad="P3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="CONN_04">
<description>1x4 connector</description>
<gates>
<gate name="G$1" symbol="CONN_04"/>
</gates>
<devices>
<device name="GOLDPIN" package="GP_04M">
<connects>
<connect gate="G$1" pin="P1" pad="1"/>
<connect gate="G$1" pin="P2" pad="2"/>
<connect gate="G$1" pin="P3" pad="3"/>
<connect gate="G$1" pin="P4" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="RAW" package="RAW_4">
<connects>
<connect gate="G$1" pin="P1" pad="P1"/>
<connect gate="G$1" pin="P2" pad="P2"/>
<connect gate="G$1" pin="P3" pad="P3"/>
<connect gate="G$1" pin="P4" pad="P4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="WS" package="JST-PH-B4">
<connects>
<connect gate="G$1" pin="P1" pad="P$1"/>
<connect gate="G$1" pin="P2" pad="P$2"/>
<connect gate="G$1" pin="P3" pad="P$3"/>
<connect gate="G$1" pin="P4" pad="P$4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="JST-SR" package="JST-SR-S4">
<connects>
<connect gate="G$1" pin="P1" pad="P1"/>
<connect gate="G$1" pin="P2" pad="P2"/>
<connect gate="G$1" pin="P3" pad="P3"/>
<connect gate="G$1" pin="P4" pad="P4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="RPI_ZERO_CONN">
<description>Raspberry Pi Zero 2x40 connector</description>
<gates>
<gate name="G$1" symbol="RPI_ZERO"/>
</gates>
<devices>
<device name="" package="GP_40M">
<connects>
<connect gate="G$1" pin="3V3" pad="P1 P17"/>
<connect gate="G$1" pin="5V" pad="P2 P4"/>
<connect gate="G$1" pin="GND" pad="P6 P9 P14 P20 P25 P30 P34 P39"/>
<connect gate="G$1" pin="P0" pad="P11"/>
<connect gate="G$1" pin="P1" pad="P12"/>
<connect gate="G$1" pin="P10" pad="P24"/>
<connect gate="G$1" pin="P11" pad="P26"/>
<connect gate="G$1" pin="P12" pad="P19"/>
<connect gate="G$1" pin="P13" pad="P21"/>
<connect gate="G$1" pin="P14" pad="P23"/>
<connect gate="G$1" pin="P15" pad="P8"/>
<connect gate="G$1" pin="P16" pad="P10"/>
<connect gate="G$1" pin="P17" pad="P29"/>
<connect gate="G$1" pin="P18" pad="P31"/>
<connect gate="G$1" pin="P19" pad="P33"/>
<connect gate="G$1" pin="P2" pad="P13"/>
<connect gate="G$1" pin="P20" pad="P35"/>
<connect gate="G$1" pin="P21" pad="P37"/>
<connect gate="G$1" pin="P22" pad="P32"/>
<connect gate="G$1" pin="P23" pad="P36"/>
<connect gate="G$1" pin="P24" pad="P38"/>
<connect gate="G$1" pin="P25" pad="P40"/>
<connect gate="G$1" pin="P26" pad="P27"/>
<connect gate="G$1" pin="P27" pad="P28"/>
<connect gate="G$1" pin="P3" pad="P15"/>
<connect gate="G$1" pin="P4" pad="P16"/>
<connect gate="G$1" pin="P5" pad="P18"/>
<connect gate="G$1" pin="P6" pad="P22"/>
<connect gate="G$1" pin="P7" pad="P7"/>
<connect gate="G$1" pin="P8" pad="P3"/>
<connect gate="G$1" pin="P9" pad="P5"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="FPC_30">
<description>30 pins FPC connector</description>
<gates>
<gate name="G$1" symbol="CONN_30"/>
<gate name="G$2" symbol="CONN_02"/>
</gates>
<devices>
<device name="" package="FPC_30_05MM">
<connects>
<connect gate="G$1" pin="P1" pad="P1"/>
<connect gate="G$1" pin="P10" pad="P10"/>
<connect gate="G$1" pin="P11" pad="P11"/>
<connect gate="G$1" pin="P12" pad="P12"/>
<connect gate="G$1" pin="P13" pad="P13"/>
<connect gate="G$1" pin="P14" pad="P14"/>
<connect gate="G$1" pin="P15" pad="P15"/>
<connect gate="G$1" pin="P16" pad="P16"/>
<connect gate="G$1" pin="P17" pad="P17"/>
<connect gate="G$1" pin="P18" pad="P18"/>
<connect gate="G$1" pin="P19" pad="P19"/>
<connect gate="G$1" pin="P2" pad="P2"/>
<connect gate="G$1" pin="P20" pad="P20"/>
<connect gate="G$1" pin="P21" pad="P21"/>
<connect gate="G$1" pin="P22" pad="P22"/>
<connect gate="G$1" pin="P23" pad="P23"/>
<connect gate="G$1" pin="P24" pad="P24"/>
<connect gate="G$1" pin="P25" pad="P25"/>
<connect gate="G$1" pin="P26" pad="P26"/>
<connect gate="G$1" pin="P27" pad="P27"/>
<connect gate="G$1" pin="P28" pad="P28"/>
<connect gate="G$1" pin="P29" pad="P29"/>
<connect gate="G$1" pin="P3" pad="P3"/>
<connect gate="G$1" pin="P30" pad="P30"/>
<connect gate="G$1" pin="P4" pad="P4"/>
<connect gate="G$1" pin="P5" pad="P5"/>
<connect gate="G$1" pin="P6" pad="P6"/>
<connect gate="G$1" pin="P7" pad="P7"/>
<connect gate="G$1" pin="P8" pad="P8"/>
<connect gate="G$1" pin="P9" pad="P9"/>
<connect gate="G$2" pin="P1" pad="G1"/>
<connect gate="G$2" pin="P2" pad="G2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="USB_OTG">
<description>USB socket</description>
<gates>
<gate name="J$1" symbol="USB_OTG"/>
</gates>
<devices>
<device name="KEYS940" package="KEYS940">
<connects>
<connect gate="J$1" pin="D+" pad="P3"/>
<connect gate="J$1" pin="D-" pad="P2"/>
<connect gate="J$1" pin="GND" pad="P5 PAD1 PAD2"/>
<connect gate="J$1" pin="OTG" pad="P4"/>
<connect gate="J$1" pin="VCC" pad="P1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="KEYS940_F" package="KEYS940_F">
<connects>
<connect gate="J$1" pin="D+" pad="P3"/>
<connect gate="J$1" pin="D-" pad="P2"/>
<connect gate="J$1" pin="GND" pad="P5 PAD1 PAD2"/>
<connect gate="J$1" pin="OTG" pad="P4"/>
<connect gate="J$1" pin="VCC" pad="P1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="" package="MX-105017-0001">
<connects>
<connect gate="J$1" pin="D+" pad="P3"/>
<connect gate="J$1" pin="D-" pad="P2"/>
<connect gate="J$1" pin="GND" pad="P5 PAD1 PAD2 PAD3 PAD4 PAD5 PAD6"/>
<connect gate="J$1" pin="OTG" pad="P4"/>
<connect gate="J$1" pin="VCC" pad="P1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="USBA-LP-SMD" package="USBA-LP-SMD">
<connects>
<connect gate="J$1" pin="D+" pad="P3"/>
<connect gate="J$1" pin="D-" pad="P2"/>
<connect gate="J$1" pin="GND" pad="P4"/>
<connect gate="J$1" pin="OTG" pad="P5 P6"/>
<connect gate="J$1" pin="VCC" pad="P1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="SERVO_CONN" uservalue="yes">
<description>Servo connector&lt;p&gt;
1x3
&lt;/p&gt;</description>
<gates>
<gate name="G$1" symbol="CONN_SERVO"/>
</gates>
<devices>
<device name="" package="GP_03M">
<connects>
<connect gate="G$1" pin="GND" pad="3"/>
<connect gate="G$1" pin="SIG" pad="1"/>
<connect gate="G$1" pin="VCC" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="CONN_06_02">
<description>2x6 connector</description>
<gates>
<gate name="G$1" symbol="CONN_02_06"/>
</gates>
<devices>
<device name="" package="GP_02_06M">
<connects>
<connect gate="G$1" pin="P1" pad="P1"/>
<connect gate="G$1" pin="P10" pad="P10"/>
<connect gate="G$1" pin="P11" pad="P11"/>
<connect gate="G$1" pin="P12" pad="P12"/>
<connect gate="G$1" pin="P2" pad="P2"/>
<connect gate="G$1" pin="P3" pad="P3"/>
<connect gate="G$1" pin="P4" pad="P4"/>
<connect gate="G$1" pin="P5" pad="P5"/>
<connect gate="G$1" pin="P6" pad="P6"/>
<connect gate="G$1" pin="P7" pad="P7"/>
<connect gate="G$1" pin="P8" pad="P8"/>
<connect gate="G$1" pin="P9" pad="P9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="CONN_04_03">
<description>3x4 connector</description>
<gates>
<gate name="G$1" symbol="CONN_03_04"/>
</gates>
<devices>
<device name="" package="GP_03_04M">
<connects>
<connect gate="G$1" pin="P1" pad="P1"/>
<connect gate="G$1" pin="P10" pad="P10"/>
<connect gate="G$1" pin="P11" pad="P11"/>
<connect gate="G$1" pin="P12" pad="P12"/>
<connect gate="G$1" pin="P2" pad="P2"/>
<connect gate="G$1" pin="P3" pad="P3"/>
<connect gate="G$1" pin="P4" pad="P4"/>
<connect gate="G$1" pin="P5" pad="P5"/>
<connect gate="G$1" pin="P6" pad="P6"/>
<connect gate="G$1" pin="P7" pad="P7"/>
<connect gate="G$1" pin="P8" pad="P8"/>
<connect gate="G$1" pin="P9" pad="P9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="CONN_06">
<description>1x6 connector</description>
<gates>
<gate name="G$1" symbol="CONN_06"/>
</gates>
<devices>
<device name="RAW" package="RAW_6">
<connects>
<connect gate="G$1" pin="P1" pad="P1"/>
<connect gate="G$1" pin="P2" pad="P2"/>
<connect gate="G$1" pin="P3" pad="P3"/>
<connect gate="G$1" pin="P4" pad="P4"/>
<connect gate="G$1" pin="P5" pad="P5"/>
<connect gate="G$1" pin="P6" pad="P6"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="GOLDPIN" package="GP_06M">
<connects>
<connect gate="G$1" pin="P1" pad="1"/>
<connect gate="G$1" pin="P2" pad="2"/>
<connect gate="G$1" pin="P3" pad="3"/>
<connect gate="G$1" pin="P4" pad="4"/>
<connect gate="G$1" pin="P5" pad="5"/>
<connect gate="G$1" pin="P6" pad="6"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="JST-PH" package="WS-06S">
<connects>
<connect gate="G$1" pin="P1" pad="P$1"/>
<connect gate="G$1" pin="P2" pad="P$2"/>
<connect gate="G$1" pin="P3" pad="P$3"/>
<connect gate="G$1" pin="P4" pad="P$4"/>
<connect gate="G$1" pin="P5" pad="P$5"/>
<connect gate="G$1" pin="P6" pad="P$6"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="JST-ZH" package="JST-ZH-S6">
<connects>
<connect gate="G$1" pin="P1" pad="P1"/>
<connect gate="G$1" pin="P2" pad="P2"/>
<connect gate="G$1" pin="P3" pad="P3"/>
<connect gate="G$1" pin="P4" pad="P4"/>
<connect gate="G$1" pin="P5" pad="P5"/>
<connect gate="G$1" pin="P6" pad="P6"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="JST-SRS" package="JST-SR-S6">
<connects>
<connect gate="G$1" pin="P1" pad="P1"/>
<connect gate="G$1" pin="P2" pad="P2"/>
<connect gate="G$1" pin="P3" pad="P3"/>
<connect gate="G$1" pin="P4" pad="P4"/>
<connect gate="G$1" pin="P5" pad="P5"/>
<connect gate="G$1" pin="P6" pad="P6"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="FPC_06">
<description>6 pins FPC connector</description>
<gates>
<gate name="G$1" symbol="FPC_06"/>
</gates>
<devices>
<device name="" package="FPC_06_05MM">
<connects>
<connect gate="G$1" pin="P1" pad="P1"/>
<connect gate="G$1" pin="P2" pad="P2"/>
<connect gate="G$1" pin="P3" pad="P3"/>
<connect gate="G$1" pin="P4" pad="P4"/>
<connect gate="G$1" pin="P5" pad="P5"/>
<connect gate="G$1" pin="P6" pad="P6"/>
<connect gate="G$1" pin="PAD" pad="P7 P8"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="SIM_6">
<description>Sim card socket</description>
<gates>
<gate name="G$1" symbol="MICROSIM"/>
</gates>
<devices>
<device name="MICRO" package="MICROSIM">
<connects>
<connect gate="G$1" pin="CLK" pad="C3"/>
<connect gate="G$1" pin="CPP" pad="C6"/>
<connect gate="G$1" pin="GND" pad="C5"/>
<connect gate="G$1" pin="IO" pad="C7"/>
<connect gate="G$1" pin="PAD" pad="P1 P2"/>
<connect gate="G$1" pin="RST" pad="C2"/>
<connect gate="G$1" pin="VCC" pad="C1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="NANO" package="NANOSIM">
<connects>
<connect gate="G$1" pin="CLK" pad="S3"/>
<connect gate="G$1" pin="CPP" pad="S5"/>
<connect gate="G$1" pin="GND" pad="S4" route="any"/>
<connect gate="G$1" pin="IO" pad="S6"/>
<connect gate="G$1" pin="PAD" pad="G1 G2 G3 G4"/>
<connect gate="G$1" pin="RST" pad="S2"/>
<connect gate="G$1" pin="VCC" pad="S1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ANTENNA">
<description>Antenna connector</description>
<gates>
<gate name="G$1" symbol="ANTENN"/>
</gates>
<devices>
<device name="U.FL" package="U.FL_ADAM_TECH">
<connects>
<connect gate="G$1" pin="GROUND" pad="PAD1 PAD2"/>
<connect gate="G$1" pin="SIG" pad="SIG"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="SMA" package="SMA_THT_ADAM_TECH">
<connects>
<connect gate="G$1" pin="GROUND" pad="P1 P2 P3 P4"/>
<connect gate="G$1" pin="SIG" pad="SIG"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="CONN_05" uservalue="yes">
<description>1x5 connector</description>
<gates>
<gate name="J$1" symbol="CONN_05"/>
</gates>
<devices>
<device name="RAW" package="RAW_5">
<connects>
<connect gate="J$1" pin="P1" pad="P1"/>
<connect gate="J$1" pin="P2" pad="P2"/>
<connect gate="J$1" pin="P3" pad="P3"/>
<connect gate="J$1" pin="P4" pad="P4"/>
<connect gate="J$1" pin="P5" pad="P5"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="GOLDPIN" package="GP_05M">
<connects>
<connect gate="J$1" pin="P1" pad="1"/>
<connect gate="J$1" pin="P2" pad="2"/>
<connect gate="J$1" pin="P3" pad="3"/>
<connect gate="J$1" pin="P4" pad="4"/>
<connect gate="J$1" pin="P5" pad="5"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="JST-PH" package="JST-PH-B5">
<connects>
<connect gate="J$1" pin="P1" pad="P$1"/>
<connect gate="J$1" pin="P2" pad="P$2"/>
<connect gate="J$1" pin="P3" pad="P$3"/>
<connect gate="J$1" pin="P4" pad="P$4"/>
<connect gate="J$1" pin="P5" pad="P$5"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="RAW_MINI" package="RAW_MINI_5">
<connects>
<connect gate="J$1" pin="P1" pad="P1"/>
<connect gate="J$1" pin="P2" pad="P2"/>
<connect gate="J$1" pin="P3" pad="P3"/>
<connect gate="J$1" pin="P4" pad="P4"/>
<connect gate="J$1" pin="P5" pad="P5"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="JST-ZH" package="JST-ZH-S5">
<connects>
<connect gate="J$1" pin="P1" pad="P1"/>
<connect gate="J$1" pin="P2" pad="P2"/>
<connect gate="J$1" pin="P3" pad="P3"/>
<connect gate="J$1" pin="P4" pad="P4"/>
<connect gate="J$1" pin="P5" pad="P5"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="JST-SR" package="JST-SR-S5">
<connects>
<connect gate="J$1" pin="P1" pad="P1"/>
<connect gate="J$1" pin="P2" pad="P2"/>
<connect gate="J$1" pin="P3" pad="P3"/>
<connect gate="J$1" pin="P4" pad="P4"/>
<connect gate="J$1" pin="P5" pad="P5"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="FPC_05">
<description>5 pins FPC connector</description>
<gates>
<gate name="G$1" symbol="CONN_05_P"/>
</gates>
<devices>
<device name="" package="S5B-SM4A">
<connects>
<connect gate="G$1" pin="P1" pad="P1"/>
<connect gate="G$1" pin="P2" pad="P2"/>
<connect gate="G$1" pin="P3" pad="P3"/>
<connect gate="G$1" pin="P4" pad="P4"/>
<connect gate="G$1" pin="P5" pad="P5"/>
<connect gate="G$1" pin="PAD" pad="PAD1 PAD2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="CONN_01">
<description>1x1 connector</description>
<gates>
<gate name="G$1" symbol="CONN_01"/>
</gates>
<devices>
<device name="" package="GP_01M">
<connects>
<connect gate="G$1" pin="P1" pad="P$1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="VERY_HIGH_AMP" package="VERY_HIGH_AMP">
<connects>
<connect gate="G$1" pin="P1" pad="P1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="CONN_10">
<description>1x10 connector</description>
<gates>
<gate name="G$1" symbol="CONN_10"/>
</gates>
<devices>
<device name="" package="GP_10M">
<connects>
<connect gate="G$1" pin="P1" pad="1"/>
<connect gate="G$1" pin="P10" pad="10"/>
<connect gate="G$1" pin="P2" pad="2"/>
<connect gate="G$1" pin="P3" pad="3"/>
<connect gate="G$1" pin="P4" pad="4"/>
<connect gate="G$1" pin="P5" pad="5"/>
<connect gate="G$1" pin="P6" pad="6"/>
<connect gate="G$1" pin="P7" pad="7"/>
<connect gate="G$1" pin="P8" pad="8"/>
<connect gate="G$1" pin="P9" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="CONN_07">
<description>1x7 connector</description>
<gates>
<gate name="G$1" symbol="CONN_07"/>
</gates>
<devices>
<device name="GOLDPIN" package="GP_07M">
<connects>
<connect gate="G$1" pin="P1" pad="1"/>
<connect gate="G$1" pin="P2" pad="2"/>
<connect gate="G$1" pin="P3" pad="3"/>
<connect gate="G$1" pin="P4" pad="4"/>
<connect gate="G$1" pin="P5" pad="5"/>
<connect gate="G$1" pin="P6" pad="6"/>
<connect gate="G$1" pin="P7" pad="7"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="JST_ZH" package="JST-ZH-S7">
<connects>
<connect gate="G$1" pin="P1" pad="P1"/>
<connect gate="G$1" pin="P2" pad="P2"/>
<connect gate="G$1" pin="P3" pad="P3"/>
<connect gate="G$1" pin="P4" pad="P4"/>
<connect gate="G$1" pin="P5" pad="P5"/>
<connect gate="G$1" pin="P6" pad="P6"/>
<connect gate="G$1" pin="P7" pad="P7"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="JST-SRS" package="JST-SR-S7">
<connects>
<connect gate="G$1" pin="P1" pad="P1"/>
<connect gate="G$1" pin="P2" pad="P2"/>
<connect gate="G$1" pin="P3" pad="P3"/>
<connect gate="G$1" pin="P4" pad="P4"/>
<connect gate="G$1" pin="P5" pad="P5"/>
<connect gate="G$1" pin="P6" pad="P6"/>
<connect gate="G$1" pin="P7" pad="P7"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="RPI_BPLUS_CONN">
<description>Raspberry Pi B+ 2x40 connector</description>
<gates>
<gate name="G$1" symbol="RPI_BPLUS"/>
</gates>
<devices>
<device name="" package="GP_40M">
<connects>
<connect gate="G$1" pin="3V3" pad="P1 P17"/>
<connect gate="G$1" pin="5V" pad="P2 P4"/>
<connect gate="G$1" pin="GND" pad="P6 P9 P14 P20 P25 P30 P34 P39"/>
<connect gate="G$1" pin="GPIO10" pad="P19"/>
<connect gate="G$1" pin="GPIO11" pad="P23"/>
<connect gate="G$1" pin="GPIO12" pad="P32"/>
<connect gate="G$1" pin="GPIO13" pad="P33"/>
<connect gate="G$1" pin="GPIO14" pad="P8"/>
<connect gate="G$1" pin="GPIO15" pad="P10"/>
<connect gate="G$1" pin="GPIO16" pad="P36"/>
<connect gate="G$1" pin="GPIO17" pad="P11"/>
<connect gate="G$1" pin="GPIO18" pad="P12"/>
<connect gate="G$1" pin="GPIO19" pad="P35"/>
<connect gate="G$1" pin="GPIO2" pad="P3"/>
<connect gate="G$1" pin="GPIO20" pad="P38"/>
<connect gate="G$1" pin="GPIO21" pad="P40"/>
<connect gate="G$1" pin="GPIO22" pad="P15"/>
<connect gate="G$1" pin="GPIO23" pad="P16"/>
<connect gate="G$1" pin="GPIO24" pad="P18"/>
<connect gate="G$1" pin="GPIO25" pad="P22"/>
<connect gate="G$1" pin="GPIO26" pad="P37"/>
<connect gate="G$1" pin="GPIO27" pad="P13"/>
<connect gate="G$1" pin="GPIO3" pad="P5"/>
<connect gate="G$1" pin="GPIO4" pad="P7"/>
<connect gate="G$1" pin="GPIO5" pad="P29"/>
<connect gate="G$1" pin="GPIO6" pad="P31"/>
<connect gate="G$1" pin="GPIO7" pad="P26"/>
<connect gate="G$1" pin="GPIO8" pad="P24"/>
<connect gate="G$1" pin="GPIO9" pad="P21"/>
<connect gate="G$1" pin="ID_SC" pad="P28"/>
<connect gate="G$1" pin="ID_SD" pad="P27"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="RPI_4_CONN">
<gates>
<gate name="G$1" symbol="RPI_4B"/>
</gates>
<devices>
<device name="" package="GP_40M">
<connects>
<connect gate="G$1" pin="(ID_SC)GPIO1" pad="P28"/>
<connect gate="G$1" pin="(PCM_CLK)GPIO18" pad="P12"/>
<connect gate="G$1" pin="(PCM_DIN)GPIO20" pad="P38"/>
<connect gate="G$1" pin="(PCM_DOUT)GPIO21" pad="P40"/>
<connect gate="G$1" pin="(PCM_FS)GPIO19" pad="P35"/>
<connect gate="G$1" pin="3V3" pad="P1 P17"/>
<connect gate="G$1" pin="5V" pad="P2 P4"/>
<connect gate="G$1" pin="GND" pad="P6 P9 P14 P20 P25 P30 P34 P39"/>
<connect gate="G$1" pin="GPIO0(ID_SD)" pad="P27"/>
<connect gate="G$1" pin="GPIO10(MOSI)" pad="P19"/>
<connect gate="G$1" pin="GPIO11(SCLK)" pad="P23"/>
<connect gate="G$1" pin="GPIO12(PWM0)" pad="P32"/>
<connect gate="G$1" pin="GPIO13(PWM1)" pad="P33"/>
<connect gate="G$1" pin="GPIO14(TXD)" pad="P8"/>
<connect gate="G$1" pin="GPIO15(RXD)" pad="P10"/>
<connect gate="G$1" pin="GPIO16" pad="P36"/>
<connect gate="G$1" pin="GPIO17" pad="P11"/>
<connect gate="G$1" pin="GPIO2(SDA)" pad="P3"/>
<connect gate="G$1" pin="GPIO22" pad="P15"/>
<connect gate="G$1" pin="GPIO23" pad="P16"/>
<connect gate="G$1" pin="GPIO24" pad="P18"/>
<connect gate="G$1" pin="GPIO25" pad="P22"/>
<connect gate="G$1" pin="GPIO26" pad="P37"/>
<connect gate="G$1" pin="GPIO27" pad="P13"/>
<connect gate="G$1" pin="GPIO3(SCL)" pad="P5"/>
<connect gate="G$1" pin="GPIO4(GPCLK0)" pad="P7"/>
<connect gate="G$1" pin="GPIO5" pad="P29"/>
<connect gate="G$1" pin="GPIO6" pad="P31"/>
<connect gate="G$1" pin="GPIO7(CE1)" pad="P26"/>
<connect gate="G$1" pin="GPIO8(CE0)" pad="P24"/>
<connect gate="G$1" pin="GPIO9(MISO)" pad="P21"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="CONN_08">
<gates>
<gate name="G$1" symbol="CONN_08"/>
</gates>
<devices>
<device name="JST-ZHS" package="JST-ZH-S8">
<connects>
<connect gate="G$1" pin="P1" pad="P1"/>
<connect gate="G$1" pin="P2" pad="P2"/>
<connect gate="G$1" pin="P3" pad="P3"/>
<connect gate="G$1" pin="P4" pad="P4"/>
<connect gate="G$1" pin="P5" pad="P5"/>
<connect gate="G$1" pin="P6" pad="P6"/>
<connect gate="G$1" pin="P7" pad="P7"/>
<connect gate="G$1" pin="P8" pad="P8"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="JST-SRS" package="JST-SR-S8">
<connects>
<connect gate="G$1" pin="P1" pad="P1"/>
<connect gate="G$1" pin="P2" pad="P2"/>
<connect gate="G$1" pin="P3" pad="P3"/>
<connect gate="G$1" pin="P4" pad="P4"/>
<connect gate="G$1" pin="P5" pad="P5"/>
<connect gate="G$1" pin="P6" pad="P6"/>
<connect gate="G$1" pin="P7" pad="P7"/>
<connect gate="G$1" pin="P8" pad="P8"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
</devicesets>
</library>
</drawing>
</eagle>
