Index of Functions: A B C D E F G H I J K L M N O P Q R S T U V W X
Index Page ckgr03_c
Table of contents
Procedure Abstract Required_Reading Keywords Brief_I/O Detailed_Input | Detailed_Output Parameters Exceptions Files Particulars Examples | Restrictions Literature_References Author_and_Institution Version Index_Entries
#### Procedure
       ckgr03_c ( C-kernel, get record, type 03 )

       void ckgr03_c ( SpiceInt            handle,
                       ConstSpiceDouble    descr  [],
                       SpiceInt            recno,
                       SpiceDouble         record [] )
#### Abstract
       Return a specified pointing instance from a CK type 03 segment.
       The segment is identified by a CK file handle and segment
       descriptor.
#### Required_Reading
       CK
       DAF
#### Keywords
       POINTING
#### Brief_I/O
       VARIABLE  I/O  DESCRIPTION
       --------  ---  --------------------------------------------------
       handle     I   The handle of the CK file containing the segment.
       descr      I   The segment descriptor.
       recno      I   The number of the pointing instance to be returned.
       record     O   The pointing record.
#### Detailed_Input
       handle      is the handle of the binary CK file containing the
                   desired segment. The file should have been opened
                   for read or write access, by cklpf_c, dafopr_c or dafopw_c.

       descr       is the packed descriptor of the data type 3 CK segment.

       recno       is the number of the discrete pointing instance to be
                   returned from the data type 3 segment.
#### Detailed_Output
       record      is the pointing instance indexed by `recno' in the
                   segment. The contents are as follows:

                      record[ 0 ] = clkout

                      record[ 1 ] = q0
                      record[ 2 ] = q1
                      record[ 3 ] = q2
                      record[ 4 ] = q3

                      record[ 5 ] = av0  |
                      record[ 6 ] = av1  |-- Returned optionally
                      record[ 7 ] = av2  |

                   `clkout' is the encoded spacecraft clock time associated
                   with the returned pointing values.

                   The quantities q0 - q3 are the components of the
                   quaternion that represents the C-matrix that transforms
                   vectors from the inertial reference frame of the
                   segment to the instrument frame at time `clkout'.

                   The quantities `av0', `av1', and `av2' represent the
                   angular velocity vector, and are returned only if
                   the segment contains angular velocity data. The
                   components of the angular velocity vector are
                   specified relative to the inertial reference
                   frame of the segment.
#### Parameters
       None.
#### Exceptions
       1)  If the segment is not of data type 3, the error
           SPICE(CKWRONGDATATYPE) is signaled by a routine in the call tree of
           this routine.

       2)  If `recno' is less than one or greater than the number of records in
           the specified segment, the error SPICE(CKNONEXISTREC) is signaled by
           a routine in the call tree of this routine.

       3)  If the specified handle does not belong to any DAF file that
           is currently known to be open, an error is signaled by a
           routine in the call tree of this routine.

       4)  If `descr' is not a valid descriptor of a segment in the CK
           file specified by `handle', the results of this routine are
           unpredictable.
#### Files
       The CK file specified by `handle' should be open for read or
       write access.
#### Particulars
       For a detailed description of the structure of a type 3 segment,
       see the CK required reading.

       This is a utility routine that may be used to read the individual
       pointing instances that make up a type 3 segment. It is normally
       used in conjunction with cknr03_c, which gives the number of
       pointing instances stored in a segment.
#### Examples
       The numerical results shown for this example may differ across
       platforms. The results depend on the SPICE kernels used as
       input, the compiler and supporting libraries, and the machine
       specific arithmetic implementation.

       1) The following code example extracts the SCLK time, boresight
          vector, and angular velocity vector for each pointing instance
          in the first segment in a CK file that contains segments of
          data type 3.

          Use the CK kernel below, available in the Venus Express PDS
          archives, as input for the code example.

             VEX_BOOM_V01.BC

          Example code begins here.

          /.
             Program ckgr03_ex1
          ./
          #include <stdio.h>
          #include "SpiceUsr.h"

          int main( )
          {

             /.
             Local variables.
             ./
             SpiceDouble          quat   [4];
             SpiceDouble          av     [3];
             SpiceDouble          bore   [3];
             SpiceDouble          cmat   [3][3];
             SpiceDouble          dcd    [2];
             SpiceDouble          descr  [5];
             SpiceDouble          record [8];
             SpiceDouble          sclkdp;

             SpiceInt             i;
             SpiceInt             icd    [6];
             SpiceInt             handle;
             SpiceInt             nrec;

             SpiceBoolean         avseg;
             SpiceBoolean         found;

             /.
             First load the file (it may also be opened by using
             cklpf_c).
             ./
             dafopr_c ( "VEX_BOOM_V01.BC", &handle );

             /.
             Begin forward search.  Find the first array.
             ./
             dafbfs_c ( handle );
             daffna_c ( &found );

             /.
             Get segment descriptor.
             ./
             dafgs_c ( descr );

             /.
             Unpack the segment descriptor into its double precision
             and integer components.
             ./
             dafus_c ( descr, 2, 6, dcd, icd );

             /.
             The data type for a segment is located in the third
             integer component of the descriptor.
             ./
             if ( icd[2] == 3 )
             {

                /.
                Does the segment contain `av' data?
                ./
                avseg =  ( icd[3] == 1 );

                /.
                How many records does this segment contain?
                ./
                cknr03_c ( handle, descr, &nrec );

                for ( i = 1; i <= nrec; i++ )
                {

                   /.
                   Get the ith pointing instance in the segment.
                   ./
                   ckgr03_c ( handle, descr, i, record );

                   /.
                   Unpack `record' into the time, quaternion, and av.
                   ./
                   sclkdp = record[0];

                   moved_c ( record+1, 4, quat );

                   if ( avseg )
                   {
                      moved_c ( record+5, 3, av );
                   }

                   /.
                   The boresight vector is the third row of the
                   C-matrix.
                   ./
                   q2m_c ( quat, cmat );

                   bore[0] = cmat[2][0];
                   bore[1] = cmat[2][1];
                   bore[2] = cmat[2][2];

                   /.
                   Write out the results.
                   ./
                   printf( "Record: %2d\n", (int)i );
                   printf( "   SCLK time       : %24.6f\n", sclkdp );
                   printf( "   Boresight       : %13.9f %13.9f %13.9f\n",
                                                bore[0], bore[1], bore[2] );

                   if ( avseg )
                   {
                      printf( "   Angular velocity: %13.9f %13.9f %13.9f\n",
                                                         av[0], av[1], av[2] );
                   }
                   printf( "\n" );
                }
             }

             return ( 0 );
          }

          When this program was executed on a Mac/Intel/cc/64-bit
          platform, the output was:

          Record:  1
             SCLK time       :           2162686.710986
             Boresight       :  -0.999122830   0.000000000   0.041875654
             Angular velocity:   0.000000000   0.000000000   0.000000000

          Record:  2
             SCLK time       :       54160369751.715164
             Boresight       :  -0.999122830   0.000000000   0.041875654
             Angular velocity:   0.000000000   1.176083393   0.000000000

          Record:  3
             SCLK time       :       54160454948.487686
             Boresight       :   0.000000000   0.000000000   1.000000000
             Angular velocity:   0.000000000   0.000000000   0.000000000

          Record:  4
             SCLK time       :      299264885854.937805
             Boresight       :   0.000000000   0.000000000   1.000000000
             Angular velocity:   0.000000000   0.000000000   0.000000000

          Record:  5
             SCLK time       :     2366007685832.532227
             Boresight       :   0.000000000   0.000000000   1.000000000
             Angular velocity:   0.000000000   0.000000000   0.000000000

          Record:  6
             SCLK time       :     4432750485810.126953
             Boresight       :   0.000000000   0.000000000   1.000000000
             Angular velocity:   0.000000000   0.000000000   0.000000000

          Record:  7
             SCLK time       :     6505155594828.757812
             Boresight       :   0.000000000   0.000000000   1.000000000
             Angular velocity:   0.000000000   0.000000000   0.000000000

          Record:  8
             SCLK time       :     8571898394806.352539
             Boresight       :   0.000000000   0.000000000   1.000000000
             Angular velocity:   0.000000000   0.000000000   0.000000000

          Record:  9
             SCLK time       :    10638641194783.947266
             Boresight       :   0.000000000   0.000000000   1.000000000
             Angular velocity:   0.000000000   0.000000000   0.000000000

          Record: 10
             SCLK time       :    12705383994761.541016
             Boresight       :   0.000000000   0.000000000   1.000000000
             Angular velocity:   0.000000000   0.000000000   0.000000000

          Record: 11
             SCLK time       :    14777789103780.169922
             Boresight       :   0.000000000   0.000000000   1.000000000
             Angular velocity:   0.000000000   0.000000000   0.000000000

          Record: 12
             SCLK time       :    16844531903757.763672
             Boresight       :   0.000000000   0.000000000   1.000000000
             Angular velocity:   0.000000000   0.000000000   0.000000000

          Record: 13
             SCLK time       :    18911274703735.359375
             Boresight       :   0.000000000   0.000000000   1.000000000
             Angular velocity:   0.000000000   0.000000000   0.000000000
#### Restrictions
       1)  The binary CK file containing the segment whose descriptor was
           passed to this routine must be opened for read or write access
           by cklpf_c, dafopr_c or dafopw_c.
#### Literature_References
       None.
#### Author_and_Institution
       J. Diaz del Rio     (ODC Space)
#### Version
       -CSPICE Version 1.0.0, 01-NOV-2021 (JDR)
#### Index_Entries
       get CK type_3 record
#### Link to routine ckgr03_c source file ckgr03_c.c

    Fri Dec 31 18:41:02 2021