Index of Functions: A B C D E F G H I J K L M N O P Q R S T U V W X
Index Page ckfrot_c
Table of contents
Procedure Abstract Required_Reading Keywords Brief_I/O Detailed_Input | Detailed_Output Parameters Exceptions Files Particulars Examples | Restrictions Literature_References Author_and_Institution Version Index_Entries
#### Procedure
       ckfrot_c ( CK frame, find position rotation )

       void ckfrot_c ( SpiceInt            inst,
                       SpiceDouble         et,
                       SpiceDouble         rotate [3][3],
                       SpiceInt          * ref,
                       SpiceBoolean      * found         )
#### Abstract
       Find the position rotation matrix from a C-kernel (CK) frame with
       the specified frame class ID (CK ID) to the base frame of the
       highest priority CK segment containing orientation data for this
       CK frame at the time requested.
#### Required_Reading
       CK
#### Keywords
       POINTING
#### Brief_I/O
       VARIABLE  I/O  DESCRIPTION
       --------  ---  --------------------------------------------------
       inst       I   Frame class ID (CK ID) of a CK frame.
       et         I   Epoch measured in seconds past J2000 TDB.
       rotate     O   Rotation matrix from CK frame to frame `ref'.
       ref        O   Frame ID of the base reference.
       found      O   SPICETRUE when requested pointing is available.
#### Detailed_Input
       inst        is the unique frame class ID (CK ID) of the CK frame for
                   which data is being requested.

       et          is the epoch for which the position rotation is desired.
                   `et' should be given in seconds past the epoch of J2000
                   TDB.
#### Detailed_Output
       rotate      is a position rotation matrix that converts positions
                   relative to the CK frame given by its frame class ID,
                   `inst', to positions relative to the base frame given by
                   its frame ID, `ref'.

                   Thus, if a position S has components x,y,z in the CK
                   frame, then S has components x', y', z' in the base
                   frame.

                      .-  -.     .-        -. .- -.
                      | x' |     |          | | x |
                      | y' |  =  |  rotate  | | y |
                      | z' |     |          | | z |
                      `-  -'     `-        -' `- -'

       ref         is the ID code of the base reference frame to which
                   `rotate' will transform positions.

       found       is SPICETRUE if a record was found to satisfy the pointing
                   request. `found' will be SPICEFALSE otherwise.
#### Parameters
       None.
#### Exceptions
       1)  If no CK files were loaded prior to calling this routine, an
           error is signaled by a routine in the call tree of this
           routine.

       2)  If no SCLK correlation data needed to read CK files were
           loaded prior to calling this routine, an error is signaled by
           a routine in the call tree of this routine.

       3)  If the input time `et' cannot be converted to an encoded SCLK
           time, using SCLK data associated with `inst', an error is
           signaled by a routine in the call tree of this routine.
#### Files
       ckfrot_c searches through loaded CK files to locate a segment that
       can satisfy the request for position rotation data for the CK
       frame with the specified frame class ID at time `et'. You must load
       a CK file containing such data before calling this routine. You
       must also load SCLK and possibly LSK files needed to convert the
       input `et' time to the encoded SCLK time with which the orientation
       data stored inside that CK is tagged.
#### Particulars
       ckfrot_c searches through loaded CK files to satisfy a pointing
       request. Last-loaded files are searched first, and individual
       files are searched in backwards order, giving priority to
       segments that were added to a file later than the others.

       The search ends when a segment is found that can give pointing
       for the specified CK frame at the request time.

       Segments with and without angular velocities are considered by
       this routine.

       This routine uses the ckmeta_c routine to determine the SCLK ID
       used to convert the input `et' time to the encoded SCLK time used
       to look up pointing data in loaded CK files.
#### Examples
       The numerical results shown for this example may differ across
       platforms. The results depend on the SPICE kernels used as
       input, the compiler and supporting libraries, and the machine
       specific arithmetic implementation.

       1) Use ckfrot_c to compute the instantaneous angular velocity
          vector for the Mars Global Surveyor (MGS) spacecraft frame,
          "MGS_SPACECRAFT", relative to the inertial frame used as the
          base frame in CK files containing MGS spacecraft orientation
          at 2003-JUL-25 13:00:00. The frame class ID (CK ID) for the
          "MGS_SPACECRAFT" frame is -94000.

          Suppose that r(t) is the rotation matrix whose columns
          represent the inertial pointing vectors of the MGS spacecraft
          axes at time `t'.

          Then the angular velocity vector points along the vector given
          by:

                                  T
              limit  axis( r(t+h)r )
              h-->0

          And the magnitude of the angular velocity at time `t' is given
          by:

                                  T
              d angle ( r(t+h)r(t) )
             ------------------------   at   h = 0
                        dh

          Use the meta-kernel shown below to load the required SPICE
          kernels.

             KPL/MK

             File name: ckfrot_ex1.tm

             This meta-kernel is intended to support operation of SPICE
             example programs. The kernels shown here should not be
             assumed to contain adequate or correct versions of data
             required by SPICE-based user applications.

             In order for an application to use this meta-kernel, the
             kernels referenced here must be present in the user's
             current working directory.

             The names and contents of the kernels referenced
             by this meta-kernel are as follows:

                File name                     Contents
                ---------                     --------
                naif0012.tls                  Leapseconds
                mgs_sclkscet_00061.tsc        MGS SCLK coefficients
                mgs_sc_ext12.bc               MGS s/c bus attitude

             \begindata

             KERNELS_TO_LOAD = ( 'naif0012.tls',
                                 'mgs_sclkscet_00061.tsc',
                                 'mgs_sc_ext12.bc' )

             \begintext

             End of meta-kernel

          Example code begins here.

          /.
             Program ckfrot_ex1
          ./
          #include <stdio.h>
          #include "SpiceUsr.h"

          int main( )
          {

             /.
             Local parameters.
             ./
             #define EPOCH        "2003-JUL-25 13:00:00"
             #define INST         -94000

             /.
             Local variables.
             ./
             SpiceDouble          angle;
             SpiceDouble          angvel [3];
             SpiceDouble          axis   [3];
             SpiceDouble          et;
             SpiceDouble          infrot [3][3];
             SpiceDouble          h;
             SpiceDouble          ret    [3][3];
             SpiceDouble          reth   [3][3];

             SpiceInt             ref;
             SpiceInt             refh;

             SpiceBoolean         found;
             SpiceBoolean         foundh;

             /.
             Load the required LSK, SCLK and CK. Use a
             meta-kernel for convenience.
             ./
             furnsh_c ( "ckfrot_ex1.tm" );

             /.
             First convert the time to seconds past J2000. Set the
             delta time (1 ms).
             ./
             str2et_c ( EPOCH, &et );
             h = 1.e-3;

             /.
             Now, look up the rotation from the MGS spacecraft
             frame specified by its frame class ID (CK ID) to a
             base reference frame (returned by ckfrot_c), at `et'
             and et+h.
             ./
             ckfrot_c ( INST, et, ret, &ref, &found );
             ckfrot_c ( INST, et+h, reth, &refh, &foundh );

             /.
             If both rotations were computed and if the base
             reference frames are the same, compute the
             instantaneous angular velocity vector.
             ./
             if ( found && foundh && ref == refh )
             {

                /.
                Compute the infinitesimal rotation r(t+h)r(t)^T.
                ./
                mxmt_c ( reth, ret, infrot );

                /.
                Compute the `axis' and `angle' of the infinitesimal
                rotation.
                ./
                raxisa_c ( infrot, axis, &angle );

                /.
                Scale `axis' to get the angular velocity vector.
                ./
                vscl_c ( angle/h, axis, angvel );

                /.
                Output the results.
                ./
                printf( "Instantaneous angular velocity vector:\n" );
                printf( "%15.10f %14.10f %14.10f\n",
                        angvel[0], angvel[1], angvel[2] );
                printf( "Reference frame ID: %4d\n", (int)ref );
             }
             else
             {
                printf( "ERROR: data not found or frame mismatch.\n" );
             }

             return ( 0 );
          }

          When this program was executed on a Mac/Intel/cc/64-bit
          platform, the output was:

          Instantaneous angular velocity vector:
             0.0001244121   0.0008314866   0.0003028634
          Reference frame ID:    1
#### Restrictions
       1)  A CK file must be loaded prior to calling this routine.

       2)  LSK and SCLK files needed for time conversions must be loaded
           prior to calling this routine.
#### Literature_References
       None.
#### Author_and_Institution
       J. Diaz del Rio     (ODC Space)
#### Version
       -CSPICE Version 1.0.0, 13-DEC-2021 (JDR)
#### Index_Entries
       get instrument frame rotation and reference frame
#### Link to routine ckfrot_c source file ckfrot_c.c

    Fri Dec 31 18:41:02 2021