Index of Functions: A B C D E F G H I J K L M N O P Q R S T U V W X
Index Page dskb02_c
Table of contents
Procedure Abstract Required_Reading Keywords Brief_I/O Detailed_Input | Detailed_Output Parameters Exceptions Files Particulars Examples | Restrictions Literature_References Author_and_Institution Version Index_Entries
#### Procedure
       dskb02_c ( DSK, fetch type 2 bookkeeping data )

       void dskb02_c ( SpiceInt               handle,
                       ConstSpiceDLADescr   * dladsc,
                       SpiceInt             * nv,
                       SpiceInt             * np,
                       SpiceInt             * nvxtot,
                       SpiceDouble            vtxbds  [3][2],
                       SpiceDouble          * voxsiz,
                       SpiceDouble            voxori  [3],
                       SpiceInt               vgrext  [3],
                       SpiceInt             * cgscal,
                       SpiceInt             * vtxnpl,
                       SpiceInt             * voxnpt,
                       SpiceInt             * voxnpl          )
#### Abstract
       Return bookkeeping data from a DSK type 2 segment.
#### Required_Reading
       DAS
       DSK
#### Keywords
       DAS
       DSK
       FILES
#### Brief_I/O
       VARIABLE  I/O  DESCRIPTION
       --------  ---  --------------------------------------------------
       handle     I   DSK file handle.
       dladsc     I   DLA descriptor.
       nv         O   Number of vertices in model.
       np         O   Number of plates in model.
       nvxtot     O   Number of voxels in fine grid.
       vtxbds     O   Vertex bounds.
       voxsiz     O   Fine voxel edge length.
       voxori     O   Fine voxel grid origin.
       vgrext     O   Fine voxel grid extent.
       cgscal     O   Coarse voxel grid scale.
       vtxnpl     O   Size of vertex-plate correspondence list.
       voxnpt     O   Size of voxel-plate pointer list.
       voxnpl     O   Size of voxel-plate correspondence list.
#### Detailed_Input
       handle      is the handle of a DSK file containing a type 2
                   segment from which data are to be fetched.

       dladsc      is the DLA descriptor associated with the segment
                   from which data are to be fetched.
#### Detailed_Output
       nv          is the number of vertices in model.

       np          is the number of plates in model.

       nvxtot      is the total number of voxels in fine grid.

       vtxbds      are the vertex bounds. This is an array of six values giving
                   the minimum and maximum values of each component of
                   the vertex set. `vtxbds' has dimensions [3][2].
                   Units are km.

       voxsiz      is the fine grid voxel size. DSK voxels are cubes; the
                   edge length of each cube is given by the voxel size.
                   This size applies to the fine voxel grid. Units are km.

       voxori      is the voxel grid origin. This is the location of the
                   voxel grid origin in the body-fixed frame associated
                   with the target body. Units are km.

       vgrext      is the voxel grid extent. This extent is an array of
                   three integers indicating the number of voxels in the
                   X, Y, and Z directions in the fine voxel grid.

       cgscal      is the coarse voxel grid scale. The extent of the fine
                   voxel grid is related to the extent of the coarse voxel
                   grid by this scale factor.

       vtxnpl      is the vertex-plate correspondence list size.

       voxnpt      is the size of the voxel-to-plate pointer list.

       voxnpl      is the voxel-plate correspondence list size.
#### Parameters
       See the header file

          SpiceDLA.h

       for declarations of DLA descriptor sizes and documentation of the
       contents of DLA descriptors.

       See the header file

          SpiceDSK.h

       for declarations of DSK descriptor sizes and documentation of the
       contents of DSK descriptors.

       See the header file

          SpiceDSK.h

       for declarations of DSK data type 2 (plate model) parameters.
#### Exceptions
       1)  If the input handle is invalid, an error is signaled by a
           routine in the call tree of this routine.

       2)  If a file read error occurs, the error is signaled by a
           routine in the call tree of this routine.

       3)  If the input DLA descriptor is invalid, the effect of this
           routine is undefined. The error *may* be diagnosed by
           routines in the call tree of this routine, but there are no
           guarantees.
#### Files
       See input argument `handle'.
#### Particulars
       This routine supports computations involving bookkeeping information
       stored in DSK type 2 segments. User applications typically will not
       need to call this routine.

       DSK files are built using the DLA low-level format and the DAS
       architecture; DLA files are a specialized type of DAS file in which
       data are organized as a doubly linked list of segments. Each
       segment's data belong to contiguous components of character, double
       precision, and integer type.
#### Examples
       The numerical results shown for this example may differ across
       platforms. The results depend on the SPICE kernels used as
       input, the compiler and supporting libraries, and the machine
       specific arithmetic implementation.

       1) Dump several parameters from the first DLA segment of
          a DSK file. The segment is assumed to be of type 2.

          Example code begins here.

          /.
             Program dskb02_ex1
          ./
          #include <stdio.h>
          #include "SpiceUsr.h"

          int main()
          {
             /.
             Constants
             ./
             #define FILSIZ          256

             /.
             Local variables
             ./
             SpiceBoolean            found;

             SpiceChar               dsk  [ FILSIZ ];

             SpiceDLADescr           dladsc;

             SpiceDouble             voxori [3];
             SpiceDouble             voxsiz;
             SpiceDouble             vtxbds [3][2];

             SpiceInt                cgscal;
             SpiceInt                handle;
             SpiceInt                np;
             SpiceInt                nv;
             SpiceInt                nvxtot;
             SpiceInt                vgrext [3];
             SpiceInt                voxnpl;
             SpiceInt                voxnpt;
             SpiceInt                vtxnpl;

             /.
             Prompt for the name of DSK to read.
             ./
             prompt_c ( "Enter DSK name > ", FILSIZ, dsk );

             /.
             Open the DSK file for read access. We use the
             DAS-level interface for this function.
             ./
             dasopr_c ( dsk, &handle );

             /.
             Begin a forward search through the kernel. In
             this example, it's a very short search.
             ./
             dlabfs_c ( handle, &dladsc, &found );

             if ( !found )
             {
                setmsg_c ( "No segment found in file #." );
                errch_c  ( "#",  dsk                     );
                sigerr_c ( "SPICE(NOSEGMENT)"            );
             }

             /.
             If we made it this far, DLADSC is the
             DLA descriptor of the first segment.
             Read and display type 2 bookkeeping data.
             ./
             dskb02_c ( handle,  &dladsc, &nv,    &np,    &nvxtot,
                        vtxbds,  &voxsiz, voxori, vgrext, &cgscal,
                        &vtxnpl, &voxnpt, &voxnpl                 );

             printf ( "\n"
                      "Number of vertices:                 %d\n"
                      "Number of plates:                   %d\n"
                      "Number of voxels:                   %d\n",
                      (int)nv,
                      (int)np,
                      (int)nvxtot                                       );

             printf ( "Vertex bounds in X direction (km):  %f : %f\n"
                      "Vertex bounds in Y direction (km):  %f : %f\n"
                      "Vertex bounds in Z direction (km):  %f : %f\n",
                      vtxbds[0][0], vtxbds[0][1],
                      vtxbds[1][0], vtxbds[1][1],
                      vtxbds[2][0], vtxbds[2][1]                        );

             printf ( "Voxel edge length (km):             %f\n"
                      "Voxel grid origin (km):           ( %f %f %f )\n"
                      "Voxel grid extents:                 %d %d %d\n"
                      "Coarse voxel grid scale:            %d\n"
                      "Size of vertex-plate list:          %d\n"
                      "Size of voxel-plate pointer array:  %d\n"
                      "Size of voxel-plate list:           %d\n",
                      voxsiz,
                      voxori[0], voxori[1], voxori[2],
                      (int)vgrext[0], (int)vgrext[1], (int)vgrext[2],
                      (int)cgscal,
                      (int)vtxnpl,
                      (int)voxnpt,
                      (int)voxnpl                                       );

             /.
             Close the kernel. This isn't necessary in a stand-
             alone program, but it's good practice in subroutines
             because it frees program and system resources.
             ./
             dascls_c ( handle );

             return ( 0 );
          }

          When this program was executed on a Mac/Intel/cc/64-bit
          platform, using the DSK file named phobos512.bds,
          the output was:

          Enter DSK name > phobos512.bds

          Number of vertices:                 1579014
          Number of plates:                   3145728
          Number of voxels:                   11914500
          Vertex bounds in X direction (km):  -13.440030 : 12.762800
          Vertex bounds in Y direction (km):  -11.520650 : 12.061140
          Vertex bounds in Z direction (km):  -9.570780 : 10.055000
          Voxel edge length (km):             0.104248
          Voxel grid origin (km):           ( -14.073520 -11.988554 -9.903588 )
          Voxel grid extents:                 260 235 195
          Coarse voxel grid scale:            5
          Size of vertex-plate list:          11010050
          Size of voxel-plate pointer array:  1151500
          Size of voxel-plate list:           6419540
#### Restrictions
       1)  The caller must verify that the segment associated with
           the input DLA descriptor is a DSK type 2 segment.
#### Literature_References
       None.
#### Author_and_Institution
       N.J. Bachman        (JPL)
       J. Diaz del Rio     (ODC Space)
#### Version
       -CSPICE Version 2.1.1, 08-FEB-2021 (JDR)

           Edited the header to comply with NAIF standard. Removed unnecessary
           include statements from example code.

           Updated example code to split printf statement in three in order to
           comply with ANSI-C maximum string literal of length.

       -CSPICE Version 2.1.0, 11-JUL-2016 (NJB)

           Edit to example program to use "%d" with explicit casts
           to int for printing SpiceInts with printf.

           Removed unnecessary include statements. Updated
           header.

           Based on:

           DSKLIB_C Version 2.0.1, 11-JUL-2014 (NJB)

              Added example program to header.

           DSKLIB_C Version 2.0.0, 13-MAY-2010 (NJB)

              Updated for compatibility with new DSK type 2 design.
              Name has been changed from dskp02_c to dskb02_c.

           DSKLIB_C Version 1.0.0, 11-FEB-2010 (NJB)
#### Index_Entries
       fetch parameters from a type 2 DSK segment
#### Link to routine dskb02_c source file dskb02_c.c

    Fri Dec 31 18:41:04 2021