Index of Functions: A B C D E F G H I J K L M N O P Q R S T U V W X
Index Page gfclrh_c
Table of contents
Procedure Abstract Required_Reading Keywords Brief_I/O Detailed_Input | Detailed_Output Parameters Exceptions Files Particulars Examples | Restrictions Literature_References Author_and_Institution Version Index_Entries
#### Procedure
       gfclrh_c ( GF, clear interrupt signal handler status )

       void gfclrh_c ( void )
#### Abstract
       Clear the interrupt signal handler status, so that future calls
       to gfbail_c will indicate no interrupt was received.
#### Required_Reading
       GF
#### Keywords
       GEOMETRY
       SEARCH
       UTILITY
#### Brief_I/O
       None. This routine operates by side effects; see -Particulars
       below.
#### Detailed_Input
       None.
#### Detailed_Output
       None.
#### Parameters
       None.
#### Exceptions
       Error free.
#### Files
       None.
#### Particulars
       This routine clears the interrupt signal handler status maintained
       by the GF subsystem. Calling this routine causes the GF interrupt
       signal receipt indicator function gfbail_c to return SPICEFALSE
       until the next interrupt signal is received by a signal handler
       established by the GF system.

       User applications that use default GF interrupt handling should call
       this routine after processing an interrupt signal.
#### Examples
       1) The code fragment below is from an example program in
          the header of gfocce_c. The code includes a search,
          a call to gfbail_c, which is made to determine whether
          an interrupt signal was received, and a call to
          gfclrh_c to clear the interrupt signal status.

                ...

                /.
                Turn on interrupt handling and progress reporting.
                ./
                bail = SPICETRUE;
                rpt  = SPICETRUE;

                /.
                Perform the search.
                ./
                gfocce_c ( "ANY",
                           "MOON",     "ellipsoid",  "IAU_MOON",
                           "SUN",      "ellipsoid",  "IAU_SUN",
                           "LT",       "EARTH",      CNVTOL,
                           gfstep_c,   gfrefn_c,     rpt,
                           gfrepi_c,   gfrepu_c,     gfrepf_c,
                           bail,       gfbail_c,     &cnfine,
                           &result                              );

                if ( gfbail_c() )
                {
                   /.
                   Clear the CSPICE interrupt indication. This is
                   an essential step for programs that continue
                   running after an interrupt; gfbail_c will
                   continue to return SPICETRUE until this step
                   has been performed.
                   ./
                   gfclrh_c();

                   /.
                   We've trapped an interrupt signal. In a realistic
                   application, the program would continue operation
                   from this point. In this simple example, we simply
                   display a message and quit.
                   ./
                   printf ( "\nSearch was interrupted.\n\nThis message "
                            "was written after an interrupt signal\n"
                            "was trapped. By default, the program "
                            "would have terminated \nbefore this message "
                            "could be written.\n\n"                       );
                }
                else

                ...
#### Restrictions
       1)  This routine has no visible effect on operation of user applications
           unless GF interrupt handling is enabled and gfbail_c is used as
           the interrupt signal receipt indicator.
#### Literature_References
       None.
#### Author_and_Institution
       N.J. Bachman        (JPL)
       J. Diaz del Rio     (ODC Space)
       L.S. Elson          (JPL)
#### Version
       -CSPICE Version 1.0.1, 05-AUG-2021 (JDR)

           Edited the header to comply with NAIF standard.

       -CSPICE Version 1.0.0, 05-FEB-2009 (NJB) (LSE)
#### Index_Entries
       GF clear interrupt signal status
#### Link to routine gfclrh_c source file gfclrh_c.c

    Fri Dec 31 18:41:07 2021