Index of Functions: A B C D E F G H I J K L M N O P Q R S T U V W X
Index Page getfvn_c
Table of contents
Procedure Abstract Required_Reading Keywords Brief_I/O Detailed_Input | Detailed_Output Parameters Exceptions Files Particulars Examples | Restrictions Literature_References Author_and_Institution Version Index_Entries
#### Procedure
       getfvn_c (Get instrument FOV parameters, by instrument name)

       void getfvn_c ( ConstSpiceChar    * inst,
                       SpiceInt            room,
                       SpiceInt            shalen,
                       SpiceInt            fralen,
                       SpiceChar         * shape,
                       SpiceChar         * frame,
                       SpiceDouble         bsight [3],
                       SpiceInt          * n,
                       SpiceDouble         bounds [][3] )
#### Abstract
       Return the field-of-view (FOV) parameters for a specified
       instrument. The instrument is specified by name.
#### Required_Reading
       NAIF_IDS
#### Keywords
       FOV
       INSTRUMENT
#### Brief_I/O
       VARIABLE  I/O  DESCRIPTION
       --------  ---  --------------------------------------------------
       inst       I   Name of an instrument.
       room       I   Maximum number of vectors that can be returned.
       shalen     I   Maximum length of output string `shape'.
       fralen     I   Maximum length of output string `frame'.
       shape      O   Instrument FOV shape.
       frame      O   Name of the frame in which FOV vectors are defined.
       bsight     O   Boresight vector.
       n          O   Number of boundary vectors returned.
       bounds     O   FOV boundary vectors.
#### Detailed_Input
       inst        is the name of an instrument, such as a
                   spacecraft-mounted framing camera, for which the field of
                   view parameters are to be retrieved from the kernel pool.
                   `inst' is case-insensitive, and leading and trailing blanks
                   in `inst' are not significant. Optionally, you may supply
                   the integer ID for the instrument as an integer string.
                   For example, both "CASSINI_ISS_NAC" and "-82360" are
                   legitimate strings that indicate the CASSINI ISS NAC
                   camera is the instrument of interest.

       room        is the maximum number of 3-dimensional vectors that can
                   be returned in `bounds'.

       shalen      is the maximum allowed length of the output string
                   `shape'. This length must be large enough to hold the
                   output string plus the null-terminator character. If the
                   output string is expected to have X characters, `shalen'
                   should be at least X+1.

       fralen      is the maximum allowed length of the output string
                   `frame'. This length must be large enough to hold the
                   output string plus the null-terminator character. If the
                   output string is expected to have X characters, `fralen'
                   should be at least X+1.
#### Detailed_Output
       shape       is a character string that describes the "shape" of
                   the field of view. Possible values returned are:

                      "POLYGON"
                      "RECTANGLE"
                      "CIRCLE"
                      "ELLIPSE"

                   If the value of `shape' is "POLYGON" the field of view
                   of the instrument is a pyramidal polyhedron. The
                   vertex of the pyramid is at the instrument focal
                   point. The rays along the edges of the pyramid are
                   parallel to the vectors returned in `bounds'.

                   If the value of `shape' is "RECTANGLE" the field of view
                   of the instrument is a rectangular pyramid. The vertex
                   of the pyramid is at the instrument focal point. The
                   rays along the edges of the pyramid are parallel to
                   the vectors returned in `bounds'. Moreover, in this
                   case, the boresight points along the axis of symmetry
                   of the rectangular pyramid.

                   If the value of `shape' is "CIRCLE" the field of view of
                   the instrument is a circular cone centered on the
                   boresight vector. The vertex of the cone is at the
                   instrument focal point. A single vector will be
                   returned in `bounds'. This vector will be parallel to a
                   ray that lies in the cone that makes up the boundary
                   of the field of view.

                   If the value of `shape' is "ELLIPSE" the field of view
                   of the instrument is an elliptical cone with the
                   boresight vector as the axis of the cone. In this
                   case two vectors are returned in `bounds'. One of the
                   vectors returned in `bounds' points to the end of the
                   semi-major axis of a perpendicular cross section of
                   the elliptic cone. The other vector points to the end
                   of the semi-minor axis of a perpendicular cross
                   section of the cone.

       frame       is the name of the reference frame in which the field
                   of view boundary vectors are defined.

       bsight      is a vector representing the principal instrument view
                   direction that can be

                      -  the central pixel view direction,
                      -  the optical axis direction,
                      -  the FOV geometric center view direction,
                      -  an axis of the FOV frame,

                   or any other vector specified for this purpose
                   in the IK FOV definition. The length of `bsight'
                   is not specified other than being non-zero.

       n           is the number of boundary vectors returned.

       bounds      is an array of vectors that point to the "corners" of
                   the instrument field of view. (See the discussion
                   accompanying `shape' for an expansion of the term
                   "corner of the field of view.") Note that the vectors
                   returned in `bounds' are not necessarily unit vectors.
                   Their magnitudes will be as set in the IK (for
                   'CORNERS'-style FOV specifications) or the same as the
                   magnitude of the boresight (for 'ANGLES'-style FOV
                   specifications.)
#### Parameters
       MINCOS      is the lower limit on the value of the cosine of the
                   cross or reference angles in the 'ANGLES' specification
                   cases. See the header of the routine getfov_c for its
                   current value.
#### Exceptions
       1)  If the name of the instrument cannot be translated to its NAIF
           ID code, the error SPICE(IDCODENOTFOUND) is signaled by a
           routine in the call tree of this routine.

       2)  If the frame associated with the instrument can not be found,
           an error is signaled by a routine in the call tree of this
           routine.

       3)  If the shape of the instrument field of view can not be found
           in the kernel pool, an error is signaled by a routine in the
           call tree of this routine.

       4)  If the FOV_SHAPE specified by the instrument kernel is not
           one of the four values: 'CIRCLE', 'POLYGON', 'ELLIPSE', or
           'RECTANGLE', an error is signaled by a routine in the call
           tree of this routine. If the 'ANGLES' specification is used,
           FOV_SHAPE must be one of the three values: 'CIRCLE',
           'ELLIPSE', or 'RECTANGLE'.

       5)  If the direction of the boresight cannot be located in the
           kernel pool, an error is signaled by a routine in the call
           tree of this routine.

       6)  If the number of components for the boresight vector in the
           kernel pool is not 3, or they are not numeric, an error is
           signaled by a routine in the call tree of this routine.

       7)  If the boresight vector is the zero vector, an error is
           is signaled by a routine in the call tree of this routine.

       8)  If the 'ANGLES' specification is not present in the kernel
           pool and the boundary vectors for the edge of the field of
           view cannot be found in the kernel pool, an error is signaled
           by a routine in the call tree of this routine.

       9)  If there is insufficient room (as specified by the argument
           `room') to return all of the vectors associated with the
           boundary of the field of view, an error is signaled by a
           routine in the call tree of this routine.

       10) If the number of components of vectors making up the field of
           view is not a multiple of 3, an error is signaled by a routine
           in the call tree of this routine.

       11) If the number of components of vectors making up the field of
           view is not compatible with the shape specified for the field
           of view, an error is signaled by a routine in the call tree of
           this routine.

       12) If the reference vector for the 'ANGLES' specification can not
           be found in the kernel pool, an error is signaled by a routine
           in the call tree of this routine.

       13) If the reference vector stored in the kernel pool to support
           the 'ANGLES' specification contains an incorrect number of
           components, contains 3 character components, or is parallel to
           the boresight, an error is signaled by a routine in the call
           tree of this routine.

       14) If the 'ANGLES' specification is present in the kernel pool
           and the reference angle stored in the kernel pool to support
           the 'ANGLES' specification is absent from the kernel pool, an
           error is signaled by a routine in the call tree of this
           routine.

       15) If the keyword that stores the angular units for the angles
           used in the 'ANGLES' specification is absent from the kernel
           pool, an error is signaled by a routine in the call tree of
           this routine.

       16) If the value used for the units in the 'ANGLES' specification
           is not one of the supported angular units of convrt_c, an error
           is signaled by a routine in the call tree of this routine.

       17) If the keyword that stores the cross angle for the 'ANGLES'
           specification is needed and is absent from the kernel pool, an
           error is signaled by a routine in the call tree of this
           routine.

       18) If the angles for the 'RECTANGLE'/'ANGLES' specification case
           have cosines that are less than those stored in the parameter
           MINCOS defined in the getfov_c routine, an error is signaled by
           a routine in the call tree of this routine.

       19) If the class specification contains something other than
           'ANGLES' or 'CORNERS', an error is signaled by a routine in
           the call tree of this routine.

       20) In the event that the CLASS_SPEC keyword is absent from the
           kernel pool for the instrument whose FOV is sought, this
           module assumes the 'CORNERS' specification is to be utilized.

       21) If the `inst' input string pointer is null, the error
           SPICE(NULLPOINTER) is signaled.

       22) If the `inst' input string has zero length, the error
           SPICE(EMPTYSTRING) is signaled.

       23) If any of the `shape' or `frame' output string pointers is
           null, the error SPICE(NULLPOINTER) is signaled.

       24) If any of the `shape' or `frame' output strings has length
           less than two characters, the error SPICE(STRINGTOOSHORT) is
           signaled, since the output string is too short to contain one
           character of output data plus a null terminator.
#### Files
       Appropriate SPICE kernels must be loaded by the calling program
       before this routine is called.

       This routine relies upon having successfully loaded an instrument
       kernel (IK file) via the routine furnsh_c prior to calling this
       routine.

       The name `inst' must be associated with an NAIF ID code, normally
       through a frames kernel (FK file) or instrument kernel (IK file).

       Kernel data are normally loaded via furnsh_c once per program run,
       NOT every time this routine is called.
#### Particulars
       This routine provides a common interface for retrieving from the
       kernel pool the geometric characteristics of an instrument field
       of view for a wide variety of remote sensing instruments
       across many different space missions.

       This routine is identical in function to the routine getfov_c except
       that it allows you to refer to an instrument by name (via a
       character string) instead of by its NAIF instrument ID.

       Given the NAIF instrument name, (and having "loaded" the
       instrument field of view description and instrument name to NAIF
       ID mapping) this routine returns the boresight of the instrument,
       the "shape" of the field of view, a collection of vectors
       that point along the edges of the field of view, and the
       name of the reference frame in which these vectors are defined.

       Currently this routine supports two classes of specifications
       for FOV definitions: "corners" and "angles".

       The "corners" specification requires that the following keywords
       defining the shape, boresight, boundary vectors, and reference
       frame of the FOV be provided in one of the text kernel files
       (normally an IK file) loaded into the kernel pool (in the
       keywords below <INSTID> is replaced with the instrument ID which
       corresponds to the `inst' name passed into the module):

          INS<INSTID>_FOV_CLASS_SPEC         must be set to 'CORNERS' or
                                             omitted to indicate the
                                             "corners"-class
                                             specification.

          INS<INSTID>_FOV_SHAPE              must be set to one of these
                                             values:

                                                'CIRCLE'
                                                'ELLIPSE'
                                                'RECTANGLE'
                                                'POLYGON'

          INS<INSTID>_FOV_FRAME              must contain the name of
                                             the frame in which the
                                             boresight and boundary
                                             corner vectors are defined.

          INS<INSTID>_BORESIGHT              must be set to a 3D vector
                                             defining the boresight in
                                             the FOV frame specified in
                                             the FOV_FRAME keyword.

          INS<INSTID>_FOV_BOUNDARY   or
          INS<INSTID>_FOV_BOUNDARY_CORNERS   must be set to one (for
                                             FOV_SHAPE = 'CIRCLE'), two
                                             (for FOV_SHAPE =
                                             'ELLIPSE'), four (for
                                             FOV_SHAPE = 'RECTANGLE'),
                                             or three or more (for
                                             'POLYGON') 3D vectors
                                             defining the corners of the
                                             FOV in the FOV frame
                                             specified in the FOV_FRAME
                                             keyword. The vectors should
                                             be listed in either
                                             clockwise or
                                             counterclockwise order.
                                             This is required by some
                                             SPICE routines that make
                                             use of FOV specifications.

       The "angles" specification requires the following keywords
       defining the shape, boresight, reference vector, reference and
       cross angular extents of the FOV be provided in one of the text
       kernel files (normally an IK file) loaded into the kernel
       pool (in the keywords below <INSTID> is replaced with the
       instrument ID which corresponds to the `inst' name passed into the
       module):

          INS<INSTID>_FOV_CLASS_SPEC         must be set to 'ANGLES' to
                                             indicate the "angles"-class
                                             specification.

          INS<INSTID>_FOV_SHAPE              must be set to one of these
                                             values:

                                                'CIRCLE'
                                                'ELLIPSE'
                                                'RECTANGLE'

          INS<INSTID>_FOV_FRAME              must contain the name of
                                             the frame in which the
                                             boresight and the computed
                                             boundary corner vectors are
                                             defined.

          INS<INSTID>_BORESIGHT              must be set to a 3D vector
                                             defining the boresight in
                                             the FOV frame specified in
                                             the FOV_FRAME keyword.

          INS<INSTID>_FOV_REF_VECTOR         must be set to a 3D vector
                                             that together with the
                                             boresight vector defines
                                             the plane in which the
                                             first angular extent of the
                                             FOV specified in the
                                             FOV_REF_ANGLE keyword is
                                             measured.

          INS<INSTID>_FOV_REF_ANGLE          must be set to the angle
                                             that is 1/2 of the total
                                             FOV angular extent in the
                                             plane defined by the
                                             boresight and the vector
                                             specified in the
                                             FOV_REF_VECTOR keyword. The
                                             the FOV angular half-extents
                                             are measured from the
                                             boresight vector.

          INS<INSTID>_FOV_CROSS_ANGLE        must be set to the angle
                                             that is 1/2 of the total
                                             FOV angular extent in the
                                             plane containing the
                                             boresight and perpendicular
                                             to the plane defined by the
                                             boresight and the vector
                                             specified in the
                                             FOV_REF_VECTOR keyword. The
                                             the FOV angular half-extents
                                             are measured from the
                                             boresight vector. This
                                             keyword is not required for
                                             FOV_SHAPE = 'CIRCLE'.

          INS<INSTID>_FOV_ANGLE_UNITS        must specify units for the
                                             angles given in the
                                             FOV_REF_ANGLE and
                                             FOV_CROSS_ANGLE keywords.
                                             Any angular units
                                             recognized by convrt_c are
                                             acceptable.

       The INS<INSTID>_FOV_REF_ANGLE and INS<INSTID>_FOV_CROSS_ANGLE
       keywords can have any values for the 'CIRCLE' and 'ELLIPSE'
       FOV shapes but must satisfy the condition cos( angle ) > 0 for
       the 'RECTANGLE' shape.

       This routine is intended to be an intermediate level routine.
       It is expected that users of this routine will be familiar
       with the SPICE frames subsystem and will be comfortable writing
       software to further manipulate the vectors retrieved by this
       routine.
#### Examples
       The numerical results shown for this example may differ across
       platforms. The results depend on the SPICE kernels used as input,
       the compiler and supporting libraries, and the machine specific
       arithmetic implementation.

       1) Load an IK, fetch the parameters for each of the FOVs defined
          within and print these parameters to the screen.

          Use the kernel shown below, an IK defining four FOVs of
          various shapes and sizes, to load the FOV definitions, and the
          mapping between their NAMES and NAIF IDs.

             KPL/IK

             File name: getfvn_ex1.ti

             The keywords below define a circular, 10-degree wide FOV
             with the boresight along the +Z axis of the 'SC999_INST001'
             frame for an instrument with ID -999001 using the
             "angles"-class specification.

             \begindata
                INS-999001_FOV_CLASS_SPEC       = 'ANGLES'
                INS-999001_FOV_SHAPE            = 'CIRCLE'
                INS-999001_FOV_FRAME            = 'SC999_INST001'
                INS-999001_BORESIGHT            = ( 0.0, 0.0, 1.0 )
                INS-999001_FOV_REF_VECTOR       = ( 1.0, 0.0, 0.0 )
                INS-999001_FOV_REF_ANGLE        = ( 5.0 )
                INS-999001_FOV_ANGLE_UNITS      = ( 'DEGREES' )
             \begintext

             The keywords below define an elliptical FOV with 2- and
             4-degree angular extents in the XZ and XY planes and the
             boresight along the +X axis of the 'SC999_INST002' frame for
             an instrument with ID -999002 using the "corners"-class
             specification.

             \begindata
                INS-999002_FOV_SHAPE            = 'ELLIPSE'
                INS-999002_FOV_FRAME            = 'SC999_INST002'
                INS-999002_BORESIGHT            = ( 1.0, 0.0, 0.0 )
                INS-999002_FOV_BOUNDARY_CORNERS = (
                                        1.0,  0.0,        0.01745506,
                                        1.0,  0.03492077, 0.0        )
             \begintext

             The keywords below define a rectangular FOV with 1.2- and
             0.2-degree angular extents in the ZX and ZY planes and the
             boresight along the +Z axis of the 'SC999_INST003' frame for
             an instrument with ID -999003 using the "angles"-class
             specification.

             \begindata
                INS-999003_FOV_CLASS_SPEC       = 'ANGLES'
                INS-999003_FOV_SHAPE            = 'RECTANGLE'
                INS-999003_FOV_FRAME            = 'SC999_INST003'
                INS-999003_BORESIGHT            = ( 0.0, 0.0, 1.0 )
                INS-999003_FOV_REF_VECTOR       = ( 1.0, 0.0, 0.0 )
                INS-999003_FOV_REF_ANGLE        = ( 0.6 )
                INS-999003_FOV_CROSS_ANGLE      = ( 0.1 )
                INS-999003_FOV_ANGLE_UNITS      = ( 'DEGREES' )
             \begintext

             The keywords below define a triangular FOV with the
             boresight along the +Y axis of the 'SC999_INST004' frame
             for an instrument with ID -999004 using the "corners"-class
             specification.

             \begindata
                INS-999004_FOV_SHAPE            = 'POLYGON'
                INS-999004_FOV_FRAME            = 'SC999_INST004'
                INS-999004_BORESIGHT            = (  0.0,  1.0,  0.0 )
                INS-999004_FOV_BOUNDARY_CORNERS = (  0.0,  0.8,  0.5,
                                                     0.4,  0.8, -0.2,
                                                    -0.4,  0.8, -0.2 )
             \begintext

             The keywords below define the INSTRUMENT name to NAIF ID
             mappings for this example. For convenience we will keep them
             in the example's IK although they could be placed elsewhere
             (normally on the mission's frames kernel)

             \begindata
                NAIF_BODY_NAME += ( 'SC999_INST001' )
                NAIF_BODY_CODE += ( -999001 )

                NAIF_BODY_NAME += ( 'SC999_INST002' )
                NAIF_BODY_CODE += ( -999002 )

                NAIF_BODY_NAME += ( 'SC999_INST003' )
                NAIF_BODY_CODE += ( -999003 )

                NAIF_BODY_NAME += ( 'SC999_INST004' )
                NAIF_BODY_CODE += ( -999004 )
             \begintext

             End of IK

          Example code begins here.

          /.
             Program getfvn_ex1
          ./
          #include <stdio.h>
          #include "SpiceUsr.h"

          int main( )
          {

             /.
             Local parameters
             ./
             #define MAXBND       4
             #define NUMINS       4
             #define WDSIZE       33

             /.
             Local variables
             ./
             SpiceChar            frame  [WDSIZE];
             SpiceChar            shape  [WDSIZE];

             SpiceDouble          bounds [MAXBND][3];
             SpiceDouble          bsight [3];

             SpiceInt             i;
             SpiceInt             j;
             SpiceInt             n;

             /.
             Define the instrument IDs.
             ./
             SpiceChar            instnm [NUMINS][WDSIZE] = { "SC999_INST001",
                                                              "SC999_INST002",
                                                              "SC999_INST003",
                                                              "SC999_INST004" };

             /.
             Load the IK file.
             ./
             furnsh_c ( "getfvn_ex1.ti" );

             /.
             For each instrument ...
             ./
             printf( "--------------------------------------\n" );
             for ( i = 0; i < NUMINS; i++ )
             {

                /.
                ... fetch FOV parameters and ...
                ./
                getfvn_c ( instnm[i], MAXBND, WDSIZE,
                           WDSIZE,    shape,  frame,
                           bsight,    &n,     bounds );

                /.
                ... print them to the screen.
                ./
                printf( "Instrument NAME: %s\n", instnm[i] );
                printf( "    FOV shape: %s\n", shape );
                printf( "    FOV frame: %s\n", frame );
                printf( "FOV boresight:  %11.8f %11.8f %11.8f\n",
                                  bsight[0], bsight[1], bsight[2] );

                printf( "  FOV corners:\n" );
                for ( j = 0; j < n; j++ )
                {
                   printf( "                %11.8f %11.8f %11.8f\n",
                            bounds[j][0], bounds[j][1], bounds[j][2] );
                }
                printf( "--------------------------------------\n" );
             }

             return ( 0 );
          }

          When this program was executed on a Mac/Intel/cc/64-bit
          platform, the output was:

          --------------------------------------
          Instrument NAME: SC999_INST001
              FOV shape: CIRCLE
              FOV frame: SC999_INST001
          FOV boresight:   0.00000000  0.00000000  1.00000000
            FOV corners:
                           0.08715574  0.00000000  0.99619470
          --------------------------------------
          Instrument NAME: SC999_INST002
              FOV shape: ELLIPSE
              FOV frame: SC999_INST002
          FOV boresight:   1.00000000  0.00000000  0.00000000
            FOV corners:
                           1.00000000  0.00000000  0.01745506
                           1.00000000  0.03492077  0.00000000
          --------------------------------------
          Instrument NAME: SC999_INST003
              FOV shape: RECTANGLE
              FOV frame: SC999_INST003
          FOV boresight:   0.00000000  0.00000000  1.00000000
            FOV corners:
                           0.01047177  0.00174523  0.99994365
                          -0.01047177  0.00174523  0.99994365
                          -0.01047177 -0.00174523  0.99994365
                           0.01047177 -0.00174523  0.99994365
          --------------------------------------
          Instrument NAME: SC999_INST004
              FOV shape: POLYGON
              FOV frame: SC999_INST004
          FOV boresight:   0.00000000  1.00000000  0.00000000
            FOV corners:
                           0.00000000  0.80000000  0.50000000
                           0.40000000  0.80000000 -0.20000000
                          -0.40000000  0.80000000 -0.20000000
          --------------------------------------
#### Restrictions
       1)  This routine will not operate unless proper mapping between
           the instrument name `inst' and a NAIF ID exists, an I-kernel for
           that instrument ID has been loaded via a call to furnsh_c prior
           to calling this routine and this IK contains the specification
           for the instrument field of view consistent with the
           expectations of this routine.
#### Literature_References
       None.
#### Author_and_Institution
       J. Diaz del Rio     (ODC Space)
#### Version
       -CSPICE Version 1.0.0, 17-DEC-2021 (JDR)
#### Index_Entries
       return instrument's FOV parameters, using instrument name
#### Link to routine getfvn_c source file getfvn_c.c

    Fri Dec 31 18:41:07 2021