Index of Functions: A B C D E F G H I J K L M N O P Q R S T U V W X
Index Page pcpool_c
Table of contents
Procedure Abstract Required_Reading Keywords Brief_I/O Detailed_Input | Detailed_Output Parameters Exceptions Files Particulars Examples | Restrictions Literature_References Author_and_Institution Version Index_Entries
#### Procedure
       pcpool_c ( Put character strings into the kernel pool )

       void pcpool_c ( ConstSpiceChar  * name,
                       SpiceInt          n,
                       SpiceInt          cvalen,
                       const void      * cvals    )
#### Abstract
       Provide toolkit programmers a method for programmatically
       inserting character data into the kernel pool.
#### Required_Reading
       None.
#### Keywords
       POOL
#### Brief_I/O
       VARIABLE  I/O  DESCRIPTION
       --------  ---  --------------------------------------------------
       name       I   The kernel pool name to associate with cvals.
       n          I   The number of values to insert.
       cvalen     I   The lengths of the strings in the array cvals.
       cvals      I   An array of strings to insert into the kernel pool.
#### Detailed_Input
       name        is the name of the kernel pool variable to associate
                   with the values supplied in the array cvals. 'name' is
                   restricted to a length of 32 characters or less.

       n           is the number of values to insert into the kernel pool.

       cvalen      is the length of the strings in the array cvals,
                   including the null terminators.

       cvals       is an array of strings to insert into the kernel
                   pool. cvals should be declared as follows:

                      char  cvals[n][cvalen];
#### Detailed_Output
       None.
#### Parameters
       None.
#### Exceptions
       1)  If `name' is already present in the kernel pool and there
           is sufficient room to hold all values supplied in `cvals',
           the old values associated with `name' will be overwritten.

       2)  If there is not sufficient room to insert a new variable into
           the kernel pool and `name' is not already present in the kernel
           pool, an error is signaled by a routine in the call tree of
           this routine.

       3)  If there is not sufficient room to insert the values
           associated with `name', the error SPICE(NOMOREROOM) is signaled
           by a routine in the call tree of this routine.

       4)  If the kernel pool variable name length exceeds its maximum
           allowed length (see Kernel Required Reading, kernel.req), the
           error SPICE(BADVARNAME) is signaled by a routine in the call
           tree of this routine.

       5)  If the `name' input string pointer is null, the error
           SPICE(NULLPOINTER) is signaled.

       6)  If the `name' input string has zero length, the error
           SPICE(EMPTYSTRING) is signaled.

       7)  If the `cvals' input array pointer is null, the error
           SPICE(NULLPOINTER) is signaled.

       8)  If the `cvals' input array strings have length less than two
           characters, the error SPICE(STRINGTOOSHORT) is signaled.
#### Files
       None.
#### Particulars
       This entry point provides a programmatic interface for inserting
       character data into the SPICE kernel pool without reading an
       external file.
#### Examples
       The numerical results shown for this example may differ across
       platforms. The results depend on the SPICE kernels used as input,
       the compiler and supporting libraries, and the machine specific
       arithmetic implementation.

       1) The following example code shows how a topocentric frame for a
          point on the surface of the earth may be defined at run time using
          pcpool_c, pdpool_c, and pipool_c. In this example, the surface
          point is associated with the body code 300000. To facilitate
          testing, the location of the surface point coincides with that of
          the DSN station DSS-12; the reference frame MYTOPO defined here
          coincides with the reference frame DSS-12_TOPO.

          Use the meta-kernel shown below to load the required SPICE
          kernels.

             KPL/MK

             File name: pcpool_ex1.tm

             This meta-kernel is intended to support operation of SPICE
             example programs. The kernels shown here should not be
             assumed to contain adequate or correct versions of data
             required by SPICE-based user applications.

             In order for an application to use this meta-kernel, the
             kernels referenced here must be present in the user's
             current working directory.

             The names and contents of the kernels referenced
             by this meta-kernel are as follows:

                File name                        Contents
                ---------                        --------
                earth_720101_070426.bpc          Earth historical
                                                 binary PCK
                earth_topo_050714.tf             DSN station FK

             \begindata

             KERNELS_TO_LOAD = ( 'earth_720101_070426.bpc',
                                 'earth_topo_050714.tf'    )

             \begintext

             End of meta-kernel.

          Example code begins here.

          /.
             Program pcpool_ex1
          ./
          #include <stdio.h>
          #include "SpiceUsr.h"

          int main()
          {
             /.
             The first angle is the negative of the longitude of the
             surface point; the second angle is the negative of the
             point's colatitude.
             ./
             SpiceDouble             angles [3]      =  { -243.1945102442646,
                                                           -54.7000629043147,
                                                           180.0              };

             SpiceDouble             et              =    0.0;
             SpiceDouble             rmat   [3][3];

             SpiceInt                axes   [3]      =  { 3, 2, 3 };
             SpiceInt                center          =    300000;
             SpiceInt                frclass         =    4;
             SpiceInt                frclsid         =    1500000;
             SpiceInt                frcode          =    1500000;

             /.
             Define the MYTOPO reference frame.

             Note that the third argument in the pcpool_c calls is
             the length of the final string argument, including the
             terminating null character.
             ./
             pipool_c ( "FRAME_MYTOPO",            1,     &frcode   );
             pcpool_c ( "FRAME_1500000_NAME",      1, 7,  "MYTOPO"  );
             pipool_c ( "FRAME_1500000_CLASS",     1,     &frclass  );
             pipool_c ( "FRAME_1500000_CLASS_ID",  1,     &frclsid  );
             pipool_c ( "FRAME_1500000_CENTER",    1,     &center   );

             pcpool_c ( "OBJECT_300000_FRAME",     1, 7,  "MYTOPO"  );

             pcpool_c ( "TKFRAME_MYTOPO_RELATIVE", 1, 7,  "ITRF93"  );
             pcpool_c ( "TKFRAME_MYTOPO_SPEC",     1, 7,  "ANGLES"  );
             pcpool_c ( "TKFRAME_MYTOPO_UNITS",    1, 8,  "DEGREES" );
             pipool_c ( "TKFRAME_MYTOPO_AXES",     3,     axes      );
             pdpool_c ( "TKFRAME_MYTOPO_ANGLES",   3,     angles    );

             /.
             Load a high precision binary earth PCK. Also load a
             topocentric frame kernel for DSN stations. Use a meta-kernel
             for convenience.
             ./
             furnsh_c ( "pcpool_ex1.tm" );

             /.
             Look up transformation from DSS-12_TOPO frame to MYTOPO frame.
             This transformation should differ by round-off error from
             the identity matrix.
             ./
             pxform_c ( "DSS-12_TOPO", "MYTOPO", et, rmat );

             printf   ( "\n"
                        "DSS-12_TOPO to MYTOPO transformation at "
                        "et %15.6f: \n"
                        "\n"
                        "   %19.16f  %19.16f  %19.16f\n"
                        "   %19.16f  %19.16f  %19.16f\n"
                        "   %19.16f  %19.16f  %19.16f\n",
                        et,
                        rmat[0][0],  rmat[0][1],  rmat[0][2],
                        rmat[1][0],  rmat[1][1],  rmat[1][2],
                        rmat[2][0],  rmat[2][1],  rmat[2][2]       );

             return ( 0 );
          }

          When this program was executed on a Mac/Intel/cc/64-bit
          platform, the output was:

          DSS-12_TOPO to MYTOPO transformation at et        0.000000:

              1.0000000000000000   0.0000000000000000   0.0000000000000001
              0.0000000000000000   1.0000000000000000  -0.0000000000000000
              0.0000000000000001  -0.0000000000000000   1.0000000000000000
#### Restrictions
       None.
#### Literature_References
       None.
#### Author_and_Institution
       N.J. Bachman        (JPL)
       J. Diaz del Rio     (ODC Space)
       W.L. Taber          (JPL)
       E.D. Wright         (JPL)
#### Version
       -CSPICE Version 1.4.0, 27-AUG-2021 (JDR)

           Changed input argument name "lenvals" to "cvalen" for
           consistency with other routines.

           Edited the header to comply with NAIF standard. Added
           example's meta-kernel. Reformatted example's output.

           Added entry #7 to -Exceptions section.

       -CSPICE Version 1.3.3, 17-JAN-2014 (NJB)

           Updated -Index_Entries section.

       -CSPICE Version 1.3.2, 10-FEB-2010 (EDW)

           Added mention of the restriction on kernel pool variable
           names to 32 characters or less.

           Reordered header sections to conform to SPICE convention.

       -CSPICE Version 1.3.1, 17-NOV-2005 (NJB)

           Replaced code fragment in -Examples section of header with
           smaller, complete program.

       -CSPICE Version 1.3.0, 12-JUL-2002 (NJB)

           Call to C2F_CreateStrArr_Sig replaced with call to C2F_MapStrArr.

       -CSPICE Version 1.2.0, 28-AUG-2001 (NJB)

           Const-qualified input array cvals.

       -CSPICE Version 1.1.0, 14-FEB-2000 (NJB)

           Calls to C2F_CreateStrArr replaced with calls to error-signaling
           version of this routine:  C2F_CreateStrArr_Sig.

       -CSPICE Version 1.0.0, 18-JUN-1999 (NJB) (WLT)
#### Index_Entries
       Set the value of a character_variable in the kernel_pool
#### Link to routine pcpool_c source file pcpool_c.c

    Fri Dec 31 18:41:10 2021