Index of Functions: A B C D E F G H I J K L M N O P Q R S T U V W X
Index Page errprt_c
Table of contents
Procedure Abstract Required_Reading Keywords Brief_I/O Detailed_Input | Detailed_Output Parameters Exceptions Files Particulars Examples | Restrictions Literature_References Author_and_Institution Version Index_Entries
#### Procedure
       errprt_c ( Get/Set Error Output Items )

       void errprt_c ( ConstSpiceChar * op,
                       SpiceInt         lislen,
                       SpiceChar      * list  )
#### Abstract
       Retrieve or set the list of error message items
       to be output when an error is detected.
#### Required_Reading
       ERROR
#### Keywords
       ERROR
#### Brief_I/O
       VARIABLE  I/O  DESCRIPTION
       --------  ---  --------------------------------------------------
       op         I   The operation:  "GET" or "SET".
       lislen     I   Length of list for output.
       list      I-O  Specification of error messages to be output.
#### Detailed_Input
       op          indicates the operation to be performed. Possible
                   values are "GET" and "SET".

                   "SET" means, "the following list specifies the default
                   selection of error messages to be output." These are
                   the messages that will be output to the default error
                   output device (selected by errdev_c) when an error is
                   detected.

                   "GET" means, "return the current list of error output
                   items." This is the exact list that was set by the
                   last call to this routine with the "SET" option.

                   The option can be specified in mixed case. For example,
                   the following call will work:

                   errprt_c ( "SeT", lislen, "ALL" )

       lislen      is the allowed length of `list' when `list' is returning a
                   the error message list. The size described by `lislen'
                   should be large enough to hold any possible output plus 1.

       list        is a list of error message items. The items
                   are delimited by commas. The items that can be
                   in the list are the words:

                   1.  SHORT        ...indicates the short error message
                   2.  EXPLAIN      ...the explanation of the short message
                   3.  LONG         ...the long error message
                   4.  TRACEBACK    ...the traceback
                   5.  ALL          ...indicates "output all messages"
                   6.  NONE         ...indicates "don't output any messages"
                   7.  DEFAULT      ...same as ALL, but includes default
                                        message

                   A "list" is a character string containing some or
                   all of the above words, delimited by commas. Examples
                   are:

                   1.  "SHORT, EXPLAIN"
                   2.  "SHORT, LONG"
                   3.  "ALL"
                   4.  "NONE"
                   5.  "ALL, NONE, ALL, SHORT, NONE"

                   Each word in the list can be thought of as
                   "flipping a switch" to enable or disable the output
                   of the message(s) indicated by the word. The
                   words are acted on in the order they occur in the
                   list, starting with the leftmost word. As examples,
                   consider the sample lists above.

                   The effect of the first list above, "SHORT, EXPLAIN",
                   is to enable the output of the short error message
                   and the explanatory text corresponding to it.

                   The effect of the second list is to enable the output
                   of the short and long messages.

                   The effect of the third list is to enable the output of
                   all of the error messages (short, long, explanation
                   of the short message, and traceback).

                   The effect of the fourth list is to disable output of
                   all of the messages.

                   The effect of the fifth list is to disable output of
                   all of the messages. The reason for this is that
                   the words in the list are responded to in order,
                   from left to right, and "NONE" is the last word.

                   If any words other than SHORT, LONG, EXPLAIN, ALL,
                   DEFAULT, TRACEBACK or NONE appear in list, those words
                   that are recognized are responded to. The words
                   that are not recognized are diagnosed as
                   erroneous, and error messages are generated
                   for each such unrecognized word.

                   The length of list is caller-defined, but only
                   the first 100 characters of list will be saved
                   for later retrieval.

                   Only the first 10 items in the list are used;
                   the rest are ignored.
#### Detailed_Output
       list        is a list of error message items. The value of
                   `list' is that set by the last call to this routine
                   using the "SET" option. See "Detailed Input"
                   for a description of the possible values and
                   meanings of `list'.

                   The initial value returned is "DEFAULT".

                   Only the first 100 characters of `list' are saved
                   when the list is set; any additional characters
                   are truncated. Therefore, the first 100
                   characters, at most, of the saved value of `list'
                   will be returned.
#### Parameters
       None.
#### Exceptions
       1)  If an invalid value of the argument `op' is supplied, the error
           SPICE(INVALIDOPERATION) is signaled.

       2)  If `op' is "SET" and an invalid word is detected within the list
           of error message items `list', the error SPICE(INVALIDLISTITEM)
           is signaled by a routine in the call tree of this routine.

       3)  If the `op' input string pointer is null, the error
           SPICE(NULLPOINTER) is signaled.

       4)  If the `op' input string has zero length, the error
           SPICE(EMPTYSTRING) is signaled, since the input string cannot
           be converted to a Fortran-style string in this case.

       5)  If the `list' string pointer is null, the error
           SPICE(NULLPOINTER) is signaled.

       6)  If `op' is "SET" and the `list' input string has zero length, the
           error SPICE(EMPTYSTRING) is signaled, since the input string cannot
           be converted to a Fortran-style string in this case.

       7)  If `op' is "GET" and the `list' output string has length less than two
           characters, the error SPICE(STRINGTOOSHORT) is signaled, since the
           output string is too short to contain one character of output data plus
           a null terminator, and therefore it cannot be passed to the underlying
           Fortran routine.
#### Files
       None.
#### Particulars
       Please read the "required reading"!

       This routine is intended to be used in conjunction with
       errdev_c, which selects the default output device to which
       the error messages selected by this routine will be
       output.

       Additionally, the error response action must be
       something other than "IGNORE" if the error messages
       are to be output. Possible choices of the error
       response action are "RETURN", "REPORT", "ABORT", "DEFAULT", and
       "IGNORE".  Use erract_c to set the error response action.

       Only the first 100 characters of list are saved.

       The default set of error messages that are output is the
       set specified by "DEFAULT"; i.e., all of them, including
       the "default" message.
#### Examples
       1. In this example, we select as the output device
           the file, SPUD.DAT, and then select the error
           messages to be output. We choose the short
           error message and the traceback. Since a
           different set of messages may have been selected
           previously, we clear the old setting by putting
           the word, "NONE", at the beginning of the list.

              /.
              Set the error output device to SPUD.DAT:
              ./
              errdev_c (  "SET", lislen, "SPUD.DAT" );

              /.
              Choose error messages:
              ./
              errprt_c (  "SET", lislen, "NONE, SHORT, TRACEBACK" );

       2. In this example we are retrieving the error message list.

              /.
              Declare the output string and its size.
              ./

             #define     LENOUT  50

             SpiceChar   list[ LENOUT ];

             errdev_c ( "GET", LENOUT, list );
#### Restrictions
       1)  The device to which the selected error messages will be
           written must be selected via errdev_c; otherwise, messages will
           be written to the initial default device.

       2)  Only the first 100 characters of `list' are saved.
#### Literature_References
       None.
#### Author_and_Institution
       N.J. Bachman        (JPL)
       J. Diaz del Rio     (ODC Space)
       E.D. Wright         (JPL)
#### Version
       -CSPICE Version 1.4.0, 10-AUG-2021 (JDR)

           Changed the input argument "lenout" to "lislen" for consistency
           with other routines.

           Edited the header to comply with NAIF standard.

       -CSPICE Version 1.3.0, 24-JUN-2003 (NJB)

           Bug fix: case of invalid operation keyword is now
           diagnosed, as per the -Exceptions section of the header.

       -CSPICE Version 2.0.0, 09-FEB-1998 (NJB) (EDW)

           Input argument op was changed to type ConstSpiceChar *.

           Re-implemented routine without dynamically allocated, temporary
           strings.

           Corrected errors in examples in which the call sequence
           was incorrect.

       -CSPICE Version 1.0.0, 25-OCT-1997 (EDW)
#### Index_Entries
       get/set error output items
#### Link to routine errprt_c source file errprt_c.c

    Fri Dec 31 18:41:06 2021