Index of Functions: A B C D E F G H I J K L M N O P Q R S T U V W X
Index Page dskx02_c
Table of contents
Procedure Abstract Required_Reading Keywords Brief_I/O Detailed_Input | Detailed_Output Parameters Exceptions Files Particulars Examples | Restrictions Literature_References Author_and_Institution Version Index_Entries
#### Procedure
       dskx02_c ( DSK, ray-surface intercept, type 2 )

       void dskx02_c ( SpiceInt               handle,
                       ConstSpiceDLADescr   * dladsc,
                       ConstSpiceDouble       vertex  [3],
                       ConstSpiceDouble       raydir  [3],
                       SpiceInt             * plid,
                       SpiceDouble            xpt     [3],
                       SpiceBoolean         * found        )
#### Abstract
       Determine the plate ID and body-fixed coordinates of the
       intersection of a specified ray with the surface defined by a
       type 2 DSK plate model.
#### Required_Reading
       None.
#### Keywords
       GEOMETRY
       SHAPES
#### Brief_I/O
       VARIABLE  I/O  DESCRIPTION
       --------  ---  --------------------------------------------------
       handle     I   Handle of DSK kernel containing plate model.
       dladsc     I   DLA descriptor of plate model segment.
       vertex     I   Ray's vertex in the  body fixed frame.
       raydir     I   Ray direction in the body fixed frame.
       plid       O   ID code of the plate intersected by the ray.
       xpt        O   Intercept.
       found      O   Flag indicating whether intercept exists.
#### Detailed_Input
       handle      is the file handle of a DSK file containing a shape
                   model for a target body. The shape model is stored
                   in a type 2 DSK segment.

       dladsc      is the DLA descriptor of a type 2 DSK segment containing
                   plate model data representing the surface of the target
                   body. Normally this descriptor will be obtained by a
                   search through a DSK file using the DLA search routines;
                   see the -Examples header section below for a working code
                   example illustrating a simple search.

       vertex      is the vertex of a ray. `vertex' is expressed relative
                   to the body fixed reference frame associated with the
                   target body. This reference frame is the same frame
                   relative to which the vertices of the plate model
                   are expressed. Units are km.

                   The vertex is required to be outside the target
                   body.

       raydir      is the ray's direction vector. `raydir' is expressed
                   relative to the body fixed reference frame associated
                   with the target body.
#### Detailed_Output
       plid        is the ID of the plate closest to the input ray's
                   vertex at which a ray-surface intercept exists.
                   If no intercept exists, `plid' is undefined.

       xpt         is the ray-target intercept closest to the ray's
                   vertex, if an intercept exists. `xpt' is expressed
                   relative to the body-fixed reference frame associated
                   with the target body. Units are km.

                   If no intercept exists, `xpt' is undefined.

       found       is a logical flag that indicates whether or not the ray
                   does indeed intersect the target. If the ray intersects a
                   plate `found' is SPICETRUE. Otherwise `found' is
                   SPICEFALSE.
#### Parameters
       See the header file

          SpiceDtl.h

       for the values of tolerance parameters used by default by the
       ray-surface intercept algorithm.

       See the header file

          SpiceDLA.h

       for declarations of DLA descriptor sizes and documentation of the
       contents of DLA descriptors.

       See the header file

          SpiceDSK.h

       for declarations of DSK descriptor sizes and documentation of the
       contents of DSK descriptors.

       See the header file

          SpiceDSK.h

       for declarations of DSK data type 2 (plate model) parameters.
#### Exceptions
       1)  If the input handle is invalid, an error is signaled by a
           routine in the call tree of this routine.

       2)  If a file read error occurs, the error is signaled by a
           routine in the call tree of this routine.

       3)  If the input DLA descriptor is invalid, the effect of this
           routine is undefined. The error *may* be diagnosed by
           routines in the call tree of this routine, but there are no
           guarantees.

       4)  If an error occurs while trying to look up any component
           of the shape model, the error is signaled by a routine in the
           call tree of this routine.

       5)  If the input ray direction is the zero vector, the error
           SPICE(ZEROVECTOR) is signaled by a routine in the call tree of
           this routine.

       6)  If the coarse voxel grid scale of the shape model is less than
           1, the error SPICE(VALUEOUTOFRANGE) is signaled by a routine
           in the call tree of this routine.

       7)  If the coarse voxel grid of the shape model contains more
           than SPICE_DSK_MAXCGR (see SpiceDSK.h) voxels, the error
           SPICE(GRIDTOOLARGE) is signaled by a routine in the call tree of
           this routine.

       8)  If the plate list for any intersected voxel is too large
           for this routine to buffer, the error SPICE(ARRAYTOOSMALL)
           is signaled by a routine in the call tree of this routine.

       9)  Due to round-off errors, results from this routine may
           differ across platforms. Results also may differ from
           those expected---and not necessarily by a small amount.
           For example, a ray may miss a plate it was expected to
           hit and instead hit another plate considerably farther
           from the ray's vertex, or miss the target entirely.

       10) In the event that an intercept point lies on multiple
           plates (that is, the point is on an edge or vertex),
           a plate will be selected. Due to round-off error, the
           selection may vary across platforms.
#### Files
       See the description of the input argument `handle'.
#### Particulars
       This routine solves the ray-surface intercept problem for
       a specified ray and a surface represented by triangular plate
       model. The surface representation is provided by data in a
       type 2 segment of a DSK file.

       This routine does not assume that the segment from which the
       surface model data are read represents the entire surface of
       the target body. A program could call this routine repeatedly
       to find the surface intercept of a ray and a shape model
       partitioned into multiple segments.

       In general, this routine should be expected to run faster
       when used with smaller shape models.
#### Examples
       The numerical results shown for this example may differ across
       platforms. The results depend on the SPICE kernels used as input,
       the compiler and supporting libraries, and the machine specific
       arithmetic implementation.

       1) Find the surface intercept points corresponding to a latitude/
          longitude grid of a specified resolution, for a specified
          target body.

          This simple program assumes the shape model for the target
          body is stored in a single type 2 DSK segment, and that this
          segment is the first one in the DSK file to which it belongs.

          Example code begins here.

          /.
             Program dskx02_ex1
          ./
          #include <stdio.h>
          #include <math.h>
          #include "SpiceUsr.h"

          int main()
          {
             /.
             Local parameters
             ./
             #define  FILSIZ             256
             #define  NLAT               9
             #define  NLON               9
             #define  TOL                ( 1.e-12 )
             #define  SPICE_MXCOR3_IDX   21

             /.
             Local variables
             ./
             SpiceBoolean            found;

             SpiceChar               dsk [ FILSIZ ];

             SpiceDLADescr           dladsc;
             SpiceDSKDescr           dskdsc;

             SpiceDouble             lat;
             SpiceDouble             lon;
             SpiceDouble             maxr;
             SpiceDouble             r;
             SpiceDouble             raydir [3];
             SpiceDouble             vertex [3];
             SpiceDouble             xlat;
             SpiceDouble             xlon;
             SpiceDouble             xpt    [3];
             SpiceDouble             xr;

             SpiceInt                handle;
             SpiceInt                i;
             SpiceInt                j;
             SpiceInt                plid;

             /.
             Prompt for the name of the DSK to read.
             ./
             prompt_c ( "Enter DSK name > ", FILSIZ, dsk );

             /.
             Open the DSK file for read access.
             We use the DAS-level interface for
             this function.
             ./
             dasopr_c ( dsk, &handle );

             /.
             Begin a forward search through the
             kernel, treating the file as a DLA.
             In this example, it's a very short
             search.
             ./
             dlabfs_c ( handle, &dladsc, &found );

             if ( !found  )
             {
                /.
                We arrive here only if the kernel
                contains no segments.  This is
                unexpected, but we're prepared for it.
                ./
                setmsg_c ( "No segments found in DSK file #.");
                errch_c  ( "#",  dsk                         );
                sigerr_c ( "SPICE(NODATA)"                   );
             }

             /.
             If we made it this far, DLADSC is the
             DLA descriptor of the first segment.

             We're going to generate the intercept points
             using a set of rays which point toward the
             origin and whose vertices are on a specified
             specified lat/lon grid.  To start out we
             must pick a reasonable range from the origin
             for the vertices:  the range must be large
             enough so that the vertices are guaranteed
             to be outside the target body but small
             enough that we don't lose too much precision
             in the surface intercept computation.

             We'll look up the upper bound for the target
             radius, then use 2 times this value as the
             vertex magnitude.
             ./

             dskgd_c ( handle, &dladsc, &dskdsc );

             maxr =  dskdsc.co3max;
             r    = 2.0 * maxr;

             /.
             Now generate the intercept points. We generate
             intercepts along latitude bounds, working from
             north to south. Latitude ranges from +80 to -80
             degrees. Longitude ranges from 0 to 320 degrees.
             The increment is 20 degrees for latitude and 40
             degrees for longitude.
             ./
             for ( i = 0;  i < NLAT;  i++  )
             {
                lat = rpd_c() * ( 80.0 - 20.0*i );

                for ( j = 0;  j < NLON;  j++  )
                {
                   lon = rpd_c() * 40.0*j;

                   /.
                   Produce a ray vertex for the current
                   lat/lon value.  Negate the vertex to
                   produce the ray's direction vector.
                   ./
                   latrec_c ( r, lon, lat, vertex );
                   vminus_c ( vertex,      raydir );

                   /.
                   Find the surface intercept for this
                   ray.
                   ./
                   dskx02_c ( handle, &dladsc, vertex, raydir,
                              &plid,  xpt,     &found          );

                   /.
                   Since the ray passes through the origin on
                   the body-fixed frame associated with the
                   target body, we'd rarely expect to find that
                   the ray failed to intersect the surface.
                   For safety, we check the FOUND flag.  (A
                   "not found" condition could be a sign of
                   a bug.)
                   ./
                   if ( ! found  )
                   {
                      printf ( "\n"
                               "Intercept not found!\n"
                               "   Ray vertex:\n"
                               "   Longitude (deg): %f\n"
                               "   Latitude  (deg): %f\n"
                               "   Radius     (km): %e\n"
                               "\n",
                               lon * dpr_c(),
                               lat * dpr_c(),
                               r                           );
                   }
                   else
                   {
                      /.
                      This is the normal case.  Display the
                      intercept plate ID and the intercept
                      point in both cartesian and latitudinal
                      coordinates.  Show the corresponding ray
                      vertex to facilitate validation of results.

                      Use recrad_c rather than reclat_c to produce
                      non-negative longitudes.
                      ./
                      recrad_c ( xpt, &xr, &xlon, &xlat );

                      printf ( "\n"
                               "Intercept found:\n"
                               "   Plate ID:                 %d\n"
                               "   Cartesian Coordinates: %12.8f %12.8f %12.8f\n"
                               "   Latitudinal Coordinates:\n"
                               "   Longitude (deg): %f\n"
                               "   Latitude  (deg): %f\n"
                               "   Radius     (km): %e\n"
                               "\n"
                               "   Ray vertex:\n"
                               "   Longitude (deg): %f\n"
                               "   Latitude  (deg): %f\n"
                               "   Radius     (km): %e\n"
                               "\n",
                               (int)plid,
                               xpt[0], xpt[1], xpt[2],
                               xlon * dpr_c(),
                               xlat * dpr_c(),
                               xr,
                               lon  * dpr_c(),
                               lat  * dpr_c(),
                               r                                           );

                      /.
                      Perform sanity checks on the intercept
                      coordinates.  Stop the program if any error
                      is larger than our tolerance value.
                      ./
                      if ( fabs(xlat-lat) > TOL )
                      {
                         sigerr_c ( "Latitude error!" );
                      }

                      if (  (xlon - lon)  > pi_c()  )
                      {
                         xlon -= twopi_c();
                      }

                      if (  (xlon - lon)  > TOL  )
                      {
                         sigerr_c ( "Longitude error!" );
                      }

                      if ( xr  > (1.0+TOL)*maxr  )
                      {
                         sigerr_c ( "Radius error!" );
                      }
                   }
                   /.
                   End of longitude loop.
                   ./
                }
                /.
                End of latitude loop.
                ./
             }

             /.
             Close the kernel.  This isn't necessary in a stand-
             alone program, but it's good practice in subroutines
             because it frees program and system resources.
             ./
             dascls_c ( handle );

             return ( 0 );
          }

          When this program was executed on a Mac/Intel/cc/64-bit
          platform, using the DSK file named phobos_3_3.bds, the output
          was:

          Enter DSK name > phobos_3_3.bds

          Intercept found:
             Plate ID:                 306238
             Cartesian Coordinates:   1.52087789   0.00000000   8.62532711
             Latitudinal Coordinates:
             Longitude (deg): 0.000000
             Latitude  (deg): 80.000000
             Radius     (km): 8.758387e+00

             Ray vertex:
             Longitude (deg): 0.000000
             Latitude  (deg): 80.000000
             Radius     (km): 2.802354e+01

          Intercept found:
             Plate ID:                 317112
             Cartesian Coordinates:   1.18970365   0.99827989   8.80777185
             Latitudinal Coordinates:
             Longitude (deg): 40.000000
             Latitude  (deg): 80.000000
             Radius     (km): 8.943646e+00

             Ray vertex:
             Longitude (deg): 40.000000
             Latitude  (deg): 80.000000
             Radius     (km): 2.802354e+01

          Intercept found:
             Plate ID:                 324141
             Cartesian Coordinates:   0.27777518   1.57534131   9.07202903
             Latitudinal Coordinates:
             Longitude (deg): 80.000000
             Latitude  (deg): 80.000000
             Radius     (km): 9.211980e+00

             Ray vertex:
             Longitude (deg): 80.000000
             Latitude  (deg): 80.000000
             Radius     (km): 2.802354e+01

          Intercept found:
             Plate ID:                 327994
             Cartesian Coordinates:  -0.81082405   1.40438846   9.19682344
             Latitudinal Coordinates:
             Longitude (deg): 120.000000
             Latitude  (deg): 80.000000
             Radius     (km): 9.338699e+00

             Ray vertex:
             Longitude (deg): 120.000000
             Latitude  (deg): 80.000000
             Radius     (km): 2.802354e+01

          Intercept found:
             Plate ID:                 329431
             Cartesian Coordinates:  -1.47820193   0.53802150   8.92132122
             Latitudinal Coordinates:
             Longitude (deg): 160.000000
             Latitude  (deg): 80.000000
             Radius     (km): 9.058947e+00

             Ray vertex:
             Longitude (deg): 160.000000
             Latitude  (deg): 80.000000
             Radius     (km): 2.802354e+01

          Intercept found:
             Plate ID:                 196042
             Cartesian Coordinates:  -1.49854761  -0.54542673   9.04411256
             Latitudinal Coordinates:
             Longitude (deg): 200.000000
             Latitude  (deg): 80.000000
             Radius     (km): 9.183633e+00

             Ray vertex:
             Longitude (deg): 200.000000
             Latitude  (deg): 80.000000
             Radius     (km): 2.802354e+01

          Intercept found:
             Plate ID:                 235899
             Cartesian Coordinates:  -0.78240454  -1.35516441   8.87447325
             Latitudinal Coordinates:
             Longitude (deg): 240.000000
             Latitude  (deg): 80.000000
             Radius     (km): 9.011376e+00

             Ray vertex:
             Longitude (deg): 240.000000
             Latitude  (deg): 80.000000
             Radius     (km): 2.802354e+01

          [...]

          Warning: incomplete output. Only 100 out of 1135 lines have
          been provided.
#### Restrictions
       None.
#### Literature_References
       [1]  A. Woo, "Fast Ray-Box Intersection", Graphic Gems I,
            395-396, Aug. 1990
#### Author_and_Institution
       N.J. Bachman        (JPL)
       J.A. Bytof          (JPL)
       J. Diaz del Rio     (ODC Space)
       W.L. Taber          (JPL)
       E.D. Wright         (JPL)
#### Version
       -CSPICE Version 1.0.3, 07-AUG-2021 (JDR)

           Edited the header to comply with NAIF standard. Updated
           code example to remove unnecessary include files.

       -CSPICE Version 1.0.2, 04-APR-2017 (EDW)

           Edit to example program to use "%d" with explicit casts
           to int for printing SpiceInts with printf.

       -CSPICE Version 1.0.1, 20-JUL-2011 (NJB)

           Header correction: the detailed input section
           now says that the ray's vertex *is* required to
           be outside the target body.

       -CSPICE Version 1.0.0, 05-JUN-2010 (NJB) (EDW) (JAB) (WLT)
#### Index_Entries
       plate and plate model point intersected by ray
       intersection of ray and surface
#### Link to routine dskx02_c source file dskx02_c.c

    Fri Dec 31 18:41:05 2021