Index of Functions: A B C D E F G H I J K L M N O P Q R S T U V W X
Index Page srfs2c_c
Table of contents
Procedure Abstract Required_Reading Keywords Brief_I/O Detailed_Input | Detailed_Output Parameters Exceptions Files Particulars Examples | Restrictions Literature_References Author_and_Institution Version Index_Entries
#### Procedure
       srfs2c_c ( Surface and body strings to surface ID code )

       void srfs2c_c ( ConstSpiceChar  * srfstr,
                       ConstSpiceChar  * bodstr,
                       SpiceInt        * code,
                       SpiceBoolean    * found )
#### Abstract
       Translate a surface string, together with a body string, to the
       corresponding surface ID code. The input strings may contain
       names or integer ID codes.
#### Required_Reading
       DSK
       NAIF_IDS
#### Keywords
       CONVERSION
       DSK
       ID
       NAME
       STRING
       SURFACE
#### Brief_I/O
       VARIABLE  I/O  DESCRIPTION
       --------  ---  --------------------------------------------------
       srfstr     I   Surface name or ID string.
       bodstr     I   Body name or ID string.
       code       O   Integer surface ID code.
       found      O   Flag indicating whether surface ID was found.
#### Detailed_Input
       srfstr      is a string designating a surface. `srfstr' may contain
                   a surface name or a string representation of the
                   surface's integer ID code.

                   If, for the body specified by `bodstr', multiple surface
                   names are associated with one surface ID code, then any
                   of these names may be used as the value of `srfstr'.

                   Case and leading and trailing blanks in a surface name
                   are not significant. Sequences of consecutive embedded
                   blanks are considered equivalent to a single blank.
                   For example, all of the strings below are considered
                   to be equivalent:

                      "MGS MOLA 128 PIXEL/DEG"
                      "MGS MOLA 128 pixel/deg"
                      "MGS MOLA 128 PIXEL/DEG   "
                      "MGS MOLA 128    PIXEL/DEG"
                      "   MGS MOLA 128 PIXEL/DEG"

                   However,

                      "MGSMOLA 128PIXEL/DEG"

                   is not equivalent to the names above.

       bodstr      is a string designating the body associated with the
                   input surface string. `bodstr' may contain a body name
                   or a string representation of the body's integer ID
                   code. For example, `bodstr' may contain

                      "1000012"

                   instead of

                      "67P/CHURYUMOV-GERASIMENKO (1969 R1)"

                   Case and leading and trailing blanks in a name are not
                   significant. The treatment of blanks in `bodstr' is the
                   same as for `srfstr'.
#### Detailed_Output
       code        is integer ID code of the surface designated by
                   `srfstr', for the body designated by `bodstr', if for this
                   body an association exists between the input surface
                   string and a surface ID code. `code' is defined if and
                   only if the output flag `found' is SPICETRUE.

       found       is a logical flag that is SPICETRUE if a surface code
                   corresponding to the input strings was found and
                   SPICEFALSE otherwise.
#### Parameters
       None.
#### Exceptions
       1)  If the input surface string does not map to an ID code
           and does not represent an integer, the output `code' is
           undefined and the output `found' is set to SPICEFALSE.

           This case is not treated as an error.

       2)  If the input body string does not map to an ID code and does
           not represent an integer, the output `code' is undefined and
           the output `found' is set to SPICEFALSE.

           This case is not treated as an error.

       3)  If any of the `srfstr' or `bodstr' input string pointers is
           null, the error SPICE(NULLPOINTER) is signaled.

       4)  If any of the `srfstr' or `bodstr' input strings has zero
           length, the error SPICE(EMPTYSTRING) is signaled.
#### Files
       Surface name-to-ID mappings may be defined at run time by loading
       text kernels containing kernel variable assignments of the form

          NAIF_SURFACE_NAME += ( <surface name 1>, ... )
          NAIF_SURFACE_CODE += ( <surface code 1>, ... )
          NAIF_SURFACE_BODY += ( <body code 1>,    ... )

       Above, the Ith elements of the lists on the assignments' right
       hand sides together define the Ith surface name/ID mapping.

       The same effect can be achieved using assignments formatted as
       follows:

          NAIF_SURFACE_NAME += <surface name 1>
          NAIF_SURFACE_CODE += <surface code 1>
          NAIF_SURFACE_BODY += <body code 1>

          NAIF_SURFACE_NAME += <surface name 2>
          NAIF_SURFACE_CODE += <surface code 2>
          NAIF_SURFACE_BODY += <body code 2>

             ...

       Note the use of the

          +=

       operator; this operator appends to rather than overwrites the
       kernel variable named on the left hand side of the assignment.
#### Particulars
       Surfaces are always associated with bodies (which usually are
       ephemeris objects). For any given body, a mapping between surface
       names and surface ID codes can be established.

       Bodies serve to disambiguate surface names and ID codes: the set
       of surface names and surface ID codes for a given body can be
       thought of as belonging to a name space. A given surface ID code
       or surface name may be used for surfaces of multiple bodies,
       without conflict.

       Associations between surface names and ID codes are always made
       via kernel pool assignments; there are no built-in associations.

       srfs2c_c is one of four related functions:

          srfs2c_c      Surface string and body string to surface ID code
          srfscc_c      Surface string and body ID code to surface ID code
          srfc2s_c      Surface ID code and body ID code to surface string
          srfcss_c      Surface ID code and body string to surface string

       srfs2c_c, srfc2s_c, srfscc_c, and srfcss_c perform translations between
       surface strings and their corresponding integer ID codes.

       Refer to naif_ids.req for details concerning adding new surface
       name/code associations at run time by loading text kernels.
#### Examples
       The numerical results shown for this example may differ across
       platforms. The results depend on the SPICE kernels used as input,
       the compiler and supporting libraries, and the machine specific
       arithmetic implementation.

       1) Suppose a text kernel has been loaded that contains
          the following assignments:

             NAIF_SURFACE_NAME += ( 'MGS MOLA  64 pixel/deg',
                                    'MGS MOLA 128 pixel/deg',
                                    'PHOBOS GASKELL Q512'     )
             NAIF_SURFACE_CODE += (   1,   2,    1 )
             NAIF_SURFACE_BODY += ( 499, 499,  401 )

          Translate each surface and body string pair to the
          associated surface ID code. Also perform a translation
          for a surface name having no matching ID and for
          a body string having no matching body ID code.

          Use the meta-kernel shown below to define the required SPICE
          kernel variables.

             KPL/MK

             File: srfs2c_ex1.tm

             This meta-kernel is intended to support operation of SPICE
             example programs. The file contents shown here should not be
             assumed to contain adequate or correct versions of data
             required by SPICE-based user applications.

             \begindata

             NAIF_SURFACE_NAME += ( 'MGS MOLA  64 pixel/deg',
                                    'MGS MOLA 128 pixel/deg',
                                    'PHOBOS GASKELL Q512'     )
             NAIF_SURFACE_CODE += (   1,   2,    1 )
             NAIF_SURFACE_BODY += ( 499, 499,  401 )

             \begintext

             End of meta-kernel

          Example code begins here.

          /.
             Program srfs2c_ex1
          ./

          #include <stdio.h>
          #include "SpiceUsr.h"

          int main()
          {
             /.
             Local constants
             ./
             #define BDNMLN          37
             #define SFNMLN          SPICE_SRF_SFNMLN
             #define NCASE           8

             /.
             Local variables
             ./
             SpiceBoolean            found;

             static SpiceChar        bodstr [NCASE][BDNMLN] =

                                       { "MARS", "PHOBOS", "MARS",
                                         "499",  "PHOBOS", "499",
                                         "MARS", "ZZZ" };

             static SpiceChar        srfstr [NCASE][SFNMLN] =

                                       { "MGS MOLA  64 pixel/deg",
                                         "PHOBOS GASKELL Q512",
                                         "MGS MOLA 128 pixel/deg",
                                         "MGS MOLA  64 pixel/deg",
                                         "1",
                                         "2",
                                         "ZZZ",
                                         "1"                      };

             static SpiceChar        tf     [2][6] =

                                       { "false", "true" };

             SpiceChar             * meta;

             SpiceInt                i;
             SpiceInt                surfid;

             meta = "srfs2c_ex1.tm";

             furnsh_c ( meta );

             printf ( "\n" );

             for ( i = 0;  i < NCASE;  i++ )
             {
                srfs2c_c ( srfstr[i], bodstr[i], &surfid, &found );

                printf ( "surface string   = %s\n"
                         "body string      = %s\n"
                         "surface ID found = %s\n",
                         srfstr[i],
                         bodstr[i],
                         tf[found]                 );

                if ( found )
                {
                   printf ( "surface ID       = %d\n", surfid );
                }
                printf ( "\n" );
             }
             return ( 0 );
          }

          When this program was executed on a Mac/Intel/cc/64-bit
          platform, the output was:

          surface string   = MGS MOLA  64 pixel/deg
          body string      = MARS
          surface ID found = true
          surface ID       = 1

          surface string   = PHOBOS GASKELL Q512
          body string      = PHOBOS
          surface ID found = true
          surface ID       = 1

          surface string   = MGS MOLA 128 pixel/deg
          body string      = MARS
          surface ID found = true
          surface ID       = 2

          surface string   = MGS MOLA  64 pixel/deg
          body string      = 499
          surface ID found = true
          surface ID       = 1

          surface string   = 1
          body string      = PHOBOS
          surface ID found = true
          surface ID       = 1

          surface string   = 2
          body string      = 499
          surface ID found = true
          surface ID       = 2

          surface string   = ZZZ
          body string      = MARS
          surface ID found = false

          surface string   = 1
          body string      = ZZZ
          surface ID found = false
#### Restrictions
       None.
#### Literature_References
       None.
#### Author_and_Institution
       N.J. Bachman        (JPL)
       J. Diaz del Rio     (ODC Space)
       B.V. Semenov        (JPL)
       E.D. Wright         (JPL)
#### Version
       -CSPICE Version 1.0.1, 01-NOV-2021 (JDR) (NJB)

           Edited the header to comply with NAIF standard.

           Updated description of "srfstr" to indicate that any
           surface name alias may be used.

       -CSPICE Version 1.0.0, 22-JAN-2016 (NJB) (BVS) (EDW)
#### Index_Entries
       surface string and body string to surface ID code
#### Link to routine srfs2c_c source file srfs2c_c.c

    Fri Dec 31 18:41:13 2021