Index of Functions: A B C D E F G H I J K L M N O P Q R S T U V W X
Index Page srfrec_c
Table of contents
Procedure Abstract Required_Reading Keywords Brief_I/O Detailed_Input | Detailed_Output Parameters Exceptions Files Particulars Examples | Restrictions Literature_References Author_and_Institution Version Index_Entries
#### Procedure
       srfrec_c ( Surface to rectangular coordinates )

       void srfrec_c ( SpiceInt      body,
                       SpiceDouble   lon,
                       SpiceDouble   lat,
                       SpiceDouble   rectan[3] )
#### Abstract
       Convert planetocentric latitude and longitude of a surface
       point on a specified body to rectangular coordinates.
#### Required_Reading
       KERNEL
       NAIF_IDS
#### Keywords
       CONVERSION
       COORDINATES
       TRANSFORMATION
#### Brief_I/O
       VARIABLE  I/O  DESCRIPTION
       --------  ---  --------------------------------------------------
       body       I   NAIF integer code of an extended body.
       lon        I   Longitude of point in radians.
       lat        I   Latitude of point in radians.
       rectan     O   Rectangular coordinates of the point.
#### Detailed_Input
       body        is the NAIF integer code of an extended body on which
                   a surface point of interest is located. The body is
                   modeled as a triaxial ellipsoid.

       lon         is the longitude of the input point. This is the
                   angle between the prime meridian and the meridian
                   containing the point. The direction of increasing
                   longitude is from the +X axis towards the +Y axis.

                   Longitude is measured in radians. On input, the
                   range of longitude is unrestricted.

       lat         is the latitude of the input point. This is the angle
                   from the XY plane of the ray from the origin through
                   the point.

                   Latitude is measured in radians. On input, the range
                   of latitude is unrestricted.
#### Detailed_Output
       rectan      are the rectangular coordinates of the input surface point.
                   `rectan' is a 3-vector.

                   Units are the same as those used to define the radii of
                   `body'. Normally, these units are km.
#### Parameters
       None.
#### Exceptions
       1)  If radii for `body' are not found in the kernel pool, an error
           is signaled by a routine in the call tree of this routine.

       2)  If the size of the `body' body radii kernel variable is not
           three, an error is signaled by a routine in the call tree of
           this routine.

       3)  If any of the three `body' body radii is less-than or equal to
           zero, an error is signaled by a routine in the call tree of
           this routine.
#### Files
       None.
#### Particulars
       This routine returns the rectangular coordinates of a surface
       point on an extended body with known radii, where the location
       of the surface point is specified in planetocentric latitudinal
       coordinates.

       Latitudinal coordinates are defined by a distance from a central
       reference point, an angle from a reference meridian, and an angle
       above the equator of a sphere centered at the central reference
       point. In this case, the distance from the central reference
       point is not required as an input because the fact that the
       point is on the body's surface allows one to deduce this quantity.

       Below are two tables that demonstrate by example the relationship
       between rectangular and latitudinal coordinates.

       Listed in the first table (under R, `lon' and `lat') are
       latitudinal coordinate triples that approximately represent
       points whose rectangular coordinates are taken from the set
       {-1, 0, 1}.  (Angular quantities are given in degrees.)

            R          lon       lat    rectan[0]   rectan[1]  rectan[2]
           --------------------------   --------------------------------
           0.0000    0.0000    0.0000      0.0000      0.0000     0.0000
           1.0000    0.0000    0.0000      1.0000      0.0000     0.0000
           1.0000   90.0000    0.0000      0.0000      1.0000     0.0000
           1.0000    0.0000   90.0000      0.0000      0.0000     1.0000
           1.0000  180.0000    0.0000     -1.0000      0.0000     0.0000
           1.0000  -90.0000    0.0000      0.0000     -1.0000     0.0000
           1.0000    0.0000  -90.0000      0.0000      0.0000    -1.0000
           1.4142   45.0000    0.0000      1.0000      1.0000     0.0000
           1.4142    0.0000   45.0000      1.0000      0.0000     1.0000
           1.4142   90.0000   45.0000      0.0000      1.0000     1.0000
           1.7320   45.0000   35.2643      1.0000      1.0000     1.0000

       This routine is related to the CSPICE routine latrec_c, which
       accepts a radius, longitude, and latitude as inputs and produces
       equivalent rectangular coordinates as outputs.
#### Examples
       The numerical results shown for this example may differ across
       platforms. The results depend on the SPICE kernels used as
       input, the compiler and supporting libraries, and the machine
       specific arithmetic implementation.

       1) Find the rectangular coordinates of the point

             100 degrees planetocentric longitude
             -35 degrees planetocentric latitude

          on the Earth; then convert these coordinates back to
          latitudinal coordinates. We should be able to recover
          our original longitude and latitude values.

          Use the PCK kernel below to load the required triaxial
          ellipsoidal shape model and orientation data for the Earth.

             pck00008.tpc

          Example code begins here.

          /.
             Program srfrec_ex1
          ./

          #include <stdio.h>
          #include "SpiceUsr.h"

          int main()
          {

             #define  EARTH          399

             SpiceDouble             lat;
             SpiceDouble             lon;
             SpiceDouble             x      [3];
             SpiceDouble             radius;

             /.
             Load the kernel pool with a PCK file that contains
             values for the radii of the Earth.
             ./
             furnsh_c ( "pck00008.tpc" );

             /.
             Find `x', the rectangular coordinates of the surface point
             defined by `lat' and `long'.  The NAIF integer code for
             the Earth is 399. (See the NAIF_IDS required reading file
             for the complete set of codes.)
             ./
             lon   =  100.0;
             lat   =  -35.0;

             printf ( "Original latitudinal coordinates\n"
                      "\n"
                      "  Longitude (deg) =  %f\n"
                      "  Latitude  (deg) =  %f\n",
                      lon,
                      lat                                   );

             /.
             Convert angles to radians forr input to srfrec_c.
             ./
             srfrec_c ( EARTH, lon*rpd_c(), lat*rpd_c(), x );

             printf ( "\n"
                      "Rectangular coordinates\n"
                      "\n"
                      "  X (km)          =  %f\n"
                      "  Y (km)          =  %f\n"
                      "  Z (km)          =  %f\n",
                      x[0],
                      x[1],
                      x[2]                         );

             /.
             Now try to recover the original latitudinal coordinates
             from the rectangular coordinates found by srfrec_c.
             ./
             reclat_c ( x, &radius, &lon, &lat );

             /.
             Convert angles back to degree for display.
             ./
             printf ( "\n"
                      "Latitudinal coordinates recovered from "
                      "rectangular coordinates\n"
                      "\n"
                      "  Longitude (deg) =  %f\n"
                      "  Latitude  (deg) =  %f\n"
                      "  Radius    (km)  =  %f\n",
                      lon * dpr_c(),
                      lat * dpr_c(),
                      radius                       );

             return ( 0 );
          }

          When this program was executed on a Mac/Intel/cc/64-bit
          platform, the output was:

          Original latitudinal coordinates

            Longitude (deg) =  100.000000
            Latitude  (deg) =  -35.000000

          Rectangular coordinates

            X (km)          =  -906.249429
            Y (km)          =  5139.595909
            Z (km)          =  -3654.300840

          Latitudinal coordinates recovered from rectangular coordinates

            Longitude (deg) =  100.000000
            Latitude  (deg) =  -35.000000
            Radius    (km)  =  6371.079089
#### Restrictions
       1)  A PCK text kernel containing the body radius definitions
           required by this routine must be loaded into the kernel
           pool prior to any calls to this routine.
#### Literature_References
       None.
#### Author_and_Institution
       N.J. Bachman        (JPL)
       J. Diaz del Rio     (ODC Space)
       W.L. Taber          (JPL)
#### Version
       -CSPICE Version 1.1.0, 01-NOV-2021 (JDR)

           Changed the input argument names "longitude" and "latitude" by
           "lon and "lat" for consistency with other routines.

           Edited the header to comply with NAIF standard.

           Modified code example output format. Added solutions to the
           -Examples section.

       -CSPICE Version 1.0.0, 03-NOV-2005 (NJB) (WLT)
#### Index_Entries
       convert body-fixed latitudinal coordinates to rectangular
       convert surface latitudinal coordinates to rectangular
       surface point latitudinal coordinates to rectangular
#### Link to routine srfrec_c source file srfrec_c.c

    Fri Dec 31 18:41:13 2021