Index of Functions: A B C D E F G H I J K L M N O P Q R S T U V W X
Index Page llgrid_pl02
Table of contents
Procedure Abstract Required_Reading Keywords Brief_I/O Detailed_Input | Detailed_Output Parameters Exceptions Files Particulars Examples | Restrictions Literature_References Author_and_Institution Version Index_Entries
#### Procedure
       llgrid_pl02 ( Lon/lat grid using DSK type 2 plate model )

       void llgrid_pl02 ( SpiceInt               handle,
                          ConstSpiceDLADescr   * dladsc,
                          SpiceInt               npts,
                          ConstSpiceDouble       grid   [][2],
                          SpiceDouble            srfpts [][3],
                          SpiceInt               pltids []     )
#### Abstract
       Deprecated: This routine has been superseded by the CSPICE routine
       latsrf_c. This routine is supported for purposes of backward
       compatibility only.

       Given the planetocentric longitude and latitude values of a set of
       surface points on a specified target body, compute the corresponding
       rectangular coordinates of those points. The target body's
       surface is represented by a triangular plate model contained in a
       type 2 DSK segment.
#### Required_Reading
       FRAMES
       PCK
       SPK
       TIME
#### Keywords
       GEOMETRY
#### Brief_I/O
       VARIABLE  I/O  DESCRIPTION
       --------  ---  --------------------------------------------------
       handle     I   DSK handle.
       dladsc     I   DLA descriptor of target body segment.
       npts       I   Number of grid coordinate pairs.
       grid       I   Lon/lat values of surface points (radians).
       srfpts     O   Rectangular coordinates of surface points.
       pltids     O   DSK plate IDs of surface points.
#### Detailed_Input
       handle      is the DAS file handle of a DSK file open for read
                   access. This kernel must contain a type 2 segment
                   that provides a plate model representing the entire
                   surface of the target body.

       dladsc      is the DLA descriptor of a DSK segment representing
                   the surface of a target body.

       npts        is the number of longitude/latitude pairs in the array
                   of grid points `grid'.

       grid        is an array of planetocentric longitude/latitude pairs
                   to be mapped to surface points on the target body.
                   `grid' should be declared by the caller

                       SpiceDouble grid [npts][2];

                   Elements

                      grid[i][0]
                      grid[i][1]

                   are, respectively, the planetocentric longitude and
                   latitude of the ith grid point.

                   Units are radians.
#### Detailed_Output
       srfpts      is an array containing the rectangular (Cartesian)
                   coordinates of the surface points on the target body,
                   expressed relative to the body-fixed reference frame of
                   the target body, corresponding to the input grid points.

                   `srfpts' should be declared by the caller

                      SpiceDouble srfpts [npts][3];

       pltids      is an array of integer ID codes of the plates on which
                   the surface points are located. The ith plate ID
                   corresponds to the ith surface point. These ID codes can
                   be use to look up data associated with the plate, such
                   as the plate's vertices or outward normal vector.

                   `pltids' should be declared by the caller

                      SpiceInt pltids [npts];
#### Parameters
       None.
#### Exceptions
       If any of the listed errors occur, the output arguments are
       left unchanged.

       1)  If a DSK providing a DSK type 2 plate model has not been
           loaded prior to calling llgrid_pl02, an error is signaled by a
           routine in the call tree of this routine.

       2)  If the segment associated with the input DLA descriptor is not
           of data type 2, the error SPICE(WRONGDATATYPE) is signaled.

       3)  If a surface point cannot be computed because the ray corresponding
           to a longitude/latitude pair fails to intersect the target
           surface as defined by the plate model, the error
           SPICE(NOINTERCEPT) is signaled.
#### Files
       The following data are required:

       -  DSK data:  a DSK file containing a plate model representing the
          target body's surface must be loaded. This kernel must contain
          a type 2 segment that contains data for the entire surface of
          the target body.

       In all cases, kernel data are normally loaded once per program
       run, NOT every time this routine is called.
#### Particulars
       See the headers of the CSPICE routines

          reclat_c
          latrec_c

       for detailed definitions of Planetocentric coordinates.
#### Examples
       The numerical results shown for this example may differ across
       platforms. The results depend on the SPICE kernels used as input,
       the compiler and supporting libraries, and the machine specific
       arithmetic implementation.

       1) Find the surface points on a target body corresponding to a given
          planetocentric longitude/latitude grid.

          Use the DSK kernel below to provide the plate model representation
          of the surface of Phobos.

             phobos_3_3.bds

          Example code begins here.

          /.
             Program llgrid_pl02_ex1
          ./
          #include <stdio.h>
          #include <math.h>
          #include "SpiceUsr.h"

          int main()
          {
             /.
             Local parameters
             ./
             #define  FILSIZ         256
             #define  NAMLEN         33
             #define  NLAT           9
             #define  NLON           9
             #define  MAXGRID        ( NLAT * NLON )
             #define  TOL            ( 1.e-12 )

             /.
             Local variables
             ./
             SpiceBoolean            found;

             SpiceChar               dsk      [ FILSIZ ];

             SpiceDLADescr           dladsc;

             SpiceDouble             grid     [ MAXGRID ][2];
             SpiceDouble             lat;
             SpiceDouble             lon;
             SpiceDouble             srfpts  [ MAXGRID ][3];
             SpiceDouble             xlat;
             SpiceDouble             xlon;
             SpiceDouble             xr;

             SpiceInt                handle;
             SpiceInt                i;
             SpiceInt                j;
             SpiceInt                n;
             SpiceInt                npts;
             SpiceInt                pltids [ MAXGRID ];

             /.
             Prompt for the name of the DSK to read and the name of
             the target body.
             ./
             prompt_c ( "Enter DSK name    > ", FILSIZ, dsk    );

             /.
             Open the DSK file for read access.
             We use the DAS-level interface for
             this function.
             ./
             dasopr_c ( dsk, &handle );

             /.
             Begin a forward search through the
             kernel, treating the file as a DLA.
             In this example, it's a very short
             search.
             ./
             dlabfs_c ( handle, &dladsc, &found );

             if ( !found  )
             {
                /.
                We arrive here only if the kernel
                contains no segments.  This is
                unexpected, but we're prepared for it.
                ./
                setmsg_c ( "No segments found in DSK file #.");
                errch_c  ( "#",  dsk                         );
                sigerr_c ( "SPICE(NODATA)"                   );
             }

             /.
             If we made it this far, DLADSC is the
             DLA descriptor of the first segment.

             Now generate the grid points.  We generate
             points along latitude bands, working from
             north to south.  The latitude range is selected
             to range from +80 to -80 degrees.  Longitude
             ranges from 0 to 350 degrees.  The increment
             is 20 degrees for latitude and 40 degrees for
             longitude.
             ./

             n = 0;

             for ( i = 0;  i < NLAT;  i++  )
             {
                lat = rpd_c() * ( 80.0 - 20.0*i );

                for ( j = 0;  j < NLON;  j++  )
                {
                   lon = rpd_c() * 40.0*j;

                   grid[n][0] = lon;
                   grid[n][1] = lat;

                   ++n;
                }
             }
             npts = n - 1;

             /.
             Find the surface points corresponding to the grid points.
             ./
             llgrid_pl02 ( handle,
                           &dladsc,
                           npts,
                           (ConstSpiceDouble (*)[2])grid,
                           srfpts,
                           pltids                        );

             /.
             Print out the surface points in latitudinal
             coordinates and compare the derived lon/lat values
             to those of the input grid.
             ./
             for ( i = 0;  i < npts;  i++  )
             {
                /.
                Use recrad_c rather than reclat_c to produce
                non-negative longitudes.
                ./
                recrad_c ( srfpts[i], &xr, &xlon, &xlat );

                printf ( "\n"
                         "Intercept for grid point %d:\n"
                         "   Plate ID:                 %d\n"
                         "   Cartesian Coordinates:    (%e %e %e)\n"
                         "   Latitudinal Coordinates:\n"
                         "   Longitude (deg): %f\n"
                         "   Latitude  (deg): %f\n"
                         "   Radius     (km): %f\n"
                         "\n"
                         "Original grid coordinates:\n"
                         "   Longitude (deg): %f\n"
                         "   Latitude  (deg): %f\n"
                         "\n",
                         (int)i,
                         (int)pltids[i],
                         srfpts[i][0], srfpts[i][1], srfpts[i][2],
                         xlon * dpr_c(),
                         xlat * dpr_c(),
                         xr,
                         grid[i][0] * dpr_c(),
                         grid[i][1] * dpr_c()                         );

                /.
                Perform sanity checks on the intercept
                coordinates.  Stop the program if any error
                is larger than our tolerance value.
                ./
                lon = grid[i][0];
                lat = grid[i][1];

                if ( fabs(xlat-lat) > TOL )
                {
                   sigerr_c ( "Latitude error!" );
                }

                if (  (xlon - lon)  > pi_c()  )
                {
                   xlon -= twopi_c();
                }

                if (  (xlon - lon)  > TOL  )
                {
                   sigerr_c ( "Longitude error!" );
                }

             }

             /.
             Close the kernel.  This isn't necessary in a stand-
             alone program, but it's good practice in subroutines
             because it frees program and system resources.
             ./
             dascls_c ( handle );

             return ( 0 );
          }

          When this program was executed on a Mac/Intel/cc/64-bit
          platform, using the DSK file named phobos_3_3.bds, the output
          was:

          Enter DSK name    > phobos_3_3.bds

          Intercept for grid point 0:
             Plate ID:                 306238
             Cartesian Coordinates:    (1.520878e+00 0.000000e+00 8.625327e+00)
             Latitudinal Coordinates:
             Longitude (deg): 0.000000
             Latitude  (deg): 80.000000
             Radius     (km): 8.758387

          Original grid coordinates:
             Longitude (deg): 0.000000
             Latitude  (deg): 80.000000

          Intercept for grid point 1:
             Plate ID:                 317112
             Cartesian Coordinates:    (1.189704e+00 9.982799e-01 8.807772e+00)
             Latitudinal Coordinates:
             Longitude (deg): 40.000000
             Latitude  (deg): 80.000000
             Radius     (km): 8.943646

          Original grid coordinates:
             Longitude (deg): 40.000000
             Latitude  (deg): 80.000000

          Intercept for grid point 2:
             Plate ID:                 324141
             Cartesian Coordinates:    (2.777752e-01 1.575341e+00 9.072029e+00)
             Latitudinal Coordinates:
             Longitude (deg): 80.000000
             Latitude  (deg): 80.000000
             Radius     (km): 9.211980

          Original grid coordinates:
             Longitude (deg): 80.000000
             Latitude  (deg): 80.000000

          Intercept for grid point 3:
             Plate ID:                 327994
             Cartesian Coordinates:    (-8.108241e-01 1.404388e+00 9.196823e+00)
             Latitudinal Coordinates:
             Longitude (deg): 120.000000
             Latitude  (deg): 80.000000
             Radius     (km): 9.338699

          Original grid coordinates:
             Longitude (deg): 120.000000
             Latitude  (deg): 80.000000

          Intercept for grid point 4:
             Plate ID:                 329431
             Cartesian Coordinates:    (-1.478202e+00 5.380215e-01 8.921321e+00)
             Latitudinal Coordinates:
             Longitude (deg): 160.000000
             Latitude  (deg): 80.000000
             Radius     (km): 9.058947

          Original grid coordinates:
             Longitude (deg): 160.000000
             Latitude  (deg): 80.000000

          Intercept for grid point 5:
             Plate ID:                 196042
             Cartesian Coordinates:    (-1.498548e+00 -5.454267e-01 9.044113e+00)
             Latitudinal Coordinates:
             Longitude (deg): 200.000000
             Latitude  (deg): 80.000000
             Radius     (km): 9.183633

          Original grid coordinates:
             Longitude (deg): 200.000000
             Latitude  (deg): 80.000000

          Intercept for grid point 6:
             Plate ID:                 235899
             Cartesian Coordinates:    (-7.824045e-01 -1.355164e+00 8.874473e+00)
             Latitudinal Coordinates:
             Longitude (deg): 240.000000
             Latitude  (deg): 80.000000
             Radius     (km): 9.011376

          Original grid coordinates:
             Longitude (deg): 240.000000
             Latitude  (deg): 80.000000

          Intercept for grid point 7:
             Plate ID:                 266998
             Cartesian Coordinates:    (2.645121e-01 -1.500123e+00 8.638862e+00)
             Latitudinal Coordinates:
             Longitude (deg): 280.000000
             Latitude  (deg): 80.000000
             Radius     (km): 8.772130

          [...]

          Warning: incomplete output. Only 100 out of 1041 lines have
          been provided.
#### Restrictions
       1)  This routine assumes that the origin of the body-fixed reference
           frame associated with the target body is located in the interior
           of that body.

       2)  The results returned by this routine may not be meaningful
           if the target surface has multiple surface points associated
           with some (longitude, latitude) coordinates.
#### Literature_References
       None.
#### Author_and_Institution
       N.J. Bachman        (JPL)
       J. Diaz del Rio     (ODC Space)
       B.V. Semenov        (JPL)
#### Version
       -CSPICE Version 2.1.0, 26-OCT-2021 (JDR)

           Changed argument names "npoints", "spoints" and "plateIDs" to
           "npts", "srfpts" and "pltids" for consistency with other routines.

           Edited the header to comply with NAIF standard.

           Index lines now state that this routine is deprecated.

       -CSPICE Version 2.0.0, 23-JUL-2016 (NJB) (BVS)

           Added failed_c calls.

           Include file references have been updated. Now calls
           zzdsksgr_ instead of dsksgr_. Integer output format
           in example program has been updated.

        Beta Version 1.3.0, 30-APR-2014 (NJB) (BVS)

           Now includes dsk_proto.h.

           Last update was 1.2.1, 07-APR-2014 (BVS)

           Changed FRAME to FRAMES in the Required_Reading section.

        Beta Version 1.2.0, 14-MAY-2010 (NJB)

           Updated for compatibility with new DSK design.
           DSK name was updated in example program.

        Beta Version 1.1.0, 09-FEB-2007 (NJB)

           Bug fix: type of local variable fDLADescr was changed to SpiceInt.

        Beta Version 1.0.0, 06-NOV-2006 (NJB)
#### Index_Entries
       DEPRECATED map latitudinal grid to DSK type 2 plate model
#### Link to routine llgrid_pl02 source file llgrid_pl02.c

    Fri Dec 31 18:41:09 2021