Index of Functions: A B C D E F G H I J K L M N O P Q R S T U V W X
Index Page erract_c
Table of contents
Procedure Abstract Required_Reading Keywords Brief_I/O Detailed_Input | Detailed_Output Parameters Exceptions Files Particulars Examples | Restrictions Literature_References Author_and_Institution Version Index_Entries
#### Procedure
       erract_c ( Get/Set Default Error Action )

       void erract_c ( ConstSpiceChar * op,
                       SpiceInt         actlen,
                       SpiceChar      * action )
#### Abstract
       Retrieve or set the default error action.
#### Required_Reading
       ERROR
#### Keywords
       ERROR
#### Brief_I/O
       VARIABLE  I/O  DESCRIPTION
       --------  ---  --------------------------------------------------
       op         I   Operation -- "GET" or "SET".
       actlen     I   Length of list for output.
       action    I-O  Error response action.
#### Detailed_Input
       op          indicates the operation -- "GET" or "SET".  "GET" means,
                   "Set action to the current value of the error response
                   action."  "SET" means, "update the error response action to
                   the value indicated by action."

                   `op' may be in mixed case; for example,

                      erract_c ( "gEt", actlen, action );

                   will work.

       actlen      is the string size of output `action' when op equals "GET".
                   The size described by `actlen' should be large enough to
                   hold all characters of any possible output string
                   plus 1 (to accommodate the C null terminator).

       action      is an input argument when `op' is "SET." It takes the
                   values,  "ABORT",  "IGNORE", "REPORT", "RETURN", and
                   "DEFAULT".

                   Briefly, the meanings of the error response
                   choices are as follows:

                   1.  "ABORT"  --  When an error is detected by a
                                    CSPICE routine, or when
                                    ANY routine signals detection
                       of an error via a call to sigerr_c, the
                       toolkit will output any error messages that
                       it has been enabled to output (see errprt_c
                       and errdev_c also ), and then execute an
                       exit statement.

                   2.  "REPORT" --  In this mode, the toolkit does
                                    NOT abort when errors are detected.
                                    When sigerr_c is called to report
                       an error, all error messages that the toolkit
                       is enabled to output will be sent to the
                       designated error output device. Similarly,
                       a call to setmsg_c will result in the long
                       error message being output, if the toolkit
                       is enabled to output it.

                   3.  "RETURN" --  In this mode, the toolkit also
                                    does NOT abort when errors are
                                    detected. Instead, error messages
                       are output if the toolkit is enabled to do
                       so, and subsequently, ALL TOOLKIT ROUTINES
                       RETURN IMMEDIATELY UPON ENTRY until the
                       error status is reset via a call to RESET.
                       (No, RESET itself doesn't return on entry).
                       Resetting the error status will cause the
                       toolkit routines to resume their normal
                       execution threads.

                   4.  "IGNORE" --  The toolkit will not take any
                                    action in response to errors;
                                    calls to sigerr_c will have no
                                    effect.

                   5.  "DEFAULT" -- This mode is the same as "ABORT",
                                    except that an additional error
                                    message is output. The additional
                                    message informs the user that the
                                    error response action can be
                                    modified, and refers to documentation
                                    of the error handling feature.

                   `action' may be in mixed case; for example,

                       erract_c ( "SET", actlen, "igNORe" );

                   will work.
#### Detailed_Output
       action      is an output argument returning the current error
                   response action when `op' equals "GET". Possible values
                   are:  "ABORT", "REPORT", "RETURN", and "IGNORE".
                   See "Detailed Input" for descriptions of these values.
#### Parameters
       None.
#### Exceptions
       1)  If an invalid value of the operation `op' is supplied, the error
           SPICE(INVALIDOPERATION) is signaled.

       2)  If `op' is "SET" and the input argument `action' does not indicate
           a valid error handling action, the error SPICE(INVALIDACTION)
           is signaled by a routine in the call tree of this routine.

       3)  If the `op' input string pointer is null, the error
           SPICE(NULLPOINTER) is signaled.

       4)  If the `op' input string has zero length, the error
           SPICE(EMPTYSTRING) is signaled, since the input string cannot
           be converted to a Fortran-style string in this case.

       5)  If the `action' string pointer is null, the error SPICE(NULLPOINTER) is
           signaled.

       6)  If `op' is "SET" and the `action' string has zero length, the error
           SPICE(EMPTYSTRING) is signaled, since the input string cannot
           be converted to a Fortran-style string in this case.

       7)  If `op is "GET" and the `action' string has length less than
           two characters, the error SPICE(STRINGTOOSHORT) is signaled,
           since the output string is too short to contain one character
           of output data plus a null terminator, and therefore it cannot
           be passed to the underlying Fortran routine.
#### Files
       None.
#### Particulars
       As indicated in the "detailed input" section above, the choices for
       the Toolkit's error handling action are designated by the strings
       "ABORT", "REPORT", "RETURN", "IGNORE", and "DEFAULT".  These
       choices control the way the toolkit behaves when an error is
       detected. The toolkit thinks an error has been detected when
       sigerr_c is called.

       1.  "ABORT"   In this mode, the toolkit sends error messages
            to the error output device and then stops.
            This is the default mode. It is probably
            the one to choose for running non-interactive programs.
            You may also wish to use this for programs which
            have many bugs, or in other cases where continued
            operation following detection of an error isn't useful.

       2.  "REPORT"  In this mode, the toolkit sends error messages
            to the error output device and keeps going. This mode
            may be useful if you are debugging a large program,
            since you can get more information from a single test run.
            You will probably want to use errdev_c to indicate a file
            where your error messages should be sent.

       3.  "RETURN"  In this mode, the toolkit also sends error messages
            to the error output device and "keeps going".  But
            instead of following their normal execution threads,
            the toolkit routines will simply return immediately upon
            entry, once an error has been detected.
            The availability of this feature makes it safe to call
            multiple toolkit routines without checking the error
            status after each one returns; if one routine detects
            an error, subsequent calls to toolkit routines will have
            no effect; therefore, no crash will occur. The error
            messages set by the routine which detected the error
            will remain available for retrieval by getmsg_.

       4.   "IGNORE"  This mode can be dangerous!  It is best
            used when running a program whose behavior you
            understand well, in cases where you wish to suppress
            annoying messages.  BUT, if an unexpected error
            occurs, you won't hear about it from anyone, except
            possibly your run-time system.

       5.  "DEFAULT"  As the name suggests, this is the default
            error handling mode. The error handling mechanism
            starts out in this mode when a program using the
            toolkit is run, and the mode remains "DEFAULT" until
            it is changed via a call to this routine.
            This mode is the same as "ABORT",
            except that an additional error message is output.
            The additional message informs the user that the
            error response action can be modified, and refers
            to documentation of the error handling feature.

       NOTE:

            By default, error messages are printed to the screen
            when errors are detected. You may want to send them
            to a different output device, or choose a subset to
            output. Use the routines errdev_c and errprt_c to choose
            the output device and select the messages to output,
            respectively.

            You can also suppress the automatic output of messages
            and retrieve them directly in your own program. getmsg_
            can be used for this. To make sure that the messages
            retrieved correspond to the FIRST error that occurred,
            use "RETURN" mode. In "REPORT" mode, new messages
            overwrite old ones in the CSPICE message storage
            area, so getmsg_ will get the messages from the LATEST
            error that occurred.
#### Examples
       1. Setting up "ABORT" mode:

              /.
              We wish to have our program abort if an error
              is detected. But instead of having the error
              messages printed on the screen, we want them
              to be written to the file, ERROR_LOG.TXT

              We want to see all of the messages, so we
              call errprt_c, using the "ALL" option.

              Finally, we call erract_c to set the action to "ABORT":
              ./

              errdev_c ( "SET", actlen, "ERROR_LOG.DAT" );

              errprt_c ( "SET", actlen, "ALL" );

              erract_c ( "SET", actlen, "ABORT" );

       2. Setting up "REPORT" mode:

              errdev_c ( "SET", actlen, "ERROR_LOG.DAT" );

              errprt_c ( "SET", actlen, "ALL"  );

              erract_c ( "SET", actlen, "REPORT" );

       3. Setting up "RETURN" mode: This is the same
           as example #2, except that the erract_c call becomes:

              erract_c ( "SET", actlen, "RETURN" );

       4. Setting up "IGNORE" mode:

              /.
              In this case, we aren't going to have
              ANY error messages (unless the call
              to erract_c itself fails), so we don't
              really need to call errprt_c and errdev_c.
              (If the call to erract_c DOES fail, which
              it can do only if we misspell "IGNORE,"
              the resulting error messages will go to
              the screen).
              ./

              erract_c ( "SET", actlen, "IGNORE" );
#### Restrictions
       None.
#### Literature_References
       None.
#### Author_and_Institution
       N.J. Bachman        (JPL)
       J. Diaz del Rio     (ODC Space)
       E.D. Wright         (JPL)
#### Version
       -CSPICE Version 1.4.0, 10-AUG-2021 (JDR)

           Changed the input argument name "lenout" to "actlen" for consistency
           with other routines.

           Edited the header to comply with NAIF standard.

       -CSPICE Version 1.3.1, 25-SEP-2003 (EDW)

           Corrected confusing description of 'actlen' argument.

       -CSPICE Version 1.3.0, 24-JUN-2003 (NJB)

           Bug fix: case of invalid operation keyword is now
           diagnosed, as per the -Exceptions section of the header.

       -CSPICE Version 1.2.0, 09-FEB-1998 (NJB)

           Re-implemented routine without dynamically allocated, temporary
           strings. Made various header fixes.

       -CSPICE Version 1.0.1, 30-OCT-1997 (EDW)

           Corrected errors in examples in which the call sequence
           was incorrect.

       -CSPICE Version 1.0.0, 25-OCT-1997 (EDW)
#### Index_Entries
       get/set default error action
#### Link to routine erract_c source file erract_c.c

    Fri Dec 31 18:41:06 2021