# Software Information
display_name = "Commodore - Amiga (UAE4ARM)"
categories = "Emulator"
authors = "TomB/Chips-fr"
supported_extensions = "adf|dms|ipf|adz|wrp|zip|uae|lha|cue|ccd|iso|hdf"
corename = "UAE4ARM"
categories = "Emulator"
license = "GPLv2"
permissions = ""
display_version = "v0.5"

# Hardware Information
manufacturer = "Commodore"
systemname = "Amiga"
systemid = "commodore_amiga"

# Libretro Features
database = "Commodore - Amiga|Commodore - CD32|Commodore - CDTV"
supports_no_game = "false"
savestate = "true"
savestate_features = "serialized"

# Firmware / BIOS
firmware_count = 6
firmware0_desc = "kick34005.A500 (Amiga 500 BIOS, Kickstart v1.3 Rev. 34.005)"
firmware0_path = "kick34005.A500"
firmware0_opt = "false"
firmware1_desc = "kick40063.A600 (Amiga 600 BIOS, Kickstart v3.1 Rev. 40.063)"
firmware1_path = "kick40063.A600"
firmware1_opt = "false"
firmware2_desc = "kick40068.A1200 (Amiga 1200 BIOS, Kickstart v3.1 Rev. 40.068)"
firmware2_path = "kick40068.A1200"
firmware2_opt = "false"
firmware3_desc = "kick34005.CDTV (Amiga CDTV extended ROM v1.00 Rev. 34.005)"
firmware3_path = "kick34005.CDTV"
firmware3_opt = "false"
firmware4_desc = "kick40060.CD32 (Amiga CD32 BIOS, Kickstart v3.1 Rev. 40.060)"
firmware4_path = "kick40060.CD32"
firmware4_opt = "false"
firmware5_desc = "kick40060.CD32.ext (Amiga CD32 Extended BIOS, CD32 Extended ROM Rev. 40.060)"
firmware5_path = "kick40060.CD32.ext"
firmware5_opt = "false"

description = "An old fork of the uae4arm Amiga emulator, ported to libretro. This core is intended only for use on very weak, low-powered hardware and should only be used in cases where the P-UAE core is not available or cannot maintain full speed."
