# Software Information
display_name = "Commodore - CBM-II 5x0 (VICE xcbm5x0)"
categories = "Emulator"
authors = "VICE Team"
corename = "VICE xcbm5x0"
supported_extensions = "d64|d71|d80|d81|d82|g64|g41|x64|t64|tap|prg|p00|crt|bin|zip|gz|d6z|d7z|d8z|g6z|g4z|x6z|cmd|m3u|vfl|vsf|nib|nbz|d2m|d4m"
license = "GPLv2"
permissions = ""
display_version = "3.7"

# Hardware Information
manufacturer = "Commodore"
systemname = "CBM-5x0"
systemid = "commodore_cbm5x0"

# Libretro Features
database = "Commodore - CBM-5x0"
supports_no_game = "true"
savestate = "true"
savestate_features = "serialized"
cheats = "true"
input_descriptors = "true"
memory_descriptors = "true"
libretro_saves = "true"
core_options = "true"
load_subsystem = "false"
hw_render = "false"
needs_fullpath = "true"
disk_control = "true"
is_experimental = "false"

description = "The VICE xcbm5x0 emulator, isolated and ported to libretro. This core provides experimental emulation for the C510 model (also known as P500) of CBM-II, which is the 'little brother' of the C600/700 machines. It runs at roughly 1 MHz and use a VIC-II chip instead of the CRTC."
