# Software Information
display_name = "Nintendo - SNES / SFC (bsnes-hd beta)"
categories = "Emulator"
authors = "Near|DerKoun"
corename = "bsnes-hd beta"
supported_extensions = "smc|sfc|swc|fig|gb|gbc|bs"
license = "GPLv3"
permissions = ""
display_version = "v112.v12"

# Hardware Information
manufacturer = "Nintendo"
systemname = "Super Nintendo Entertainment System"
systemid = "super_nes"

# BIOS / Firmware
firmware_count = 19
firmware0_desc = "dsp1.data.rom"
firmware0_path = "dsp1.data.rom"
firmware0_opt = "true"
firmware1_desc = "dsp1.program.rom"
firmware1_path = "dsp1.program.rom"
firmware1_opt = "true"
firmware2_desc = "dsp1b.data.rom"
firmware2_path = "dsp1b.data.rom"
firmware2_opt = "true"
firmware3_desc = "dsp1b.program.rom"
firmware3_path = "dsp1b.program.rom"
firmware3_opt = "true"
firmware4_desc = "dsp2.data.rom"
firmware4_path = "dsp2.data.rom"
firmware4_opt = "true"
firmware5_desc = "dsp2.program.rom"
firmware5_path = "dsp2.program.rom"
firmware5_opt = "true"
firmware6_desc = "dsp3.data.rom"
firmware6_path = "dsp3.data.rom"
firmware6_opt = "true"
firmware7_desc = "dsp3.program.rom"
firmware7_path = "dsp3.program.rom"
firmware7_opt = "true"
firmware8_desc = "dsp4.data.rom"
firmware8_path = "dsp4.data.rom"
firmware8_opt = "true"
firmware9_desc = "dsp4.program.rom"
firmware9_path = "dsp4.program.rom"
firmware9_opt = "true"
firmware10_desc = "cx4.data.rom"
firmware10_path = "cx4.data.rom"
firmware10_opt = "true"
firmware11_desc = "st010.data.rom"
firmware11_path = "st010.data.rom"
firmware11_opt = "true"
firmware12_desc = "st010.program.rom"
firmware12_path = "st010.program.rom"
firmware12_opt = "true"
firmware13_desc = "st011.data.rom"
firmware13_path = "st011.data.rom"
firmware13_opt = "true"
firmware14_desc = "st011.program.rom"
firmware14_path = "st011.program.rom"
firmware14_opt = "true"
firmware15_desc = "st018.data.rom"
firmware15_path = "st018.data.rom"
firmware15_opt = "true"
firmware16_desc = "st018.program.rom"
firmware16_path = "st018.program.rom"
firmware16_opt = "true"
firmware17_desc = "SGB1.sfc (SGB Boot Image)"
firmware17_path = "SGB1.sfc"
firmware17_opt = "true"
firmware18_desc = "SGB2.sfc (SGB Boot Image)"
firmware18_path = "SGB2.sfc"
firmware18_opt = "true"
notes = "[1] bsnes uses split ROMS for special chip games.|[*] Notable DSP1/DSP1B Games: Super Mario Kart,  Pilotwings|[*] Notable DSP2 Games: Dungeon Master|[*] Notable DSP3 Games: SD Gundam GX|[*] Notable DSP4 Games: Top Gear 3000|[*] Notable Cx4 Games: Mega Man X2,  Mega Man X3|[2] SGB Emulation needs No-Intro Super Game Boy ROMs renamed to SGB1.sfc or SGB2.sfc|(!) SGB1.sfc (md5): b15ddb15721c657d82c5bab6db982ee9|(!) SGB2.sfc (md5): 8ecd73eb4edf7ed7e81aef1be80031d5"

# Libretro Features
savestate = "true"
savestate_features = "serialized"
cheats = "false"
input_descriptors = "true"
memory_descriptors = "false"
libretro_saves = "true"
core_options = "true"
core_options_version = "1.0"
load_subsystem = "true"
supports_no_game = "false"
database = "Nintendo - Super Nintendo Entertainment System|Nintendo - Sufami Turbo|Nintendo - Satellaview"
hw_render = "false"
needs_fullpath = "false"
disk_control = "false"

description = "bsnes HD Beta is based on the latest code from the bsnes emulator, but it serves as a test-bed for some additional features that are not considered stable enough for inclusion in the standard bsnes core. These features include true widescreen support and increased color depth (i.e., without dithering), among others. Aside from these additional experimental features, this core is identical to the standard bsnes core in both accuracy and performance (and libretro features/limitations)."
