# Software Information
display_name = "The 3DO Company - 3DO (Opera)"
authors = "trapexit|JohnnyDude|FreeDO team"
supported_extensions = "iso|bin|chd|cue"
corename = "Opera"
categories = "Emulator"
license = "LGPL/Non-commercial"
permissions = ""
display_version = "1.0.0"

# Hardware Information
manufacturer = "Panasonic|GoldStar|Sanyo"
systemname = "3DO"
systemid = "3do"

# Libretro Features
database = "The 3DO Company - 3DO"
supports_no_game = "true"
savestate = "true"
savestate_features = "basic"
cheats = "false"
input_descriptors = "true"
memory_descriptors = "false"
libretro_saves = "true"
core_options = "true"
load_subsystem = "false"
hw_render = "false"
needs_fullpath = "true"
disk_control = "false"
is_experimental = "false"

# BIOS/Firmware
firmware_count = 13

firmware0_desc = "panafz1.bin (Panasonic FZ-1 BIOS)"
firmware0_path = "panafz1.bin"
firmware0_opt = "true"

firmware1_desc = "panafz10.bin (Panasonic FZ-10 BIOS)"
firmware1_path = "panafz10.bin"
firmware1_opt = "true"

firmware2_desc = "panafz10-norsa.bin (Panasonic FZ-10 BIOS [Encryption Check Disabled])"
firmware2_path = "panafz10-norsa.bin"
firmware2_opt = "true"

firmware3_desc = "panafz10e-anvil.bin (Panasonic FZ-10E ANVIL BIOS)"
firmware3_path = "panafz10e-anvil.bin"
firmware3_opt = "true"

firmware4_desc = "panafz10e-anvil-norsa.bin (Panasonic FZ-10E ANVIL BIOS [Encryption Check Disabled])"
firmware4_path = "panafz10e-anvil-norsa.bin"
firmware4_opt = "true"

firmware5_desc = "goldstar.bin (Goldstar GDO-101M BIOS)"
firmware5_path = "goldstar.bin"
firmware5_opt = "true"

firmware6_desc = "sanyotry.bin (Sanyo Try IMP-21J BIOS)"
firmware6_path = "sanyotry.bin"
firmware6_opt = "true"

firmware7_desc = "3do_arcade_saot.bin (Shootout At Old Tucson BIOS)"
firmware7_path = "3do_arcade_saot.bin"
firmware7_opt = "true"

firmware8_desc = "panafz1-kanji.bin (Panasonic FZ-1 Kanji Font ROM)"
firmware8_path = "panafz1-kanji.bin"
firmware8_opt = "true"

firmware9_desc = "panafz10ja-anvil-kanji.bin (Panasonic FZ-10JA Kanji Font ROM)"
firmware9_path = "panafz10ja-anvil-kanji.bin"
firmware9_opt = "true"

firmware10_desc = "panafz1j.bin (Panasonic FZ-1J BIOS)"
firmware10_path = "panafz1j.bin"
firmware10_opt = "true"

firmware11_desc = "panafz1j-norsa.bin (Panasonic FZ-1J BIOS [Encryption Check Disabled])"
firmware11_path = "panafz1j-norsa.bin"
firmware11_opt = "true"

firmware12_desc = "panafz1j-kanji.bin (Panasonic FZ-1J Kanji Font ROM)"
firmware12_path = "panafz1j-kanji.bin"
firmware12_opt = "true"

notes = "(!) panafz1.bin (md5): f47264dd47fe30f73ab3c010015c155b|(!) panafz10.bin (md5): 51f2f43ae2f3508a14d9f56597e2d3ce|(!) panafz10-norsa.bin (md5): 1477bda80dc33731a65468c1f5bcbee9|(!) panafz10e-anvil.bin (md5): a48e6746bd7edec0f40cff078f0bb19f|(!) panafz10e-anvil-norsa.bin (md5): cf11bbb5a16d7af9875cca9de9a15e09|(!) goldstar.bin (md5): 8639fd5e549bd6238cfee79e3e749114|(!) sanyotry.bin (md5): 35fa1a1ebaaeea286dc5cd15487c13ea|(!) 3do_arcade_saot.bin (md5): 8970fc987ab89a7f64da9f8a8c4333ff|(!) panafz1-kanji.bin (md5): b8dc97f778a6245c58e064b0312e8281|(!) panafz10ja-anvil-kanji.bin (md5): 428577250f43edc902ea239c50d2240d|(!) panafz1j.bin (md5): a496cfdded3da562759be3561317b605|(!) panafz1j-norsa.bin (md5): f6c71de7470d16abe4f71b1444883dc8|(!) panafz1j-kanji.bin (md5): c23fb5d5e6bb1c240d02cf968972be37"

description = "A port and continuation of the 4DO emulator, which itself is a fork of the FreeDO 3DO emulator, to libretro. This core is the best option for users seeking to play 3DO games, as it is the only one still under development."
