# Software Information
display_name = "Commodore - C64 (VICE x64, fast)"
categories = "Emulator"
authors = "VICE Team"
corename = "VICE x64"
supported_extensions = "d64|d71|d80|d81|d82|g64|g41|x64|t64|tap|prg|p00|crt|bin|zip|gz|d6z|d7z|d8z|g6z|g4z|x6z|cmd|m3u|vfl|vsf|nib|nbz|d2m|d4m"
license = "GPLv2"
permissions = ""
display_version = "3.7"

# Hardware Information
manufacturer = "Commodore"
systemname = "C64"
systemid = "commodore_c64"

# Libretro Features
database = "Commodore - 64"
supports_no_game = "true"
savestate = "true"
savestate_features = "serialized"
cheats = "true"
input_descriptors = "true"
memory_descriptors = "true"
libretro_saves = "true"
core_options = "true"
load_subsystem = "false"
hw_render = "false"
needs_fullpath = "true"
disk_control = "true"
is_experimental = "false"

# Firmware
firmware_count = 4
firmware0_desc = "vice/JiffyDOS_C64.bin (JiffyDOS C64 Kernal)"
firmware0_path = "vice/JiffyDOS_C64.bin"
firmware0_opt = "true"
firmware1_desc = "vice/JiffyDOS_1541-II.bin (JiffyDOS 1541 drive BIOS)"
firmware1_path = "vice/JiffyDOS_1541-II.bin"
firmware1_opt = "true"
firmware2_desc = "vice/JiffyDOS_1571_repl310654.bin (JiffyDOS 1571 drive BIOS)"
firmware2_path = "vice/JiffyDOS_1571_repl310654.bin"
firmware2_opt = "true"
firmware3_desc = "vice/JiffyDOS_1581.bin (JiffyDOS 1581 drive BIOS)"
firmware3_path = "vice/JiffyDOS_1581.bin"
firmware3_opt = "true"
notes = "(!) JiffyDOS_C64.bin (md5): be09394f0576cf81fa8bacf634daf9a2|(!) JiffyDOS_1541-II.bin (md5): 1b1e985ea5325a1f46eb7fd9681707bf|(!) JiffyDOS_1571_repl310654.bin (md5): 41c6cc528e9515ffd0ed9b180f8467c0|(!) JiffyDOS_1581.bin (md5): 20b6885c6dc2d42c38754a365b043d71"

description = "The VICE x64 (fast) Commodore 64 emulator, isolated and ported to libretro. This core features a fairly complete emulation of the VIC-II video chip, with all sprites, registers and video modes emulated in a fully cycle-accurate manner. However, the 'x64sc' core's VIC-II emulation is both cycle-based and pixel-accurate, making it a better choice for devices powerful enough to run it. Both cores include options to switch between the original 'fastSID' sound chip emulation and the slower but much more accurate 'reSID' module."
