# Software Information
display_name = "MSX/SVI/ColecoVision/SG-1000 (blueMSX)"
authors = "Daniel Vik"
supported_extensions = "rom|ri|mx1|mx2|col|dsk|cas|sg|sc|sf|m3u"
corename = "blueMSX"
categories = "Emulator"
license = "GPLv2"
permissions = ""
display_version = "SVN"

# Hardware Information
manufacturer = "Spectravideo|Philips|Al Alamiah|Sony|Sanyo|Mitsubishi|Toshiba|Hitachi|Panasonic|Canon|Casio|Pioneer|Fujitsu|Yamaha|JVC|Kyocera|GoldStar|Samsung|Daewoo|Gradiente|Sharp|Talent|NTT|ACVS/CIEL|DDX|AGE Labs"
systemname = "MSX/SVI/ColecoVision/SG-1000"
systemid = "msx"

# Libretro Features
database = "Microsoft - MSX|Microsoft - MSX2|Coleco - ColecoVision|Sega - SG-1000|Spectravideo - SVI-318 - SVI-328"
supports_no_game = "false"
savestate = "true"
savestate_features = "serialized"
cheats = "false"
input_descriptors = "true"
memory_descriptors = "false"
libretro_saves = "false"
core_options = "true"
core_options_version = "1.0"
load_subsystem = "false"
hw_render = "false"
needs_fullpath = "true"
disk_control = "true"
is_experimental = "false"
needs_kbd_mouse_focus = "true"

# BIOS/Firmware
firmware_count = 2
firmware0_desc = "'Databases' folder"
firmware0_path = "Databases/msxromdb.xml"
firmware0_opt = "false"
firmware1_desc = "'Machines' folder"
firmware1_path = "Machines/Shared Roms/MSX.rom"
firmware1_opt = "false"
notes = "(!) The libretro port of blueMSX requires the BIOS files|from full standalone package inside the 'System\Machines' directory |and media database files into 'System\Databases' directory.|https://docs.libretro.com/library/bluemsx/#bios|(!) ColecoVision Gamepad Mapping is as follow:|Button 1 as Retropad A|Button 2 as Retropad B|Dial keys 1 to 8 as X, Y, R, L, R2, L2, R3, L3|Star as Select, Hash as Start|0 & 9 are on keyboard 1 & 2 for Player 1|0 & 9 are on keyboard 3 & 4 for Player 2.|(!) To play SpectraVideo cassettes type 'cload' then 'run'|or BLOAD ''CAS:'',R depending of game."

description = "A port of the blueMSX emulator to libretro. This emulator is cycle accurate and covers all generations of MSX computers, as well as SVI, ColecoVision and Sega SG-1000 machines. This core requires the 'Databases' and 'Machines' folders from a standalone installation of blueMSX to be placed in the frontend's system directory to function."
