# Software Information
display_name = "NEC - PC-8000 / PC-8800 series (QUASI88)"
authors = "Showzoh Fukunaga"
supported_extensions = "d88|u88|m3u"
corename = "QUASI88"
license = "BSD 3-Clause and MAME non-commercial"
permissions = ""
display_version = "0.6.4"
categories = "Emulator"

# Hardware Information
manufacturer = "NEC"
systemname = "PC-8000 / PC-8800 series"
systemid = "pc_88"

# Libretro Features
database = "NEC - PC-8001 - PC-8801"
supports_no_game = "true"
savestate = "true"
savestate_features = "deterministic"
cheats = "true"
input_descriptors = "true"
memory_descriptors = "true"
libretro_saves = "true"
core_options = "true"
load_subsystem = "true"
hw_render = "false"
needs_fullpath = "false"
disk_control = "false"
is_experimental = "false"

# Firmware / BIOS
firmware_count = 10
firmware0_desc = "n88.rom (Main BIOS)"
firmware0_path = "quasi88/n88.rom"
firmware0_opt = "false"
firmware1_desc = "n88_0.rom (Extension BIOS 1)"
firmware1_path = "quasi88/n88_0.rom"
firmware1_opt = "false"
firmware2_desc = "n88_1.rom (Extension BIOS 2)"
firmware2_path = "quasi88/n88_1.rom"
firmware2_opt = "true"
firmware3_desc = "n88_2.rom (Extension BIOS 3)"
firmware3_path = "quasi88/n88_2.rom"
firmware3_opt = "true"
firmware4_desc = "n88_3.rom (Extension BIOS 4)"
firmware4_path = "quasi88/n88_3.rom"
firmware4_opt = "true"
firmware5_desc = "n88n.rom (N Basic BIOS)"
firmware5_path = "quasi88/n88n.rom"
firmware5_opt = "true"
firmware6_desc = "disk.rom (Sub BIOS)"
firmware6_path = "quasi88/disk.rom"
firmware6_opt = "true"
firmware7_desc = "n88knj1.rom (Kanji Font 1)"
firmware7_path = "quasi88/n88knj1.rom"
firmware7_opt = "true"
firmware8_desc = "n88knj2.rom (Kanji Font 2)"
firmware8_path = "quasi88/n88knj2.rom"
firmware8_opt = "true"
firmware9_desc = "n88jisho.rom (Jisho)"
firmware9_path = "quasi88/n88jisho.rom"
firmware9_opt = "true"
notes = "QUASI88 by Showzoh Fukunaga.|Sound driver by MAME team.|fmgen and PC-8801 pseudo BIOS by cisc.|libretro port by Celerizer.| |BSD 3-Clause License| |Redistribution and use in source and binary|forms, with or without modification, are permitted|provided that the following conditions are met:| |1. Redistributions of source code must retain the|   above copyright notice, this list of conditions and|   the following disclaimer.| |2. Redistributions in binary form must reproduce the|   above copyright notice, this list of conditions and|   the following disclaimer in the documentation and/or|   other materials provided with the distribution.| |3. Neither the name of the copyright holder nor the|   names of its contributors may be used to endorse or|   promote products derived from this software without|   specific prior written permission.| |THIS SOFTWARE IS PROVIDED BY THE COPYRIGHT HOLDERS AND|CONTRIBUTORS ''AS IS'' AND ANY EXPRESS OR IMPLIED WARRANTIES,|INCLUDING, BUT NOT LIMITED TO, THE IMPLIED WARRANTIES OF|MERCHANTABILITY AND FITNESS FOR A PARTICULAR PURPOSE ARE|DISCLAIMED. IN NO EVENT SHALL THE COPYRIGHT HOLDER OR|CONTRIBUTORS BE LIABLE FOR ANY DIRECT, INDIRECT, INCIDENTAL,|SPECIAL, EXEMPLARY, OR CONSEQUENTIAL DAMAGES (INCLUDING, BUT|NOT LIMITED TO, PROCUREMENT OF SUBSTITUTE GOODS OR SERVICES;|LOSS OF USE, DATA, OR PROFITS; OR BUSINESS INTERRUPTION)|HOWEVER CAUSED AND ON ANY THEORY OF LIABILITY, WHETHER IN|CONTRACT, STRICT LIABILITY, OR TORT (INCLUDING NEGLIGENCE OR|OTHERWISE) ARISING IN ANY WAY OUT OF THE USE OF THIS SOFTWARE,|EVEN IF ADVISED OF THE POSSIBILITY OF SUCH DAMAGE."

description = "A port of the Quasi88 emulator for NEC's PC-8000 computer platform to libretro. This core supports built-in BIOS and fonts as fallbacks if the user does not supply their own dumps, and it can start using between 0 and 6 disks as content using the subsystem interface. It does not support the disk control interface but instead uses the dpad in conjunction with the L and R shoulder buttons to cycle among disks in the first and second drive positions, respectively."
