# Software Information
display_name = "Sharp - X68000 (PX68k)"
authors = "hissorii"
supported_extensions = "dim|zip|img|d88|88d|hdm|dup|2hd|xdf|hdf|cmd|m3u"
corename = "PX68k"
license = "Custom Non-Commercial"
permissions = ""
display_version = "0.15+"
categories = "Emulator"

# Hardware Information
manufacturer = "Sharp"
systemname = "Sharp X68000"
systemid = "sharp_x68000"

# Libretro Features
supports_no_game = "true"
database = "Sharp - X68000"
savestate = "false"
cheats = "false"
input_descriptors = "true"
memory_descriptors = "false"
libretro_saves = "false"
core_options = "true"
load_subsystem = "false"
hw_render = "false"
needs_fullpath = "true"
disk_control = "true"
is_experimental = "false"

# Firmware / BIOS
firmware_count = 3
firmware0_desc = "iplrom.dat (X68000 BIOS)"
firmware0_path = "keropi/iplrom.dat"
firmware0_opt = "false"
firmware1_desc = "cgrom.dat (X68000 BIOS 2)"
firmware1_path = "keropi/cgrom.dat"
firmware1_opt = "false"
firmware2_desc = "iplrom30.dat (X68000 BIOS 3)"
firmware2_path = "keropi/iplrom30.dat"
firmware2_opt = "true"
notes = "[i] Place BIOS files in system/keropi folder.|[i] F12 or Retropad L2 for Emulator Menu.|[i] Define your disks path in system/keropi/config StartDir line."

description = "A port of the Portable Sharp X68000 Emulator to libretro. The core can launch games directly or can be launched with no content and then use the built-in OSD menu via retropad-L2 or F12 key."
