<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="6.5.0">
<drawing>
<library>
<description>Beagle Bone Black pinout</description>
<packages>
<package name="TQFP64">
</package>
<package name="OSCILLATOR-3.2X2.5">
<description>3.2x2.5 MM Chrystal Oscillator

http://www.txccrystal.com/images/pdf/7m-accuracy.pdf</description>
</package>
<package name="SO08">
<description>&lt;b&gt;Small Outline Package&lt;/b&gt; Fits JEDEC packages (narrow SOIC-8)</description>
</package>
<package name="CAP-PTH-SMALL">
</package>
<package name="CAP-PTH-SMALL2">
</package>
<package name="0805">
</package>
<package name="CAP-PTH-LARGE">
</package>
<package name="GRM43D">
</package>
<package name="0603-CAP">
</package>
<package name="0402-CAP">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;&lt;p&gt;
chip</description>
</package>
<package name="CAP-PTH-5MM">
</package>
<package name="AXIAL-5MM">
</package>
<package name="1210">
</package>
<package name="1206">
</package>
<package name="AXIAL-0.3">
</package>
<package name="R2010">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
chip</description>
</package>
<package name="0603-RES">
</package>
<package name="0402-RES">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;&lt;p&gt;
chip</description>
</package>
<package name="1/6W-RES">
<description>1/6W Thru-hole Resistor - *UNPROVEN*</description>
</package>
<package name="R2512">
</package>
<package name="SOT223">
<description>&lt;b&gt;SOT-223&lt;/b&gt;</description>
</package>
<package name="EIA3216">
</package>
<package name="EIA3528">
</package>
<package name="CPOL-RADIAL-100UF-25V">
</package>
<package name="CPOL-RADIAL-10UF-25V">
</package>
<package name="EIA7343">
</package>
<package name="PANASONIC_G">
<description>&lt;b&gt;Panasonic Aluminium Electrolytic Capacitor VS-Serie Package G&lt;/b&gt;</description>
</package>
<package name="PANASONIC_E">
<description>&lt;b&gt;Panasonic Aluminium Electrolytic Capacitor VS-Serie Package E&lt;/b&gt;</description>
</package>
<package name="PANASONIC_C">
<description>&lt;b&gt;Panasonic Aluminium Electrolytic Capacitor VS-Serie Package E&lt;/b&gt;</description>
</package>
<package name="NIPPON_F80">
</package>
<package name="PANASONIC_D">
</package>
<package name="CPOL-RADIAL-1000UF-63V">
</package>
<package name="CPOL-RADIAL-1000UF-25V">
</package>
<package name="VISHAY_C">
</package>
<package name="PANASONIC_H13">
</package>
<package name="SOT23-5">
<description>&lt;b&gt;Small Outline Transistor&lt;/b&gt;</description>
</package>
<package name="SC70">
</package>
<package name="SOT-223">
</package>
<package name="SMA-DIODE">
<description>&lt;B&gt;Diode&lt;/B&gt;&lt;p&gt;
Basic SMA packaged diode. Good for reverse polarization protection. Common part #: MBRA140</description>
</package>
<package name="PTC">
</package>
<package name="PTC-1206">
</package>
<package name="0603">
</package>
<package name="MOLEX-47346-0001">
</package>
<package name="53047-15">
<description>&lt;b&gt;CONNECTOR&lt;/b&gt;&lt;p&gt;
wire to board 1.25 mm (.049 inch) pitch header&lt;p&gt;
straight</description>
</package>
<package name="53048-15">
<description>&lt;b&gt;CONNECTOR&lt;/b&gt;&lt;p&gt;
wire to board 1.25 mm (.049 inch) pitch header&lt;p&gt;
right angle</description>
</package>
<package name="53261-15">
<description>&lt;b&gt;CONNECTOR&lt;/b&gt;&lt;p&gt;
wire to board 1.25 mm (.049 inch) pitch header&lt;p&gt;
SMT&lt;p&gt;
right angle</description>
</package>
<package name="53398-15">
<description>&lt;b&gt;CONNECTOR&lt;/b&gt;&lt;p&gt;
wire to board 1.25 mm (.049 inch) pitch header&lt;p&gt;
SMT&lt;p&gt;
straight</description>
</package>
<package name="CTS742C083">
<description>&lt;b&gt;Chip Resistor Array&lt;/b&gt;&lt;p&gt;
Source: http://www.ctscorp.com/components/Datasheets/CTSChipArrayDs.pdf</description>
</package>
<package name="MSOP-8">
</package>
<package name="53047-04">
<description>&lt;b&gt;CONNECTOR&lt;/b&gt;&lt;p&gt;
wire to board 1.25 mm (.049 inch) pitch header&lt;p&gt;
straight</description>
</package>
<package name="53048-04">
<description>&lt;b&gt;CONNECTOR&lt;/b&gt;&lt;p&gt;
wire to board 1.25 mm (.049 inch) pitch header&lt;p&gt;
right angle</description>
</package>
<package name="53261-04">
<description>&lt;b&gt;CONNECTOR&lt;/b&gt;&lt;p&gt;
wire to board 1.25 mm (.049 inch) pitch header&lt;p&gt;
SMT&lt;p&gt;
right angle</description>
</package>
<package name="53398-04">
<description>&lt;b&gt;CONNECTOR&lt;/b&gt;&lt;p&gt;
wire to board 1.25 mm (.049 inch) pitch header&lt;p&gt;
SMT&lt;p&gt;
straight</description>
</package>
<package name="FTSH-105-01-XXX-DV-K">
<description>TERMINAL STRIP, .050 inch(1.27mm) PITCH, 10 PINS, KEYED</description>
</package>
<package name="53047-10">
<description>&lt;b&gt;CONNECTOR&lt;/b&gt;&lt;p&gt;
wire to board 1.25 mm (.049 inch) pitch header&lt;p&gt;
straight</description>
</package>
<package name="53048-10">
<description>&lt;b&gt;CONNECTOR&lt;/b&gt;&lt;p&gt;
wire to board 1.25 mm (.049 inch) pitch header&lt;p&gt;
right angle</description>
</package>
<package name="53261-10">
<description>&lt;b&gt;CONNECTOR&lt;/b&gt;&lt;p&gt;
wire to board 1.25 mm (.049 inch) pitch header&lt;p&gt;
SMT&lt;p&gt;
right angle</description>
</package>
<package name="53398-10">
<description>&lt;b&gt;CONNECTOR&lt;/b&gt;&lt;p&gt;
wire to board 1.25 mm (.049 inch) pitch header&lt;p&gt;
SMT&lt;p&gt;
straight</description>
</package>
<package name="TACTILE-PTH">
<description>&lt;b&gt;OMRON SWITCH&lt;/b&gt;</description>
</package>
<package name="TACTILE_SWITCH_SMD">
</package>
<package name="TACTILE_SWITCH_SMD-2">
</package>
<package name="TACTILE-PTH-12MM">
</package>
<package name="TACTILE-SWITCH-1101NE">
<description>Sparkfun SKU# COM-08229</description>
</package>
<package name="53047-03">
<description>&lt;b&gt;CONNECTOR&lt;/b&gt;&lt;p&gt;
wire to board 1.25 mm (.049 inch) pitch header&lt;p&gt;
straight</description>
</package>
<package name="53048-03">
<description>&lt;b&gt;CONNECTOR&lt;/b&gt;&lt;p&gt;
wire to board 1.25 mm (.049 inch) pitch header&lt;p&gt;
right angle</description>
</package>
<package name="53261-03">
<description>&lt;b&gt;CONNECTOR&lt;/b&gt;&lt;p&gt;
wire to board 1.25 mm (.049 inch) pitch header&lt;p&gt;
SMT&lt;p&gt;
right angle</description>
</package>
<package name="53398-03">
<description>&lt;b&gt;CONNECTOR&lt;/b&gt;&lt;p&gt;
wire to board 1.25 mm (.049 inch) pitch header&lt;p&gt;
SMT&lt;p&gt;
straight</description>
</package>
<package name="S3B-ZR-SM4A-TF">
<description>JST ZH series side-entry SMD, 3 pins plus solder tabs.</description>
</package>
<package name="1206-IND">
</package>
<package name="CR54">
</package>
<package name="CDRH125">
</package>
<package name="0402-IND">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;&lt;p&gt;
chip</description>
</package>
<package name="B82462G">
</package>
<package name="CR75">
</package>
<package name="1007">
<description>1007 (2518 metric) package</description>
</package>
<package name="COOPER_UP4B">
</package>
<package name="CDRH3D28">
</package>
<package name="SO014">
</package>
<package name="MICROSD">
</package>
<package name="LGA-16-3PX5P">
<description>&lt;b&gt;LGA-16 3x3 mm package (3x5 pin layout)&lt;/b&gt;&lt;br /&gt;
This layout follows the ST Micro design guidelines for LGA packages found at:&lt;br /&gt;
&lt;br /&gt;
&lt;a href="http://www.st.com/internet/com/TECHNICAL_RESOURCES/TECHNICAL_LITERATURE/TECHNICAL_NOTE/CD00134799.pdf"&gt;ST Micro LGA surface mounting guidelines&lt;/a&gt;</description>
</package>
<package name="LGA-16L_SMALL_PADS">
<description>&lt;h3&gt;Description&lt;/h3&gt;
LGA-16 5x5 mm package (4x4 pin layout)
This layout follows the ST Micro design guidelines for LGA packages found at:&lt;br /&gt;
&lt;br /&gt;

&lt;a href="http://www.st.com/internet/com/TECHNICAL_RESOURCES/TECHNICAL_LITERATURE/TECHNICAL_NOTE/CD00134799.pdf"&gt;ST Micro LGA surface mounting guidelines&lt;/a&gt;</description>
</package>
<package name="LPCC20-OLD">
</package>
<package name="BMP085">
</package>
<package name="HEADER_2MM_2X15">
<description>2mm Surface Mount Box Connector Strip Assembly</description>
</package>
<package name="QFN10">
</package>
<package name="QFN10L">
</package>
<package name="SJ_3">
</package>
<package name="1X03">
</package>
<package name="SJ_3_PASTE1&amp;2">
</package>
<package name="SJ_3_PASTE2&amp;3">
</package>
<package name="QFN16">
</package>
<package name="DO214AC">
<description>&lt;b&gt;DIODE&lt;/b&gt;</description>
</package>
<package name="FTSH-105-01-XXX-DV">
</package>
<package name="EVQP7J01K">
</package>
<package name="SOT996-2">
</package>
<package name="LED5MM">
<description>&lt;B&gt;LED&lt;/B&gt;&lt;p&gt;
5 mm, round</description>
</package>
<package name="LED3MM">
<description>&lt;B&gt;LED&lt;/B&gt;&lt;p&gt;
3 mm, round</description>
</package>
<package name="LED-1206">
</package>
<package name="LED10MM">
</package>
<package name="MOUNT-HOLE2.1">
<description>Mounting hole to suit M2 fastener and Richco R937-x spacer.</description>
</package>
<package name="TQFP48">
</package>
<package name="SO14">
<description>&lt;b&gt;SMALL OUTLINE INTEGRATED CIRCUIT&lt;/b&gt;&lt;p&gt;
body 3.9 mm/JEDEC MS-012AC</description>
</package>
<package name="3X8RA">
</package>
<package name="3X1RA">
</package>
<package name="FREESCALE-1351-01">
</package>
<package name="SOP4-2.54">
<description>2.54SOP4 Toshiba package

Footprint is from:
http://www.semicon.toshiba.co.jp/docs/catalog/en/BCE0034_catalog.pdf</description>
</package>
<package name="R-PDSO-G08">
<description>&lt;b&gt;PLASTIC SMALL-OUTLINE PACKAGE, SO 8&lt;/b&gt; JEDEC MO-153&lt;p&gt;
Source: www.ti.com/.. slvs087l.pdf</description>
</package>
<package name="53047-02">
<description>&lt;b&gt;CONNECTOR&lt;/b&gt;&lt;p&gt;
wire to board 1.25 mm (.049 inch) pitch header&lt;p&gt;
straight</description>
</package>
<package name="53048-02">
<description>&lt;b&gt;CONNECTOR&lt;/b&gt;&lt;p&gt;
wire to board 1.25 mm (.049 inch) pitch header&lt;p&gt;
right angle</description>
</package>
<package name="53261-02">
<description>&lt;b&gt;CONNECTOR&lt;/b&gt;&lt;p&gt;
wire to board 1.25 mm (.049 inch) pitch header&lt;p&gt;
SMT&lt;p&gt;
right angle</description>
</package>
<package name="53398-02">
<description>&lt;b&gt;CONNECTOR&lt;/b&gt;&lt;p&gt;
wire to board 1.25 mm (.049 inch) pitch header&lt;p&gt;
SMT&lt;p&gt;
straight</description>
</package>
<package name="XBEE-1">
</package>
<package name="XBEE-SILK">
</package>
<package name="XBEE-SMD">
</package>
<package name="XBEE-1_LOCK">
</package>
<package name="SOT23-5L">
<description>&lt;b&gt;Small Outline Transistor&lt;/b&gt;&lt;p&gt;
package type OT</description>
</package>
<package name="R-PDSO-G24">
<description>&lt;b&gt;PLASTIC SMALL-OUTLINE PACKAGE SO 24&lt;/b&gt; JEDEC MO-153&lt;p&gt;
Source: www.ti.com/.. slvs087l.pdf</description>
</package>
<package name="53047-06">
<description>&lt;b&gt;CONNECTOR&lt;/b&gt;&lt;p&gt;
wire to board 1.25 mm (.049 inch) pitch header&lt;p&gt;
straight</description>
</package>
<package name="53048-06">
<description>&lt;b&gt;CONNECTOR&lt;/b&gt;&lt;p&gt;
wire to board 1.25 mm (.049 inch) pitch header&lt;p&gt;
right angle</description>
</package>
<package name="53261-06">
<description>&lt;b&gt;CONNECTOR&lt;/b&gt;&lt;p&gt;
wire to board 1.25 mm (.049 inch) pitch header&lt;p&gt;
SMT&lt;p&gt;
right angle</description>
</package>
<package name="53398-06">
<description>&lt;b&gt;CONNECTOR&lt;/b&gt;&lt;p&gt;
wire to board 1.25 mm (.049 inch) pitch header&lt;p&gt;
SMT&lt;p&gt;
straight</description>
</package>
<package name="53047-07">
<description>&lt;b&gt;CONNECTOR&lt;/b&gt;&lt;p&gt;
wire to board 1.25 mm (.049 inch) pitch header&lt;p&gt;
straight</description>
</package>
<package name="53048-07">
<description>&lt;b&gt;CONNECTOR&lt;/b&gt;&lt;p&gt;
wire to board 1.25 mm (.049 inch) pitch header&lt;p&gt;
right angle</description>
</package>
<package name="53261-07">
<description>&lt;b&gt;CONNECTOR&lt;/b&gt;&lt;p&gt;
wire to board 1.25 mm (.049 inch) pitch header&lt;p&gt;
SMT&lt;p&gt;
right angle</description>
</package>
<package name="53398-07">
<description>&lt;b&gt;CONNECTOR&lt;/b&gt;&lt;p&gt;
wire to board 1.25 mm (.049 inch) pitch header&lt;p&gt;
SMT&lt;p&gt;
straight</description>
</package>
<package name="MICROSMP">
<description>MicroSMP Package

&lt;br /&gt;
&lt;a href="http://www.vishay.com/docs/89019/mss1p4.pdf"&gt;http://www.vishay.com/docs/89019/mss1p4.pdf&lt;/a&gt;</description>
</package>
<package name="SOT363_PHILIPS">
<description>&lt;b&gt;Small Outline Transistor; 6 leads&lt;/b&gt;&lt;p&gt;
Philips Semiconductors, SOT363.pdf</description>
</package>
<package name="XBEE-MINIMAL">
</package>
<package name="PTH08080W_SMD">
</package>
<package name="PTH08080W_TH">
</package>
<package name="L3G4200DH-MAN">
<description>LGA-16L Case for manual assembly</description>
</package>
<package name="LIS331DLH-MAN">
<description>ST LIS331DLH Accelerometer package
&lt;br /&gt;
&lt;br /&gt;
Adapted based on:&lt;br /&gt;
&lt;a href="http://www.st.com/stonline/products/literature/tn/12707.pdf"&gt;http://www.st.com/stonline/products/literature/tn/12707.pdf&lt;/a&gt;</description>
</package>
<package name="LPCC20">
</package>
<package name="HEADER_2MM_2X15_REVERSE">
<description>2mm Surface Mount Connector Strip Assembly, reversed for board-to-board mating</description>
</package>
<package name="PAD.02X.02">
</package>
<package name="PAD.03X.03">
</package>
<package name="EM406">
</package>
<package name="0402-PTC">
</package>
<package name="BM06B-SRSS-TB">
<description>&lt;b&gt;Shrouded Header, top entry type&lt;/b&gt;</description>
</package>
<package name="SM06B-SRSS-TB">
<description>&lt;b&gt;Shrouded Header, side entry type&lt;/b&gt;</description>
</package>
<package name="OSCILLATOR-5.0X3.2">
</package>
<package name="1,6/0,8">
<description>&lt;b&gt;THROUGH-HOLE PAD&lt;/b&gt;</description>
</package>
<package name="1,6/0,9">
<description>&lt;b&gt;THROUGH-HOLE PAD&lt;/b&gt;</description>
</package>
<package name="2,15/1,0">
<description>&lt;b&gt;THROUGH-HOLE PAD&lt;/b&gt;</description>
</package>
<package name="2,54/0,8">
<description>&lt;b&gt;THROUGH-HOLE PAD&lt;/b&gt;</description>
</package>
<package name="2,54/0,9">
<description>&lt;b&gt;THROUGH-HOLE PAD&lt;/b&gt;</description>
</package>
<package name="2,54/1,0">
<description>&lt;b&gt;THROUGH-HOLE PAD&lt;/b&gt;</description>
</package>
<package name="2,54/1,1">
<description>&lt;b&gt;THROUGH-HOLE PAD&lt;/b&gt;</description>
</package>
<package name="3,17/1,1">
<description>&lt;b&gt;THROUGH-HOLE PAD&lt;/b&gt;</description>
</package>
<package name="3,17/1,2">
<description>&lt;b&gt;THROUGH-HOLE PAD&lt;/b&gt;</description>
</package>
<package name="3,17/1,3">
<description>&lt;b&gt;THROUGH-HOLE PAD&lt;/b&gt;</description>
</package>
<package name="3,81/1,1">
<description>&lt;b&gt;THROUGH-HOLE PAD&lt;/b&gt;</description>
</package>
<package name="3,81/1,3">
<description>&lt;b&gt;THROUGH-HOLE PAD&lt;/b&gt;</description>
</package>
<package name="3,81/1,4">
<description>&lt;b&gt;THROUGH-HOLE PAD&lt;/b&gt;</description>
</package>
<package name="4,16O1,6">
<description>&lt;b&gt;THROUGH-HOLE PAD&lt;/b&gt;</description>
</package>
<package name="5-1,8">
<description>&lt;b&gt;THROUGH-HOLE PAD&lt;/b&gt;</description>
</package>
<package name="5-2,5">
<description>&lt;b&gt;THROUGH-HOLE PAD&lt;/b&gt;</description>
</package>
<package name="3,5-2">
</package>
<package name="53047-05">
<description>&lt;b&gt;CONNECTOR&lt;/b&gt;&lt;p&gt;
wire to board 1.25 mm (.049 inch) pitch header&lt;p&gt;
straight</description>
</package>
<package name="53048-05">
<description>&lt;b&gt;CONNECTOR&lt;/b&gt;&lt;p&gt;
wire to board 1.25 mm (.049 inch) pitch header&lt;p&gt;
right angle</description>
</package>
<package name="53261-05">
<description>&lt;b&gt;CONNECTOR&lt;/b&gt;&lt;p&gt;
wire to board 1.25 mm (.049 inch) pitch header&lt;p&gt;
SMT&lt;p&gt;
right angle</description>
</package>
<package name="53398-05">
<description>&lt;b&gt;CONNECTOR&lt;/b&gt;&lt;p&gt;
wire to board 1.25 mm (.049 inch) pitch header&lt;p&gt;
SMT&lt;p&gt;
straight</description>
</package>
<package name="MOUNT-HOLE3.1">
</package>
<package name="MEDIATEK_MT3329">
</package>
<package name="HMC5883L-MAN">
</package>
<package name="ADH8066">
<description>FP for ADH8066 cell modules. Uses 50-pin connector with 0.5mm pitch Hirose part# DF12(3.0)-50DP-0.5V</description>
</package>
<package name="B3B-ZR">
<description>&lt;b&gt;JST ZH Series 3-pos top entry&lt;/b&gt;
&lt;br /&gt;
&lt;br /&gt;
Datasheet: &lt;a href="http://www.jst-mfg.com/product/pdf/eng/eZH.pdf"&gt;http://www.jst-mfg.com/product/pdf/eng/eZH.pdf&lt;/a&gt;</description>
</package>
<package name="S4B-PH-SM4-TB">
</package>
<package name="B4B-PH-K-S">
<description>JST PH top-entry through-hole 4-pos connector</description>
</package>
<package name="S02B-PASK-2">
<description>JST PA Series

2 position, 2 mm pitch, 3A max.</description>
</package>
<package name="TI-DCU">
</package>
<package name="PAD-2.5-1.8">
</package>
<package name="LENSMOUNT_M12">
<description>Point Grey compatible M12 lensmount</description>
</package>
<package name="ADNS-2080">
</package>
<package name="SOT23-3">
</package>
<package name="HEADER_2MM_2X8">
</package>
<package name="SJ_2">
</package>
<package name="PAD-2.5-1.3">
</package>
<package name="SJ_3_0805_PASTE1&amp;2">
</package>
<package name="SJ_3_0603_PASTE1&amp;2">
</package>
<package name="SOD323">
</package>
<package name="HEADER_2MM_2X15_REVERSE_POGO">
</package>
<package name="HEADER_2MM_2X15_POGO">
</package>
<package name="POGO">
<description>Pogo-Testpin</description>
</package>
<package name="HEADER_2.54MM-2X10-SHROUDED_LOCK">
</package>
<package name="HEADER_1X06-SIP_LOCK">
<description>This footprint was designed to help hold the alignment of a through-hole component (i.e.  6-pin header) while soldering it into place.  
You may notice that each hole has been shifted either up or down by 0.005 of an inch from it's more standard position (which is a perfectly straight line).  
This slight alteration caused the pins (the squares in the middle) to touch the edges of the holes.  Because they are alternating, it causes a "brace" 
to hold the component in place.  0.005 has proven to be the perfect amount of "off-center" position when using our standard breakaway headers.
Although looks a little odd when you look at the bare footprint, once you have a header in there, the alteration is very hard to notice.  Also,
if you push a header all the way into place, it is covered up entirely on the bottom side.  This idea of altering the position of holes to aid alignment 
will be further integrated into the Sparkfun Library for other footprints.  It can help hold any component with 3 or more connection pins.</description>
</package>
<package name="POGO-HOLE">
<description>&lt;h2&gt;Pogo-pin-head hole&lt;/h2&gt;
&lt;br /&gt;
This footprint allows the head of the pogo-pin to pass through. It should be uses for the PCB-mount, not for mounting the pogo pin (use footprint POGO for the pogo-pin solder footprint).</description>
</package>
<package name="HEADER_2.54MM-2X15-SHROUDED_LOCK">
</package>
<package name="POWER_JACK_SMD">
</package>
<package name="POWER_JACK_SLOT">
</package>
<package name="POWER_JACK_PTH">
</package>
<package name="POWER_JACK_COMBO">
</package>
<package name="RCA">
</package>
<package name="POWER_JACK_PTH_LOCK">
</package>
<package name="RCA_LOCK">
</package>
<package name="TSOP-6">
</package>
<package name="TI-DGS">
<description>TI DGS / MAXIM 10L uMAX/uSOP

0.5 mm pin spacing, 5 mm pin span</description>
</package>
<package name="SWITCH-SPDT">
</package>
<package name="AYZ0202">
<description>&lt;b&gt;DPDT Slide Switch SMD&lt;/b&gt;
www.SparkFun.com SKU : Comp-SMDS</description>
</package>
<package name="SWITCHE-DPDT">
</package>
<package name="R_SW_TH">
</package>
<package name="SWITCH-SPDT-SMD">
</package>
<package name="SWITCH-SPDT_LOCK.007S">
</package>
<package name="USB-A-H">
<description>&lt;b&gt;USB Series A Hole Mounted&lt;/b&gt;</description>
</package>
<package name="USB-A-S">
<description>&lt;b&gt;USB Series A Surface Mounted&lt;/b&gt;</description>
</package>
<package name="USB-MB-H">
<description>&lt;b&gt;USB Series Mini-B Hole Mounted&lt;/b&gt;</description>
</package>
<package name="USB-B-SMT">
<description>USB Series B Surface Mounted</description>
</package>
<package name="USB-MINIB-OLD">
<description>&lt;b&gt;USB Series Mini-B Surface Mounted&lt;/b&gt;</description>
</package>
<package name="USB-B-PTH">
<description>&lt;b&gt;USB Series B Hole Mounted&lt;/b&gt;</description>
</package>
<package name="S4B-PH">
</package>
<package name="USB-MINIB">
<description>&lt;b&gt;USB Series Mini-B Surface Mounted&lt;/b&gt;</description>
</package>
<package name="USB-A-PCB">
</package>
<package name="USB-B-PTH-VERTICAL">
<description>&lt;b&gt;USB Series B Hole Mounted&lt;/b&gt;</description>
</package>
<package name="USB-A-S-NOSILK">
</package>
<package name="USB-A-S-NOSILK-FEMALE">
</package>
<package name="USB-MICROB">
<description>Micro USB Package</description>
</package>
<package name="USB-MINIB-NOSTOP">
</package>
<package name="USB-A-S-SILK-FEMALE">
</package>
<package name="TSSOP-8">
</package>
<package name="SOT23-6">
</package>
<package name="AMPHENOL_114-00841-68">
</package>
<package name="MOUNT-HOLE2.6">
<description>Mounting hole to suit M2.5 fastener and Richco R907-series spacer</description>
</package>
<package name="LGA12">
</package>
<package name="OSHW-LOGO-S">
</package>
<package name="OSHW-LOGO-M">
</package>
<package name="OSHW-LOGO-L">
</package>
<package name="3X1-BOARD-EDGE">
</package>
<package name="DF13A-15P-1.25H">
<description>Hirose DF13 A

15 pos 1.25 mm pitch 1A connector</description>
</package>
<package name="DF13A-4P-1.25H">
</package>
<package name="DF13A-3P-1.25H">
</package>
<package name="DF13-15P-1.25DSA">
</package>
<package name="DF13-2P-1.25DSA">
</package>
<package name="DF13-3P-1.25DSA">
</package>
<package name="DF13-4P-1.25DSA">
</package>
<package name="DF13-5P-1.25DSA">
</package>
<package name="DF13-6P-1.25DSA">
</package>
<package name="HEADER_2MM_2X15_TH_REVERSE">
<description>2 MM 30 pos Dual-Row Header

e.g. 3M product 951230-8622-AR</description>
</package>
<package name="HEADER_2MM_2X15_TH">
<description>2 mm 30 pos Dual-Row Through-Hole Header
e.g. 3M product 951230-8622-AR</description>
</package>
<package name="HEADER_2.54MM_2X15_PROTO">
</package>
<package name="HEADER_1X06-FTDI">
</package>
<package name="MS5611-01BA">
</package>
<package name="TO-92">
<description>&lt;b&gt;TO 92&lt;/b&gt;</description>
</package>
<package name="SOT89">
</package>
<package name="TO-92-AMMO">
</package>
<package name="78XXL">
<description>&lt;b&gt;VOLTAGE REGULATOR&lt;/b&gt;</description>
</package>
<package name="CPOL-RADIAL-100UF-50V-3.5MM-8MM">
</package>
<package name="DO201AD">
<description>&lt;B&gt;DIODE&lt;/B&gt;&lt;p&gt;
diameter 5.3 mm, horizontal, grid 15.24 mm</description>
</package>
<package name="DO204AR">
<description>DO-204AR Package

&lt;a href="http://www.vishay.com/docs/95243/ado204ar.pdf"&gt;Dimensions Datasheet Link&lt;/a&gt;</description>
</package>
<package name="TO220">
<description>&lt;b&gt;TO 220 Vertical&lt;/b&gt; Package works with various parts including N-Channel MOSFET SparkFun SKU: COM-10213</description>
</package>
<package name="TO220-2POS">
</package>
<package name="CLCC-48">
</package>
<package name="TQFP100">
</package>
<package name="MAXSONAR">
</package>
<package name="LENSMOUNT_LARGE_M12">
</package>
<package name="QFN-24">
</package>
<package name="QUALIFIED_1_OVERO">
</package>
<package name="BM12B-SRSS-TB">
</package>
<package name="B8B-PH-K-S">
</package>
<package name="HEADER_2MM_2X4_TH">
</package>
<package name="HEADER_2MM_2X4_TH_REVERSE">
</package>
<package name="PX4FLOW">
</package>
<package name="CASPA">
</package>
<package name="DF13A-6P-1.25H">
</package>
<package name="DF13A-5P-1.25H">
</package>
<package name="DF13A-7P-1.25H">
</package>
<package name="3DROBOTICS_1296-12">
<description>&lt;b&gt;1.27mm SINGLE ROW FEMALE SOCKET&lt;/b&gt;&lt;p&gt;
Source: http://www.leotronics.co.uk/Conexcon/Data%20Sheets/sec.%20A/1296ing.pdf</description>
</package>
<package name="3DROBOTICS_2MM-DUAL-ROW-MALE-HEADER-SMT-2X6">
</package>
<package name="HEADER_2.54MM-1X04">
</package>
<package name="DPAK">
</package>
<package name="F/TMB">
<description>&lt;b&gt;BUZZER&lt;/b&gt;</description>
</package>
<package name="SWITCH-SPDT-TH-HORZ">
</package>
<package name="SM12B-SRSS-TB">
</package>
<package name="LVK24-CURRENT-SENSE">
</package>
<package name="HEADER_2MM_2X15_POGO-HOLE">
</package>
<package name="WIREPAD-TH-1.5MM">
</package>
<package name="WIREPAD-TH-2.0MM">
</package>
<package name="HEADER_3X01_SMD_H_BOARD_EDGE">
</package>
<package name="MOUNTING-BRACKET-4-40">
</package>
<package name="MECH-MINI-SERVO">
</package>
<package name="PAD.05X.05">
</package>
<package name="DF13-7P-1.25DSA">
</package>
<package name="QUALIFIED_1_DUOVERO">
</package>
<package name="QUALIFIED_1_USB-B-SMT">
<description>&lt;b&gt;USB&lt;/b&gt; YAMAICHI CONNECTOR</description>
</package>
<package name="QUALIFIED_1_USB-MINI-AB-SMT">
</package>
<package name="R-PDSO-G20">
</package>
<package name="DF13A-2P-1.25H">
</package>
<package name="KRUBERG_HVQFN32">
</package>
<package name="MOLEX-HDMI_47151-001">
</package>
<package name="MOLEX-HDMI-46765-0001">
</package>
<package name="CTS-219-4MST">
</package>
<package name="COPAL-CHS-04TA">
</package>
<package name="USB-MINI-B-SMT">
</package>
<package name="PX4-LOGO-5MM">
</package>
<package name="PX4-LOGO-10MM">
</package>
<package name="PX4-LOGO-15MM">
</package>
<package name="PX4-LOGO-20MM">
</package>
<package name="PX4-LOGO-30MM">
</package>
<package name="SOT23">
<description>&lt;B&gt;DIODE&lt;/B&gt;</description>
</package>
<package name="PAD.04X.04">
</package>
<package name="FTSH-105-01-XXX-DV-K-POGO-PINS">
</package>
<package name="FTSH-105-01-XXX-DV-K-POGO-HOLES">
</package>
<package name="DMS-20LCD">
</package>
<package name="KEYSTONE-5016">
</package>
<package name="PAD-2MM-PROBE-HORZ">
<description>2MM Probe Tip Diameter

For 2MM multimeter / scope standard probes. Similar to:

Keystone 6050 and Emerson 105-1102-001

http://emersonconnectivity.com/OA_MEDIA/specs/pi-1051102001.pdf</description>
</package>
<package name="HARWIN-S1751-46R">
</package>
<package name="BMA280">
</package>
<package name="TSSOP-16">
<description>&lt;b&gt;Thin Shrink Small Outline Plastic 16&lt;/b&gt;&lt;p&gt;
MAX3223-MAX3243.pdf</description>
</package>
<package name="R-78X.0-1.0">
</package>
<package name="MOUNT-HOLE3.3">
</package>
<package name="HEADER_2MM_2X15_TH_FMU_MOUNTING">
</package>
<package name="HEADER_2MM_2X15_TH_REVERSE_FMU_MOUNTING">
</package>
<package name="3X4RA">
</package>
<package name="DO41-7">
<description>&lt;B&gt;DIODE&lt;/B&gt;&lt;p&gt;
diameter 2.54 mm, horizontal, grid 7.62 mm</description>
</package>
<package name="3X1-BOARD-EDGE-NOLABEL">
</package>
<package name="LGA-16L">
</package>
<package name="0603-LED">
</package>
<package name="0402-LED">
</package>
<package name="DFN16+GND_5X3">
<description>DFN16 5mm x 3mm with ground pad</description>
</package>
<package name="QFN20-RGY">
<description>Texas Instruments RGY (QFN20) package</description>
</package>
<package name="SOT23-8">
<description>SOT23-8</description>
</package>
<package name="QFN24-RHL">
</package>
<package name="3X6RA">
</package>
<package name="3X16RA">
</package>
<package name="MS621FE">
</package>
<package name="MSOP-8-EPAD">
<description>MSOP-8 ePad (Micrel)</description>
</package>
<package name="6-PLCC">
</package>
<package name="SOT353">
</package>
<package name="SON10">
</package>
<package name="KYOCERA-KNH10">
<description>Kyocera KNH10 series EMI filter</description>
</package>
<package name="KYOCERA-KNH16-DA">
<description>Kyocera KNH16-DA EMI filter</description>
</package>
<package name="3528/B-DIO">
</package>
<package name="MELF-MLL41">
<description>&lt;h4&gt;Diode in MELF package&lt;/h4&gt;
&lt;p&gt;
MELF = MLL41 = DO-213AB&lt;br /&gt;&lt;br /&gt;

http://www.diotec.com/produkte/files/loetpads.pdf
&lt;/p&gt;</description>
</package>
<package name="SOD-123-DIO">
</package>
<package name="0603-DIO">
</package>
<package name="MLF-8-EPAD">
</package>
<package name="SOT563-6">
</package>
<package name="QFN8-DSG">
</package>
<package name="MLP08W">
</package>
<package name="0402-TVS">
</package>
<package name="1210-IND">
</package>
<package name="1206-CAP">
</package>
<package name="1812-CAP">
</package>
<package name="SO08-DDA-EPAD">
</package>
<package name="0805-IND">
</package>
<package name="0805-CAP">
</package>
<package name="0603-IND">
</package>
<package name="0805-POL-CAP">
</package>
<package name="51281-1094">
<description>Molex 51281-1094 10-way 0.5mm RA LIF FPC connector.</description>
</package>
<package name="78119-0108">
<description>Molex 78119-0108 0.5mm 10pos vertical LIF FPC connector</description>
</package>
<package name="FIDUCIAL-1.5X3">
</package>
<package name="FIDUCIAL-1X2">
</package>
<package name="FIDUCIAL-1X2.5">
</package>
<package name="MICRO-FIDUCIAL">
</package>
<package name="TSSOP8_SOT505-2">
</package>
<package name="HEADER_3X01_SMD_H_BOARD_EDGE_SHORT">
</package>
<package name="MO-220">
<description>JEDEC MO-220, aka LTC UF package</description>
</package>
<package name="1206-8">
<description>1206-8 ChipFet</description>
</package>
<package name="4525DO-DS5AI001DP">
</package>
<package name="HEADER_2.54MM_2X23_TH">
</package>
<package name="HEADER_2.54MM-1X10">
</package>
<package name="LGA-24">
</package>
<package name="BEAGLEBONE_SHIELD">
</package>
<package name="3X14RA">
</package>
<package name="MPU-6500">
</package>
<package name="WDFN8">
</package>
<package name="DFN8+OUT_3X3MM">
</package>
<package name="4525DO-DSXAI001DS">
</package>
</packages>
<symbols>
<symbol name="PORT_A_L">
<pin name="PA0"/>
<pin name="PA1"/>
<pin name="PA2"/>
<pin name="PA3"/>
<pin name="PA4"/>
<pin name="PA5"/>
<pin name="PA6"/>
<pin name="PA7"/>
</symbol>
<symbol name="PORT_A_H">
<pin name="PA8"/>
<pin name="PA9"/>
<pin name="PA10"/>
<pin name="PA11"/>
<pin name="PA12"/>
<pin name="PA13"/>
<pin name="PA14"/>
<pin name="PA15"/>
</symbol>
<symbol name="PORT_B_L">
<pin name="PB0"/>
<pin name="PB1"/>
<pin name="PB2"/>
<pin name="PB3"/>
<pin name="PB4"/>
<pin name="PB5"/>
<pin name="PB6"/>
<pin name="PB7"/>
</symbol>
<symbol name="PORT_B_H">
<pin name="PB8"/>
<pin name="PB9"/>
<pin name="PB10"/>
<pin name="PB11"/>
<pin name="PB12"/>
<pin name="PB13"/>
<pin name="PB14"/>
<pin name="PB15"/>
</symbol>
<symbol name="PORT_C_L">
<pin name="PC0"/>
<pin name="PC1"/>
<pin name="PC2"/>
<pin name="PC3"/>
<pin name="PC4"/>
<pin name="PC5"/>
<pin name="PC6"/>
<pin name="PC7"/>
</symbol>
<symbol name="PORT_C_H">
<pin name="PC13"/>
<pin name="PC14"/>
<pin name="PC15"/>
<pin name="PC8"/>
<pin name="PC9"/>
<pin name="PC10"/>
<pin name="PC11"/>
<pin name="PC12"/>
</symbol>
<symbol name="VCC_VDD_M">
<pin name="VDD_1" direction="pwr"/>
<pin name="VDD_2" direction="pwr"/>
<pin name="VDD_3" direction="pwr"/>
<pin name="VCAP_1" direction="pwr"/>
<pin name="VCAP_2" direction="pwr"/>
<pin name="VSS_3" direction="pwr"/>
<pin name="VDD_4" direction="pwr"/>
<pin name="VSS_4" direction="pwr"/>
</symbol>
<symbol name="PORT_D_3">
<pin name="PH0/OSC&lt;="/>
<pin name="PH1/OSC=&gt;"/>
<pin name="PD2"/>
</symbol>
<symbol name="BAT_AN_M">
<pin name="VBAT" direction="pwr"/>
<pin name="VSSA" direction="pwr"/>
<pin name="VDDA" direction="pwr"/>
</symbol>
<symbol name="BOOT_RST">
<pin name="NRST" direction="in" function="dot"/>
<pin name="BOOT0" direction="in"/>
</symbol>
<symbol name="XTAL">
<pin name="3"/>
<pin name="1"/>
<pin name="NC_4" direction="sup"/>
<pin name="NC_2" direction="sup"/>
</symbol>
<symbol name="EEPROM-I2C">
<pin name="VSS" direction="pwr"/>
<pin name="WP"/>
<pin name="VCC" direction="pwr"/>
<pin name="SCL"/>
<pin name="SDA"/>
<pin name="A2"/>
<pin name="A0"/>
<pin name="A1"/>
</symbol>
<symbol name="A3L-LOC">
</symbol>
<symbol name="A4L-LOC">
</symbol>
<symbol name="CAP">
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
</symbol>
<symbol name="RESISTOR">
<pin name="2" direction="pas"/>
<pin name="1" direction="pas"/>
</symbol>
<symbol name="78XX">
<pin name="IN" direction="in"/>
<pin name="GND" direction="in"/>
<pin name="OUT" direction="out"/>
</symbol>
<symbol name="CAP_POL">
<pin name="+" direction="pas"/>
<pin name="-" direction="pas"/>
</symbol>
<symbol name="GND">
<pin name="GND" direction="sup"/>
</symbol>
<symbol name="V-REG-LDO">
<pin name="IN" direction="in"/>
<pin name="GND" direction="in"/>
<pin name="OUT" direction="pas"/>
<pin name="EN" direction="in"/>
<pin name="BP" direction="in"/>
</symbol>
<symbol name="LD1117A">
<pin name="VIN"/>
<pin name="GND(ADJ)"/>
<pin name="VOUT"/>
</symbol>
<symbol name="DIODE-SCHOTTKY">
<pin name="A" direction="pas"/>
<pin name="C" direction="pas"/>
</symbol>
<symbol name="PTC">
<pin name="1"/>
<pin name="2"/>
</symbol>
<symbol name="MINI-USB">
<pin name="1" direction="sup"/>
<pin name="2"/>
<pin name="3"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="sup"/>
<pin name="GND1"/>
<pin name="GND2"/>
<pin name="GND3"/>
<pin name="GND4"/>
</symbol>
<symbol name="MV">
<pin name="S" direction="pas"/>
</symbol>
<symbol name="M">
<pin name="S" direction="pas"/>
</symbol>
<symbol name="RN4">
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="1" direction="pas"/>
<pin name="8" direction="pas"/>
</symbol>
<symbol name="SN74LVC2T45">
<pin name="VCCA" direction="pas"/>
<pin name="A1"/>
<pin name="A2"/>
<pin name="GND" direction="sup"/>
<pin name="DIR" direction="in"/>
<pin name="B2"/>
<pin name="B1"/>
<pin name="VCCB" direction="pas"/>
</symbol>
<symbol name="NOT-CONNECTED">
</symbol>
<symbol name="SN65HVD232">
<pin name="D" direction="in"/>
<pin name="R" direction="out"/>
<pin name="VCC" direction="in"/>
<pin name="GND" direction="sup"/>
<pin name="CANH"/>
<pin name="CANL"/>
<pin name="NC2" direction="nc"/>
<pin name="NC" direction="nc"/>
</symbol>
<symbol name="SWITCH-MOMENTARY-2">
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
</symbol>
<symbol name="INDUCTOR">
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
</symbol>
<symbol name="TXB0104">
<pin name="A1"/>
<pin name="A2"/>
<pin name="A3"/>
<pin name="A4"/>
<pin name="B1"/>
<pin name="B2"/>
<pin name="B3"/>
<pin name="B4"/>
<pin name="VCCA" direction="in"/>
<pin name="VCCB" direction="in"/>
<pin name="OE" direction="in"/>
<pin name="GND" direction="sup"/>
<pin name="P$1" direction="nc"/>
<pin name="P$2" direction="nc"/>
</symbol>
<symbol name="TX?0102">
<pin name="A1"/>
<pin name="A2"/>
<pin name="B1"/>
<pin name="B2"/>
<pin name="VCCA" direction="in"/>
<pin name="VCCB" direction="in"/>
<pin name="GND" direction="sup"/>
<pin name="OE" direction="in"/>
</symbol>
<symbol name="MICROSD">
<pin name="CS"/>
<pin name="DI"/>
<pin name="VCC" direction="pas"/>
<pin name="CLK" function="clk"/>
<pin name="GND" direction="sup"/>
<pin name="DO"/>
</symbol>
<symbol name="LIS331DLH">
<pin name="RES_P15_VDD"/>
<pin name="NC_P2" direction="nc"/>
<pin name="NC_P3" direction="nc"/>
<pin name="GND1"/>
<pin name="GND2"/>
<pin name="GND3"/>
<pin name="GND4"/>
<pin name="VDD_IO"/>
<pin name="SCL/SPC" direction="in"/>
<pin name="SDA/SDI/SDO"/>
<pin name="SDO/SA0"/>
<pin name="CS" direction="in"/>
<pin name="INT1" direction="out"/>
<pin name="INT2" direction="out"/>
<pin name="VDD"/>
<pin name="RES_P10_GND" direction="in"/>
</symbol>
<symbol name="L3G4200DH">
<pin name="RES_P11_GND"/>
<pin name="RES_P8_GND"/>
<pin name="RES_P9_GND"/>
<pin name="RES_P10_GND"/>
<pin name="RES_P12_GND"/>
<pin name="PLLFILT"/>
<pin name="RES_P15_VDD"/>
<pin name="VDD_IO"/>
<pin name="SCL/SPC" direction="in"/>
<pin name="SDA/SDI/SDO"/>
<pin name="SDO/SA0"/>
<pin name="CS" direction="in"/>
<pin name="INT1" direction="out"/>
<pin name="DRDY/INT2" direction="out"/>
<pin name="VDD"/>
<pin name="GND"/>
</symbol>
<symbol name="HMC5843">
<pin name="AVDD"/>
<pin name="DRDY"/>
<pin name="SDA"/>
<pin name="AGND"/>
<pin name="VREN"/>
<pin name="SCLP"/>
<pin name="SDAP"/>
<pin name="SCL"/>
<pin name="C1"/>
<pin name="SETC"/>
<pin name="DVDD"/>
<pin name="DGND"/>
<pin name="SVDD"/>
<pin name="SETN"/>
<pin name="SETP"/>
<pin name="OFFN"/>
<pin name="OFFP"/>
</symbol>
<symbol name="BMP085">
<pin name="XCLR"/>
<pin name="SDA"/>
<pin name="SCL"/>
<pin name="NC"/>
<pin name="VDDD"/>
<pin name="VDDA"/>
<pin name="EOC"/>
<pin name="GND"/>
</symbol>
<symbol name="ST2329A">
<pin name="VL1"/>
<pin name="VL2"/>
<pin name="VCC1"/>
<pin name="VCC2"/>
<pin name="VL" direction="sup"/>
<pin name="VCC" direction="sup"/>
<pin name="GND" direction="sup"/>
<pin name="OE" direction="in"/>
<pin name="NC4" direction="nc"/>
<pin name="NC5" direction="nc"/>
</symbol>
<symbol name="ST2349A">
<pin name="VL_PIN6" direction="sup"/>
<pin name="VL1"/>
<pin name="VL2"/>
<pin name="VL3"/>
<pin name="VL4"/>
<pin name="VCC_PIN7" direction="sup"/>
<pin name="VCC1"/>
<pin name="VCC2"/>
<pin name="VCC3"/>
<pin name="VCC4"/>
<pin name="GND"/>
<pin name="OE" direction="in"/>
<pin name="NC1" direction="nc"/>
<pin name="NC2" direction="nc"/>
<pin name="VL_PIN15" direction="sup"/>
<pin name="VCC_PIN14" direction="sup"/>
</symbol>
<symbol name="JUMPER-3">
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
</symbol>
<symbol name="LED">
<pin name="C" direction="pas"/>
<pin name="A" direction="pas"/>
</symbol>
<symbol name="MOUNT-HOLE">
</symbol>
<symbol name="PORT_A_L-1">
<pin name="PA0"/>
<pin name="PA1"/>
<pin name="PA2"/>
<pin name="PA3"/>
<pin name="PA4"/>
<pin name="PA5"/>
<pin name="PA6"/>
<pin name="PA7"/>
</symbol>
<symbol name="PORT_A_H-1">
<pin name="PA8"/>
<pin name="PA9"/>
<pin name="PA10"/>
<pin name="PA11"/>
<pin name="PA12"/>
<pin name="PA13"/>
<pin name="PA14"/>
<pin name="PA15"/>
</symbol>
<symbol name="PORT_B_L-1">
<pin name="PB0"/>
<pin name="PB1"/>
<pin name="PB2"/>
<pin name="PB3"/>
<pin name="PB4"/>
<pin name="PB5"/>
<pin name="PB6"/>
<pin name="PB7"/>
</symbol>
<symbol name="PORT_B_H-1">
<pin name="PB8"/>
<pin name="PB9"/>
<pin name="PB10"/>
<pin name="PB11"/>
<pin name="PB12"/>
<pin name="PB13"/>
<pin name="PB14"/>
<pin name="PB15"/>
</symbol>
<symbol name="VCC_VDD_S">
<pin name="VDD_1" direction="pwr"/>
<pin name="VDD_2" direction="pwr"/>
<pin name="VDD_3" direction="pwr"/>
<pin name="VSS_1" direction="pwr"/>
<pin name="VSS_2" direction="pwr"/>
<pin name="VSS_3" direction="pwr"/>
</symbol>
<symbol name="PORT_C_3">
<pin name="PC13"/>
<pin name="PC14"/>
<pin name="PC15"/>
</symbol>
<symbol name="PORT_D_2">
<pin name="PD0/OSC&lt;="/>
<pin name="PD1/OSC=&gt;"/>
</symbol>
<symbol name="BAT_AN_M-1">
<pin name="VBAT" direction="pwr"/>
<pin name="VSSA" direction="pwr"/>
<pin name="VDDA" direction="pwr"/>
</symbol>
<symbol name="BOOT_RST-1">
<pin name="NRST" direction="in" function="dot"/>
<pin name="BOOT0" direction="in"/>
</symbol>
<symbol name="SERVO8">
<pin name="PPM8"/>
<pin name="PPM7"/>
<pin name="PPM6"/>
<pin name="PPM5"/>
<pin name="PPM4"/>
<pin name="PPM3"/>
<pin name="PPM2"/>
<pin name="PPM1"/>
<pin name="+5V@1"/>
<pin name="+5V@2"/>
<pin name="+5V@3"/>
<pin name="+5V@4"/>
<pin name="+5V@5"/>
<pin name="+5V@6"/>
<pin name="+5V@7"/>
<pin name="+5V@8"/>
<pin name="GND@1"/>
<pin name="GND@2"/>
<pin name="GND@3"/>
<pin name="GND@4"/>
<pin name="GND@5"/>
<pin name="GND@7"/>
<pin name="GND@6"/>
<pin name="GND@8"/>
</symbol>
<symbol name="SERVO1">
<pin name="PPM"/>
<pin name="+5V"/>
<pin name="GND"/>
</symbol>
<symbol name="INVERTER">
<pin name="NC"/>
<pin name="A"/>
<pin name="GND"/>
<pin name="Y"/>
<pin name="VCC"/>
</symbol>
<symbol name="PHOTO-MOSFET">
<pin name="1"/>
<pin name="2"/>
<pin name="4"/>
<pin name="3"/>
</symbol>
<symbol name="XBEE-1">
<pin name="VDD" direction="pwr"/>
<pin name="DOUT" direction="out"/>
<pin name="DIN" direction="in"/>
<pin name="DIO12"/>
<pin name="RESET" direction="in" function="dot"/>
<pin name="RSSI"/>
<pin name="DIO11"/>
<pin name="RES@8"/>
<pin name="DTR" function="dot"/>
<pin name="GND" direction="pwr"/>
<pin name="DIO4"/>
<pin name="CTS" direction="out" function="dot"/>
<pin name="DIO9"/>
<pin name="RES@14"/>
<pin name="DIO5"/>
<pin name="RTS" direction="in" function="dot"/>
<pin name="DIO3"/>
<pin name="DIO2"/>
<pin name="DIO1"/>
<pin name="DIO0"/>
</symbol>
<symbol name="SN74LVC8T245">
<pin name="VCCA"/>
<pin name="DIR"/>
<pin name="A1"/>
<pin name="A2"/>
<pin name="A3"/>
<pin name="A4"/>
<pin name="A5"/>
<pin name="A6"/>
<pin name="A7"/>
<pin name="A8"/>
<pin name="GND@1"/>
<pin name="GND@2"/>
<pin name="VCCB@1"/>
<pin name="VCCB@2"/>
<pin name="OE"/>
<pin name="B1"/>
<pin name="B2"/>
<pin name="B3"/>
<pin name="B4"/>
<pin name="B5"/>
<pin name="B6"/>
<pin name="B7"/>
<pin name="B8"/>
<pin name="GND@3"/>
</symbol>
<symbol name="TPS2051">
<pin name="IN" direction="sup"/>
<pin name="EN" direction="in"/>
<pin name="GND" direction="sup"/>
<pin name="!OC" direction="oc"/>
<pin name="OUT" direction="out"/>
</symbol>
<symbol name="74LVC2GU04">
<pin name="VCC" direction="sup"/>
<pin name="GND" direction="sup"/>
<pin name="1A"/>
<pin name="2A"/>
<pin name="1Y"/>
<pin name="2Y"/>
</symbol>
<symbol name="XBEE">
<pin name="VDD" direction="pwr"/>
<pin name="DOUT" direction="out"/>
<pin name="DIN" direction="in"/>
<pin name="RSSI"/>
<pin name="GND" direction="pwr"/>
<pin name="DIO4"/>
<pin name="CTS" direction="out" function="dot"/>
<pin name="RTS" direction="in" function="dot"/>
<pin name="DIO0"/>
</symbol>
<symbol name="PTH08080W">
<pin name="VIN" direction="sup"/>
<pin name="VOUT" direction="sup"/>
<pin name="IHN"/>
<pin name="GND" direction="sup"/>
<pin name="ADJ"/>
</symbol>
<symbol name="PRESSURE-SENSOR">
<pin name="+5V"/>
<pin name="VOUT"/>
<pin name="GND"/>
</symbol>
<symbol name="PAD">
<pin name="P$1" direction="pas"/>
</symbol>
<symbol name="EM406">
<pin name="GND1"/>
<pin name="GND2"/>
<pin name="TX"/>
<pin name="RX"/>
<pin name="NC"/>
<pin name="VCC"/>
</symbol>
<symbol name="KV">
<pin name="S" direction="pas"/>
</symbol>
<symbol name="K">
<pin name="S" direction="pas"/>
</symbol>
<symbol name="74LVC2G240">
<pin name="VCC" direction="sup"/>
<pin name="GND" direction="sup"/>
<pin name="1A"/>
<pin name="2A"/>
<pin name="1Y"/>
<pin name="2Y"/>
<pin name="!1OE" direction="in"/>
<pin name="!2OE" direction="in"/>
</symbol>
<symbol name="PAD-1">
<pin name="P" direction="pas"/>
</symbol>
<symbol name="MEDIATEK_MT3329">
<pin name="3D-FIX" direction="out"/>
<pin name="D+"/>
<pin name="D-"/>
<pin name="ENABLE" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="GND2" direction="pas"/>
<pin name="NC" direction="nc"/>
<pin name="NC2" direction="nc"/>
<pin name="RXD-I" direction="in"/>
<pin name="TXD-O" direction="out"/>
<pin name="VBACKUP" direction="pwr"/>
<pin name="VCC" direction="pwr"/>
</symbol>
<symbol name="HMC5883L">
<pin name="VDD"/>
<pin name="DRDY"/>
<pin name="SDA"/>
<pin name="GND1"/>
<pin name="SCL"/>
<pin name="C1"/>
<pin name="SETC"/>
<pin name="VDDIO"/>
<pin name="GND2"/>
<pin name="SETP"/>
<pin name="S1_VDDIO"/>
<pin name="NC_P3" direction="nc"/>
<pin name="NC_P5" direction="nc"/>
<pin name="NC_P6" direction="nc"/>
<pin name="NC_P7" direction="nc"/>
<pin name="NC_P14" direction="nc"/>
</symbol>
<symbol name="ADH8066">
<pin name="1.8V"/>
<pin name="ADC1"/>
<pin name="AUXOUTN"/>
<pin name="AUXOUTP"/>
<pin name="BATTTEMP"/>
<pin name="CHV_DRV"/>
<pin name="CHV_MAX"/>
<pin name="CTS0"/>
<pin name="DCD0"/>
<pin name="DSR0"/>
<pin name="DTR0"/>
<pin name="EARN"/>
<pin name="EARP"/>
<pin name="GND@6"/>
<pin name="GND@21"/>
<pin name="GND@22"/>
<pin name="GND@23"/>
<pin name="GND@24"/>
<pin name="GND@25"/>
<pin name="GND@42"/>
<pin name="GPIO3"/>
<pin name="GPIO10"/>
<pin name="MIC1_N"/>
<pin name="MIC1_P"/>
<pin name="MIC2_N"/>
<pin name="MIC2_P"/>
<pin name="ON_KEY"/>
<pin name="PCMCLK"/>
<pin name="PCMDI"/>
<pin name="PCMDO"/>
<pin name="PCMFSO"/>
<pin name="RI0"/>
<pin name="RTS0"/>
<pin name="RXD0"/>
<pin name="RXD1"/>
<pin name="SCL(NC)"/>
<pin name="SDA(NC)"/>
<pin name="SIMCLK"/>
<pin name="SIMIO"/>
<pin name="SIMRST"/>
<pin name="SIMVDD"/>
<pin name="TXD0"/>
<pin name="TXD1"/>
<pin name="VBAT@26"/>
<pin name="VBAT@27"/>
<pin name="VBAT@28"/>
<pin name="VBAT@29"/>
<pin name="VBAT@30"/>
<pin name="VCHAR@18"/>
<pin name="VCHAR@19"/>
</symbol>
<symbol name="LENSMOUNT_M12">
</symbol>
<symbol name="ADNS-2080">
<pin name="SDIO"/>
<pin name="LED" direction="in"/>
<pin name="MOTION" direction="out"/>
<pin name="VDDIO" direction="in"/>
<pin name="SCLK" direction="in"/>
<pin name="GND" direction="in"/>
<pin name="VDD" direction="out"/>
<pin name="VDDA" direction="in"/>
</symbol>
<symbol name="MOSFET-NCHANNEL">
<pin name="G" direction="pas"/>
<pin name="D" direction="pas"/>
<pin name="S" direction="pas"/>
</symbol>
<symbol name="JUMPER-2">
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
</symbol>
<symbol name="POWERJACK">
<pin name="GNDBREAK"/>
<pin name="GND"/>
<pin name="PWR"/>
</symbol>
<symbol name="MOSFET-PCHANNEL-6POS">
<pin name="G" direction="pas"/>
<pin name="D" direction="pas"/>
<pin name="S" direction="pas"/>
<pin name="D1" direction="pas"/>
<pin name="D2" direction="pas"/>
<pin name="D3" direction="pas"/>
</symbol>
<symbol name="TS3A24157">
<pin name="NC2"/>
<pin name="IN1"/>
<pin name="NO1"/>
<pin name="NC1"/>
<pin name="NO2"/>
<pin name="GND"/>
<pin name="V+"/>
<pin name="COM1"/>
<pin name="IN2"/>
<pin name="COM2"/>
</symbol>
<symbol name="FT4232H">
<pin name="!RESET"/>
<pin name="REF"/>
<pin name="DP"/>
<pin name="DM"/>
<pin name="VREGOUT"/>
<pin name="VREGIN"/>
<pin name="EECS"/>
<pin name="EECLK"/>
<pin name="EEDATA"/>
<pin name="OSCI"/>
<pin name="OSCO"/>
<pin name="TEST"/>
<pin name="AGND"/>
<pin name="GND1"/>
<pin name="GND2"/>
<pin name="GND3"/>
<pin name="GND4"/>
<pin name="GND5"/>
<pin name="GND6"/>
<pin name="GND7"/>
<pin name="GND8"/>
<pin name="!SUSPEND"/>
<pin name="!PWREN"/>
<pin name="DDBUS7"/>
<pin name="DDBUS6"/>
<pin name="DDBUS5"/>
<pin name="DDBUS4"/>
<pin name="DDBUS3"/>
<pin name="DDBUS2"/>
<pin name="DDBUS1"/>
<pin name="DDBUS0"/>
<pin name="CDBUS7"/>
<pin name="CDBUS6"/>
<pin name="CDBUS5"/>
<pin name="CDBUS4"/>
<pin name="CDBUS3"/>
<pin name="CDBUS2"/>
<pin name="CDBUS1"/>
<pin name="CDBUS0"/>
<pin name="BDBUS7"/>
<pin name="BDBUS6"/>
<pin name="BDBUS5"/>
<pin name="BDBUS4"/>
<pin name="BDBUS3"/>
<pin name="BDBUS2"/>
<pin name="BDBUS1"/>
<pin name="BDBUS0"/>
<pin name="ADBUS7"/>
<pin name="ADBUS6"/>
<pin name="ADBUS5"/>
<pin name="ADBUS4"/>
<pin name="ADBUS3"/>
<pin name="ADBUS2"/>
<pin name="ADBUS1"/>
<pin name="ADBUS0"/>
<pin name="VCCIO4"/>
<pin name="VCCIO3"/>
<pin name="VCCIO2"/>
<pin name="VCCIO1"/>
<pin name="VCORE3"/>
<pin name="VCORE2"/>
<pin name="VCORE1"/>
<pin name="VPLL"/>
<pin name="VPHY"/>
</symbol>
<symbol name="TOGGLE">
<pin name="P" direction="pas"/>
<pin name="S" direction="pas"/>
<pin name="O" direction="pas"/>
</symbol>
<symbol name="USB">
<pin name="D+"/>
<pin name="D-"/>
<pin name="VBUS"/>
<pin name="GND"/>
</symbol>
<symbol name="1.8V">
<pin name="VDD_1V8" direction="sup"/>
</symbol>
<symbol name="2.8V">
<pin name="VDD_2V8" direction="sup"/>
</symbol>
<symbol name="3.3V">
<pin name="VDD_3V3" direction="sup"/>
</symbol>
<symbol name="5V">
<pin name="VDD_5V" direction="sup"/>
</symbol>
<symbol name="EEPROM-SERIAL">
<pin name="DO" direction="out"/>
<pin name="NC" direction="nc"/>
<pin name="VCC" direction="pwr"/>
<pin name="ORG"/>
<pin name="VSS" direction="pwr"/>
<pin name="DI" direction="in"/>
<pin name="CS" direction="in"/>
<pin name="CLK" direction="in"/>
</symbol>
<symbol name="BMA180">
<pin name="NC"/>
<pin name="VDD"/>
<pin name="VSS"/>
<pin name="INT"/>
<pin name="CSB"/>
<pin name="NC1"/>
<pin name="SCK"/>
<pin name="SDO"/>
<pin name="SDI"/>
<pin name="VDDIO"/>
<pin name="NC2"/>
<pin name="NC3"/>
</symbol>
<symbol name="ITG-3200">
<pin name="CLKIN"/>
<pin name="VLOGIC"/>
<pin name="AD0"/>
<pin name="REGOUT"/>
<pin name="RESV-G"/>
<pin name="INT"/>
<pin name="SDA"/>
<pin name="SCL"/>
<pin name="CPOUT"/>
<pin name="GND"/>
<pin name="VDD"/>
</symbol>
<symbol name="OSHW-LOGO">
</symbol>
<symbol name="MS5611-01BA">
<pin name="CSB1"/>
<pin name="VDD"/>
<pin name="PS"/>
<pin name="GND"/>
<pin name="SCLK"/>
<pin name="SDO"/>
<pin name="SDI/SDA"/>
<pin name="CSB2"/>
</symbol>
<symbol name="PNP">
<pin name="B" direction="pas"/>
<pin name="C" direction="pas"/>
<pin name="E" direction="pas"/>
</symbol>
<symbol name="NPN">
<pin name="B" direction="pas"/>
<pin name="E" direction="pas"/>
<pin name="C" direction="pas"/>
</symbol>
<symbol name="MT9V034">
</symbol>
<symbol name="MT9V032">
<pin name="!RESET" direction="in"/>
<pin name="AGND@34" direction="pwr"/>
<pin name="AGND@38" direction="pwr"/>
<pin name="BYPASS_CLKIN_N" direction="in"/>
<pin name="BYPASS_CLKIN_P" direction="in"/>
<pin name="DGND@13" direction="pwr"/>
<pin name="DGND@48" direction="pwr"/>
<pin name="DOUT0" direction="out"/>
<pin name="DOUT1" direction="out"/>
<pin name="DOUT2" direction="out"/>
<pin name="DOUT3" direction="out"/>
<pin name="DOUT4" direction="out"/>
<pin name="DOUT5" direction="out"/>
<pin name="DOUT6" direction="out"/>
<pin name="DOUT7" direction="out"/>
<pin name="DOUT8" direction="out"/>
<pin name="DOUT9" direction="out"/>
<pin name="EXPOSURE" direction="in"/>
<pin name="FRAME_VALID" direction="out"/>
<pin name="LED_OUT" direction="out"/>
<pin name="LINE_VALID" direction="out"/>
<pin name="LVDS_GND@7" direction="pwr"/>
<pin name="LVDS_GND@12" direction="pwr"/>
<pin name="NC@36" direction="nc"/>
<pin name="NC@37" direction="nc"/>
<pin name="OE" direction="in"/>
<pin name="PIXCLK" direction="out"/>
<pin name="RSVD" direction="in"/>
<pin name="SCLK" direction="in"/>
<pin name="SCTRL_ADR0" direction="in"/>
<pin name="SCTRL_ADR1" direction="in"/>
<pin name="SDATA"/>
<pin name="SER_DATAIN_N" direction="in"/>
<pin name="SER_DATAIN_P" direction="in"/>
<pin name="SER_DATAOUT_N" direction="out"/>
<pin name="SER_DATAOUT_P" direction="out"/>
<pin name="SHFT_CLKOUT_N" direction="out"/>
<pin name="SHFT_CLKOUT_P" direction="out"/>
<pin name="STANDBY" direction="in"/>
<pin name="STFRM_OUT"/>
<pin name="STLN_OUT"/>
<pin name="SYSCLK" direction="in"/>
<pin name="VAA@35" direction="in"/>
<pin name="VAA@39" direction="in"/>
<pin name="VAA_PIX" direction="in"/>
<pin name="VDD@1" direction="in"/>
<pin name="VDD@14" direction="in"/>
<pin name="VDD_LVDS" direction="in"/>
</symbol>
<symbol name="PORT_C_L-1">
<pin name="PC0"/>
<pin name="PC1"/>
<pin name="PC2"/>
<pin name="PC3"/>
<pin name="PC4"/>
<pin name="PC5"/>
<pin name="PC6"/>
<pin name="PC7"/>
</symbol>
<symbol name="PORT_C_H-1">
<pin name="PC13"/>
<pin name="PC14"/>
<pin name="PC15"/>
<pin name="PC8"/>
<pin name="PC9"/>
<pin name="PC10"/>
<pin name="PC11"/>
<pin name="PC12"/>
</symbol>
<symbol name="PORT_D_L">
<pin name="PD0"/>
<pin name="PD1"/>
<pin name="PD2"/>
<pin name="PD3"/>
<pin name="PD4"/>
<pin name="PD5"/>
<pin name="PD6"/>
<pin name="PD7"/>
</symbol>
<symbol name="PORT_D_H">
<pin name="PD8"/>
<pin name="PD9"/>
<pin name="PD10"/>
<pin name="PD11"/>
<pin name="PD12"/>
<pin name="PD13"/>
<pin name="PD14"/>
<pin name="PD15"/>
</symbol>
<symbol name="PORT_E_L">
<pin name="PE0"/>
<pin name="PE1"/>
<pin name="PE2"/>
<pin name="PE3"/>
<pin name="PE4"/>
<pin name="PE5"/>
<pin name="PE6"/>
<pin name="PE7"/>
</symbol>
<symbol name="PORT_E_H">
<pin name="PE8"/>
<pin name="PE9"/>
<pin name="PE10"/>
<pin name="PE11"/>
<pin name="PE12"/>
<pin name="PE13"/>
<pin name="PE14"/>
<pin name="PE15"/>
</symbol>
<symbol name="VCC_VSS_L">
<pin name="VDD@1" direction="pwr"/>
<pin name="VDD@2" direction="pwr"/>
<pin name="VDD@3" direction="pwr"/>
<pin name="VSS@1" direction="pwr"/>
<pin name="VSS_4" direction="pwr"/>
<pin name="VSS@3" direction="pwr"/>
<pin name="VDD@4" direction="pwr"/>
<pin name="VCAP_1" direction="pwr"/>
<pin name="VDD@5" direction="pwr"/>
<pin name="VCAP_2" direction="pwr"/>
<pin name="VDD@6" direction="pwr"/>
</symbol>
<symbol name="BAT_AN_L">
<pin name="VBAT" direction="pwr"/>
<pin name="VSSA" direction="pwr"/>
<pin name="VDDA" direction="pwr"/>
<pin name="VREF+" direction="in"/>
<pin name="VREF-" direction="in"/>
<pin name="NC" direction="nc"/>
</symbol>
<symbol name="OSC">
<pin name="OSC_IN" direction="in"/>
<pin name="OSC_OUT" direction="out"/>
</symbol>
<symbol name="STM32F4X_VCC_VSS_L">
<pin name="VDD" direction="pwr"/>
<pin name="VSS" direction="pwr"/>
<pin name="VCAP_1" direction="pwr"/>
<pin name="VCAP_2" direction="pwr"/>
</symbol>
<symbol name="STM32F4X_BAT_AN_L">
<pin name="VBAT" direction="pwr"/>
<pin name="VSSA" direction="pwr"/>
<pin name="VDDA" direction="pwr"/>
<pin name="VREF+" direction="in"/>
</symbol>
<symbol name="MPU-6000">
<pin name="CLKIN"/>
<pin name="NC1"/>
<pin name="NC2"/>
<pin name="NC3"/>
<pin name="NC4"/>
<pin name="AUX_DA"/>
<pin name="AUX_CL"/>
<pin name="/CS"/>
<pin name="AD0/SDO"/>
<pin name="REGOUT"/>
<pin name="FSYNC"/>
<pin name="INT"/>
<pin name="VDD"/>
<pin name="NC5"/>
<pin name="NC6"/>
<pin name="NC7"/>
<pin name="NC8"/>
<pin name="GND"/>
<pin name="RESV1"/>
<pin name="CPOUT"/>
<pin name="RESV2"/>
<pin name="CLKOUT"/>
<pin name="SCL/SCLK"/>
<pin name="SDA/SDI"/>
</symbol>
<symbol name="MAX4634EUB+">
<pin name="COM"/>
<pin name="A0" direction="in"/>
<pin name="A1" direction="in"/>
<pin name="EN" direction="in"/>
<pin name="NO1"/>
<pin name="NO2"/>
<pin name="NO3"/>
<pin name="NO4"/>
<pin name="GND"/>
<pin name="V+"/>
</symbol>
<symbol name="QUALIFIED_1_OVERO">
<pin name="ADCIN2"/>
<pin name="ADCIN3"/>
<pin name="ADCIN4"/>
<pin name="ADCIN5"/>
<pin name="ADCIN6"/>
<pin name="ADCIN7"/>
<pin name="AGND"/>
<pin name="AUXLF"/>
<pin name="AUXRF"/>
<pin name="EM_A1"/>
<pin name="EM_A2"/>
<pin name="EM_A3"/>
<pin name="EM_A4"/>
<pin name="EM_A5"/>
<pin name="EM_A6"/>
<pin name="EM_A7"/>
<pin name="EM_A8"/>
<pin name="EM_A9"/>
<pin name="EM_A10"/>
<pin name="EM_CLK"/>
<pin name="EM_D0"/>
<pin name="EM_D1"/>
<pin name="EM_D2"/>
<pin name="EM_D3"/>
<pin name="EM_D4"/>
<pin name="EM_D5"/>
<pin name="EM_D6"/>
<pin name="EM_D7"/>
<pin name="EM_D8"/>
<pin name="EM_D9"/>
<pin name="EM_D10"/>
<pin name="EM_D11"/>
<pin name="EM_D12"/>
<pin name="EM_D13"/>
<pin name="EM_D14"/>
<pin name="EM_D15"/>
<pin name="EM_NADV_ALE"/>
<pin name="EM_NBE0"/>
<pin name="EM_NBE1"/>
<pin name="EM_NCS0"/>
<pin name="EM_NCS1"/>
<pin name="EM_NCS4"/>
<pin name="EM_NCS5_ETH0"/>
<pin name="EM_NCS6"/>
<pin name="EM_NOE"/>
<pin name="EM_NWE"/>
<pin name="EM_NWP"/>
<pin name="EM_WAIT0"/>
<pin name="GND"/>
<pin name="GND@33"/>
<pin name="GND@56"/>
<pin name="GND@70"/>
<pin name="GPIO0_WAKEUP"/>
<pin name="GPIO12_MMC3_CLK"/>
<pin name="GPIO13_MMC3_CMD"/>
<pin name="GPIO14_MMC3_DAT4"/>
<pin name="GPIO17_MMC3_D3"/>
<pin name="GPIO18_MMC3_D0"/>
<pin name="GPIO19_MMC3_D1"/>
<pin name="GPIO20_MMC3_D2"/>
<pin name="GPIO21_MMC3_DAT7"/>
<pin name="GPIO22_MMC3_DAT6"/>
<pin name="GPIO23_MMC3_DAT5"/>
<pin name="GPIO64_ETH0_NRESET"/>
<pin name="GPIO65_ETH1_IRQ1"/>
<pin name="GPIO66_L_PCLK"/>
<pin name="GPIO67_L_LCLK"/>
<pin name="GPIO68_L_FCLK"/>
<pin name="GPIO69_L_BIAS"/>
<pin name="GPIO70_L_DD00"/>
<pin name="GPIO71_L_DD01"/>
<pin name="GPIO72_L_DD02"/>
<pin name="GPIO73_L_DD03"/>
<pin name="GPIO74_L_DD04"/>
<pin name="GPIO75_L_DD05"/>
<pin name="GPIO76_L_DD06"/>
<pin name="GPIO77_L_DD07"/>
<pin name="GPIO78_L_DD08"/>
<pin name="GPIO79_L_DD09"/>
<pin name="GPIO80_L_DD10"/>
<pin name="GPIO81_L_DD11"/>
<pin name="GPIO82_L_DD12"/>
<pin name="GPIO83_L_DD13"/>
<pin name="GPIO84_L_DD14"/>
<pin name="GPIO85_L_DD15"/>
<pin name="GPIO86_L_DD16"/>
<pin name="GPIO87_L_DD17"/>
<pin name="GPIO88_L_DD18"/>
<pin name="GPIO89_L_DD19"/>
<pin name="GPIO90_L_DD20"/>
<pin name="GPIO91_L_DD21"/>
<pin name="GPIO92_L_DD22"/>
<pin name="GPIO93_L_DD23"/>
<pin name="GPIO114_SPI1_NIRQ"/>
<pin name="GPIO127_TS_IRQ"/>
<pin name="GPIO128_GPS_PPS"/>
<pin name="GPIO144_GPT9_PWM"/>
<pin name="GPIO145_GPT10_PWM"/>
<pin name="GPIO146_GPT11_PWM"/>
<pin name="GPIO147_GPT8_PWM"/>
<pin name="GPIO148_TXD1"/>
<pin name="GPIO149_MMC3_CD"/>
<pin name="GPIO150_MMC3_WP"/>
<pin name="GPIO151_RXD1"/>
<pin name="GPIO163_IR_CTS3"/>
<pin name="GPIO165_IR_RXD3"/>
<pin name="GPIO166_IR_TXD3"/>
<pin name="GPIO168_USBH_CPEN"/>
<pin name="GPIO170_HDQ_1WIRE"/>
<pin name="GPIO171_SPI1_CLK"/>
<pin name="GPIO172_SPI1_MOSI"/>
<pin name="GPIO173_SPI1_MISO"/>
<pin name="GPIO174_SPI1_CS0"/>
<pin name="GPIO175_SPI1_CS1"/>
<pin name="GPIO176_ETH0_IRQ"/>
<pin name="GPIO184_I2C3_SCL"/>
<pin name="GPIO185_I2C3_SDA"/>
<pin name="HSOLF"/>
<pin name="HSORF"/>
<pin name="MIC_MAIN_MF"/>
<pin name="MIC_SUB_MF"/>
<pin name="NC@62"/>
<pin name="NC@63"/>
<pin name="N_MANUAL_RESET"/>
<pin name="POWERON"/>
<pin name="PWM0"/>
<pin name="PWM1"/>
<pin name="SYSEN"/>
<pin name="USBH_DM"/>
<pin name="USBH_DP"/>
<pin name="USBH_VBUS"/>
<pin name="USBOTG_DM"/>
<pin name="USBOTG_DP"/>
<pin name="USBOTG_ID"/>
<pin name="USBOTG_VBUS"/>
<pin name="VBACKUP"/>
<pin name="VSYSTEM@1"/>
<pin name="VSYSTEM@2"/>
<pin name="VSYSTEM@66"/>
<pin name="VSYSTEM@67"/>
</symbol>
<symbol name="MAX3051">
<pin name="DIN" direction="in"/>
<pin name="DOUT" direction="out"/>
<pin name="VCC" direction="in"/>
<pin name="GND" direction="sup"/>
<pin name="CANH"/>
<pin name="CANL"/>
<pin name="SHDN" direction="in"/>
<pin name="RS" direction="in"/>
</symbol>
<symbol name="3DROBOTICS_FVAL">
<pin name="B" direction="pas"/>
</symbol>
<symbol name="3DROBOTICS_F">
<pin name="B" direction="pas"/>
</symbol>
<symbol name="MOSFET-PCHANNEL">
<pin name="G" direction="pas"/>
<pin name="D" direction="pas"/>
<pin name="S" direction="pas"/>
</symbol>
<symbol name="B">
<pin name="-" direction="pas"/>
<pin name="+" direction="pas"/>
</symbol>
<symbol name="INA169">
<pin name="OUT"/>
<pin name="GND"/>
<pin name="VIN+"/>
<pin name="VIN-"/>
<pin name="V+"/>
</symbol>
<symbol name="CURRENT-SENSE-KELVIN">
<pin name="V+"/>
<pin name="V-"/>
<pin name="I_IN"/>
<pin name="I_OUT"/>
</symbol>
<symbol name="EEPROM-I2C-5PIN">
<pin name="VSS" direction="pwr"/>
<pin name="WP"/>
<pin name="VCC" direction="pwr"/>
<pin name="SCL"/>
<pin name="SDA"/>
</symbol>
<symbol name="MECH-SERVO">
</symbol>
<symbol name="DUOVERO">
<pin name="ABE_BSP2_CLKX"/>
<pin name="ABE_BSP2_DR"/>
<pin name="ABE_BSP2_DX"/>
<pin name="ABE_BSP2_FSX"/>
<pin name="ADCIN2"/>
<pin name="ADCIN3"/>
<pin name="ADCIN4"/>
<pin name="ADCIN5"/>
<pin name="ADCIN6"/>
<pin name="AGND"/>
<pin name="AUXLF"/>
<pin name="AUXRF"/>
<pin name="BT_EN"/>
<pin name="CAM2_DX0"/>
<pin name="CAM2_DX1"/>
<pin name="CAM2_DY0"/>
<pin name="CAM2_DY1"/>
<pin name="CAM_DX0"/>
<pin name="CAM_DX1"/>
<pin name="CAM_DX2"/>
<pin name="CAM_DX3"/>
<pin name="CAM_DX4"/>
<pin name="CAM_DY0"/>
<pin name="CAM_DY1"/>
<pin name="CAM_DY2"/>
<pin name="CAM_DY3"/>
<pin name="CAM_DY4"/>
<pin name="CAM_RESET"/>
<pin name="CAM_SHUTTER"/>
<pin name="CAM_STROBE"/>
<pin name="DMIC_CLK1"/>
<pin name="DMIC_IN1"/>
<pin name="DMIC_IN2"/>
<pin name="DMIC_IN3"/>
<pin name="EM_CLK"/>
<pin name="EM_D0"/>
<pin name="EM_D1"/>
<pin name="EM_D2"/>
<pin name="EM_D3"/>
<pin name="EM_D4"/>
<pin name="EM_D5"/>
<pin name="EM_D6"/>
<pin name="EM_D7"/>
<pin name="EM_D8"/>
<pin name="EM_D9"/>
<pin name="EM_D10"/>
<pin name="EM_D11"/>
<pin name="EM_D12"/>
<pin name="EM_D13"/>
<pin name="EM_D14"/>
<pin name="EM_D15"/>
<pin name="EM_NADV_ALE"/>
<pin name="EM_NBE0"/>
<pin name="EM_NBE1"/>
<pin name="EM_NCS0"/>
<pin name="EM_NCS1"/>
<pin name="EM_NCS4"/>
<pin name="EM_NCS5_ETH0"/>
<pin name="EM_NCS6"/>
<pin name="EM_NOE"/>
<pin name="EM_NWE"/>
<pin name="EM_NWP"/>
<pin name="EM_WAIT0"/>
<pin name="GND@22"/>
<pin name="GND@24"/>
<pin name="GND@31"/>
<pin name="GND@44"/>
<pin name="GP40"/>
<pin name="GP42"/>
<pin name="GP44"/>
<pin name="GP45"/>
<pin name="GP47"/>
<pin name="GP48"/>
<pin name="GPIO31_WAKEUP"/>
<pin name="GPIO64_ETH0_NRESET"/>
<pin name="GPIO65_ETH1_IRQ1"/>
<pin name="GPIO114_SPI1_NIRQ"/>
<pin name="GPIO127_TS_IRQ"/>
<pin name="GPIO128_GPS_PPS"/>
<pin name="GPIO144_GPT9_PWM"/>
<pin name="GPIO145_GPT10_PWM"/>
<pin name="GPIO146_GPT11_PWM"/>
<pin name="GPIO147_GPT8_PWM"/>
<pin name="GPIO148_TXD1"/>
<pin name="GPIO151_RXD1"/>
<pin name="GPIO163_IR_CTS3"/>
<pin name="GPIO165_IR_RXD3"/>
<pin name="GPIO166_IR_TXD3"/>
<pin name="GPIO170_HDQ_1WIRE"/>
<pin name="GPIO171_SPI1_CLK"/>
<pin name="GPIO172_SPI1_MOSI"/>
<pin name="GPIO173_SPI1_MISO"/>
<pin name="GPIO174_SPI1_CS0"/>
<pin name="GPIO175_SPI1_CS1"/>
<pin name="GPIO176_ETH0_IRQ"/>
<pin name="GPIO184_I2C3_SCL"/>
<pin name="GPIO185_I2C3_SDA"/>
<pin name="HDMI_CEC"/>
<pin name="HDMI_CLOCKX"/>
<pin name="HDMI_CLOCKY"/>
<pin name="HDMI_D0X"/>
<pin name="HDMI_D0Y"/>
<pin name="HDMI_D1X"/>
<pin name="HDMI_D1Y"/>
<pin name="HDMI_D2X"/>
<pin name="HDMI_D2Y"/>
<pin name="HDMI_DDC_SCL"/>
<pin name="HDMI_DDC_SDA"/>
<pin name="HDMI_HPD"/>
<pin name="HDMI_LS_OE"/>
<pin name="HSMIC_PF"/>
<pin name="HSOLF"/>
<pin name="HSORF"/>
<pin name="I2C2_SCL"/>
<pin name="I2C2_SDA"/>
<pin name="I2C4_SCL"/>
<pin name="I2C4_SDA"/>
<pin name="IR_RTS3"/>
<pin name="MIC_MAIN_MF"/>
<pin name="NRESPWRON"/>
<pin name="POWERON"/>
<pin name="PWM1"/>
<pin name="PWM2"/>
<pin name="SYSEN"/>
<pin name="USBH_CPEN"/>
<pin name="USBH_DM"/>
<pin name="USBH_DP"/>
<pin name="USBH_RESET"/>
<pin name="USBH_VBUS"/>
<pin name="USBOTG_CE"/>
<pin name="USBOTG_DM"/>
<pin name="USBOTG_DP"/>
<pin name="USBOTG_ID"/>
<pin name="USBOTG_VBUS_IN"/>
<pin name="VBACKUP"/>
<pin name="VSYSTEM@1"/>
<pin name="VSYSTEM@2"/>
<pin name="VSYSTEM@41"/>
<pin name="VSYSTEM@42"/>
<pin name="WIFI_EN"/>
</symbol>
<symbol name="QUALIFIED_1_USB">
<pin name="1_VBUS" direction="pas"/>
<pin name="2_D-" direction="pas"/>
<pin name="3_D+" direction="pas"/>
<pin name="4_ID" direction="pas"/>
<pin name="5_GND" direction="pas"/>
</symbol>
<symbol name="QUALIFIED_1_M">
<pin name="S" direction="pas"/>
</symbol>
<symbol name="TX?0108">
<pin name="A1"/>
<pin name="A2"/>
<pin name="B1"/>
<pin name="B2"/>
<pin name="VCCA" direction="in"/>
<pin name="VCCB" direction="in"/>
<pin name="GND" direction="sup"/>
<pin name="OE" direction="in"/>
<pin name="A3"/>
<pin name="A4"/>
<pin name="A5"/>
<pin name="A6"/>
<pin name="A7"/>
<pin name="A8"/>
<pin name="B3"/>
<pin name="B4"/>
<pin name="B5"/>
<pin name="B6"/>
<pin name="B7"/>
<pin name="B8"/>
</symbol>
<symbol name="IP4786CZ32">
<pin name="CEC_A"/>
<pin name="CEC_B"/>
<pin name="CON_5V0" direction="pwr"/>
<pin name="ESD_BYP\" direction="pwr"/>
<pin name="HPD_A"/>
<pin name="HPD_B"/>
<pin name="LS_OE"/>
<pin name="NC@30"/>
<pin name="NC@31"/>
<pin name="PGND@PAD" direction="pwr"/>
<pin name="SCL_A"/>
<pin name="SCL_B"/>
<pin name="SDA_A"/>
<pin name="SDA_B"/>
<pin name="SYS_TXC+"/>
<pin name="SYS_TXC-"/>
<pin name="SYS_TXD0+"/>
<pin name="SYS_TXD0-"/>
<pin name="SYS_TXD1+"/>
<pin name="SYS_TXD1-\"/>
<pin name="SYS_TXD2+"/>
<pin name="SYS_TXD2-"/>
<pin name="TXC+"/>
<pin name="TXC-"/>
<pin name="TXD0+"/>
<pin name="TXD0-"/>
<pin name="TXD1+"/>
<pin name="TXD1-"/>
<pin name="TXD2+"/>
<pin name="TXD2-"/>
<pin name="UTILITY" direction="pwr"/>
<pin name="VCC_1.8" direction="pwr"/>
<pin name="VCC_5.0" direction="pwr"/>
</symbol>
<symbol name="MOLEX-HDMI">
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="10" direction="pas"/>
<pin name="11" direction="pas"/>
<pin name="12" direction="pas"/>
<pin name="13" direction="pas"/>
<pin name="14" direction="pas"/>
<pin name="15" direction="pas"/>
<pin name="16" direction="pas"/>
<pin name="17" direction="pas"/>
<pin name="18" direction="pas"/>
<pin name="19" direction="pas"/>
<pin name="20" direction="pas"/>
<pin name="21" direction="pas"/>
<pin name="22" direction="pas"/>
<pin name="23" direction="pas"/>
</symbol>
<symbol name="SWITCH-SPST-4POS">
<pin name="S1A" direction="pas"/>
<pin name="S1B" direction="pas"/>
<pin name="S2A" direction="pas"/>
<pin name="S3A" direction="pas"/>
<pin name="S4A" direction="pas"/>
<pin name="S2B" direction="pas"/>
<pin name="S3B" direction="pas"/>
<pin name="S4B" direction="pas"/>
</symbol>
<symbol name="PX4-LOGO">
</symbol>
<symbol name="SDD_KAAK">
<pin name="K1" direction="pas"/>
<pin name="K2" direction="pas"/>
<pin name="AA" direction="pas"/>
</symbol>
<symbol name="SDD_AKKA">
<pin name="A1" direction="pas"/>
<pin name="A2" direction="pas"/>
<pin name="CC" direction="pas"/>
</symbol>
<symbol name="SCHOTTKY">
<pin name="A" direction="pas"/>
<pin name="C" direction="pas"/>
</symbol>
<symbol name="SDD_AKAK">
<pin name="A1" direction="pas"/>
<pin name="C2" direction="pas"/>
<pin name="C1A2" direction="pas"/>
</symbol>
<symbol name="DMS-20LCD">
<pin name="+5V/+BATTERY"/>
<pin name="-5V/-BATTERY"/>
<pin name="!DP3"/>
<pin name="!DP2"/>
<pin name="!DP1"/>
<pin name="(-)INPUT_LO"/>
<pin name="(+)INPUT_HI"/>
<pin name="AN_COMMON"/>
<pin name="!BACKLIGHT"/>
<pin name="REF_OUT"/>
<pin name="REF_IN"/>
</symbol>
<symbol name="BMA280">
<pin name="VDD"/>
<pin name="INT2"/>
<pin name="INT1"/>
<pin name="CSB"/>
<pin name="GNDIO"/>
<pin name="SCK/SCL"/>
<pin name="SDO"/>
<pin name="SDI/SDA"/>
<pin name="VDDIO"/>
<pin name="GND"/>
<pin name="PS"/>
</symbol>
<symbol name="CD4017">
<pin name="Q0"/>
<pin name="Q1"/>
<pin name="Q2"/>
<pin name="Q3"/>
<pin name="Q4"/>
<pin name="Q5"/>
<pin name="Q6"/>
<pin name="Q7"/>
<pin name="Q8"/>
<pin name="Q9"/>
<pin name="TC"/>
<pin name="GND"/>
<pin name="CLK"/>
<pin name="RST"/>
<pin name="!CLK_EN"/>
<pin name="VCC"/>
</symbol>
<symbol name="STM32F407_BAT_AN">
<pin name="VBAT" direction="pwr"/>
<pin name="VSSA" direction="pwr"/>
<pin name="VDDA" direction="pwr"/>
<pin name="VREF+" direction="in"/>
<pin name="VSS"/>
</symbol>
<symbol name="SERVO4">
<pin name="PPM4"/>
<pin name="PPM3"/>
<pin name="PPM2"/>
<pin name="PPM1"/>
<pin name="VCC_5V@1"/>
<pin name="VCC_5V@2"/>
<pin name="VCC_5V@3"/>
<pin name="VCC_5V@4"/>
<pin name="GND@1"/>
<pin name="GND2@2"/>
<pin name="GND@3"/>
<pin name="GND@4"/>
</symbol>
<symbol name="FM25V01">
<pin name="VDD"/>
<pin name="VSS"/>
<pin name="C"/>
<pin name="D"/>
<pin name="Q"/>
<pin name="!S"/>
<pin name="!W"/>
<pin name="!HOLD"/>
</symbol>
<symbol name="L3GD20H">
<pin name="VDD"/>
<pin name="VDD_IO"/>
<pin name="GND"/>
<pin name="CS"/>
<pin name="DEN"/>
<pin name="SCL/SPC"/>
<pin name="SDA/SDI/SDO"/>
<pin name="SDO/SA0"/>
<pin name="INT1"/>
<pin name="DRDY/INT2"/>
<pin name="CAP"/>
</symbol>
<symbol name="LPS331AP">
<pin name="VDD"/>
<pin name="VDD_IO"/>
<pin name="VCCA"/>
<pin name="GND4"/>
<pin name="GND3"/>
<pin name="GND2"/>
<pin name="GND1"/>
<pin name="RSRV"/>
<pin name="SCL/SPC"/>
<pin name="SDA/SDI/SDO"/>
<pin name="SDO/SA0"/>
<pin name="CS"/>
<pin name="INT1"/>
<pin name="INT2"/>
</symbol>
<symbol name="LSM303D">
<pin name="GND@4"/>
<pin name="GND@3"/>
<pin name="GND@2"/>
<pin name="C1"/>
<pin name="SETP"/>
<pin name="SETC"/>
<pin name="GND@1"/>
<pin name="CS"/>
<pin name="SCL/SPC"/>
<pin name="SDA/SDI/SDO"/>
<pin name="SDO/SA0"/>
<pin name="INT1"/>
<pin name="INT2"/>
<pin name="RSRV"/>
<pin name="VDD"/>
<pin name="VDD_IO"/>
</symbol>
<symbol name="LT3028">
<description>LT3028 dual 100mA/500mA low-dropout regulator</description>
<pin name="IN1" direction="pwr"/>
<pin name="!SHDN1" direction="in"/>
<pin name="IN2" direction="pwr"/>
<pin name="!SHDN2" direction="in"/>
<pin name="OUT1" direction="pwr"/>
<pin name="BYP1"/>
<pin name="ADJ1" direction="in"/>
<pin name="OUT2" direction="pwr"/>
<pin name="BYP2"/>
<pin name="ADJ2" direction="in"/>
<pin name="GND" direction="pwr"/>
</symbol>
<symbol name="TPS76701Q">
<description>TPS76701Q 1A Adjustable LDO</description>
<pin name="IN" direction="pwr"/>
<pin name="!EN" direction="in"/>
<pin name="GND" direction="pwr"/>
<pin name="FB"/>
<pin name="!RESET" direction="oc"/>
<pin name="OUT" direction="pwr"/>
</symbol>
<symbol name="SERVO6">
<pin name="PPM6"/>
<pin name="PPM5"/>
<pin name="PPM4"/>
<pin name="PPM3"/>
<pin name="PPM2"/>
<pin name="PPM1"/>
<pin name="+5V@1"/>
<pin name="+5V@2"/>
<pin name="+5V@3"/>
<pin name="+5V@4"/>
<pin name="+5V@5"/>
<pin name="+5V@6"/>
<pin name="GND@1"/>
<pin name="GND@2"/>
<pin name="GND@3"/>
<pin name="GND@4"/>
<pin name="GND@5"/>
<pin name="GND@6"/>
</symbol>
<symbol name="BATTERY">
<pin name="NEG"/>
<pin name="POS"/>
</symbol>
<symbol name="LTC4411">
<pin name="IN" direction="pwr"/>
<pin name="CTL" direction="pas"/>
<pin name="GND" direction="pwr"/>
<pin name="OUT" direction="pwr"/>
<pin name="STAT" direction="oc"/>
</symbol>
<symbol name="MIC5357">
<description>MIC5357 low-noise dual 500mA LDO</description>
<pin name="IN"/>
<pin name="EN1"/>
<pin name="EN2"/>
<pin name="BYP"/>
<pin name="GND"/>
<pin name="OUT1"/>
<pin name="OUT2"/>
</symbol>
<symbol name="MC14504B">
<description>Hex level shifter</description>
<pin name="VCC" direction="pwr"/>
<pin name="AIN"/>
<pin name="BIN"/>
<pin name="CIN"/>
<pin name="DIN"/>
<pin name="EIN"/>
<pin name="FIN"/>
<pin name="MODE"/>
<pin name="GND"/>
<pin name="FOUT"/>
<pin name="EOUT"/>
<pin name="DOUT"/>
<pin name="COUT"/>
<pin name="BOUT"/>
<pin name="AOUT"/>
<pin name="VDD"/>
</symbol>
<symbol name="LT3469">
<description>LT3469 Piezo Microactuator Driver with Boost Regulator</description>
<pin name="VIN" direction="pwr"/>
<pin name="SW" direction="pas"/>
<pin name="VCC"/>
<pin name="FB"/>
<pin name="GND" direction="pwr"/>
<pin name="OUT" direction="out"/>
<pin name="-IN" direction="in"/>
<pin name="+IN" direction="in"/>
</symbol>
<symbol name="74LVC1G125">
<pin name="VCC" direction="sup"/>
<pin name="GND" direction="sup"/>
<pin name="A"/>
<pin name="Y"/>
<pin name="!OE" direction="in"/>
</symbol>
<symbol name="TCA62724">
<description>TCA62725 I2C RGB LED driver</description>
<pin name="!SHDN" direction="in"/>
<pin name="SDA"/>
<pin name="SCL"/>
<pin name="!RESET" direction="in"/>
<pin name="GND" direction="pwr"/>
<pin name="REXT"/>
<pin name="OUT2" direction="oc"/>
<pin name="OUT1" direction="oc"/>
<pin name="OUT0" direction="oc"/>
<pin name="VIN" direction="pwr"/>
</symbol>
<symbol name="CAP-FEEDTHROUGH">
<description>Feed-through capacitor / EMI filter</description>
<pin name="P$1"/>
<pin name="P$2"/>
<pin name="P$3"/>
</symbol>
<symbol name="IR2301">
<pin name="VCC"/>
<pin name="HIN"/>
<pin name="LIN"/>
<pin name="COM"/>
<pin name="LO"/>
<pin name="VS"/>
<pin name="HO"/>
<pin name="VB"/>
</symbol>
<symbol name="INA169-1">
<pin name="GND"/>
<pin name="OUT"/>
<pin name="V+"/>
<pin name="VIN+"/>
<pin name="VIN-"/>
</symbol>
<symbol name="DIODE">
<pin name="A" direction="pas"/>
<pin name="C" direction="pas"/>
</symbol>
<symbol name="MIC5332">
<pin name="VIN"/>
<pin name="EN1"/>
<pin name="EN2"/>
<pin name="CSET"/>
<pin name="GND"/>
<pin name="VOUT1"/>
<pin name="VOUT2"/>
<pin name="POR2"/>
</symbol>
<symbol name="NUF20X0XV6">
<pin name="D1I"/>
<pin name="GND"/>
<pin name="D2I"/>
<pin name="D2O"/>
<pin name="VBUS"/>
<pin name="D1O"/>
</symbol>
<symbol name="BQ24313">
<pin name="IN"/>
<pin name="OUT"/>
<pin name="VBAT"/>
<pin name="!FAULT"/>
<pin name="!CE"/>
<pin name="VSS"/>
<pin name="ILIM"/>
</symbol>
<symbol name="FR014H5JZ">
<pin name="POS"/>
<pin name="NEG"/>
<pin name="CTL"/>
</symbol>
<symbol name="DIODE-TVS">
<pin name="A" direction="pas"/>
<pin name="C" direction="pas"/>
</symbol>
<symbol name="ZXCT1051">
<pin name="VSENSE+"/>
<pin name="VSENSE-"/>
<pin name="VCC"/>
<pin name="GND"/>
<pin name="VOUT"/>
</symbol>
<symbol name="TPS54332">
<pin name="VIN"/>
<pin name="EN"/>
<pin name="COMP"/>
<pin name="SS"/>
<pin name="GND"/>
<pin name="VSENSE"/>
<pin name="PH"/>
<pin name="BOOT"/>
</symbol>
<symbol name="FIDUCIAL">
</symbol>
<symbol name="LTC4417">
<pin name="V1"/>
<pin name="UV1"/>
<pin name="OV1"/>
<pin name="V2"/>
<pin name="UV2"/>
<pin name="OV2"/>
<pin name="V3"/>
<pin name="UV3"/>
<pin name="OV3"/>
<pin name="GND"/>
<pin name="CAS"/>
<pin name="HYS"/>
<pin name="!SHDN"/>
<pin name="EN"/>
<pin name="VOUT"/>
<pin name="!VALID1"/>
<pin name="!VALID2"/>
<pin name="!VALID3"/>
<pin name="VS1"/>
<pin name="G1"/>
<pin name="VS2"/>
<pin name="G2"/>
<pin name="VS3"/>
<pin name="G3"/>
</symbol>
<symbol name="4525DO">
<pin name="GND"/>
<pin name="VCC"/>
<pin name="SDA/MISO"/>
<pin name="SCL/SCLK"/>
<pin name="INT/SS"/>
</symbol>
<symbol name="MV-1">
<pin name="S" direction="pas"/>
</symbol>
<symbol name="VDD_VSS_M_F1X">
<pin name="VDD@1" direction="pwr"/>
<pin name="VDD@2" direction="pwr"/>
<pin name="VDD@3" direction="pwr"/>
<pin name="VSS@1" direction="pwr"/>
<pin name="VSS@2" direction="pwr"/>
<pin name="VSS@3" direction="pwr"/>
<pin name="VDD@4" direction="pwr"/>
<pin name="VSS@4" direction="pwr"/>
</symbol>
<symbol name="M-1">
<pin name="S" direction="pas"/>
</symbol>
<symbol name="BBB_PLUG_8">
<description>Header</description>
<pin name="P$1"/>
<pin name="P$2"/>
<pin name="P$3"/>
<pin name="P$4"/>
<pin name="P$5"/>
<pin name="P$6"/>
<pin name="P$7"/>
<pin name="P$8"/>
<pin name="P$9"/>
<pin name="P$10"/>
<pin name="P$11"/>
<pin name="P$12"/>
<pin name="P$13"/>
<pin name="P$14"/>
<pin name="P$15"/>
<pin name="P$16"/>
<pin name="P$17"/>
<pin name="P$18"/>
<pin name="P$19"/>
<pin name="P$20"/>
<pin name="P$21"/>
<pin name="P$22"/>
<pin name="P$23"/>
<pin name="P$24"/>
<pin name="P$25"/>
<pin name="P$26"/>
<pin name="P$27"/>
<pin name="P$28"/>
<pin name="P$29"/>
<pin name="P$30"/>
<pin name="P$31"/>
<pin name="P$32"/>
<pin name="P$33"/>
<pin name="P$34"/>
<pin name="P$35"/>
<pin name="P$36"/>
<pin name="P$37"/>
<pin name="P$38"/>
<pin name="P$39"/>
<pin name="P$40"/>
<pin name="P$41"/>
<pin name="P$42"/>
<pin name="P$43"/>
<pin name="P$44"/>
<pin name="P$45"/>
<pin name="P$46"/>
</symbol>
<symbol name="HEAD_10">
<pin name="P$1"/>
<pin name="P$2"/>
<pin name="P$3"/>
<pin name="P$4"/>
<pin name="P$5"/>
<pin name="P$6"/>
</symbol>
<symbol name="LSM9DS0">
<pin name="NC"/>
<pin name="GND@1"/>
<pin name="GND@2"/>
<pin name="GND@3"/>
<pin name="GND@4"/>
<pin name="GND@5"/>
<pin name="C1_XM"/>
<pin name="SETC_XM"/>
<pin name="SETP_XM"/>
<pin name="DEN_G"/>
<pin name="INT_G"/>
<pin name="DRDY_G"/>
<pin name="INT1_XM"/>
<pin name="INT2_XM"/>
<pin name="VDD@1"/>
<pin name="VDD@2"/>
<pin name="VDD@3"/>
<pin name="VDD_IO"/>
<pin name="CS_G"/>
<pin name="CS_XM"/>
<pin name="SPC"/>
<pin name="SDO_G"/>
<pin name="SDO_XM"/>
<pin name="SDA"/>
</symbol>
<symbol name="BEAGLEBONE-1">
<pin name="GND@1" direction="pwr" function="dot"/>
<pin name="GND@2" direction="pwr" function="dot"/>
<pin name="VDD_3V3EXP@1" direction="pwr" function="dot"/>
<pin name="VDD_3V3EXP@2" direction="pwr" function="dot"/>
<pin name="VDD_5V@1" direction="pwr" function="dot"/>
<pin name="VDD_5V@2" direction="pwr" function="dot"/>
<pin name="SYS_5V@1" direction="pwr" function="dot"/>
<pin name="SYS_5V@2" direction="pas" function="dot"/>
<pin name="PWR_BUT" direction="pas" function="dot"/>
<pin name="SYS_RESETN" direction="pas" function="dot"/>
<pin name="UART4_RXD" direction="pas" function="dot"/>
<pin name="GPIO1_28" direction="pas" function="dot"/>
<pin name="UART4_TXD" direction="pas" function="dot"/>
<pin name="EHRPWM1A" direction="pas" function="dot"/>
<pin name="GPIO1_16" direction="pas" function="dot"/>
<pin name="EHRPWM1B" direction="pas" function="dot"/>
<pin name="I2C1_SCL" direction="pas" function="dot"/>
<pin name="I2C1_SDA" direction="pas" function="dot"/>
<pin name="I2C2_SCL" direction="pas" function="dot"/>
<pin name="I2C2_SDA" direction="pas" function="dot"/>
<pin name="UART2_TXD" direction="pas" function="dot"/>
<pin name="UART2_RXD" direction="pas" function="dot"/>
<pin name="GPIO1_17" direction="pas" function="dot"/>
<pin name="UART1_TXD" direction="pas" function="dot"/>
<pin name="GPIO3_21" direction="pas" function="dot"/>
<pin name="UART1_RXD" direction="pas" function="dot"/>
<pin name="GPIO3_19" direction="pas" function="dot"/>
<pin name="SPI1_CS0" direction="pas" function="dot"/>
<pin name="SPI1_DO" direction="pas" function="dot"/>
<pin name="SPI1_DI" direction="pas" function="dot"/>
<pin name="SPI1_SCLK" direction="pas" function="dot"/>
<pin name="VDD_ADC" direction="pas" function="dot"/>
<pin name="AIN4" direction="pas" function="dot"/>
<pin name="GNDA_ADC" direction="pas" function="dot"/>
<pin name="AIN6" direction="pas" function="dot"/>
<pin name="AIN5" direction="pas" function="dot"/>
<pin name="AIN2" direction="pas" function="dot"/>
<pin name="AIN3" direction="pas" function="dot"/>
<pin name="AIN0" direction="pwr" function="dot"/>
<pin name="AIN1" direction="pas" function="dot"/>
<pin name="CLKOUT2" direction="in" function="dot"/>
<pin name="GPIO0_7" direction="pas" function="dot"/>
<pin name="GND@3" direction="pwr" function="dot"/>
<pin name="GND@5" direction="pwr" function="dot"/>
<pin name="GND@4" direction="pwr" function="dot"/>
<pin name="GND@6" direction="pwr" function="dot"/>
<pin name="GND@7" direction="pwr" function="dot"/>
<pin name="GND@8" direction="pwr" function="dot"/>
<pin name="GPIO1_6" direction="pas" function="dot"/>
<pin name="GPIO1_7" direction="pas" function="dot"/>
<pin name="GPIO1_2" direction="pas" function="dot"/>
<pin name="GPIO1_3" direction="pas" function="dot"/>
<pin name="TIMER4" direction="pas" function="dot"/>
<pin name="TIMER7" direction="pas" function="dot"/>
<pin name="TIMER5" direction="pas" function="dot"/>
<pin name="TIMER6" direction="pas" function="dot"/>
<pin name="GPIO1_13" direction="pas" function="dot"/>
<pin name="GPIO1_12" direction="pas" function="dot"/>
<pin name="EHRPWM2B" direction="pas" function="dot"/>
<pin name="GPIO0_26" direction="pas" function="dot"/>
<pin name="GPIO1_15" direction="pas" function="dot"/>
<pin name="GPIO1_14" direction="pas" function="dot"/>
<pin name="GPIO0_27" direction="pas" function="dot"/>
<pin name="GPIO2_1" direction="pas" function="dot"/>
<pin name="EHRPWM2A" direction="pas" function="dot"/>
<pin name="GPIO1_31" direction="pas" function="dot"/>
<pin name="GPIO1_30" direction="pas" function="dot"/>
<pin name="GPIO1_5" direction="pas" function="dot"/>
<pin name="GPIO1_4" direction="pas" function="dot"/>
<pin name="GPIO1_1" direction="pas" function="dot"/>
<pin name="GPIO1_0" direction="pas" function="dot"/>
<pin name="GPIO1_29" direction="pas" function="dot"/>
<pin name="GPIO2_22" direction="pas" function="dot"/>
<pin name="GPIO2_24" direction="pas" function="dot"/>
<pin name="GPIO2_23" direction="pas" function="dot"/>
<pin name="GPIO2_25" direction="pas" function="dot"/>
<pin name="UART5_CTSN" direction="pas" function="dot"/>
<pin name="UART5_RTSN" direction="pas" function="dot"/>
<pin name="UART4_RTSN" direction="pas" function="dot"/>
<pin name="UART3_RTSN" direction="pas" function="dot"/>
<pin name="UART4_CTSN" direction="pas" function="dot"/>
<pin name="UART3_CTSN" direction="pas" function="dot"/>
<pin name="UART5_TXD" direction="pas" function="dot"/>
<pin name="UART5_RXD" direction="pas" function="dot"/>
<pin name="GPIO2_12" direction="pas" function="dot"/>
<pin name="GPIO2_13" direction="pas" function="dot"/>
<pin name="GPIO2_10" direction="pas" function="dot"/>
<pin name="GPIO2_11" direction="pas" function="dot"/>
<pin name="GPIO2_8" direction="pas" function="dot"/>
<pin name="GPIO2_9" direction="pas" function="dot"/>
<pin name="GPIO2_6" direction="pas" function="dot"/>
<pin name="GPIO2_7" direction="pas" function="dot"/>
<pin name="GND@9" function="dot"/>
<pin name="NC@1" function="dot"/>
<pin name="NC@3" function="dot"/>
<pin name="NC@2" function="dot"/>
<pin name="UART0_TXD" function="dot"/>
<pin name="UART0_RXD" function="dot"/>
<pin name="SCREW$1"/>
<pin name="SCREW$2"/>
<pin name="SCREW$3"/>
<pin name="SCREW$4"/>
<pin name="BAT_+_LIPO_1_S"/>
<pin name="BAT_SENSE"/>
<pin name="TEMP_SENSE"/>
<pin name="BATT_GND"/>
</symbol>
<symbol name="3X14RA_SERVO">
<pin name="CH12"/>
<pin name="5V@1"/>
<pin name="GND@1"/>
<pin name="CH11"/>
<pin name="5V@2"/>
<pin name="CH_10"/>
<pin name="CH_9"/>
<pin name="CH_8"/>
<pin name="CH_7"/>
<pin name="CH_6"/>
<pin name="CH_5"/>
<pin name="CH_4"/>
<pin name="CH_3"/>
<pin name="CH_2"/>
<pin name="CH_1"/>
<pin name="PPM/S.BUS_OUT"/>
<pin name="PPM/S.BUS_IN"/>
<pin name="5V@3"/>
<pin name="5V@4"/>
<pin name="5V@5"/>
<pin name="5V@6"/>
<pin name="5V@7"/>
<pin name="5V@8"/>
<pin name="5V@9"/>
<pin name="5V@10"/>
<pin name="5V@11"/>
<pin name="5V@12"/>
<pin name="5V@13"/>
<pin name="5V@14"/>
<pin name="GND@2"/>
<pin name="GND@3"/>
<pin name="GND@4"/>
<pin name="GND@5"/>
<pin name="GND@6"/>
<pin name="GND@7"/>
<pin name="GND@8"/>
<pin name="GND@9"/>
<pin name="GND@10"/>
<pin name="GND@11"/>
<pin name="GND@12"/>
<pin name="GND@13"/>
<pin name="GND@14"/>
</symbol>
<symbol name="MPU-6500">
<pin name="VDDIO"/>
<pin name="NC@1"/>
<pin name="NC@2"/>
<pin name="NC@3"/>
<pin name="NC@4"/>
<pin name="AUX_DA"/>
<pin name="AUX_CL"/>
<pin name="!CS"/>
<pin name="AD0/SDO"/>
<pin name="REGOUT"/>
<pin name="FSYNC"/>
<pin name="INT"/>
<pin name="VDD"/>
<pin name="NC@5"/>
<pin name="NC@6"/>
<pin name="NC@7"/>
<pin name="NC@8"/>
<pin name="GND"/>
<pin name="RESV@1"/>
<pin name="NC@10"/>
<pin name="RESV@2"/>
<pin name="NC@9"/>
<pin name="SCL/SCLK"/>
<pin name="SDA/SDI"/>
</symbol>
<symbol name="LTC3080">
<pin name="IN" direction="in"/>
<pin name="VCONTROL"/>
<pin name="SET"/>
<pin name="OUT" direction="out"/>
</symbol>
<symbol name="MCP14700">
<pin name="VCC" direction="in"/>
<pin name="HI" direction="in"/>
<pin name="LO" direction="in"/>
<pin name="GND" direction="in"/>
<pin name="HIGHDR" direction="in"/>
<pin name="BOOT" direction="in"/>
<pin name="PHASE" direction="in"/>
<pin name="LOWDR" direction="in"/>
</symbol>
</symbols>
<devicesets>
<deviceset name="STM32F20X_TQFP64" prefix="U">
<description>STM32F20x 64pin LQFP</description>
<gates>
<gate name="PORTA_L" symbol="PORT_A_L"/>
<gate name="PORTA_H" symbol="PORT_A_H"/>
<gate name="PORTB_L" symbol="PORT_B_L"/>
<gate name="PORTB_H" symbol="PORT_B_H"/>
<gate name="PORTC_L" symbol="PORT_C_L"/>
<gate name="PORTC_H" symbol="PORT_C_H"/>
<gate name="POWER" symbol="VCC_VDD_M"/>
<gate name="PORTD/OSC" symbol="PORT_D_3"/>
<gate name="AN_POWER" symbol="BAT_AN_M"/>
<gate name="RESET" symbol="BOOT_RST"/>
</gates>
<devices>
<device name="" package="TQFP64">
<connects>
<connect gate="AN_POWER" pin="VBAT" pad="1"/>
<connect gate="AN_POWER" pin="VDDA" pad="13"/>
<connect gate="AN_POWER" pin="VSSA" pad="12"/>
<connect gate="PORTA_H" pin="PA10" pad="43"/>
<connect gate="PORTA_H" pin="PA11" pad="44"/>
<connect gate="PORTA_H" pin="PA12" pad="45"/>
<connect gate="PORTA_H" pin="PA13" pad="46"/>
<connect gate="PORTA_H" pin="PA14" pad="49"/>
<connect gate="PORTA_H" pin="PA15" pad="50"/>
<connect gate="PORTA_H" pin="PA8" pad="41"/>
<connect gate="PORTA_H" pin="PA9" pad="42"/>
<connect gate="PORTA_L" pin="PA0" pad="14"/>
<connect gate="PORTA_L" pin="PA1" pad="15"/>
<connect gate="PORTA_L" pin="PA2" pad="16"/>
<connect gate="PORTA_L" pin="PA3" pad="17"/>
<connect gate="PORTA_L" pin="PA4" pad="20"/>
<connect gate="PORTA_L" pin="PA5" pad="21"/>
<connect gate="PORTA_L" pin="PA6" pad="22"/>
<connect gate="PORTA_L" pin="PA7" pad="23"/>
<connect gate="PORTB_H" pin="PB10" pad="29"/>
<connect gate="PORTB_H" pin="PB11" pad="30"/>
<connect gate="PORTB_H" pin="PB12" pad="33"/>
<connect gate="PORTB_H" pin="PB13" pad="34"/>
<connect gate="PORTB_H" pin="PB14" pad="35"/>
<connect gate="PORTB_H" pin="PB15" pad="36"/>
<connect gate="PORTB_H" pin="PB8" pad="61"/>
<connect gate="PORTB_H" pin="PB9" pad="62"/>
<connect gate="PORTB_L" pin="PB0" pad="26"/>
<connect gate="PORTB_L" pin="PB1" pad="27"/>
<connect gate="PORTB_L" pin="PB2" pad="28"/>
<connect gate="PORTB_L" pin="PB3" pad="55"/>
<connect gate="PORTB_L" pin="PB4" pad="56"/>
<connect gate="PORTB_L" pin="PB5" pad="57"/>
<connect gate="PORTB_L" pin="PB6" pad="58"/>
<connect gate="PORTB_L" pin="PB7" pad="59"/>
<connect gate="PORTC_H" pin="PC10" pad="51"/>
<connect gate="PORTC_H" pin="PC11" pad="52"/>
<connect gate="PORTC_H" pin="PC12" pad="53"/>
<connect gate="PORTC_H" pin="PC13" pad="2"/>
<connect gate="PORTC_H" pin="PC14" pad="3"/>
<connect gate="PORTC_H" pin="PC15" pad="4"/>
<connect gate="PORTC_H" pin="PC8" pad="39"/>
<connect gate="PORTC_H" pin="PC9" pad="40"/>
<connect gate="PORTC_L" pin="PC0" pad="8"/>
<connect gate="PORTC_L" pin="PC1" pad="9"/>
<connect gate="PORTC_L" pin="PC2" pad="10"/>
<connect gate="PORTC_L" pin="PC3" pad="11"/>
<connect gate="PORTC_L" pin="PC4" pad="24"/>
<connect gate="PORTC_L" pin="PC5" pad="25"/>
<connect gate="PORTC_L" pin="PC6" pad="37"/>
<connect gate="PORTC_L" pin="PC7" pad="38"/>
<connect gate="PORTD/OSC" pin="PD2" pad="54"/>
<connect gate="PORTD/OSC" pin="PH0/OSC&lt;=" pad="5"/>
<connect gate="PORTD/OSC" pin="PH1/OSC=&gt;" pad="6"/>
<connect gate="POWER" pin="VCAP_1" pad="31"/>
<connect gate="POWER" pin="VCAP_2" pad="47"/>
<connect gate="POWER" pin="VDD_1" pad="32"/>
<connect gate="POWER" pin="VDD_2" pad="48"/>
<connect gate="POWER" pin="VDD_3" pad="64"/>
<connect gate="POWER" pin="VDD_4" pad="19"/>
<connect gate="POWER" pin="VSS_3" pad="63"/>
<connect gate="POWER" pin="VSS_4" pad="18"/>
<connect gate="RESET" pin="BOOT0" pad="60"/>
<connect gate="RESET" pin="NRST" pad="7"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="OSCILLATOR" prefix="X" uservalue="yes">
<description>Crystal Oscillator in 3.2x2.5 SMD</description>
<gates>
<gate name="G$1" symbol="XTAL"/>
</gates>
<devices>
<device name="-3.2X2.5" package="OSCILLATOR-3.2X2.5">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="NC_2" pad="2"/>
<connect gate="G$1" pin="NC_4" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="" package="OSCILLATOR-5.0X3.2">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="NC_2" pad="2"/>
<connect gate="G$1" pin="NC_4" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="EEPROM-I2C" prefix="U">
<description>&lt;h3&gt;I2C EEPROM&lt;/h3&gt;

Generic footprint for I2C EEPROMS. Compatible types include:

&lt;ul&gt;
  &lt;li&gt;Microchip 24FC128-I/MS&lt;/li&gt;
  &lt;li&gt;Microchip 24AA256-I/MS&lt;/li&gt;
  &lt;li&gt;ST Microelectronics M24128-BWDW6TP&lt;/li&gt;
&lt;/ul&gt;</description>
<gates>
<gate name="G$1" symbol="EEPROM-I2C"/>
</gates>
<devices>
<device name="SMD" package="SO08">
<connects>
<connect gate="G$1" pin="A0" pad="1"/>
<connect gate="G$1" pin="A1" pad="2"/>
<connect gate="G$1" pin="A2" pad="3"/>
<connect gate="G$1" pin="SCL" pad="6"/>
<connect gate="G$1" pin="SDA" pad="5"/>
<connect gate="G$1" pin="VCC" pad="8"/>
<connect gate="G$1" pin="VSS" pad="4"/>
<connect gate="G$1" pin="WP" pad="7"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="MSOP" package="MSOP-8">
<connects>
<connect gate="G$1" pin="A0" pad="1"/>
<connect gate="G$1" pin="A1" pad="2"/>
<connect gate="G$1" pin="A2" pad="3"/>
<connect gate="G$1" pin="SCL" pad="6"/>
<connect gate="G$1" pin="SDA" pad="5"/>
<connect gate="G$1" pin="VCC" pad="8"/>
<connect gate="G$1" pin="VSS" pad="4"/>
<connect gate="G$1" pin="WP" pad="7"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="A3L-LOC" prefix="FRAME" uservalue="yes">
<description>&lt;b&gt;FRAME&lt;/b&gt;&lt;p&gt;
DIN A3, landscape with location and doc. field</description>
<gates>
<gate name="G$1" symbol="A3L-LOC"/>
</gates>
<devices>
<device name="">
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="A4L-LOC" prefix="FRAME" uservalue="yes">
<description>&lt;b&gt;FRAME&lt;/b&gt;&lt;p&gt;
DIN A4, landscape with location and doc. field</description>
<gates>
<gate name="G$1" symbol="A4L-LOC"/>
</gates>
<devices>
<device name="">
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="CAP" prefix="C" uservalue="yes">
<description>&lt;b&gt;Capacitor&lt;/b&gt;
Standard 0603 ceramic capacitor, and 0.1" leaded capacitor.</description>
<gates>
<gate name="G$1" symbol="CAP"/>
</gates>
<devices>
<device name="PTH" package="CAP-PTH-SMALL">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="PTH2" package="CAP-PTH-SMALL2">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="PTH3" package="CAP-PTH-LARGE">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="SMD" package="GRM43D">
<connects>
<connect gate="G$1" pin="1" pad="A"/>
<connect gate="G$1" pin="2" pad="C"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="0402" package="0402-CAP">
<connects>
<connect gate="G$1" pin="1" pad="P$1"/>
<connect gate="G$1" pin="2" pad="P$2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="PTH1" package="CAP-PTH-5MM">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_" package="AXIAL-5MM">
<connects>
<connect gate="G$1" pin="1" pad="P$1"/>
<connect gate="G$1" pin="2" pad="P$2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="1210" package="1210">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="1812" package="1812-CAP">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="1206" package="1206-CAP">
<connects>
<connect gate="G$1" pin="1" pad="P$1"/>
<connect gate="G$1" pin="2" pad="P$2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="0603" package="0603-CAP">
<connects>
<connect gate="G$1" pin="1" pad="P$1"/>
<connect gate="G$1" pin="2" pad="P$2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="0805" package="0805-CAP">
<connects>
<connect gate="G$1" pin="1" pad="P$1"/>
<connect gate="G$1" pin="2" pad="P$2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="RESISTOR" prefix="R" uservalue="yes">
<description>&lt;b&gt;Resistor&lt;/b&gt;
Basic schematic elements and footprints for 0603, 1206, and PTH 1/10th watt (small) resistors.</description>
<gates>
<gate name="G$1" symbol="RESISTOR"/>
</gates>
<devices>
<device name="1206" package="1206">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="PTH1" package="AXIAL-0.3">
<connects>
<connect gate="G$1" pin="1" pad="P$1"/>
<connect gate="G$1" pin="2" pad="P$2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="2010" package="R2010">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="0805" package="0805">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="0603-RES" package="0603-RES">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="0402-RES" package="0402-RES">
<connects>
<connect gate="G$1" pin="1" pad="P$1"/>
<connect gate="G$1" pin="2" pad="P$2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="PTH-1/6W" package="1/6W-RES">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="2512" package="R2512">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="CAP_POL" prefix="C" uservalue="yes">
<description>&lt;b&gt;Capacitor Polarized&lt;/b&gt;
These are standard SMD and PTH capacitors. Normally 10uF, 47uF, and 100uF in electrolytic and tantalum varieties. Always verify the external diameter of the through hole cap, it varies with capacity, voltage, and manufacturer. The EIA devices should be standard.</description>
<gates>
<gate name="G$1" symbol="CAP_POL"/>
</gates>
<devices>
<device name="1206" package="EIA3216">
<connects>
<connect gate="G$1" pin="+" pad="A"/>
<connect gate="G$1" pin="-" pad="C"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="3528" package="EIA3528">
<connects>
<connect gate="G$1" pin="+" pad="A"/>
<connect gate="G$1" pin="-" pad="C"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="PTH1" package="CPOL-RADIAL-100UF-25V">
<connects>
<connect gate="G$1" pin="+" pad="1"/>
<connect gate="G$1" pin="-" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="PTH2" package="CPOL-RADIAL-10UF-25V">
<connects>
<connect gate="G$1" pin="+" pad="1"/>
<connect gate="G$1" pin="-" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="7343" package="EIA7343">
<connects>
<connect gate="G$1" pin="+" pad="A"/>
<connect gate="G$1" pin="-" pad="C"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="G" package="PANASONIC_G">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="E" package="PANASONIC_E">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="C" package="PANASONIC_C">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="F80" package="NIPPON_F80">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="D" package="PANASONIC_D">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="PTH3" package="CPOL-RADIAL-1000UF-63V">
<connects>
<connect gate="G$1" pin="+" pad="1"/>
<connect gate="G$1" pin="-" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="PTH4" package="CPOL-RADIAL-1000UF-25V">
<connects>
<connect gate="G$1" pin="+" pad="1"/>
<connect gate="G$1" pin="-" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="SMD" package="VISHAY_C">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="H13" package="PANASONIC_H13">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="PTH5" package="CPOL-RADIAL-100UF-50V-3.5MM-8MM">
<connects>
<connect gate="G$1" pin="+" pad="1"/>
<connect gate="G$1" pin="-" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="GND" prefix="GND">
<description>&lt;b&gt;SUPPLY SYMBOL&lt;/b&gt;</description>
<gates>
<gate name="1" symbol="GND"/>
</gates>
<devices>
<device name="">
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="V_REG_LDO" prefix="U">
<description>&lt;b&gt;Voltage Regulator LDO&lt;/b&gt;
Standard 150mA LDO voltage regulator in SOT-23 layout. Micrel part MIC5205. BP (by-pass) pin is used to lower output noise with 470pF cap.</description>
<gates>
<gate name="G$1" symbol="V-REG-LDO"/>
</gates>
<devices>
<device name="SMD" package="SOT23-5">
<connects>
<connect gate="G$1" pin="BP" pad="4"/>
<connect gate="G$1" pin="EN" pad="3"/>
<connect gate="G$1" pin="GND" pad="2"/>
<connect gate="G$1" pin="IN" pad="1"/>
<connect gate="G$1" pin="OUT" pad="5"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="SMD2" package="SC70">
<connects>
<connect gate="G$1" pin="BP" pad="4"/>
<connect gate="G$1" pin="EN" pad="3"/>
<connect gate="G$1" pin="GND" pad="2"/>
<connect gate="G$1" pin="IN" pad="1"/>
<connect gate="G$1" pin="OUT" pad="5"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LD1117A">
<description>LD1117A LDO

Datasheet:
http://www.st.com/stonline/books/pdf/docs/7194.pdf</description>
<gates>
<gate name="G$1" symbol="LD1117A"/>
</gates>
<devices>
<device name="S33" package="SOT-223">
<connects>
<connect gate="G$1" pin="GND(ADJ)" pad="1"/>
<connect gate="G$1" pin="VIN" pad="3"/>
<connect gate="G$1" pin="VOUT" pad="2 4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="STR" package="SOT-223">
<connects>
<connect gate="G$1" pin="GND(ADJ)" pad="1"/>
<connect gate="G$1" pin="VIN" pad="3"/>
<connect gate="G$1" pin="VOUT" pad="2 4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="DIODE-SCHOTTKY" prefix="D">
<description>Schottky barrier diode in DO214AC, e.g. Fairchild SS14.</description>
<gates>
<gate name="G$1" symbol="DIODE-SCHOTTKY"/>
</gates>
<devices>
<device name="_SMA" package="SMA-DIODE">
<connects>
<connect gate="G$1" pin="A" pad="A"/>
<connect gate="G$1" pin="C" pad="C"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_DO214" package="DO214AC">
<connects>
<connect gate="G$1" pin="A" pad="A"/>
<connect gate="G$1" pin="C" pad="C"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_MSMP" package="MICROSMP">
<connects>
<connect gate="G$1" pin="A" pad="ANODE"/>
<connect gate="G$1" pin="C" pad="CATHODE"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_SOD323" package="SOD323">
<connects>
<connect gate="G$1" pin="A" pad="A"/>
<connect gate="G$1" pin="C" pad="C"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_DO201" package="DO201AD">
<connects>
<connect gate="G$1" pin="A" pad="A"/>
<connect gate="G$1" pin="C" pad="C"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_TO220" package="TO220-2POS">
<connects>
<connect gate="G$1" pin="A" pad="2"/>
<connect gate="G$1" pin="C" pad="1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_DO41" package="DO41-7">
<connects>
<connect gate="G$1" pin="A" pad="A"/>
<connect gate="G$1" pin="C" pad="C"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="PTC" prefix="F">
<description>&lt;b&gt;Resettable Fuse PTC&lt;/b&gt;
Resettable Fuse. Spark Fun Electronics SKU : COM-08357</description>
<gates>
<gate name="G$1" symbol="PTC"/>
</gates>
<devices>
<device name="PTH" package="PTC">
<connects>
<connect gate="G$1" pin="1" pad="P$1"/>
<connect gate="G$1" pin="2" pad="P$2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="SMD" package="PTC-1206">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="0603" package="0603">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="0402" package="0402-PTC">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MOLEX-47346-0001" prefix="USB">
<description>MICRO USB B, BOTTOM MOUNT</description>
<gates>
<gate name="G$1" symbol="MINI-USB"/>
</gates>
<devices>
<device name="" package="MOLEX-47346-0001">
<connects>
<connect gate="G$1" pin="1" pad="VBUS"/>
<connect gate="G$1" pin="2" pad="D-"/>
<connect gate="G$1" pin="3" pad="D+"/>
<connect gate="G$1" pin="4" pad="ID"/>
<connect gate="G$1" pin="5" pad="GND"/>
<connect gate="G$1" pin="GND1" pad="GND1"/>
<connect gate="G$1" pin="GND2" pad="GND2"/>
<connect gate="G$1" pin="GND3" pad="GND3"/>
<connect gate="G$1" pin="GND4" pad="GND4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="53?-15" prefix="X" uservalue="yes">
<description>&lt;b&gt;CONNECTOR&lt;/b&gt;&lt;p&gt;
wire to board 1.25 mm (.049 inch) pitch header</description>
<gates>
<gate name="-1" symbol="MV"/>
<gate name="-2" symbol="M"/>
<gate name="-3" symbol="M"/>
<gate name="-4" symbol="M"/>
<gate name="-5" symbol="M"/>
<gate name="-6" symbol="M"/>
<gate name="-7" symbol="M"/>
<gate name="-8" symbol="M"/>
<gate name="-9" symbol="M"/>
<gate name="-10" symbol="M"/>
<gate name="-11" symbol="M"/>
<gate name="-12" symbol="M"/>
<gate name="-13" symbol="M"/>
<gate name="-14" symbol="M"/>
<gate name="-15" symbol="M"/>
</gates>
<devices>
<device name="047" package="53047-15">
<connects>
<connect gate="-1" pin="S" pad="1"/>
<connect gate="-10" pin="S" pad="10"/>
<connect gate="-11" pin="S" pad="11"/>
<connect gate="-12" pin="S" pad="12"/>
<connect gate="-13" pin="S" pad="13"/>
<connect gate="-14" pin="S" pad="14"/>
<connect gate="-15" pin="S" pad="15"/>
<connect gate="-2" pin="S" pad="2"/>
<connect gate="-3" pin="S" pad="3"/>
<connect gate="-4" pin="S" pad="4"/>
<connect gate="-5" pin="S" pad="5"/>
<connect gate="-6" pin="S" pad="6"/>
<connect gate="-7" pin="S" pad="7"/>
<connect gate="-8" pin="S" pad="8"/>
<connect gate="-9" pin="S" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="048" package="53048-15">
<connects>
<connect gate="-1" pin="S" pad="1"/>
<connect gate="-10" pin="S" pad="10"/>
<connect gate="-11" pin="S" pad="11"/>
<connect gate="-12" pin="S" pad="12"/>
<connect gate="-13" pin="S" pad="13"/>
<connect gate="-14" pin="S" pad="14"/>
<connect gate="-15" pin="S" pad="15"/>
<connect gate="-2" pin="S" pad="2"/>
<connect gate="-3" pin="S" pad="3"/>
<connect gate="-4" pin="S" pad="4"/>
<connect gate="-5" pin="S" pad="5"/>
<connect gate="-6" pin="S" pad="6"/>
<connect gate="-7" pin="S" pad="7"/>
<connect gate="-8" pin="S" pad="8"/>
<connect gate="-9" pin="S" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="261" package="53261-15">
<connects>
<connect gate="-1" pin="S" pad="1"/>
<connect gate="-10" pin="S" pad="10"/>
<connect gate="-11" pin="S" pad="11"/>
<connect gate="-12" pin="S" pad="12"/>
<connect gate="-13" pin="S" pad="13"/>
<connect gate="-14" pin="S" pad="14"/>
<connect gate="-15" pin="S" pad="15"/>
<connect gate="-2" pin="S" pad="2"/>
<connect gate="-3" pin="S" pad="3"/>
<connect gate="-4" pin="S" pad="4"/>
<connect gate="-5" pin="S" pad="5"/>
<connect gate="-6" pin="S" pad="6"/>
<connect gate="-7" pin="S" pad="7"/>
<connect gate="-8" pin="S" pad="8"/>
<connect gate="-9" pin="S" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="398" package="53398-15">
<connects>
<connect gate="-1" pin="S" pad="1"/>
<connect gate="-10" pin="S" pad="10"/>
<connect gate="-11" pin="S" pad="11"/>
<connect gate="-12" pin="S" pad="12"/>
<connect gate="-13" pin="S" pad="13"/>
<connect gate="-14" pin="S" pad="14"/>
<connect gate="-15" pin="S" pad="15"/>
<connect gate="-2" pin="S" pad="2"/>
<connect gate="-3" pin="S" pad="3"/>
<connect gate="-4" pin="S" pad="4"/>
<connect gate="-5" pin="S" pad="5"/>
<connect gate="-6" pin="S" pad="6"/>
<connect gate="-7" pin="S" pad="7"/>
<connect gate="-8" pin="S" pad="8"/>
<connect gate="-9" pin="S" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="CTS742C083" prefix="RN">
<description>&lt;b&gt;Chip Resistor Array&lt;/b&gt; 4 Single Resistor&lt;p&gt;
Source: http://www.ctscorp.com/components/Datasheets/CTSChipArrayDs.pdf</description>
<gates>
<gate name="G$1" symbol="RN4"/>
</gates>
<devices>
<device name="" package="CTS742C083">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="SN74LVC2T45" prefix="U" uservalue="yes">
<description>DUAL-BIT DUAL-SUPPLY BUS TRANSCEIVER WITH CONFIGURABLE VOLTAGE TRANSLATION AND 3-STATE OUTPUTS</description>
<gates>
<gate name="G$1" symbol="SN74LVC2T45"/>
</gates>
<devices>
<device name="DCUR" package="TI-DCU">
<connects>
<connect gate="G$1" pin="A1" pad="2"/>
<connect gate="G$1" pin="A2" pad="3"/>
<connect gate="G$1" pin="B1" pad="7"/>
<connect gate="G$1" pin="B2" pad="6"/>
<connect gate="G$1" pin="DIR" pad="5"/>
<connect gate="G$1" pin="GND" pad="4"/>
<connect gate="G$1" pin="VCCA" pad="1"/>
<connect gate="G$1" pin="VCCB" pad="8"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="NOT-CONNECTED">
<description>Symbol for unconnected pins

NC</description>
<gates>
<gate name="G$1" symbol="NOT-CONNECTED"/>
</gates>
<devices>
<device name="">
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="53?-04" prefix="X" uservalue="yes">
<description>&lt;b&gt;CONNECTOR&lt;/b&gt;&lt;p&gt;
wire to board 1.25 mm (.049 inch) pitch header</description>
<gates>
<gate name="-1" symbol="MV"/>
<gate name="-2" symbol="M"/>
<gate name="-3" symbol="M"/>
<gate name="-4" symbol="M"/>
</gates>
<devices>
<device name="047" package="53047-04">
<connects>
<connect gate="-1" pin="S" pad="1"/>
<connect gate="-2" pin="S" pad="2"/>
<connect gate="-3" pin="S" pad="3"/>
<connect gate="-4" pin="S" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="048" package="53048-04">
<connects>
<connect gate="-1" pin="S" pad="1"/>
<connect gate="-2" pin="S" pad="2"/>
<connect gate="-3" pin="S" pad="3"/>
<connect gate="-4" pin="S" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="261" package="53261-04">
<connects>
<connect gate="-1" pin="S" pad="1"/>
<connect gate="-2" pin="S" pad="2"/>
<connect gate="-3" pin="S" pad="3"/>
<connect gate="-4" pin="S" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="398" package="53398-04">
<connects>
<connect gate="-1" pin="S" pad="1"/>
<connect gate="-2" pin="S" pad="2"/>
<connect gate="-3" pin="S" pad="3"/>
<connect gate="-4" pin="S" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MAX3051" prefix="U" uservalue="yes">
<description>3.3-V CAN TRANSCEIVER</description>
<gates>
<gate name="G$1" symbol="MAX3051"/>
</gates>
<devices>
<device name="MAX3051ESA" package="SO08">
<connects>
<connect gate="G$1" pin="CANH" pad="7"/>
<connect gate="G$1" pin="CANL" pad="6"/>
<connect gate="G$1" pin="DIN" pad="1"/>
<connect gate="G$1" pin="DOUT" pad="4"/>
<connect gate="G$1" pin="GND" pad="2"/>
<connect gate="G$1" pin="RS" pad="8"/>
<connect gate="G$1" pin="SHDN" pad="5"/>
<connect gate="G$1" pin="VCC" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="MAX3051EKA" package="SOT23-8">
<connects>
<connect gate="G$1" pin="CANH" pad="7"/>
<connect gate="G$1" pin="CANL" pad="6"/>
<connect gate="G$1" pin="DIN" pad="1"/>
<connect gate="G$1" pin="DOUT" pad="4"/>
<connect gate="G$1" pin="GND" pad="2"/>
<connect gate="G$1" pin="RS" pad="8"/>
<connect gate="G$1" pin="SHDN" pad="5"/>
<connect gate="G$1" pin="VCC" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ARM_MINI_JTAG" prefix="J">
<description>&lt;b&gt;CONNECTOR&lt;/b&gt;&lt;p&gt;
wire to board 1.25 mm (.049 inch) pitch header</description>
<gates>
<gate name="-VTREF" symbol="MV"/>
<gate name="-TMS/SWDIO" symbol="M"/>
<gate name="-GND1" symbol="M"/>
<gate name="-TCK/SWCLK" symbol="M"/>
<gate name="-GND2" symbol="M"/>
<gate name="-TDO/SWO" symbol="M"/>
<gate name="-TDI/EXTB" symbol="M"/>
<gate name="-GND3" symbol="M"/>
<gate name="-!RESET" symbol="M"/>
</gates>
<devices>
<device name="-SMT" package="FTSH-105-01-XXX-DV-K">
<connects>
<connect gate="-!RESET" pin="S" pad="10"/>
<connect gate="-GND1" pin="S" pad="3"/>
<connect gate="-GND2" pin="S" pad="5"/>
<connect gate="-GND3" pin="S" pad="9"/>
<connect gate="-TCK/SWCLK" pin="S" pad="4"/>
<connect gate="-TDI/EXTB" pin="S" pad="8"/>
<connect gate="-TDO/SWO" pin="S" pad="6"/>
<connect gate="-TMS/SWDIO" pin="S" pad="2"/>
<connect gate="-VTREF" pin="S" pad="1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-TH" package="FTSH-105-01-XXX-DV">
<connects>
<connect gate="-!RESET" pin="S" pad="10"/>
<connect gate="-GND1" pin="S" pad="3"/>
<connect gate="-GND2" pin="S" pad="5"/>
<connect gate="-GND3" pin="S" pad="9"/>
<connect gate="-TCK/SWCLK" pin="S" pad="4"/>
<connect gate="-TDI/EXTB" pin="S" pad="8"/>
<connect gate="-TDO/SWO" pin="S" pad="6"/>
<connect gate="-TMS/SWDIO" pin="S" pad="2"/>
<connect gate="-VTREF" pin="S" pad="1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-POGO-PINS" package="FTSH-105-01-XXX-DV-K-POGO-PINS">
<connects>
<connect gate="-!RESET" pin="S" pad="10"/>
<connect gate="-GND1" pin="S" pad="3"/>
<connect gate="-GND2" pin="S" pad="5"/>
<connect gate="-GND3" pin="S" pad="9"/>
<connect gate="-TCK/SWCLK" pin="S" pad="4"/>
<connect gate="-TDI/EXTB" pin="S" pad="8"/>
<connect gate="-TDO/SWO" pin="S" pad="6"/>
<connect gate="-TMS/SWDIO" pin="S" pad="2"/>
<connect gate="-VTREF" pin="S" pad="1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-POGO-HOLES" package="FTSH-105-01-XXX-DV-K-POGO-HOLES">
<connects>
<connect gate="-!RESET" pin="S" pad="P$1"/>
<connect gate="-GND1" pin="S" pad="P$2"/>
<connect gate="-GND2" pin="S" pad="P$3"/>
<connect gate="-GND3" pin="S" pad="P$4"/>
<connect gate="-TCK/SWCLK" pin="S" pad="P$5"/>
<connect gate="-TDI/EXTB" pin="S" pad="P$6"/>
<connect gate="-TDO/SWO" pin="S" pad="P$7"/>
<connect gate="-TMS/SWDIO" pin="S" pad="P$8"/>
<connect gate="-VTREF" pin="S" pad="P$9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="SWITCH-MOMENTARY-2" prefix="S">
<gates>
<gate name="G$1" symbol="SWITCH-MOMENTARY-2"/>
</gates>
<devices>
<device name="PTH" package="TACTILE-PTH">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="SMD" package="TACTILE_SWITCH_SMD">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="SMD-2" package="TACTILE_SWITCH_SMD-2">
<connects>
<connect gate="G$1" pin="1" pad="2"/>
<connect gate="G$1" pin="2" pad="1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="12MM" package="TACTILE-PTH-12MM">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-SMD-1101NE" package="TACTILE-SWITCH-1101NE">
<connects>
<connect gate="G$1" pin="1" pad="P$1"/>
<connect gate="G$1" pin="2" pad="P$2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="" package="EVQP7J01K">
<connects>
<connect gate="G$1" pin="1" pad="A1"/>
<connect gate="G$1" pin="2" pad="B3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="53?-03" prefix="X" uservalue="yes">
<description>&lt;b&gt;CONNECTOR&lt;/b&gt;&lt;p&gt;
wire to board 1.25 mm (.049 inch) pitch header</description>
<gates>
<gate name="-1" symbol="MV"/>
<gate name="-2" symbol="M"/>
<gate name="-3" symbol="M"/>
</gates>
<devices>
<device name="047" package="53047-03">
<connects>
<connect gate="-1" pin="S" pad="1"/>
<connect gate="-2" pin="S" pad="2"/>
<connect gate="-3" pin="S" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="048" package="53048-03">
<connects>
<connect gate="-1" pin="S" pad="1"/>
<connect gate="-2" pin="S" pad="2"/>
<connect gate="-3" pin="S" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="261" package="53261-03">
<connects>
<connect gate="-1" pin="S" pad="1"/>
<connect gate="-2" pin="S" pad="2"/>
<connect gate="-3" pin="S" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="398" package="53398-03">
<connects>
<connect gate="-1" pin="S" pad="1"/>
<connect gate="-2" pin="S" pad="2"/>
<connect gate="-3" pin="S" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="DF13" package="DF13-3P-1.25DSA">
<connects>
<connect gate="-1" pin="S" pad="1"/>
<connect gate="-2" pin="S" pad="2"/>
<connect gate="-3" pin="S" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="CONN_SPEKTRUM_RX" prefix="J">
<description>Spektrum RX connector; JST ZH series S3B-ZR-SM4A-TF</description>
<gates>
<gate name="-VCC" symbol="M"/>
<gate name="-GND" symbol="M"/>
<gate name="-DATA" symbol="M"/>
</gates>
<devices>
<device name="-SMD" package="S3B-ZR-SM4A-TF">
<connects>
<connect gate="-DATA" pin="S" pad="P$3"/>
<connect gate="-GND" pin="S" pad="P$2"/>
<connect gate="-VCC" pin="S" pad="P$1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-TH" package="B3B-ZR">
<connects>
<connect gate="-DATA" pin="S" pad="1"/>
<connect gate="-GND" pin="S" pad="2"/>
<connect gate="-VCC" pin="S" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="INDUCTOR" prefix="L" uservalue="yes">
<description>&lt;b&gt;Inductors&lt;/b&gt;
Basic Inductor/Choke - 0603 and 1210. Footprints are not proven and vary greatly between part numbers.
SRR1210: Bourns SRR1210 parts, e.g. SRR1210-100M</description>
<gates>
<gate name="G$1" symbol="INDUCTOR"/>
</gates>
<devices>
<device name="H*" package="1206-IND">
<connects>
<connect gate="G$1" pin="1" pad="P$1"/>
<connect gate="G$1" pin="2" pad="P$2"/>
</connects>
<technologies>
<technology name="1206"/>
</technologies>
</device>
<device name="CR54" package="CR54">
<connects>
<connect gate="G$1" pin="1" pad="P$1"/>
<connect gate="G$1" pin="2" pad="P$2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-CDRH125" package="CDRH125">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="0402" package="0402-IND">
<connects>
<connect gate="G$1" pin="1" pad="P$1"/>
<connect gate="G$1" pin="2" pad="P$2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-B82462G" package="B82462G">
<connects>
<connect gate="G$1" pin="1" pad="P$1"/>
<connect gate="G$1" pin="2" pad="P$2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="CR75" package="CR75">
<connects>
<connect gate="G$1" pin="1" pad="P$1"/>
<connect gate="G$1" pin="2" pad="P$2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="1210" package="1210">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="1007" package="1007">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_" package="COOPER_UP4B">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-CDRH3D28" package="CDRH3D28">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-SRR1210" package="1210-IND">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="0805" package="0805-IND">
<connects>
<connect gate="G$1" pin="1" pad="P$1"/>
<connect gate="G$1" pin="2" pad="P$2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="0603" package="0603-IND">
<connects>
<connect gate="G$1" pin="1" pad="P$1"/>
<connect gate="G$1" pin="2" pad="P$2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="TXB0104" prefix="U" uservalue="yes">
<description>4-BIT BIDIRECTIONAL VOLTAGE-LEVEL TRANSLATOR
WITH AUTOMATIC DIRECTION SENSING AND ±15-kV ESD PROTECTION</description>
<gates>
<gate name="G$1" symbol="TXB0104"/>
</gates>
<devices>
<device name="" package="SO14">
<connects>
<connect gate="G$1" pin="A1" pad="2"/>
<connect gate="G$1" pin="A2" pad="3"/>
<connect gate="G$1" pin="A3" pad="4"/>
<connect gate="G$1" pin="A4" pad="5"/>
<connect gate="G$1" pin="B1" pad="13"/>
<connect gate="G$1" pin="B2" pad="12"/>
<connect gate="G$1" pin="B3" pad="11"/>
<connect gate="G$1" pin="B4" pad="10"/>
<connect gate="G$1" pin="GND" pad="7"/>
<connect gate="G$1" pin="OE" pad="8"/>
<connect gate="G$1" pin="P$1" pad="6"/>
<connect gate="G$1" pin="P$2" pad="9"/>
<connect gate="G$1" pin="VCCA" pad="1"/>
<connect gate="G$1" pin="VCCB" pad="14"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="TXB0102" prefix="U">
<description>2-BIT BIDIRECTIONAL VOLTAGE-LEVEL TRANSLATOR
WITH AUTO DIRECTION SENSING AND ±15-kV ESD PROTECTION</description>
<gates>
<gate name="G$1" symbol="TX?0102"/>
</gates>
<devices>
<device name="DCUR" package="TI-DCU">
<connects>
<connect gate="G$1" pin="A1" pad="5"/>
<connect gate="G$1" pin="A2" pad="4"/>
<connect gate="G$1" pin="B1" pad="8"/>
<connect gate="G$1" pin="B2" pad="1"/>
<connect gate="G$1" pin="GND" pad="2"/>
<connect gate="G$1" pin="OE" pad="6"/>
<connect gate="G$1" pin="VCCA" pad="3"/>
<connect gate="G$1" pin="VCCB" pad="7"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="SF-MICROSD">
<gates>
<gate name="G$1" symbol="MICROSD"/>
</gates>
<devices>
<device name="" package="MICROSD">
<connects>
<connect gate="G$1" pin="CLK" pad="5"/>
<connect gate="G$1" pin="CS" pad="2"/>
<connect gate="G$1" pin="DI" pad="3"/>
<connect gate="G$1" pin="DO" pad="7"/>
<connect gate="G$1" pin="GND" pad="6"/>
<connect gate="G$1" pin="VCC" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="AMP-114-00841-68" package="AMPHENOL_114-00841-68">
<connects>
<connect gate="G$1" pin="CLK" pad="P$5"/>
<connect gate="G$1" pin="CS" pad="P$2"/>
<connect gate="G$1" pin="DI" pad="P$3"/>
<connect gate="G$1" pin="DO" pad="P$7"/>
<connect gate="G$1" pin="GND" pad="P$6"/>
<connect gate="G$1" pin="VCC" pad="P$4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LIS331DLH" prefix="U" uservalue="yes">
<description>&lt;h3&gt;LIS331DLH - Digital 3-axis accelerometer&lt;/h3&gt;

The LIS331DLH is an ultra low-power high 
performance three axes linear accelerometer 
belonging to the ?nano? family, with digital I2C/SPI 
serial interface standard output. The LIS331DLH has dynamically user selectable full scales of ±2g/±4g/±8g and it is capable of 
measuring accelerations with output data rates 
from 0.5 Hz to 1 kHz. It is 
guaranteed to operate over an extended 
temperature range from -40 °C to +85 °C.&lt;br /&gt;
&lt;br /&gt;
&lt;a href="http://www.st.com/internet/com/TECHNICAL_RESOURCES/TECHNICAL_LITERATURE/DATASHEET/CD00213470.pdf"&gt;LIS331DLH Datasheet&lt;/a&gt;</description>
<gates>
<gate name="G$1" symbol="LIS331DLH"/>
</gates>
<devices>
<device name="" package="LGA-16-3PX5P">
<connects>
<connect gate="G$1" pin="CS" pad="8"/>
<connect gate="G$1" pin="GND1" pad="5"/>
<connect gate="G$1" pin="GND2" pad="12"/>
<connect gate="G$1" pin="GND3" pad="13"/>
<connect gate="G$1" pin="GND4" pad="16"/>
<connect gate="G$1" pin="INT1" pad="11"/>
<connect gate="G$1" pin="INT2" pad="9"/>
<connect gate="G$1" pin="NC_P2" pad="2"/>
<connect gate="G$1" pin="NC_P3" pad="3"/>
<connect gate="G$1" pin="RES_P10_GND" pad="10"/>
<connect gate="G$1" pin="RES_P15_VDD" pad="15"/>
<connect gate="G$1" pin="SCL/SPC" pad="4"/>
<connect gate="G$1" pin="SDA/SDI/SDO" pad="6"/>
<connect gate="G$1" pin="SDO/SA0" pad="7"/>
<connect gate="G$1" pin="VDD" pad="14"/>
<connect gate="G$1" pin="VDD_IO" pad="1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-LL" package="LIS331DLH-MAN">
<connects>
<connect gate="G$1" pin="CS" pad="8"/>
<connect gate="G$1" pin="GND1" pad="5"/>
<connect gate="G$1" pin="GND2" pad="12"/>
<connect gate="G$1" pin="GND3" pad="13"/>
<connect gate="G$1" pin="GND4" pad="16"/>
<connect gate="G$1" pin="INT1" pad="11"/>
<connect gate="G$1" pin="INT2" pad="9"/>
<connect gate="G$1" pin="NC_P2" pad="2"/>
<connect gate="G$1" pin="NC_P3" pad="3"/>
<connect gate="G$1" pin="RES_P10_GND" pad="10"/>
<connect gate="G$1" pin="RES_P15_VDD" pad="15"/>
<connect gate="G$1" pin="SCL/SPC" pad="4"/>
<connect gate="G$1" pin="SDA/SDI/SDO" pad="6"/>
<connect gate="G$1" pin="SDO/SA0" pad="7"/>
<connect gate="G$1" pin="VDD" pad="14"/>
<connect gate="G$1" pin="VDD_IO" pad="1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="L3G4200DH" prefix="U" uservalue="yes">
<description>&lt;h3&gt;L3G4200DH - Digital 3-axis Gyroscope&lt;/h3&gt;

The L3G4200DH is a low-power three-axis 
angular rate sensor. The L3G4200DH has a full scale of ±250/±500/ 
±2000 dps and is capable of measuring rates with 
a user-selectable bandwidth. It can operate within a 
temperature range from -40 °C to +85 °C. Supply voltage: 2.4 V to 3.6 V. Full datasheet:&lt;br /&gt;&lt;br /&gt;
&lt;a href="http://www.st.com/stonline/products/literature/ds/17300.pdf"&gt;L3G4200DH Datasheet&lt;/a&gt;</description>
<gates>
<gate name="G$1" symbol="L3G4200DH"/>
</gates>
<devices>
<device name="" package="LGA-16L_SMALL_PADS">
<connects>
<connect gate="G$1" pin="CS" pad="5"/>
<connect gate="G$1" pin="DRDY/INT2" pad="6"/>
<connect gate="G$1" pin="GND" pad="13"/>
<connect gate="G$1" pin="INT1" pad="7"/>
<connect gate="G$1" pin="PLLFILT" pad="14"/>
<connect gate="G$1" pin="RES_P10_GND" pad="10"/>
<connect gate="G$1" pin="RES_P11_GND" pad="11"/>
<connect gate="G$1" pin="RES_P12_GND" pad="12"/>
<connect gate="G$1" pin="RES_P15_VDD" pad="15"/>
<connect gate="G$1" pin="RES_P8_GND" pad="8"/>
<connect gate="G$1" pin="RES_P9_GND" pad="9"/>
<connect gate="G$1" pin="SCL/SPC" pad="2"/>
<connect gate="G$1" pin="SDA/SDI/SDO" pad="3"/>
<connect gate="G$1" pin="SDO/SA0" pad="4"/>
<connect gate="G$1" pin="VDD" pad="16"/>
<connect gate="G$1" pin="VDD_IO" pad="1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-LL" package="L3G4200DH-MAN">
<connects>
<connect gate="G$1" pin="CS" pad="5"/>
<connect gate="G$1" pin="DRDY/INT2" pad="6"/>
<connect gate="G$1" pin="GND" pad="13"/>
<connect gate="G$1" pin="INT1" pad="7"/>
<connect gate="G$1" pin="PLLFILT" pad="14"/>
<connect gate="G$1" pin="RES_P10_GND" pad="10"/>
<connect gate="G$1" pin="RES_P11_GND" pad="11"/>
<connect gate="G$1" pin="RES_P12_GND" pad="12"/>
<connect gate="G$1" pin="RES_P15_VDD" pad="15"/>
<connect gate="G$1" pin="RES_P8_GND" pad="8"/>
<connect gate="G$1" pin="RES_P9_GND" pad="9"/>
<connect gate="G$1" pin="SCL/SPC" pad="2"/>
<connect gate="G$1" pin="SDA/SDI/SDO" pad="3"/>
<connect gate="G$1" pin="SDO/SA0" pad="4"/>
<connect gate="G$1" pin="VDD" pad="16"/>
<connect gate="G$1" pin="VDD_IO" pad="1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="HMC5843" prefix="U">
<gates>
<gate name="G$1" symbol="HMC5843"/>
</gates>
<devices>
<device name="" package="LPCC20">
<connects>
<connect gate="G$1" pin="AGND" pad="17"/>
<connect gate="G$1" pin="AVDD" pad="18"/>
<connect gate="G$1" pin="C1" pad="13"/>
<connect gate="G$1" pin="DGND" pad="12"/>
<connect gate="G$1" pin="DRDY" pad="19"/>
<connect gate="G$1" pin="DVDD" pad="15"/>
<connect gate="G$1" pin="OFFN" pad="7"/>
<connect gate="G$1" pin="OFFP" pad="6"/>
<connect gate="G$1" pin="SCL" pad="1"/>
<connect gate="G$1" pin="SCLP" pad="3"/>
<connect gate="G$1" pin="SDA" pad="20"/>
<connect gate="G$1" pin="SDAP" pad="2"/>
<connect gate="G$1" pin="SETC" pad="14"/>
<connect gate="G$1" pin="SETN" pad="10"/>
<connect gate="G$1" pin="SETP" pad="9"/>
<connect gate="G$1" pin="SVDD" pad="11"/>
<connect gate="G$1" pin="VREN" pad="16"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="BMP085" prefix="U" uservalue="yes">
<gates>
<gate name="G$1" symbol="BMP085"/>
</gates>
<devices>
<device name="" package="BMP085">
<connects>
<connect gate="G$1" pin="EOC" pad="2"/>
<connect gate="G$1" pin="GND" pad="1"/>
<connect gate="G$1" pin="NC" pad="5"/>
<connect gate="G$1" pin="SCL" pad="6"/>
<connect gate="G$1" pin="SDA" pad="7"/>
<connect gate="G$1" pin="VDDA" pad="3"/>
<connect gate="G$1" pin="VDDD" pad="4"/>
<connect gate="G$1" pin="XCLR" pad="8"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="HEADER_2X15" prefix="J">
<description>2X15 header</description>
<gates>
<gate name="-1" symbol="M"/>
<gate name="-2" symbol="M"/>
<gate name="-3" symbol="M"/>
<gate name="-4" symbol="M"/>
<gate name="-5" symbol="M"/>
<gate name="-6" symbol="M"/>
<gate name="-7" symbol="M"/>
<gate name="-8" symbol="M"/>
<gate name="-9" symbol="M"/>
<gate name="-10" symbol="M"/>
<gate name="-11" symbol="M"/>
<gate name="-12" symbol="M"/>
<gate name="-13" symbol="M"/>
<gate name="-14" symbol="M"/>
<gate name="-15" symbol="M"/>
<gate name="-16" symbol="M"/>
<gate name="-17" symbol="M"/>
<gate name="-18" symbol="M"/>
<gate name="-19" symbol="M"/>
<gate name="-20" symbol="M"/>
<gate name="-21" symbol="M"/>
<gate name="-22" symbol="M"/>
<gate name="-23" symbol="M"/>
<gate name="-24" symbol="M"/>
<gate name="-25" symbol="M"/>
<gate name="-26" symbol="M"/>
<gate name="-27" symbol="M"/>
<gate name="-28" symbol="M"/>
<gate name="-29" symbol="M"/>
<gate name="-30" symbol="M"/>
</gates>
<devices>
<device name="-SMD" package="HEADER_2MM_2X15">
<connects>
<connect gate="-1" pin="S" pad="1"/>
<connect gate="-10" pin="S" pad="10"/>
<connect gate="-11" pin="S" pad="11"/>
<connect gate="-12" pin="S" pad="12"/>
<connect gate="-13" pin="S" pad="13"/>
<connect gate="-14" pin="S" pad="14"/>
<connect gate="-15" pin="S" pad="15"/>
<connect gate="-16" pin="S" pad="16"/>
<connect gate="-17" pin="S" pad="17"/>
<connect gate="-18" pin="S" pad="18"/>
<connect gate="-19" pin="S" pad="19"/>
<connect gate="-2" pin="S" pad="2"/>
<connect gate="-20" pin="S" pad="20"/>
<connect gate="-21" pin="S" pad="21"/>
<connect gate="-22" pin="S" pad="22"/>
<connect gate="-23" pin="S" pad="23"/>
<connect gate="-24" pin="S" pad="24"/>
<connect gate="-25" pin="S" pad="25"/>
<connect gate="-26" pin="S" pad="26"/>
<connect gate="-27" pin="S" pad="27"/>
<connect gate="-28" pin="S" pad="28"/>
<connect gate="-29" pin="S" pad="29"/>
<connect gate="-3" pin="S" pad="3"/>
<connect gate="-30" pin="S" pad="30"/>
<connect gate="-4" pin="S" pad="4"/>
<connect gate="-5" pin="S" pad="5"/>
<connect gate="-6" pin="S" pad="6"/>
<connect gate="-7" pin="S" pad="7"/>
<connect gate="-8" pin="S" pad="8"/>
<connect gate="-9" pin="S" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-REV" package="HEADER_2MM_2X15_REVERSE">
<connects>
<connect gate="-1" pin="S" pad="1"/>
<connect gate="-10" pin="S" pad="10"/>
<connect gate="-11" pin="S" pad="11"/>
<connect gate="-12" pin="S" pad="12"/>
<connect gate="-13" pin="S" pad="13"/>
<connect gate="-14" pin="S" pad="14"/>
<connect gate="-15" pin="S" pad="15"/>
<connect gate="-16" pin="S" pad="16"/>
<connect gate="-17" pin="S" pad="17"/>
<connect gate="-18" pin="S" pad="18"/>
<connect gate="-19" pin="S" pad="19"/>
<connect gate="-2" pin="S" pad="2"/>
<connect gate="-20" pin="S" pad="20"/>
<connect gate="-21" pin="S" pad="21"/>
<connect gate="-22" pin="S" pad="22"/>
<connect gate="-23" pin="S" pad="23"/>
<connect gate="-24" pin="S" pad="24"/>
<connect gate="-25" pin="S" pad="25"/>
<connect gate="-26" pin="S" pad="26"/>
<connect gate="-27" pin="S" pad="27"/>
<connect gate="-28" pin="S" pad="28"/>
<connect gate="-29" pin="S" pad="29"/>
<connect gate="-3" pin="S" pad="3"/>
<connect gate="-30" pin="S" pad="30"/>
<connect gate="-4" pin="S" pad="4"/>
<connect gate="-5" pin="S" pad="5"/>
<connect gate="-6" pin="S" pad="6"/>
<connect gate="-7" pin="S" pad="7"/>
<connect gate="-8" pin="S" pad="8"/>
<connect gate="-9" pin="S" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-POGO" package="HEADER_2MM_2X15_POGO">
<connects>
<connect gate="-1" pin="S" pad="1"/>
<connect gate="-10" pin="S" pad="10"/>
<connect gate="-11" pin="S" pad="11"/>
<connect gate="-12" pin="S" pad="12"/>
<connect gate="-13" pin="S" pad="13"/>
<connect gate="-14" pin="S" pad="14"/>
<connect gate="-15" pin="S" pad="15"/>
<connect gate="-16" pin="S" pad="16"/>
<connect gate="-17" pin="S" pad="17"/>
<connect gate="-18" pin="S" pad="18"/>
<connect gate="-19" pin="S" pad="19"/>
<connect gate="-2" pin="S" pad="2"/>
<connect gate="-20" pin="S" pad="20"/>
<connect gate="-21" pin="S" pad="21"/>
<connect gate="-22" pin="S" pad="22"/>
<connect gate="-23" pin="S" pad="23"/>
<connect gate="-24" pin="S" pad="24"/>
<connect gate="-25" pin="S" pad="25"/>
<connect gate="-26" pin="S" pad="26"/>
<connect gate="-27" pin="S" pad="27"/>
<connect gate="-28" pin="S" pad="28"/>
<connect gate="-29" pin="S" pad="29"/>
<connect gate="-3" pin="S" pad="3"/>
<connect gate="-30" pin="S" pad="30"/>
<connect gate="-4" pin="S" pad="4"/>
<connect gate="-5" pin="S" pad="5"/>
<connect gate="-6" pin="S" pad="6"/>
<connect gate="-7" pin="S" pad="7"/>
<connect gate="-8" pin="S" pad="8"/>
<connect gate="-9" pin="S" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-POGO-REV" package="HEADER_2MM_2X15_REVERSE_POGO">
<connects>
<connect gate="-1" pin="S" pad="1"/>
<connect gate="-10" pin="S" pad="10"/>
<connect gate="-11" pin="S" pad="11"/>
<connect gate="-12" pin="S" pad="12"/>
<connect gate="-13" pin="S" pad="13"/>
<connect gate="-14" pin="S" pad="14"/>
<connect gate="-15" pin="S" pad="15"/>
<connect gate="-16" pin="S" pad="16"/>
<connect gate="-17" pin="S" pad="17"/>
<connect gate="-18" pin="S" pad="18"/>
<connect gate="-19" pin="S" pad="19"/>
<connect gate="-2" pin="S" pad="2"/>
<connect gate="-20" pin="S" pad="20"/>
<connect gate="-21" pin="S" pad="21"/>
<connect gate="-22" pin="S" pad="22"/>
<connect gate="-23" pin="S" pad="23"/>
<connect gate="-24" pin="S" pad="24"/>
<connect gate="-25" pin="S" pad="25"/>
<connect gate="-26" pin="S" pad="26"/>
<connect gate="-27" pin="S" pad="27"/>
<connect gate="-28" pin="S" pad="28"/>
<connect gate="-29" pin="S" pad="29"/>
<connect gate="-3" pin="S" pad="3"/>
<connect gate="-30" pin="S" pad="30"/>
<connect gate="-4" pin="S" pad="4"/>
<connect gate="-5" pin="S" pad="5"/>
<connect gate="-6" pin="S" pad="6"/>
<connect gate="-7" pin="S" pad="7"/>
<connect gate="-8" pin="S" pad="8"/>
<connect gate="-9" pin="S" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-2.54-TH-SHROUDED" package="HEADER_2.54MM-2X15-SHROUDED_LOCK">
<connects>
<connect gate="-1" pin="S" pad="1"/>
<connect gate="-10" pin="S" pad="10"/>
<connect gate="-11" pin="S" pad="11"/>
<connect gate="-12" pin="S" pad="12"/>
<connect gate="-13" pin="S" pad="13"/>
<connect gate="-14" pin="S" pad="14"/>
<connect gate="-15" pin="S" pad="15"/>
<connect gate="-16" pin="S" pad="16"/>
<connect gate="-17" pin="S" pad="17"/>
<connect gate="-18" pin="S" pad="18"/>
<connect gate="-19" pin="S" pad="19"/>
<connect gate="-2" pin="S" pad="2"/>
<connect gate="-20" pin="S" pad="20"/>
<connect gate="-21" pin="S" pad="21"/>
<connect gate="-22" pin="S" pad="22"/>
<connect gate="-23" pin="S" pad="23"/>
<connect gate="-24" pin="S" pad="24"/>
<connect gate="-25" pin="S" pad="25"/>
<connect gate="-26" pin="S" pad="26"/>
<connect gate="-27" pin="S" pad="27"/>
<connect gate="-28" pin="S" pad="28"/>
<connect gate="-29" pin="S" pad="29"/>
<connect gate="-3" pin="S" pad="3"/>
<connect gate="-30" pin="S" pad="30"/>
<connect gate="-4" pin="S" pad="4"/>
<connect gate="-5" pin="S" pad="5"/>
<connect gate="-6" pin="S" pad="6"/>
<connect gate="-7" pin="S" pad="7"/>
<connect gate="-8" pin="S" pad="8"/>
<connect gate="-9" pin="S" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-TH" package="HEADER_2MM_2X15_TH">
<connects>
<connect gate="-1" pin="S" pad="1"/>
<connect gate="-10" pin="S" pad="10"/>
<connect gate="-11" pin="S" pad="11"/>
<connect gate="-12" pin="S" pad="12"/>
<connect gate="-13" pin="S" pad="13"/>
<connect gate="-14" pin="S" pad="14"/>
<connect gate="-15" pin="S" pad="15"/>
<connect gate="-16" pin="S" pad="16"/>
<connect gate="-17" pin="S" pad="17"/>
<connect gate="-18" pin="S" pad="18"/>
<connect gate="-19" pin="S" pad="19"/>
<connect gate="-2" pin="S" pad="2"/>
<connect gate="-20" pin="S" pad="20"/>
<connect gate="-21" pin="S" pad="21"/>
<connect gate="-22" pin="S" pad="22"/>
<connect gate="-23" pin="S" pad="23"/>
<connect gate="-24" pin="S" pad="24"/>
<connect gate="-25" pin="S" pad="25"/>
<connect gate="-26" pin="S" pad="26"/>
<connect gate="-27" pin="S" pad="27"/>
<connect gate="-28" pin="S" pad="28"/>
<connect gate="-29" pin="S" pad="29"/>
<connect gate="-3" pin="S" pad="3"/>
<connect gate="-30" pin="S" pad="30"/>
<connect gate="-4" pin="S" pad="4"/>
<connect gate="-5" pin="S" pad="5"/>
<connect gate="-6" pin="S" pad="6"/>
<connect gate="-7" pin="S" pad="7"/>
<connect gate="-8" pin="S" pad="8"/>
<connect gate="-9" pin="S" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-TH-REV" package="HEADER_2MM_2X15_TH_REVERSE">
<connects>
<connect gate="-1" pin="S" pad="1"/>
<connect gate="-10" pin="S" pad="10"/>
<connect gate="-11" pin="S" pad="11"/>
<connect gate="-12" pin="S" pad="12"/>
<connect gate="-13" pin="S" pad="13"/>
<connect gate="-14" pin="S" pad="14"/>
<connect gate="-15" pin="S" pad="15"/>
<connect gate="-16" pin="S" pad="16"/>
<connect gate="-17" pin="S" pad="17"/>
<connect gate="-18" pin="S" pad="18"/>
<connect gate="-19" pin="S" pad="19"/>
<connect gate="-2" pin="S" pad="2"/>
<connect gate="-20" pin="S" pad="20"/>
<connect gate="-21" pin="S" pad="21"/>
<connect gate="-22" pin="S" pad="22"/>
<connect gate="-23" pin="S" pad="23"/>
<connect gate="-24" pin="S" pad="24"/>
<connect gate="-25" pin="S" pad="25"/>
<connect gate="-26" pin="S" pad="26"/>
<connect gate="-27" pin="S" pad="27"/>
<connect gate="-28" pin="S" pad="28"/>
<connect gate="-29" pin="S" pad="29"/>
<connect gate="-3" pin="S" pad="3"/>
<connect gate="-30" pin="S" pad="30"/>
<connect gate="-4" pin="S" pad="4"/>
<connect gate="-5" pin="S" pad="5"/>
<connect gate="-6" pin="S" pad="6"/>
<connect gate="-7" pin="S" pad="7"/>
<connect gate="-8" pin="S" pad="8"/>
<connect gate="-9" pin="S" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-2.54-PROTO" package="HEADER_2.54MM_2X15_PROTO">
<connects>
<connect gate="-1" pin="S" pad="1"/>
<connect gate="-10" pin="S" pad="10"/>
<connect gate="-11" pin="S" pad="11"/>
<connect gate="-12" pin="S" pad="12"/>
<connect gate="-13" pin="S" pad="13"/>
<connect gate="-14" pin="S" pad="14"/>
<connect gate="-15" pin="S" pad="15"/>
<connect gate="-16" pin="S" pad="16"/>
<connect gate="-17" pin="S" pad="17"/>
<connect gate="-18" pin="S" pad="18"/>
<connect gate="-19" pin="S" pad="19"/>
<connect gate="-2" pin="S" pad="2"/>
<connect gate="-20" pin="S" pad="20"/>
<connect gate="-21" pin="S" pad="21"/>
<connect gate="-22" pin="S" pad="22"/>
<connect gate="-23" pin="S" pad="23"/>
<connect gate="-24" pin="S" pad="24"/>
<connect gate="-25" pin="S" pad="25"/>
<connect gate="-26" pin="S" pad="26"/>
<connect gate="-27" pin="S" pad="27"/>
<connect gate="-28" pin="S" pad="28"/>
<connect gate="-29" pin="S" pad="29"/>
<connect gate="-3" pin="S" pad="3"/>
<connect gate="-30" pin="S" pad="30"/>
<connect gate="-4" pin="S" pad="4"/>
<connect gate="-5" pin="S" pad="5"/>
<connect gate="-6" pin="S" pad="6"/>
<connect gate="-7" pin="S" pad="7"/>
<connect gate="-8" pin="S" pad="8"/>
<connect gate="-9" pin="S" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-POGO-HOLE" package="HEADER_2MM_2X15_POGO-HOLE">
<connects>
<connect gate="-1" pin="S" pad="P$1"/>
<connect gate="-10" pin="S" pad="P$10"/>
<connect gate="-11" pin="S" pad="P$11"/>
<connect gate="-12" pin="S" pad="P$12"/>
<connect gate="-13" pin="S" pad="P$13"/>
<connect gate="-14" pin="S" pad="P$14"/>
<connect gate="-15" pin="S" pad="P$15"/>
<connect gate="-16" pin="S" pad="P$16"/>
<connect gate="-17" pin="S" pad="P$17"/>
<connect gate="-18" pin="S" pad="P$18"/>
<connect gate="-19" pin="S" pad="P$19"/>
<connect gate="-2" pin="S" pad="P$2"/>
<connect gate="-20" pin="S" pad="P$20"/>
<connect gate="-21" pin="S" pad="P$21"/>
<connect gate="-22" pin="S" pad="P$22"/>
<connect gate="-23" pin="S" pad="P$23"/>
<connect gate="-24" pin="S" pad="P$24"/>
<connect gate="-25" pin="S" pad="P$25"/>
<connect gate="-26" pin="S" pad="P$26"/>
<connect gate="-27" pin="S" pad="P$27"/>
<connect gate="-28" pin="S" pad="P$28"/>
<connect gate="-29" pin="S" pad="P$29"/>
<connect gate="-3" pin="S" pad="P$3"/>
<connect gate="-30" pin="S" pad="P$30"/>
<connect gate="-4" pin="S" pad="P$4"/>
<connect gate="-5" pin="S" pad="P$5"/>
<connect gate="-6" pin="S" pad="P$6"/>
<connect gate="-7" pin="S" pad="P$7"/>
<connect gate="-8" pin="S" pad="P$8"/>
<connect gate="-9" pin="S" pad="P$9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-TH-FMU-MOUNTING" package="HEADER_2MM_2X15_TH_FMU_MOUNTING">
<connects>
<connect gate="-1" pin="S" pad="1"/>
<connect gate="-10" pin="S" pad="10"/>
<connect gate="-11" pin="S" pad="11"/>
<connect gate="-12" pin="S" pad="12"/>
<connect gate="-13" pin="S" pad="13"/>
<connect gate="-14" pin="S" pad="14"/>
<connect gate="-15" pin="S" pad="15"/>
<connect gate="-16" pin="S" pad="16"/>
<connect gate="-17" pin="S" pad="17"/>
<connect gate="-18" pin="S" pad="18"/>
<connect gate="-19" pin="S" pad="19"/>
<connect gate="-2" pin="S" pad="2"/>
<connect gate="-20" pin="S" pad="20"/>
<connect gate="-21" pin="S" pad="21"/>
<connect gate="-22" pin="S" pad="22"/>
<connect gate="-23" pin="S" pad="23"/>
<connect gate="-24" pin="S" pad="24"/>
<connect gate="-25" pin="S" pad="25"/>
<connect gate="-26" pin="S" pad="26"/>
<connect gate="-27" pin="S" pad="27"/>
<connect gate="-28" pin="S" pad="28"/>
<connect gate="-29" pin="S" pad="29"/>
<connect gate="-3" pin="S" pad="3"/>
<connect gate="-30" pin="S" pad="30"/>
<connect gate="-4" pin="S" pad="4"/>
<connect gate="-5" pin="S" pad="5"/>
<connect gate="-6" pin="S" pad="6"/>
<connect gate="-7" pin="S" pad="7"/>
<connect gate="-8" pin="S" pad="8"/>
<connect gate="-9" pin="S" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-TH-REVERSE-FMU-MOUNTING" package="HEADER_2MM_2X15_TH_REVERSE_FMU_MOUNTING">
<connects>
<connect gate="-1" pin="S" pad="1"/>
<connect gate="-10" pin="S" pad="10"/>
<connect gate="-11" pin="S" pad="11"/>
<connect gate="-12" pin="S" pad="12"/>
<connect gate="-13" pin="S" pad="13"/>
<connect gate="-14" pin="S" pad="14"/>
<connect gate="-15" pin="S" pad="15"/>
<connect gate="-16" pin="S" pad="16"/>
<connect gate="-17" pin="S" pad="17"/>
<connect gate="-18" pin="S" pad="18"/>
<connect gate="-19" pin="S" pad="19"/>
<connect gate="-2" pin="S" pad="2"/>
<connect gate="-20" pin="S" pad="20"/>
<connect gate="-21" pin="S" pad="21"/>
<connect gate="-22" pin="S" pad="22"/>
<connect gate="-23" pin="S" pad="23"/>
<connect gate="-24" pin="S" pad="24"/>
<connect gate="-25" pin="S" pad="25"/>
<connect gate="-26" pin="S" pad="26"/>
<connect gate="-27" pin="S" pad="27"/>
<connect gate="-28" pin="S" pad="28"/>
<connect gate="-29" pin="S" pad="29"/>
<connect gate="-3" pin="S" pad="3"/>
<connect gate="-30" pin="S" pad="30"/>
<connect gate="-4" pin="S" pad="4"/>
<connect gate="-5" pin="S" pad="5"/>
<connect gate="-6" pin="S" pad="6"/>
<connect gate="-7" pin="S" pad="7"/>
<connect gate="-8" pin="S" pad="8"/>
<connect gate="-9" pin="S" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ST2329A">
<gates>
<gate name="G$1" symbol="ST2329A"/>
</gates>
<devices>
<device name="" package="QFN10">
<connects>
<connect gate="G$1" pin="GND" pad="6"/>
<connect gate="G$1" pin="NC4" pad="4"/>
<connect gate="G$1" pin="NC5" pad="5"/>
<connect gate="G$1" pin="OE" pad="3"/>
<connect gate="G$1" pin="VCC" pad="9"/>
<connect gate="G$1" pin="VCC1" pad="8"/>
<connect gate="G$1" pin="VCC2" pad="7"/>
<connect gate="G$1" pin="VL" pad="10"/>
<connect gate="G$1" pin="VL1" pad="1"/>
<connect gate="G$1" pin="VL2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-MANUAL-SOLDERING" package="QFN10L">
<connects>
<connect gate="G$1" pin="GND" pad="6"/>
<connect gate="G$1" pin="NC4" pad="4"/>
<connect gate="G$1" pin="NC5" pad="5"/>
<connect gate="G$1" pin="OE" pad="3"/>
<connect gate="G$1" pin="VCC" pad="9"/>
<connect gate="G$1" pin="VCC1" pad="8"/>
<connect gate="G$1" pin="VCC2" pad="7"/>
<connect gate="G$1" pin="VL" pad="10"/>
<connect gate="G$1" pin="VL1" pad="1"/>
<connect gate="G$1" pin="VL2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="JUMPER-3" prefix="JP">
<gates>
<gate name="G$1" symbol="JUMPER-3"/>
</gates>
<devices>
<device name="SMD" package="SJ_3">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="PTH" package="1X03">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="1-2" package="SJ_3_PASTE1&amp;2">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="2-3" package="SJ_3_PASTE2&amp;3">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="0603" package="SJ_3_0603_PASTE1&amp;2">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ST2349A">
<gates>
<gate name="G$1" symbol="ST2349A"/>
</gates>
<devices>
<device name="" package="QFN16">
<connects>
<connect gate="G$1" pin="GND" pad="11"/>
<connect gate="G$1" pin="NC1" pad="5"/>
<connect gate="G$1" pin="NC2" pad="8"/>
<connect gate="G$1" pin="OE" pad="2"/>
<connect gate="G$1" pin="VCC1" pad="13"/>
<connect gate="G$1" pin="VCC2" pad="12"/>
<connect gate="G$1" pin="VCC3" pad="10"/>
<connect gate="G$1" pin="VCC4" pad="9"/>
<connect gate="G$1" pin="VCC_PIN14" pad="14"/>
<connect gate="G$1" pin="VCC_PIN7" pad="7"/>
<connect gate="G$1" pin="VL1" pad="16"/>
<connect gate="G$1" pin="VL2" pad="1"/>
<connect gate="G$1" pin="VL3" pad="3"/>
<connect gate="G$1" pin="VL4" pad="4"/>
<connect gate="G$1" pin="VL_PIN15" pad="15"/>
<connect gate="G$1" pin="VL_PIN6" pad="6"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LED" prefix="LED" uservalue="yes">
<description>&lt;b&gt;LEDs&lt;/b&gt;
Standard schematic elements and footprints for 5mm, 3mm, 1206, and 0603 sized LEDs. 5mm - Spark Fun Electronics SKU : COM-00529 (and others)</description>
<gates>
<gate name="G$1" symbol="LED"/>
</gates>
<devices>
<device name="5MM" package="LED5MM">
<connects>
<connect gate="G$1" pin="A" pad="A"/>
<connect gate="G$1" pin="C" pad="K"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="3MM" package="LED3MM">
<connects>
<connect gate="G$1" pin="A" pad="A"/>
<connect gate="G$1" pin="C" pad="K"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="1206" package="LED-1206">
<connects>
<connect gate="G$1" pin="A" pad="A"/>
<connect gate="G$1" pin="C" pad="C"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="10MM" package="LED10MM">
<connects>
<connect gate="G$1" pin="A" pad="A"/>
<connect gate="G$1" pin="C" pad="C"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="0402" package="0402-LED">
<connects>
<connect gate="G$1" pin="A" pad="A"/>
<connect gate="G$1" pin="C" pad="C"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="0603" package="0603-LED">
<connects>
<connect gate="G$1" pin="A" pad="A"/>
<connect gate="G$1" pin="C" pad="C"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MOUNT-HOLE">
<gates>
<gate name="G$1" symbol="MOUNT-HOLE"/>
</gates>
<devices>
<device name="2.1MM" package="MOUNT-HOLE2.1">
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="3.1MM" package="MOUNT-HOLE3.1">
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="2.6MM" package="MOUNT-HOLE2.6">
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-BRACKET#4-40" package="MOUNTING-BRACKET-4-40">
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="" package="MOUNT-HOLE3.3">
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="STM32F10XCXT6" prefix="IC">
<description>ST STM32F101/103 48pin LQFP</description>
<gates>
<gate name="PORTA_L" symbol="PORT_A_L-1"/>
<gate name="PORTA_H" symbol="PORT_A_H-1"/>
<gate name="PORTB_L" symbol="PORT_B_L-1"/>
<gate name="PORTB_H" symbol="PORT_B_H-1"/>
<gate name="POWER" symbol="VCC_VDD_S"/>
<gate name="PORTC" symbol="PORT_C_3"/>
<gate name="PORTD/OSC" symbol="PORT_D_2"/>
<gate name="AN_POWER" symbol="BAT_AN_M-1"/>
<gate name="RESET" symbol="BOOT_RST-1"/>
</gates>
<devices>
<device name="" package="TQFP48">
<connects>
<connect gate="AN_POWER" pin="VBAT" pad="1"/>
<connect gate="AN_POWER" pin="VDDA" pad="9"/>
<connect gate="AN_POWER" pin="VSSA" pad="8"/>
<connect gate="PORTA_H" pin="PA10" pad="31"/>
<connect gate="PORTA_H" pin="PA11" pad="32"/>
<connect gate="PORTA_H" pin="PA12" pad="33"/>
<connect gate="PORTA_H" pin="PA13" pad="34"/>
<connect gate="PORTA_H" pin="PA14" pad="37"/>
<connect gate="PORTA_H" pin="PA15" pad="38"/>
<connect gate="PORTA_H" pin="PA8" pad="29"/>
<connect gate="PORTA_H" pin="PA9" pad="30"/>
<connect gate="PORTA_L" pin="PA0" pad="10"/>
<connect gate="PORTA_L" pin="PA1" pad="11"/>
<connect gate="PORTA_L" pin="PA2" pad="12"/>
<connect gate="PORTA_L" pin="PA3" pad="13"/>
<connect gate="PORTA_L" pin="PA4" pad="14"/>
<connect gate="PORTA_L" pin="PA5" pad="15"/>
<connect gate="PORTA_L" pin="PA6" pad="16"/>
<connect gate="PORTA_L" pin="PA7" pad="17"/>
<connect gate="PORTB_H" pin="PB10" pad="21"/>
<connect gate="PORTB_H" pin="PB11" pad="22"/>
<connect gate="PORTB_H" pin="PB12" pad="25"/>
<connect gate="PORTB_H" pin="PB13" pad="26"/>
<connect gate="PORTB_H" pin="PB14" pad="27"/>
<connect gate="PORTB_H" pin="PB15" pad="28"/>
<connect gate="PORTB_H" pin="PB8" pad="45"/>
<connect gate="PORTB_H" pin="PB9" pad="46"/>
<connect gate="PORTB_L" pin="PB0" pad="18"/>
<connect gate="PORTB_L" pin="PB1" pad="19"/>
<connect gate="PORTB_L" pin="PB2" pad="20"/>
<connect gate="PORTB_L" pin="PB3" pad="39"/>
<connect gate="PORTB_L" pin="PB4" pad="40"/>
<connect gate="PORTB_L" pin="PB5" pad="41"/>
<connect gate="PORTB_L" pin="PB6" pad="42"/>
<connect gate="PORTB_L" pin="PB7" pad="43"/>
<connect gate="PORTC" pin="PC13" pad="2"/>
<connect gate="PORTC" pin="PC14" pad="3"/>
<connect gate="PORTC" pin="PC15" pad="4"/>
<connect gate="PORTD/OSC" pin="PD0/OSC&lt;=" pad="5"/>
<connect gate="PORTD/OSC" pin="PD1/OSC=&gt;" pad="6"/>
<connect gate="POWER" pin="VDD_1" pad="24"/>
<connect gate="POWER" pin="VDD_2" pad="36"/>
<connect gate="POWER" pin="VDD_3" pad="48"/>
<connect gate="POWER" pin="VSS_1" pad="23"/>
<connect gate="POWER" pin="VSS_2" pad="35"/>
<connect gate="POWER" pin="VSS_3" pad="47"/>
<connect gate="RESET" pin="BOOT0" pad="44"/>
<connect gate="RESET" pin="NRST" pad="7"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="HEADER-3X8">
<gates>
<gate name="G$1" symbol="SERVO8"/>
</gates>
<devices>
<device name="SERVO" package="3X8RA">
<connects>
<connect gate="G$1" pin="+5V@1" pad="2"/>
<connect gate="G$1" pin="+5V@2" pad="5"/>
<connect gate="G$1" pin="+5V@3" pad="8"/>
<connect gate="G$1" pin="+5V@4" pad="11"/>
<connect gate="G$1" pin="+5V@5" pad="14"/>
<connect gate="G$1" pin="+5V@6" pad="17"/>
<connect gate="G$1" pin="+5V@7" pad="20"/>
<connect gate="G$1" pin="+5V@8" pad="23"/>
<connect gate="G$1" pin="GND@1" pad="3"/>
<connect gate="G$1" pin="GND@2" pad="6"/>
<connect gate="G$1" pin="GND@3" pad="9"/>
<connect gate="G$1" pin="GND@4" pad="12"/>
<connect gate="G$1" pin="GND@5" pad="15"/>
<connect gate="G$1" pin="GND@6" pad="18"/>
<connect gate="G$1" pin="GND@7" pad="21"/>
<connect gate="G$1" pin="GND@8" pad="24"/>
<connect gate="G$1" pin="PPM1" pad="22"/>
<connect gate="G$1" pin="PPM2" pad="19"/>
<connect gate="G$1" pin="PPM3" pad="16"/>
<connect gate="G$1" pin="PPM4" pad="13"/>
<connect gate="G$1" pin="PPM5" pad="10"/>
<connect gate="G$1" pin="PPM6" pad="7"/>
<connect gate="G$1" pin="PPM7" pad="4"/>
<connect gate="G$1" pin="PPM8" pad="1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="HEADER-3X1">
<description>&lt;h3&gt;Single row 0.1" servo header&lt;/h3&gt;</description>
<gates>
<gate name="G$1" symbol="SERVO1"/>
</gates>
<devices>
<device name="RA" package="3X1RA">
<connects>
<connect gate="G$1" pin="+5V" pad="2"/>
<connect gate="G$1" pin="GND" pad="3"/>
<connect gate="G$1" pin="PPM" pad="1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="BOARDEDGE" package="3X1-BOARD-EDGE">
<connects>
<connect gate="G$1" pin="+5V" pad="+5V"/>
<connect gate="G$1" pin="GND" pad="GND"/>
<connect gate="G$1" pin="PPM" pad="PPM"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="SMD-BOARDEDGE" package="HEADER_3X01_SMD_H_BOARD_EDGE">
<connects>
<connect gate="G$1" pin="+5V" pad="2"/>
<connect gate="G$1" pin="GND" pad="3"/>
<connect gate="G$1" pin="PPM" pad="1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="BOARDEDGE-NOLABEL" package="3X1-BOARD-EDGE-NOLABEL">
<connects>
<connect gate="G$1" pin="+5V" pad="+5V"/>
<connect gate="G$1" pin="GND" pad="GND"/>
<connect gate="G$1" pin="PPM" pad="PPM"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="BOARDEDGE-SHORT" package="HEADER_3X01_SMD_H_BOARD_EDGE_SHORT">
<connects>
<connect gate="G$1" pin="+5V" pad="2"/>
<connect gate="G$1" pin="GND" pad="3"/>
<connect gate="G$1" pin="PPM" pad="1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="INVERTER">
<description>Single inverter, SOT23-5</description>
<gates>
<gate name="G$1" symbol="INVERTER"/>
</gates>
<devices>
<device name="" package="SOT23-5">
<connects>
<connect gate="G$1" pin="A" pad="2"/>
<connect gate="G$1" pin="GND" pad="3"/>
<connect gate="G$1" pin="NC" pad="1"/>
<connect gate="G$1" pin="VCC" pad="5"/>
<connect gate="G$1" pin="Y" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="&quot;&quot;" package="SC70">
<connects>
<connect gate="G$1" pin="A" pad="2"/>
<connect gate="G$1" pin="GND" pad="3"/>
<connect gate="G$1" pin="NC" pad="1"/>
<connect gate="G$1" pin="VCC" pad="5"/>
<connect gate="G$1" pin="Y" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="TLP3123" prefix="SSR">
<description>&lt;h3&gt;TLP3123 Solid State Relay&lt;/h3&gt;

The TOSHIBA TLP3123 consists of a gallium arsenide infrared emitting diode optically coupled to a photo-MOS FET in a plastic SOP package. The TLP3123 is a bi-directional switch, which can replace mechanical relays in many applications. And its high on-state current maximum rating and low on-state resistance is suitable to control a power line.

http://www.semicon.toshiba.co.jp/docs/datasheet/en/Opto/TLP3123_en_datasheet_071001.pdf</description>
<gates>
<gate name="G$1" symbol="PHOTO-MOSFET"/>
</gates>
<devices>
<device name="SO" package="SOP4-2.54">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="53?-02" prefix="X" uservalue="yes">
<description>&lt;b&gt;CONNECTOR&lt;/b&gt;&lt;p&gt;
wire to board 1.25 mm (.049 inch) pitch header</description>
<gates>
<gate name="-1" symbol="MV"/>
<gate name="-2" symbol="M"/>
</gates>
<devices>
<device name="047" package="53047-02">
<connects>
<connect gate="-1" pin="S" pad="1"/>
<connect gate="-2" pin="S" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="048" package="53048-02">
<connects>
<connect gate="-1" pin="S" pad="1"/>
<connect gate="-2" pin="S" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="261" package="53261-02">
<connects>
<connect gate="-1" pin="S" pad="1"/>
<connect gate="-2" pin="S" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="398" package="53398-02">
<connects>
<connect gate="-1" pin="S" pad="1"/>
<connect gate="-2" pin="S" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="DF13" package="DF13-2P-1.25DSA">
<connects>
<connect gate="-1" pin="S" pad="1"/>
<connect gate="-2" pin="S" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="XBEE-1">
<gates>
<gate name="G$1" symbol="XBEE-1"/>
</gates>
<devices>
<device name="B1" package="XBEE-1">
<connects>
<connect gate="G$1" pin="CTS" pad="12"/>
<connect gate="G$1" pin="DIN" pad="3"/>
<connect gate="G$1" pin="DIO0" pad="20"/>
<connect gate="G$1" pin="DIO1" pad="19"/>
<connect gate="G$1" pin="DIO11" pad="7"/>
<connect gate="G$1" pin="DIO12" pad="4"/>
<connect gate="G$1" pin="DIO2" pad="18"/>
<connect gate="G$1" pin="DIO3" pad="17"/>
<connect gate="G$1" pin="DIO4" pad="11"/>
<connect gate="G$1" pin="DIO5" pad="15"/>
<connect gate="G$1" pin="DIO9" pad="13"/>
<connect gate="G$1" pin="DOUT" pad="2"/>
<connect gate="G$1" pin="DTR" pad="9"/>
<connect gate="G$1" pin="GND" pad="10"/>
<connect gate="G$1" pin="RES@14" pad="14"/>
<connect gate="G$1" pin="RES@8" pad="8"/>
<connect gate="G$1" pin="RESET" pad="5"/>
<connect gate="G$1" pin="RSSI" pad="6"/>
<connect gate="G$1" pin="RTS" pad="16"/>
<connect gate="G$1" pin="VDD" pad="1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="B2" package="XBEE-SILK">
<connects>
<connect gate="G$1" pin="CTS" pad="12"/>
<connect gate="G$1" pin="DIN" pad="3"/>
<connect gate="G$1" pin="DIO0" pad="20"/>
<connect gate="G$1" pin="DIO1" pad="19"/>
<connect gate="G$1" pin="DIO11" pad="7"/>
<connect gate="G$1" pin="DIO12" pad="4"/>
<connect gate="G$1" pin="DIO2" pad="18"/>
<connect gate="G$1" pin="DIO3" pad="17"/>
<connect gate="G$1" pin="DIO4" pad="11"/>
<connect gate="G$1" pin="DIO5" pad="15"/>
<connect gate="G$1" pin="DIO9" pad="13"/>
<connect gate="G$1" pin="DOUT" pad="2"/>
<connect gate="G$1" pin="DTR" pad="9"/>
<connect gate="G$1" pin="GND" pad="10"/>
<connect gate="G$1" pin="RES@14" pad="14"/>
<connect gate="G$1" pin="RES@8" pad="8"/>
<connect gate="G$1" pin="RESET" pad="5"/>
<connect gate="G$1" pin="RSSI" pad="6"/>
<connect gate="G$1" pin="RTS" pad="16"/>
<connect gate="G$1" pin="VDD" pad="1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="B3" package="XBEE-SMD">
<connects>
<connect gate="G$1" pin="CTS" pad="12"/>
<connect gate="G$1" pin="DIN" pad="3"/>
<connect gate="G$1" pin="DIO0" pad="20"/>
<connect gate="G$1" pin="DIO1" pad="19"/>
<connect gate="G$1" pin="DIO11" pad="7"/>
<connect gate="G$1" pin="DIO12" pad="4"/>
<connect gate="G$1" pin="DIO2" pad="18"/>
<connect gate="G$1" pin="DIO3" pad="17"/>
<connect gate="G$1" pin="DIO4" pad="11"/>
<connect gate="G$1" pin="DIO5" pad="15"/>
<connect gate="G$1" pin="DIO9" pad="13"/>
<connect gate="G$1" pin="DOUT" pad="2"/>
<connect gate="G$1" pin="DTR" pad="9"/>
<connect gate="G$1" pin="GND" pad="10"/>
<connect gate="G$1" pin="RES@14" pad="14"/>
<connect gate="G$1" pin="RES@8" pad="8"/>
<connect gate="G$1" pin="RESET" pad="5"/>
<connect gate="G$1" pin="RSSI" pad="6"/>
<connect gate="G$1" pin="RTS" pad="16"/>
<connect gate="G$1" pin="VDD" pad="1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="XBEE-1_LOCK" package="XBEE-1_LOCK">
<connects>
<connect gate="G$1" pin="CTS" pad="12"/>
<connect gate="G$1" pin="DIN" pad="3"/>
<connect gate="G$1" pin="DIO0" pad="20"/>
<connect gate="G$1" pin="DIO1" pad="19"/>
<connect gate="G$1" pin="DIO11" pad="7"/>
<connect gate="G$1" pin="DIO12" pad="4"/>
<connect gate="G$1" pin="DIO2" pad="18"/>
<connect gate="G$1" pin="DIO3" pad="17"/>
<connect gate="G$1" pin="DIO4" pad="11"/>
<connect gate="G$1" pin="DIO5" pad="15"/>
<connect gate="G$1" pin="DIO9" pad="13"/>
<connect gate="G$1" pin="DOUT" pad="2"/>
<connect gate="G$1" pin="DTR" pad="9"/>
<connect gate="G$1" pin="GND" pad="10"/>
<connect gate="G$1" pin="RES@14" pad="14"/>
<connect gate="G$1" pin="RES@8" pad="8"/>
<connect gate="G$1" pin="RESET" pad="5"/>
<connect gate="G$1" pin="RSSI" pad="6"/>
<connect gate="G$1" pin="RTS" pad="16"/>
<connect gate="G$1" pin="VDD" pad="1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="SN74LVC8T245">
<gates>
<gate name="G$1" symbol="SN74LVC8T245"/>
</gates>
<devices>
<device name="R-PDSO-G24" package="R-PDSO-G24">
<connects>
<connect gate="G$1" pin="A1" pad="3"/>
<connect gate="G$1" pin="A2" pad="4"/>
<connect gate="G$1" pin="A3" pad="5"/>
<connect gate="G$1" pin="A4" pad="6"/>
<connect gate="G$1" pin="A5" pad="7"/>
<connect gate="G$1" pin="A6" pad="8"/>
<connect gate="G$1" pin="A7" pad="9"/>
<connect gate="G$1" pin="A8" pad="10"/>
<connect gate="G$1" pin="B1" pad="21"/>
<connect gate="G$1" pin="B2" pad="20"/>
<connect gate="G$1" pin="B3" pad="19"/>
<connect gate="G$1" pin="B4" pad="18"/>
<connect gate="G$1" pin="B5" pad="17"/>
<connect gate="G$1" pin="B6" pad="16"/>
<connect gate="G$1" pin="B7" pad="15"/>
<connect gate="G$1" pin="B8" pad="14"/>
<connect gate="G$1" pin="DIR" pad="2"/>
<connect gate="G$1" pin="GND@1" pad="11"/>
<connect gate="G$1" pin="GND@2" pad="12"/>
<connect gate="G$1" pin="GND@3" pad="13"/>
<connect gate="G$1" pin="OE" pad="22"/>
<connect gate="G$1" pin="VCCA" pad="1"/>
<connect gate="G$1" pin="VCCB@1" pad="24"/>
<connect gate="G$1" pin="VCCB@2" pad="23"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="RHL" package="QFN24-RHL">
<connects>
<connect gate="G$1" pin="A1" pad="3"/>
<connect gate="G$1" pin="A2" pad="4"/>
<connect gate="G$1" pin="A3" pad="5"/>
<connect gate="G$1" pin="A4" pad="6"/>
<connect gate="G$1" pin="A5" pad="7"/>
<connect gate="G$1" pin="A6" pad="8"/>
<connect gate="G$1" pin="A7" pad="9"/>
<connect gate="G$1" pin="A8" pad="10"/>
<connect gate="G$1" pin="B1" pad="21"/>
<connect gate="G$1" pin="B2" pad="20"/>
<connect gate="G$1" pin="B3" pad="19"/>
<connect gate="G$1" pin="B4" pad="18"/>
<connect gate="G$1" pin="B5" pad="17"/>
<connect gate="G$1" pin="B6" pad="16"/>
<connect gate="G$1" pin="B7" pad="15"/>
<connect gate="G$1" pin="B8" pad="14"/>
<connect gate="G$1" pin="DIR" pad="2"/>
<connect gate="G$1" pin="GND@1" pad="11"/>
<connect gate="G$1" pin="GND@2" pad="12"/>
<connect gate="G$1" pin="GND@3" pad="13"/>
<connect gate="G$1" pin="OE" pad="22"/>
<connect gate="G$1" pin="VCCA" pad="1"/>
<connect gate="G$1" pin="VCCB@1" pad="23"/>
<connect gate="G$1" pin="VCCB@2" pad="24"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="53?-06" prefix="X" uservalue="yes">
<description>&lt;b&gt;CONNECTOR&lt;/b&gt;&lt;p&gt;
wire to board 1.25 mm (.049 inch) pitch header</description>
<gates>
<gate name="-1" symbol="MV"/>
<gate name="-2" symbol="M"/>
<gate name="-3" symbol="M"/>
<gate name="-4" symbol="M"/>
<gate name="-5" symbol="M"/>
<gate name="-6" symbol="M"/>
</gates>
<devices>
<device name="047" package="53047-06">
<connects>
<connect gate="-1" pin="S" pad="1"/>
<connect gate="-2" pin="S" pad="2"/>
<connect gate="-3" pin="S" pad="3"/>
<connect gate="-4" pin="S" pad="4"/>
<connect gate="-5" pin="S" pad="5"/>
<connect gate="-6" pin="S" pad="6"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="048" package="53048-06">
<connects>
<connect gate="-1" pin="S" pad="1"/>
<connect gate="-2" pin="S" pad="2"/>
<connect gate="-3" pin="S" pad="3"/>
<connect gate="-4" pin="S" pad="4"/>
<connect gate="-5" pin="S" pad="5"/>
<connect gate="-6" pin="S" pad="6"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="261" package="53261-06">
<connects>
<connect gate="-1" pin="S" pad="1"/>
<connect gate="-2" pin="S" pad="2"/>
<connect gate="-3" pin="S" pad="3"/>
<connect gate="-4" pin="S" pad="4"/>
<connect gate="-5" pin="S" pad="5"/>
<connect gate="-6" pin="S" pad="6"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="398" package="53398-06">
<connects>
<connect gate="-1" pin="S" pad="1"/>
<connect gate="-2" pin="S" pad="2"/>
<connect gate="-3" pin="S" pad="3"/>
<connect gate="-4" pin="S" pad="4"/>
<connect gate="-5" pin="S" pad="5"/>
<connect gate="-6" pin="S" pad="6"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="53?-07" prefix="X" uservalue="yes">
<description>&lt;b&gt;CONNECTOR&lt;/b&gt;&lt;p&gt;
wire to board 1.25 mm (.049 inch) pitch header</description>
<gates>
<gate name="-1" symbol="MV"/>
<gate name="-2" symbol="M"/>
<gate name="-3" symbol="M"/>
<gate name="-4" symbol="M"/>
<gate name="-5" symbol="M"/>
<gate name="-6" symbol="M"/>
<gate name="-7" symbol="M"/>
</gates>
<devices>
<device name="047" package="53047-07">
<connects>
<connect gate="-1" pin="S" pad="1"/>
<connect gate="-2" pin="S" pad="2"/>
<connect gate="-3" pin="S" pad="3"/>
<connect gate="-4" pin="S" pad="4"/>
<connect gate="-5" pin="S" pad="5"/>
<connect gate="-6" pin="S" pad="6"/>
<connect gate="-7" pin="S" pad="7"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="048" package="53048-07">
<connects>
<connect gate="-1" pin="S" pad="1"/>
<connect gate="-2" pin="S" pad="2"/>
<connect gate="-3" pin="S" pad="3"/>
<connect gate="-4" pin="S" pad="4"/>
<connect gate="-5" pin="S" pad="5"/>
<connect gate="-6" pin="S" pad="6"/>
<connect gate="-7" pin="S" pad="7"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="261" package="53261-07">
<connects>
<connect gate="-1" pin="S" pad="1"/>
<connect gate="-2" pin="S" pad="2"/>
<connect gate="-3" pin="S" pad="3"/>
<connect gate="-4" pin="S" pad="4"/>
<connect gate="-5" pin="S" pad="5"/>
<connect gate="-6" pin="S" pad="6"/>
<connect gate="-7" pin="S" pad="7"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="398" package="53398-07">
<connects>
<connect gate="-1" pin="S" pad="1"/>
<connect gate="-2" pin="S" pad="2"/>
<connect gate="-3" pin="S" pad="3"/>
<connect gate="-4" pin="S" pad="4"/>
<connect gate="-5" pin="S" pad="5"/>
<connect gate="-6" pin="S" pad="6"/>
<connect gate="-7" pin="S" pad="7"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="TPS2051B">
<description>&lt;h3&gt;CURRENT-LIMITED, POWER-DISTRIBUTION SWITCH&lt;/h3&gt;
&lt;br /&gt;
The TPS204xB/TPS205xB power-distribution switches are intended for applications where heavy capacitive loads and short circuits are likely to be encountered. 500-mA continuous current, accurate Current Limit (0.75 A min, 1.25 A max), operating range: 2.7 V to 5.5 V. These devices incorporates 70-m? N-channel MOSFET power switches for power-distribution systems that require multiple power switches in a single package. Each switch is controlled by a logic enable input. Gate drive is provided by an internal charge pump designed to control the power-switch rise times and fall times to minimize current surges during switching. The charge pump requires no external components and allows operation from supplies as low as 2.7 V.
&lt;br /&gt;
&lt;br /&gt;
&lt;a href="http://focus.ti.com/lit/ds/symlink/tps2051b.pdf"&gt;http://focus.ti.com/lit/ds/symlink/tps2051b.pdf&lt;/a&gt;</description>
<gates>
<gate name="G$1" symbol="TPS2051"/>
</gates>
<devices>
<device name="" package="SOT23-5L">
<connects>
<connect gate="G$1" pin="!OC" pad="3"/>
<connect gate="G$1" pin="EN" pad="4"/>
<connect gate="G$1" pin="GND" pad="2"/>
<connect gate="G$1" pin="IN" pad="5"/>
<connect gate="G$1" pin="OUT" pad="1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="74LVC2GU04">
<description>&lt;h3&gt;DUAL INVERTER GATE&lt;/h3&gt;
&lt;br /&gt;

This dual inverter is designed for 1.65-V to 5.5-V VCC operation.
The SN74LVC2GU04 contains two inverters with unbuffered outputs and performs the Boolean function Y = A. It is available from NXP and TI.
&lt;br /&gt;
&lt;br /&gt;
&lt;a href="http://www.nxp.com/documents/data_sheet/74LVC2GU04.pdf"&gt;http://www.nxp.com/documents/data_sheet/74LVC2GU04.pdf&lt;/a&gt;&lt;br /&gt;
&lt;a href="http://focus.ti.com/lit/ds/symlink/sn74lvc2gu04.pdf"&gt;http://focus.ti.com/lit/ds/symlink/sn74lvc2gu04.pdf&lt;/a&gt;</description>
<gates>
<gate name="G$1" symbol="74LVC2GU04"/>
</gates>
<devices>
<device name="" package="SOT363_PHILIPS">
<connects>
<connect gate="G$1" pin="1A" pad="1"/>
<connect gate="G$1" pin="1Y" pad="6"/>
<connect gate="G$1" pin="2A" pad="3"/>
<connect gate="G$1" pin="2Y" pad="4"/>
<connect gate="G$1" pin="GND" pad="2"/>
<connect gate="G$1" pin="VCC" pad="5"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="XBEE-MINIMAL">
<gates>
<gate name="G$1" symbol="XBEE"/>
</gates>
<devices>
<device name="" package="XBEE-MINIMAL">
<connects>
<connect gate="G$1" pin="CTS" pad="12"/>
<connect gate="G$1" pin="DIN" pad="3"/>
<connect gate="G$1" pin="DIO0" pad="20"/>
<connect gate="G$1" pin="DIO4" pad="11"/>
<connect gate="G$1" pin="DOUT" pad="2"/>
<connect gate="G$1" pin="GND" pad="10"/>
<connect gate="G$1" pin="RSSI" pad="6"/>
<connect gate="G$1" pin="RTS" pad="16"/>
<connect gate="G$1" pin="VDD" pad="1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-SMD" package="XBEE-SMD">
<connects>
<connect gate="G$1" pin="CTS" pad="12"/>
<connect gate="G$1" pin="DIN" pad="3"/>
<connect gate="G$1" pin="DIO0" pad="20"/>
<connect gate="G$1" pin="DIO4" pad="11"/>
<connect gate="G$1" pin="DOUT" pad="2"/>
<connect gate="G$1" pin="GND" pad="10"/>
<connect gate="G$1" pin="RSSI" pad="6"/>
<connect gate="G$1" pin="RTS" pad="16"/>
<connect gate="G$1" pin="VDD" pad="1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="PTH08080W">
<description>&lt;h3&gt;2.25-A, WIDE-INPUT ADJUSTABLE SWITCHING REGULATOR&lt;/h3&gt;

The input voltage range of the PTH08080W is from 4.5 V to 18 V, allowing operation from either a 5-V or 12-V input bus. Using state-of-the-art switched-mode power-conversion technology, the PTH08080W can step down to voltages as low as 0.9 V from a 5-V input bus, with less than 1 W of power dissipation. The output voltage can be adjusted to any voltage over the range, 0.9 V to 5.5 V, using a single external resistor. Operating features include an undervoltage lockout (UVLO), on/off inhibit, overcurrent protection, and overtemperature protection.
&lt;br /&gt;
&lt;br /&gt;
&lt;a href="http://focus.ti.com/lit/ds/symlink/pth08080w.pdf"&gt;http://focus.ti.com/lit/ds/symlink/pth08080w.pdf&lt;/a&gt;</description>
<gates>
<gate name="G$1" symbol="PTH08080W"/>
</gates>
<devices>
<device name="AZ" package="PTH08080W_SMD">
<connects>
<connect gate="G$1" pin="ADJ" pad="4"/>
<connect gate="G$1" pin="GND" pad="2"/>
<connect gate="G$1" pin="IHN" pad="5"/>
<connect gate="G$1" pin="VIN" pad="1"/>
<connect gate="G$1" pin="VOUT" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="AH" package="PTH08080W_TH">
<connects>
<connect gate="G$1" pin="ADJ" pad="4"/>
<connect gate="G$1" pin="GND" pad="2"/>
<connect gate="G$1" pin="IHN" pad="5"/>
<connect gate="G$1" pin="VIN" pad="1"/>
<connect gate="G$1" pin="VOUT" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="AS" package="PTH08080W_SMD">
<connects>
<connect gate="G$1" pin="ADJ" pad="4"/>
<connect gate="G$1" pin="GND" pad="2"/>
<connect gate="G$1" pin="IHN" pad="5"/>
<connect gate="G$1" pin="VIN" pad="1"/>
<connect gate="G$1" pin="VOUT" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MPXV" uservalue="yes">
<gates>
<gate name="G$1" symbol="PRESSURE-SENSOR"/>
</gates>
<devices>
<device name="5004DP" package="FREESCALE-1351-01">
<connects>
<connect gate="G$1" pin="+5V" pad="2"/>
<connect gate="G$1" pin="GND" pad="3"/>
<connect gate="G$1" pin="VOUT" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="7002DP" package="FREESCALE-1351-01">
<connects>
<connect gate="G$1" pin="+5V" pad="2"/>
<connect gate="G$1" pin="GND" pad="3"/>
<connect gate="G$1" pin="VOUT" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="PAD" prefix="TP">
<description>&lt;h3&gt;Test pad&lt;/h3&gt;

This footprint includes three classes: The actual test pads, a pogo-pin footprint to mount the pogo-pin as through-hole part and a hole footprint which allows the head of the pogo-pin to pass through (do NOT use the hole to mount the pogo-pin). In a typical test setup, the stack would consist of three PCBs: The actual PCB under testing with a test pad on the bottom, then a second PCB with the hole for the pogo-pin head where the PCB under testing is pressed on and a third PCB at 30 mm / 1.2" distance with the pogo-pin footprints. The pogo-pins are soldered to the last PCB. To create the stack, copy the board under testing and exchange the footprints - this way the correct positioning is ensured.</description>
<gates>
<gate name="G$1" symbol="PAD"/>
</gates>
<devices>
<device name=".02" package="PAD.02X.02">
<connects>
<connect gate="G$1" pin="P$1" pad="P$1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name=".03" package="PAD.03X.03">
<connects>
<connect gate="G$1" pin="P$1" pad="P$1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-POGO" package="POGO">
<connects>
<connect gate="G$1" pin="P$1" pad="P$1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-HOLE" package="POGO-HOLE">
<connects>
<connect gate="G$1" pin="P$1" pad="P$2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name=".05" package="PAD.05X.05">
<connects>
<connect gate="G$1" pin="P$1" pad="P$1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name=".04" package="PAD.04X.04">
<connects>
<connect gate="G$1" pin="P$1" pad="P$1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-SCOPE-RING-L" package="KEYSTONE-5016">
<connects>
<connect gate="G$1" pin="P$1" pad="P$1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-PROBE-2MM" package="PAD-2MM-PROBE-HORZ">
<connects>
<connect gate="G$1" pin="P$1" pad="P$1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-SCOPE-RING-S" package="HARWIN-S1751-46R">
<connects>
<connect gate="G$1" pin="P$1" pad="P$1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="EM406">
<description>&lt;b&gt;EM406 Connector&lt;/b&gt;
Proven layout and schematic for EM406 connector. Spark Fun Electronics SKU : GPS-00579</description>
<gates>
<gate name="G$1" symbol="EM406"/>
</gates>
<devices>
<device name="" package="EM406">
<connects>
<connect gate="G$1" pin="GND1" pad="1"/>
<connect gate="G$1" pin="GND2" pad="5"/>
<connect gate="G$1" pin="NC" pad="6"/>
<connect gate="G$1" pin="RX" pad="3"/>
<connect gate="G$1" pin="TX" pad="4"/>
<connect gate="G$1" pin="VCC" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="?M06B-SRSS-TB" prefix="X">
<description>&lt;b&gt;Disconnectable Crimp style connector, 1.0mm pitch&lt;/b&gt;&lt;br&gt;6 contacts</description>
<gates>
<gate name="-1" symbol="KV"/>
<gate name="-2" symbol="K"/>
<gate name="-3" symbol="K"/>
<gate name="-4" symbol="K"/>
<gate name="-5" symbol="K"/>
<gate name="-6" symbol="K"/>
</gates>
<devices>
<device name="B" package="BM06B-SRSS-TB">
<connects>
<connect gate="-1" pin="S" pad="1"/>
<connect gate="-2" pin="S" pad="2"/>
<connect gate="-3" pin="S" pad="3"/>
<connect gate="-4" pin="S" pad="4"/>
<connect gate="-5" pin="S" pad="5"/>
<connect gate="-6" pin="S" pad="6"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="S" package="SM06B-SRSS-TB">
<connects>
<connect gate="-1" pin="S" pad="1"/>
<connect gate="-2" pin="S" pad="2"/>
<connect gate="-3" pin="S" pad="3"/>
<connect gate="-4" pin="S" pad="4"/>
<connect gate="-5" pin="S" pad="5"/>
<connect gate="-6" pin="S" pad="6"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="53?-10" prefix="X" uservalue="yes">
<description>&lt;b&gt;CONNECTOR&lt;/b&gt;&lt;p&gt;
wire to board 1.25 mm (.049 inch) pitch header</description>
<gates>
<gate name="-1" symbol="MV"/>
<gate name="-2" symbol="M"/>
<gate name="-3" symbol="M"/>
<gate name="-4" symbol="M"/>
<gate name="-5" symbol="M"/>
<gate name="-6" symbol="M"/>
<gate name="-7" symbol="M"/>
<gate name="-8" symbol="M"/>
<gate name="-9" symbol="M"/>
<gate name="-10" symbol="M"/>
</gates>
<devices>
<device name="047" package="53047-10">
<connects>
<connect gate="-1" pin="S" pad="1"/>
<connect gate="-10" pin="S" pad="10"/>
<connect gate="-2" pin="S" pad="2"/>
<connect gate="-3" pin="S" pad="3"/>
<connect gate="-4" pin="S" pad="4"/>
<connect gate="-5" pin="S" pad="5"/>
<connect gate="-6" pin="S" pad="6"/>
<connect gate="-7" pin="S" pad="7"/>
<connect gate="-8" pin="S" pad="8"/>
<connect gate="-9" pin="S" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="048" package="53048-10">
<connects>
<connect gate="-1" pin="S" pad="1"/>
<connect gate="-10" pin="S" pad="10"/>
<connect gate="-2" pin="S" pad="2"/>
<connect gate="-3" pin="S" pad="3"/>
<connect gate="-4" pin="S" pad="4"/>
<connect gate="-5" pin="S" pad="5"/>
<connect gate="-6" pin="S" pad="6"/>
<connect gate="-7" pin="S" pad="7"/>
<connect gate="-8" pin="S" pad="8"/>
<connect gate="-9" pin="S" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="261" package="53261-10">
<connects>
<connect gate="-1" pin="S" pad="1"/>
<connect gate="-10" pin="S" pad="10"/>
<connect gate="-2" pin="S" pad="2"/>
<connect gate="-3" pin="S" pad="3"/>
<connect gate="-4" pin="S" pad="4"/>
<connect gate="-5" pin="S" pad="5"/>
<connect gate="-6" pin="S" pad="6"/>
<connect gate="-7" pin="S" pad="7"/>
<connect gate="-8" pin="S" pad="8"/>
<connect gate="-9" pin="S" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="398" package="53398-10">
<connects>
<connect gate="-1" pin="S" pad="1"/>
<connect gate="-10" pin="S" pad="10"/>
<connect gate="-2" pin="S" pad="2"/>
<connect gate="-3" pin="S" pad="3"/>
<connect gate="-4" pin="S" pad="4"/>
<connect gate="-5" pin="S" pad="5"/>
<connect gate="-6" pin="S" pad="6"/>
<connect gate="-7" pin="S" pad="7"/>
<connect gate="-8" pin="S" pad="8"/>
<connect gate="-9" pin="S" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="74LVC2G240">
<description>Dual inverter tri-state, 3.3V/5V compatible
&lt;br /&gt;
&lt;a href="http://www.nxp.com/documents/data_sheet/74LVC2G240.pdf"&gt;http://www.nxp.com/documents/data_sheet/74LVC2G240.pdf&lt;/a&gt;&lt;br /&gt;
&lt;a href="http://focus.ti.com/lit/ds/symlink/sn74lvc2g240.pdf"&gt;http://focus.ti.com/lit/ds/symlink/sn74lvc2g240.pdf&lt;/a&gt;</description>
<gates>
<gate name="G$1" symbol="74LVC2G240"/>
</gates>
<devices>
<device name="-TSSOP-8" package="TSSOP8_SOT505-2">
<connects>
<connect gate="G$1" pin="!1OE" pad="1"/>
<connect gate="G$1" pin="!2OE" pad="7"/>
<connect gate="G$1" pin="1A" pad="2"/>
<connect gate="G$1" pin="1Y" pad="6"/>
<connect gate="G$1" pin="2A" pad="5"/>
<connect gate="G$1" pin="2Y" pad="3"/>
<connect gate="G$1" pin="GND" pad="4"/>
<connect gate="G$1" pin="VCC" pad="8"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WIREPAD" prefix="PAD">
<description>&lt;b&gt;Wire PAD&lt;/b&gt; connect wire on PCB</description>
<gates>
<gate name="G$1" symbol="PAD-1"/>
</gates>
<devices>
<device name="1,6/0,8" package="1,6/0,8">
<connects>
<connect gate="G$1" pin="P" pad="1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="1,6/0,9" package="1,6/0,9">
<connects>
<connect gate="G$1" pin="P" pad="1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="2,15/1,0" package="2,15/1,0">
<connects>
<connect gate="G$1" pin="P" pad="1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="2,54/0,8" package="2,54/0,8">
<connects>
<connect gate="G$1" pin="P" pad="1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="2,54/0,9" package="2,54/0,9">
<connects>
<connect gate="G$1" pin="P" pad="1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="2,54/1,0" package="2,54/1,0">
<connects>
<connect gate="G$1" pin="P" pad="1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="2,54/1,1" package="2,54/1,1">
<connects>
<connect gate="G$1" pin="P" pad="1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="3,17/1,1" package="3,17/1,1">
<connects>
<connect gate="G$1" pin="P" pad="1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="3,17/1,2" package="3,17/1,2">
<connects>
<connect gate="G$1" pin="P" pad="1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="3,17/1,3" package="3,17/1,3">
<connects>
<connect gate="G$1" pin="P" pad="1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="3,81/1,1" package="3,81/1,1">
<connects>
<connect gate="G$1" pin="P" pad="1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="3,81/1,3" package="3,81/1,3">
<connects>
<connect gate="G$1" pin="P" pad="1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="3,81/1,4" package="3,81/1,4">
<connects>
<connect gate="G$1" pin="P" pad="1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="4,16O1,6" package="4,16O1,6">
<connects>
<connect gate="G$1" pin="P" pad="1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="SMD5-1,8" package="5-1,8">
<connects>
<connect gate="G$1" pin="P" pad="1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="SMD5-2,5" package="5-2,5">
<connects>
<connect gate="G$1" pin="P" pad="1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="SMD3,5-2" package="3,5-2">
<connects>
<connect gate="G$1" pin="P" pad="1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="SMD2.5-1.8" package="PAD-2.5-1.8">
<connects>
<connect gate="G$1" pin="P" pad="P$1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="TH-1.5MM" package="WIREPAD-TH-1.5MM">
<connects>
<connect gate="G$1" pin="P" pad="1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="TH-2.0MM" package="WIREPAD-TH-2.0MM">
<connects>
<connect gate="G$1" pin="P" pad="1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="53?-05" prefix="X" uservalue="yes">
<description>&lt;b&gt;CONNECTOR&lt;/b&gt;&lt;p&gt;
wire to board 1.25 mm (.049 inch) pitch header</description>
<gates>
<gate name="-1" symbol="MV"/>
<gate name="-2" symbol="M"/>
<gate name="-3" symbol="M"/>
<gate name="-4" symbol="M"/>
<gate name="-5" symbol="M"/>
</gates>
<devices>
<device name="047" package="53047-05">
<connects>
<connect gate="-1" pin="S" pad="1"/>
<connect gate="-2" pin="S" pad="2"/>
<connect gate="-3" pin="S" pad="3"/>
<connect gate="-4" pin="S" pad="4"/>
<connect gate="-5" pin="S" pad="5"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="048" package="53048-05">
<connects>
<connect gate="-1" pin="S" pad="1"/>
<connect gate="-2" pin="S" pad="2"/>
<connect gate="-3" pin="S" pad="3"/>
<connect gate="-4" pin="S" pad="4"/>
<connect gate="-5" pin="S" pad="5"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="261" package="53261-05">
<connects>
<connect gate="-1" pin="S" pad="1"/>
<connect gate="-2" pin="S" pad="2"/>
<connect gate="-3" pin="S" pad="3"/>
<connect gate="-4" pin="S" pad="4"/>
<connect gate="-5" pin="S" pad="5"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="398" package="53398-05">
<connects>
<connect gate="-1" pin="S" pad="1"/>
<connect gate="-2" pin="S" pad="2"/>
<connect gate="-3" pin="S" pad="3"/>
<connect gate="-4" pin="S" pad="4"/>
<connect gate="-5" pin="S" pad="5"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MEDIATEK_MT3329_PADS" prefix="MT3329" uservalue="yes">
<description>Based on MediaTek Single Chip Architecture.
Dimension?16mm x 16mm x 6mm.
L1 Frequency, C/A code, 66 channels.
High Sensitivity?Up to -165dBm tracking, superior urban performances.</description>
<gates>
<gate name="G$1" symbol="MEDIATEK_MT3329"/>
</gates>
<devices>
<device name="" package="MEDIATEK_MT3329">
<connects>
<connect gate="G$1" pin="3D-FIX" pad="5"/>
<connect gate="G$1" pin="D+" pad="6"/>
<connect gate="G$1" pin="D-" pad="7"/>
<connect gate="G$1" pin="ENABLE" pad="2"/>
<connect gate="G$1" pin="GND" pad="3"/>
<connect gate="G$1" pin="GND2" pad="8"/>
<connect gate="G$1" pin="NC" pad="11"/>
<connect gate="G$1" pin="NC2" pad="12"/>
<connect gate="G$1" pin="RXD-I" pad="10"/>
<connect gate="G$1" pin="TXD-O" pad="9"/>
<connect gate="G$1" pin="VBACKUP" pad="4"/>
<connect gate="G$1" pin="VCC" pad="1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="HMC5883L">
<description>&lt;b&gt;Honeywell HMC5883L 12bit Magnetometer&lt;/b&gt;</description>
<gates>
<gate name="G$1" symbol="HMC5883L"/>
</gates>
<devices>
<device name="" package="HMC5883L-MAN">
<connects>
<connect gate="G$1" pin="C1" pad="10"/>
<connect gate="G$1" pin="DRDY" pad="15"/>
<connect gate="G$1" pin="GND1" pad="9"/>
<connect gate="G$1" pin="GND2" pad="11"/>
<connect gate="G$1" pin="NC_P14" pad="14"/>
<connect gate="G$1" pin="NC_P3" pad="3"/>
<connect gate="G$1" pin="NC_P5" pad="5"/>
<connect gate="G$1" pin="NC_P6" pad="6"/>
<connect gate="G$1" pin="NC_P7" pad="7"/>
<connect gate="G$1" pin="S1_VDDIO" pad="4"/>
<connect gate="G$1" pin="SCL" pad="1"/>
<connect gate="G$1" pin="SDA" pad="16"/>
<connect gate="G$1" pin="SETC" pad="12"/>
<connect gate="G$1" pin="SETP" pad="8"/>
<connect gate="G$1" pin="VDD" pad="2"/>
<connect gate="G$1" pin="VDDIO" pad="13"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ADH8066" prefix="U">
<description>8066-GSM-GPRS module from ADH-Tech</description>
<gates>
<gate name="G$1" symbol="ADH8066"/>
</gates>
<devices>
<device name="_SMD" package="ADH8066">
<connects>
<connect gate="G$1" pin="1.8V" pad="31"/>
<connect gate="G$1" pin="ADC1" pad="11"/>
<connect gate="G$1" pin="AUXOUTN" pad="48"/>
<connect gate="G$1" pin="AUXOUTP" pad="47"/>
<connect gate="G$1" pin="BATTTEMP" pad="12"/>
<connect gate="G$1" pin="CHV_DRV" pad="20"/>
<connect gate="G$1" pin="CHV_MAX" pad="40"/>
<connect gate="G$1" pin="CTS0" pad="34"/>
<connect gate="G$1" pin="DCD0" pad="39"/>
<connect gate="G$1" pin="DSR0" pad="35"/>
<connect gate="G$1" pin="DTR0" pad="33"/>
<connect gate="G$1" pin="EARN" pad="50"/>
<connect gate="G$1" pin="EARP" pad="49"/>
<connect gate="G$1" pin="GND@21" pad="21"/>
<connect gate="G$1" pin="GND@22" pad="22"/>
<connect gate="G$1" pin="GND@23" pad="23"/>
<connect gate="G$1" pin="GND@24" pad="24"/>
<connect gate="G$1" pin="GND@25" pad="25"/>
<connect gate="G$1" pin="GND@42" pad="42"/>
<connect gate="G$1" pin="GND@6" pad="6"/>
<connect gate="G$1" pin="GPIO10" pad="5"/>
<connect gate="G$1" pin="GPIO3" pad="13"/>
<connect gate="G$1" pin="MIC1_N" pad="44"/>
<connect gate="G$1" pin="MIC1_P" pad="43"/>
<connect gate="G$1" pin="MIC2_N" pad="46"/>
<connect gate="G$1" pin="MIC2_P" pad="45"/>
<connect gate="G$1" pin="ON_KEY" pad="41"/>
<connect gate="G$1" pin="PCMCLK" pad="9"/>
<connect gate="G$1" pin="PCMDI" pad="7"/>
<connect gate="G$1" pin="PCMDO" pad="10"/>
<connect gate="G$1" pin="PCMFSO" pad="8"/>
<connect gate="G$1" pin="RI0" pad="32"/>
<connect gate="G$1" pin="RTS0" pad="37"/>
<connect gate="G$1" pin="RXD0" pad="17"/>
<connect gate="G$1" pin="RXD1" pad="16"/>
<connect gate="G$1" pin="SCL(NC)" pad="36"/>
<connect gate="G$1" pin="SDA(NC)" pad="38"/>
<connect gate="G$1" pin="SIMCLK" pad="1"/>
<connect gate="G$1" pin="SIMIO" pad="3"/>
<connect gate="G$1" pin="SIMRST" pad="4"/>
<connect gate="G$1" pin="SIMVDD" pad="2"/>
<connect gate="G$1" pin="TXD0" pad="15"/>
<connect gate="G$1" pin="TXD1" pad="14"/>
<connect gate="G$1" pin="VBAT@26" pad="26"/>
<connect gate="G$1" pin="VBAT@27" pad="27"/>
<connect gate="G$1" pin="VBAT@28" pad="28"/>
<connect gate="G$1" pin="VBAT@29" pad="29"/>
<connect gate="G$1" pin="VBAT@30" pad="30"/>
<connect gate="G$1" pin="VCHAR@18" pad="18"/>
<connect gate="G$1" pin="VCHAR@19" pad="19"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="?3B-ZR">
<gates>
<gate name="-1" symbol="KV"/>
<gate name="-2" symbol="K"/>
<gate name="-3" symbol="K"/>
</gates>
<devices>
<device name="S" package="S3B-ZR-SM4A-TF">
<connects>
<connect gate="-1" pin="S" pad="P$1"/>
<connect gate="-2" pin="S" pad="P$2"/>
<connect gate="-3" pin="S" pad="P$3"/>
</connects>
<technologies>
<technology name="-SM4A-TF"/>
</technologies>
</device>
<device name="B" package="B3B-ZR">
<connects>
<connect gate="-1" pin="S" pad="1"/>
<connect gate="-2" pin="S" pad="2"/>
<connect gate="-3" pin="S" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="?4B-PH">
<gates>
<gate name="-1" symbol="KV"/>
<gate name="-2" symbol="K"/>
<gate name="-3" symbol="K"/>
<gate name="-4" symbol="K"/>
</gates>
<devices>
<device name="S" package="S4B-PH-SM4-TB">
<connects>
<connect gate="-1" pin="S" pad="1"/>
<connect gate="-2" pin="S" pad="2"/>
<connect gate="-3" pin="S" pad="3"/>
<connect gate="-4" pin="S" pad="4"/>
</connects>
<technologies>
<technology name="-SM4-TB"/>
</technologies>
</device>
<device name="" package="B4B-PH-K-S">
<connects>
<connect gate="-1" pin="S" pad="1"/>
<connect gate="-2" pin="S" pad="2"/>
<connect gate="-3" pin="S" pad="3"/>
<connect gate="-4" pin="S" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="CONN_CAN">
<gates>
<gate name="-CAN_V+" symbol="KV"/>
<gate name="-CAN_H" symbol="K"/>
<gate name="-CAN_L" symbol="K"/>
<gate name="-CAN_GND" symbol="K"/>
</gates>
<devices>
<device name="-TH" package="B4B-PH-K-S">
<connects>
<connect gate="-CAN_GND" pin="S" pad="4"/>
<connect gate="-CAN_H" pin="S" pad="2"/>
<connect gate="-CAN_L" pin="S" pad="3"/>
<connect gate="-CAN_V+" pin="S" pad="1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-SMD" package="S4B-PH-SM4-TB">
<connects>
<connect gate="-CAN_GND" pin="S" pad="4"/>
<connect gate="-CAN_H" pin="S" pad="2"/>
<connect gate="-CAN_L" pin="S" pad="3"/>
<connect gate="-CAN_V+" pin="S" pad="1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="JST-PA-02">
<description>JST PA Series

&lt;a href="http://www.jst-mfg.com/product/pdf/eng/ePA-F.pdf"&gt;http://www.jst-mfg.com/product/pdf/eng/ePA-F.pdf&lt;/a&gt;</description>
<gates>
<gate name="-1" symbol="MV"/>
<gate name="-2" symbol="M"/>
</gates>
<devices>
<device name="" package="S02B-PASK-2">
<connects>
<connect gate="-1" pin="S" pad="1"/>
<connect gate="-2" pin="S" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LENSMOUNT_M12">
<description>Point Grey compatible M12 lens mount</description>
<gates>
<gate name="G$1" symbol="LENSMOUNT_M12"/>
</gates>
<devices>
<device name="PTGREY" package="LENSMOUNT_M12">
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="" package="LENSMOUNT_LARGE_M12">
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ADNS-2080">
<gates>
<gate name="G$1" symbol="ADNS-2080"/>
</gates>
<devices>
<device name="" package="ADNS-2080">
<connects>
<connect gate="G$1" pin="GND" pad="6"/>
<connect gate="G$1" pin="LED" pad="2"/>
<connect gate="G$1" pin="MOTION" pad="3"/>
<connect gate="G$1" pin="SCLK" pad="5"/>
<connect gate="G$1" pin="SDIO" pad="1"/>
<connect gate="G$1" pin="VDD" pad="7"/>
<connect gate="G$1" pin="VDDA" pad="8"/>
<connect gate="G$1" pin="VDDIO" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MOSFET-NCHANNEL" prefix="Q">
<gates>
<gate name="G$1" symbol="MOSFET-NCHANNEL"/>
</gates>
<devices>
<device name="SMD" package="SOT23-3">
<connects>
<connect gate="G$1" pin="D" pad="3"/>
<connect gate="G$1" pin="G" pad="1"/>
<connect gate="G$1" pin="S" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-PTH" package="TO-92">
<connects>
<connect gate="G$1" pin="D" pad="1"/>
<connect gate="G$1" pin="G" pad="3"/>
<connect gate="G$1" pin="S" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-DPAK" package="DPAK">
<connects>
<connect gate="G$1" pin="D" pad="4"/>
<connect gate="G$1" pin="G" pad="1"/>
<connect gate="G$1" pin="S" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-WDFN8" package="WDFN8">
<connects>
<connect gate="G$1" pin="D" pad="D@1 D@2 D@3 D@4"/>
<connect gate="G$1" pin="G" pad="G"/>
<connect gate="G$1" pin="S" pad="S@1 S@2 S@3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="HEADER_2X8">
<gates>
<gate name="-1" symbol="KV"/>
<gate name="-2" symbol="K"/>
<gate name="-3" symbol="K"/>
<gate name="-4" symbol="K"/>
<gate name="-5" symbol="K"/>
<gate name="-6" symbol="K"/>
<gate name="-7" symbol="K"/>
<gate name="-8" symbol="K"/>
<gate name="-9" symbol="K"/>
<gate name="-10" symbol="K"/>
<gate name="-11" symbol="K"/>
<gate name="-12" symbol="K"/>
<gate name="-13" symbol="K"/>
<gate name="-14" symbol="K"/>
<gate name="-15" symbol="K"/>
<gate name="-16" symbol="K"/>
</gates>
<devices>
<device name="" package="HEADER_2MM_2X8">
<connects>
<connect gate="-1" pin="S" pad="1"/>
<connect gate="-10" pin="S" pad="10"/>
<connect gate="-11" pin="S" pad="11"/>
<connect gate="-12" pin="S" pad="12"/>
<connect gate="-13" pin="S" pad="13"/>
<connect gate="-14" pin="S" pad="14"/>
<connect gate="-15" pin="S" pad="15"/>
<connect gate="-16" pin="S" pad="16"/>
<connect gate="-2" pin="S" pad="2"/>
<connect gate="-3" pin="S" pad="3"/>
<connect gate="-4" pin="S" pad="4"/>
<connect gate="-5" pin="S" pad="5"/>
<connect gate="-6" pin="S" pad="6"/>
<connect gate="-7" pin="S" pad="7"/>
<connect gate="-8" pin="S" pad="8"/>
<connect gate="-9" pin="S" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="JUMPER-2">
<gates>
<gate name="G$1" symbol="JUMPER-2"/>
</gates>
<devices>
<device name="" package="SJ_2">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ARM_JTAG">
<gates>
<gate name="-VREF" symbol="KV"/>
<gate name="-VSUPPLY" symbol="K"/>
<gate name="-!TRST" symbol="K"/>
<gate name="-GND1" symbol="K"/>
<gate name="-TDI" symbol="K"/>
<gate name="-GND2" symbol="K"/>
<gate name="-TMS" symbol="K"/>
<gate name="-GND3" symbol="K"/>
<gate name="-TCK" symbol="K"/>
<gate name="-GND4" symbol="K"/>
<gate name="-RTCK" symbol="K"/>
<gate name="-GND5" symbol="K"/>
<gate name="-TDO" symbol="K"/>
<gate name="-GND6" symbol="K"/>
<gate name="-!SRST" symbol="K"/>
<gate name="-GND7" symbol="K"/>
<gate name="-DBGRQ" symbol="K"/>
<gate name="-GND8" symbol="K"/>
<gate name="-DBGACK" symbol="K"/>
<gate name="-GND9" symbol="K"/>
</gates>
<devices>
<device name="" package="HEADER_2.54MM-2X10-SHROUDED_LOCK">
<connects>
<connect gate="-!SRST" pin="S" pad="15"/>
<connect gate="-!TRST" pin="S" pad="3"/>
<connect gate="-DBGACK" pin="S" pad="19"/>
<connect gate="-DBGRQ" pin="S" pad="17"/>
<connect gate="-GND1" pin="S" pad="4"/>
<connect gate="-GND2" pin="S" pad="6"/>
<connect gate="-GND3" pin="S" pad="8"/>
<connect gate="-GND4" pin="S" pad="10"/>
<connect gate="-GND5" pin="S" pad="12"/>
<connect gate="-GND6" pin="S" pad="14"/>
<connect gate="-GND7" pin="S" pad="16"/>
<connect gate="-GND8" pin="S" pad="18"/>
<connect gate="-GND9" pin="S" pad="20"/>
<connect gate="-RTCK" pin="S" pad="11"/>
<connect gate="-TCK" pin="S" pad="9"/>
<connect gate="-TDI" pin="S" pad="5"/>
<connect gate="-TDO" pin="S" pad="13"/>
<connect gate="-TMS" pin="S" pad="7"/>
<connect gate="-VREF" pin="S" pad="1"/>
<connect gate="-VSUPPLY" pin="S" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="FTDI-CABLE-3V3">
<gates>
<gate name="-GND" symbol="KV"/>
<gate name="-CTS#" symbol="K"/>
<gate name="-VCC_5V" symbol="K"/>
<gate name="-TXD" symbol="K"/>
<gate name="-RXD" symbol="K"/>
<gate name="-RTS#" symbol="K"/>
</gates>
<devices>
<device name="" package="HEADER_1X06-SIP_LOCK">
<connects>
<connect gate="-CTS#" pin="S" pad="2"/>
<connect gate="-GND" pin="S" pad="1"/>
<connect gate="-RTS#" pin="S" pad="6"/>
<connect gate="-RXD" pin="S" pad="5"/>
<connect gate="-TXD" pin="S" pad="4"/>
<connect gate="-VCC_5V" pin="S" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="POWER_JACK" prefix="J">
<description>&lt;b&gt;Power Jack&lt;/b&gt;
This is the standard 5.5mm barrel jack for power. The PTH is the most common, proven, reliable, footprint. All others are experimental. The Slot footprint only works if the mill layer is transmitted to the PCB fab house so be warned. Spark Fun Electronics SKU : PRT-00119. Mating wall wart : TOL-00298 (and others)</description>
<gates>
<gate name="G$1" symbol="POWERJACK"/>
</gates>
<devices>
<device name="SMD" package="POWER_JACK_SMD">
<connects>
<connect gate="G$1" pin="GND" pad="P$4"/>
<connect gate="G$1" pin="GNDBREAK" pad="GND"/>
<connect gate="G$1" pin="PWR" pad="VIN0"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="SLT" package="POWER_JACK_SLOT">
<connects>
<connect gate="G$1" pin="GND" pad="GND@2"/>
<connect gate="G$1" pin="GNDBREAK" pad="GND@1"/>
<connect gate="G$1" pin="PWR" pad="PWR"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="PTH" package="POWER_JACK_PTH">
<connects>
<connect gate="G$1" pin="GND" pad="GND"/>
<connect gate="G$1" pin="GNDBREAK" pad="GNDBREAK"/>
<connect gate="G$1" pin="PWR" pad="PWR"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="COMBO" package="POWER_JACK_COMBO">
<connects>
<connect gate="G$1" pin="GND" pad="GND@1"/>
<connect gate="G$1" pin="GNDBREAK" pad="GND"/>
<connect gate="G$1" pin="PWR" pad="POWER"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="RCA" package="RCA">
<connects>
<connect gate="G$1" pin="GND" pad="BARREL"/>
<connect gate="G$1" pin="GNDBREAK" pad="SPRING"/>
<connect gate="G$1" pin="PWR" pad="BREAK"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="PTH_LOCK" package="POWER_JACK_PTH_LOCK">
<connects>
<connect gate="G$1" pin="GND" pad="GND"/>
<connect gate="G$1" pin="GNDBREAK" pad="GNDBREAK"/>
<connect gate="G$1" pin="PWR" pad="PWR"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="RCA_LOCK" package="RCA_LOCK">
<connects>
<connect gate="G$1" pin="GND" pad="BARREL"/>
<connect gate="G$1" pin="GNDBREAK" pad="SPRING"/>
<connect gate="G$1" pin="PWR" pad="BREAK"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MOSFET-PCHANNEL-NTGS4111P">
<gates>
<gate name="G$1" symbol="MOSFET-PCHANNEL-6POS"/>
</gates>
<devices>
<device name="" package="TSOP-6">
<connects>
<connect gate="G$1" pin="D" pad="1"/>
<connect gate="G$1" pin="D1" pad="2"/>
<connect gate="G$1" pin="D2" pad="5"/>
<connect gate="G$1" pin="D3" pad="6"/>
<connect gate="G$1" pin="G" pad="3"/>
<connect gate="G$1" pin="S" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="TS3A24157">
<description>&lt;h3&gt;2:1 Multiplexer / Demultiplexer&lt;/h3&gt;

This part is an analog multiplexer / demultiplexer for a wide range of signals, including audio and UART.

&lt;a href="http://focus.ti.com/lit/ds/symlink/ts3a24157.pdf"&gt;Datasheet&lt;/a&gt;</description>
<gates>
<gate name="G$1" symbol="TS3A24157"/>
</gates>
<devices>
<device name="" package="TI-DGS">
<connects>
<connect gate="G$1" pin="COM1" pad="9"/>
<connect gate="G$1" pin="COM2" pad="6"/>
<connect gate="G$1" pin="GND" pad="5"/>
<connect gate="G$1" pin="IN1" pad="8"/>
<connect gate="G$1" pin="IN2" pad="7"/>
<connect gate="G$1" pin="NC1" pad="1"/>
<connect gate="G$1" pin="NC2" pad="3"/>
<connect gate="G$1" pin="NO1" pad="2"/>
<connect gate="G$1" pin="NO2" pad="4"/>
<connect gate="G$1" pin="V+" pad="10"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="FT4232H">
<gates>
<gate name="G$1" symbol="FT4232H"/>
</gates>
<devices>
<device name="" package="TQFP64">
<connects>
<connect gate="G$1" pin="!PWREN" pad="60"/>
<connect gate="G$1" pin="!RESET" pad="14"/>
<connect gate="G$1" pin="!SUSPEND" pad="36"/>
<connect gate="G$1" pin="ADBUS0" pad="16"/>
<connect gate="G$1" pin="ADBUS1" pad="17"/>
<connect gate="G$1" pin="ADBUS2" pad="18"/>
<connect gate="G$1" pin="ADBUS3" pad="19"/>
<connect gate="G$1" pin="ADBUS4" pad="21"/>
<connect gate="G$1" pin="ADBUS5" pad="22"/>
<connect gate="G$1" pin="ADBUS6" pad="23"/>
<connect gate="G$1" pin="ADBUS7" pad="24"/>
<connect gate="G$1" pin="AGND" pad="10"/>
<connect gate="G$1" pin="BDBUS0" pad="26"/>
<connect gate="G$1" pin="BDBUS1" pad="27"/>
<connect gate="G$1" pin="BDBUS2" pad="28"/>
<connect gate="G$1" pin="BDBUS3" pad="29"/>
<connect gate="G$1" pin="BDBUS4" pad="30"/>
<connect gate="G$1" pin="BDBUS5" pad="32"/>
<connect gate="G$1" pin="BDBUS6" pad="33"/>
<connect gate="G$1" pin="BDBUS7" pad="34"/>
<connect gate="G$1" pin="CDBUS0" pad="38"/>
<connect gate="G$1" pin="CDBUS1" pad="39"/>
<connect gate="G$1" pin="CDBUS2" pad="40"/>
<connect gate="G$1" pin="CDBUS3" pad="41"/>
<connect gate="G$1" pin="CDBUS4" pad="43"/>
<connect gate="G$1" pin="CDBUS5" pad="44"/>
<connect gate="G$1" pin="CDBUS6" pad="45"/>
<connect gate="G$1" pin="CDBUS7" pad="46"/>
<connect gate="G$1" pin="DDBUS0" pad="48"/>
<connect gate="G$1" pin="DDBUS1" pad="52"/>
<connect gate="G$1" pin="DDBUS2" pad="53"/>
<connect gate="G$1" pin="DDBUS3" pad="54"/>
<connect gate="G$1" pin="DDBUS4" pad="55"/>
<connect gate="G$1" pin="DDBUS5" pad="57"/>
<connect gate="G$1" pin="DDBUS6" pad="58"/>
<connect gate="G$1" pin="DDBUS7" pad="59"/>
<connect gate="G$1" pin="DM" pad="7"/>
<connect gate="G$1" pin="DP" pad="8"/>
<connect gate="G$1" pin="EECLK" pad="62"/>
<connect gate="G$1" pin="EECS" pad="63"/>
<connect gate="G$1" pin="EEDATA" pad="61"/>
<connect gate="G$1" pin="GND1" pad="1"/>
<connect gate="G$1" pin="GND2" pad="5"/>
<connect gate="G$1" pin="GND3" pad="11"/>
<connect gate="G$1" pin="GND4" pad="15"/>
<connect gate="G$1" pin="GND5" pad="25"/>
<connect gate="G$1" pin="GND6" pad="35"/>
<connect gate="G$1" pin="GND7" pad="47"/>
<connect gate="G$1" pin="GND8" pad="51"/>
<connect gate="G$1" pin="OSCI" pad="2"/>
<connect gate="G$1" pin="OSCO" pad="3"/>
<connect gate="G$1" pin="REF" pad="6"/>
<connect gate="G$1" pin="TEST" pad="13"/>
<connect gate="G$1" pin="VCCIO1" pad="20"/>
<connect gate="G$1" pin="VCCIO2" pad="31"/>
<connect gate="G$1" pin="VCCIO3" pad="42"/>
<connect gate="G$1" pin="VCCIO4" pad="56"/>
<connect gate="G$1" pin="VCORE1" pad="12"/>
<connect gate="G$1" pin="VCORE2" pad="37"/>
<connect gate="G$1" pin="VCORE3" pad="64"/>
<connect gate="G$1" pin="VPHY" pad="4"/>
<connect gate="G$1" pin="VPLL" pad="9"/>
<connect gate="G$1" pin="VREGIN" pad="50"/>
<connect gate="G$1" pin="VREGOUT" pad="49"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="SWITCH-SPST" prefix="S" uservalue="yes">
<description>&lt;b&gt;SPST Switch&lt;/b&gt;
Simple slide switch. Spark Fun Electronics SKU : COM-00102</description>
<gates>
<gate name="1" symbol="TOGGLE"/>
</gates>
<devices>
<device name="PTH" package="SWITCH-SPDT">
<connects>
<connect gate="1" pin="O" pad="1"/>
<connect gate="1" pin="P" pad="2"/>
<connect gate="1" pin="S" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="SMD" package="AYZ0202">
<connects>
<connect gate="1" pin="O" pad="1"/>
<connect gate="1" pin="P" pad="2"/>
<connect gate="1" pin="S" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="PTH2" package="SWITCHE-DPDT">
<connects>
<connect gate="1" pin="O" pad="1"/>
<connect gate="1" pin="P" pad="2"/>
<connect gate="1" pin="S" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="PTH3" package="R_SW_TH">
<connects>
<connect gate="1" pin="O" pad="P$1"/>
<connect gate="1" pin="P" pad="P$2"/>
<connect gate="1" pin="S" pad="P$3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="SMD2" package="SWITCH-SPDT-SMD">
<connects>
<connect gate="1" pin="O" pad="1"/>
<connect gate="1" pin="P" pad="2"/>
<connect gate="1" pin="S" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="PTH_LOCK" package="SWITCH-SPDT_LOCK.007S">
<connects>
<connect gate="1" pin="O" pad="1"/>
<connect gate="1" pin="P" pad="2"/>
<connect gate="1" pin="S" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="PTH-HORZ" package="SWITCH-SPDT-TH-HORZ">
<connects>
<connect gate="1" pin="O" pad="1"/>
<connect gate="1" pin="P" pad="2"/>
<connect gate="1" pin="S" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="USB" prefix="X">
<description>&lt;b&gt;USB Connectors&lt;/b&gt;
&lt;p&gt;USB-B-PTH is fully proven SKU : PRT-00139
&lt;p&gt;USB-miniB is fully proven SKU : PRT-00587
&lt;p&gt;USB-A-PCB is untested.
&lt;p&gt;USB-A-H is throughly reviewed, but untested. Spark Fun Electronics SKU : PRT-00437
&lt;p&gt;USB-B-SMT is throughly reviewed, but untested. Needs silkscreen touching up.
&lt;p&gt;USB-A-S has not been used/tested
&lt;p&gt;USB-MB-H has not been used/tested</description>
<gates>
<gate name="G$1" symbol="USB"/>
</gates>
<devices>
<device name="-A-H" package="USB-A-H">
<connects>
<connect gate="G$1" pin="D+" pad="D-"/>
<connect gate="G$1" pin="D-" pad="D+"/>
<connect gate="G$1" pin="GND" pad="VBUS"/>
<connect gate="G$1" pin="VBUS" pad="GND"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-A-S" package="USB-A-S">
<connects>
<connect gate="G$1" pin="D+" pad="D+"/>
<connect gate="G$1" pin="D-" pad="D-"/>
<connect gate="G$1" pin="GND" pad="GND"/>
<connect gate="G$1" pin="VBUS" pad="VBUS"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-MB-H" package="USB-MB-H">
<connects>
<connect gate="G$1" pin="D+" pad="D+"/>
<connect gate="G$1" pin="D-" pad="D-"/>
<connect gate="G$1" pin="GND" pad="GND"/>
<connect gate="G$1" pin="VBUS" pad="VBUS"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-B-S" package="USB-B-SMT">
<connects>
<connect gate="G$1" pin="D+" pad="D+"/>
<connect gate="G$1" pin="D-" pad="D-"/>
<connect gate="G$1" pin="GND" pad="GND"/>
<connect gate="G$1" pin="VBUS" pad="VUSB"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="PTH" package="USB-B-PTH">
<connects>
<connect gate="G$1" pin="D+" pad="D+"/>
<connect gate="G$1" pin="D-" pad="D-"/>
<connect gate="G$1" pin="GND" pad="GND"/>
<connect gate="G$1" pin="VBUS" pad="VBUS"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-JST-2MM-SMT" package="S4B-PH">
<connects>
<connect gate="G$1" pin="D+" pad="2"/>
<connect gate="G$1" pin="D-" pad="3"/>
<connect gate="G$1" pin="GND" pad="1"/>
<connect gate="G$1" pin="VBUS" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="SMD" package="USB-MINIB">
<connects>
<connect gate="G$1" pin="D+" pad="D+"/>
<connect gate="G$1" pin="D-" pad="D-"/>
<connect gate="G$1" pin="GND" pad="GND"/>
<connect gate="G$1" pin="VBUS" pad="VBUS"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="PCB" package="USB-A-PCB">
<connects>
<connect gate="G$1" pin="D+" pad="USB_P"/>
<connect gate="G$1" pin="D-" pad="USB_M"/>
<connect gate="G$1" pin="GND" pad="GND"/>
<connect gate="G$1" pin="VBUS" pad="5V"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="PTH-VERTICAL" package="USB-B-PTH-VERTICAL">
<connects>
<connect gate="G$1" pin="D+" pad="D+"/>
<connect gate="G$1" pin="D-" pad="D-"/>
<connect gate="G$1" pin="GND" pad="GND"/>
<connect gate="G$1" pin="VBUS" pad="VBUS"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="USB-A-S-NOSILK" package="USB-A-S-NOSILK">
<connects>
<connect gate="G$1" pin="D+" pad="D+"/>
<connect gate="G$1" pin="D-" pad="D-"/>
<connect gate="G$1" pin="GND" pad="GND"/>
<connect gate="G$1" pin="VBUS" pad="VBUS"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-A-SMD" package="USB-A-S-NOSILK-FEMALE">
<connects>
<connect gate="G$1" pin="D+" pad="D+"/>
<connect gate="G$1" pin="D-" pad="D-"/>
<connect gate="G$1" pin="GND" pad="GND"/>
<connect gate="G$1" pin="VBUS" pad="VBUS"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-MICROB" package="USB-MICROB">
<connects>
<connect gate="G$1" pin="D+" pad="D+"/>
<connect gate="G$1" pin="D-" pad="D-"/>
<connect gate="G$1" pin="GND" pad="GND"/>
<connect gate="G$1" pin="VBUS" pad="VBUS"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_" package="USB-A-S-SILK-FEMALE">
<connects>
<connect gate="G$1" pin="D+" pad="D+"/>
<connect gate="G$1" pin="D-" pad="D-"/>
<connect gate="G$1" pin="GND" pad="GND"/>
<connect gate="G$1" pin="VBUS" pad="VBUS"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="1.8V">
<gates>
<gate name="G$1" symbol="1.8V"/>
</gates>
<devices>
<device name="">
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="2.8V">
<gates>
<gate name="G$1" symbol="2.8V"/>
</gates>
<devices>
<device name="">
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="3.3V" prefix="P+">
<description>&lt;b&gt;SUPPLY SYMBOL&lt;/b&gt;</description>
<gates>
<gate name="G$1" symbol="3.3V"/>
</gates>
<devices>
<device name="">
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="5V">
<gates>
<gate name="G$1" symbol="5V"/>
</gates>
<devices>
<device name="">
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="EEPROM-SERIAL">
<description>&lt;h3&gt;Serial EEPROM (SPI / Microwire)&lt;/h3&gt;

This is a standard footprint for SPI / Microwire serial EEPROMs. Matching parts include:

&lt;ul&gt;
  &lt;li&gt;Microchip Technology 93LC46BT-I/ST: 1K, 16 bit (64x16), 2 MHz, 2.5 - 5.5 V&lt;/li&gt;
&lt;/ul&gt;</description>
<gates>
<gate name="G$1" symbol="EEPROM-SERIAL"/>
</gates>
<devices>
<device name="-TSSOP-8" package="TSSOP-8">
<connects>
<connect gate="G$1" pin="CLK" pad="2"/>
<connect gate="G$1" pin="CS" pad="1"/>
<connect gate="G$1" pin="DI" pad="3"/>
<connect gate="G$1" pin="DO" pad="4"/>
<connect gate="G$1" pin="NC" pad="7"/>
<connect gate="G$1" pin="ORG" pad="6"/>
<connect gate="G$1" pin="VCC" pad="8"/>
<connect gate="G$1" pin="VSS" pad="5"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="TXS0102">
<description>&lt;h3&gt;TI TXS0102 Level Shifter&lt;/h3&gt;

Auto-sensing level shifter, e.g. for I2C or UART.</description>
<gates>
<gate name="G$1" symbol="TX?0102"/>
</gates>
<devices>
<device name="DCUR" package="TI-DCU">
<connects>
<connect gate="G$1" pin="A1" pad="5"/>
<connect gate="G$1" pin="A2" pad="4"/>
<connect gate="G$1" pin="B1" pad="8"/>
<connect gate="G$1" pin="B2" pad="1"/>
<connect gate="G$1" pin="GND" pad="2"/>
<connect gate="G$1" pin="OE" pad="6"/>
<connect gate="G$1" pin="VCCA" pad="3"/>
<connect gate="G$1" pin="VCCB" pad="7"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="BMA180">
<description>&lt;h3&gt;BOSCH BMA180 Accelerometer&lt;/h3&gt;&lt;br /&gt;

High-resolution sensor from Bosch Sensortec, featuring 14 bit resolution.&lt;br /&gt;
&lt;br /&gt;

&lt;a href="http://www.google.ch/url?sa=t&amp;rct=j&amp;q=bma180&amp;source=web&amp;cd=1&amp;ved=0CB0QFjAA&amp;url=http%3A%2F%2Fwww.bosch-sensortec.com%2Fcontent%2Flanguage1%2Fdownloads%2FBST-BMA180-FL000-03.pdf&amp;ei=pwWtTsCPLYGIhQedisnvDw&amp;usg=AFQjCNFhPrGTrqbWNeRaOdpmwdQXBTwpZQ&amp;cad=rja"&gt;Datasheet Link&lt;/a&gt;</description>
<gates>
<gate name="G$1" symbol="BMA180"/>
</gates>
<devices>
<device name="" package="LGA12">
<connects>
<connect gate="G$1" pin="CSB" pad="5"/>
<connect gate="G$1" pin="INT" pad="4"/>
<connect gate="G$1" pin="NC" pad="1"/>
<connect gate="G$1" pin="NC1" pad="6"/>
<connect gate="G$1" pin="NC2" pad="11"/>
<connect gate="G$1" pin="NC3" pad="12"/>
<connect gate="G$1" pin="SCK" pad="7"/>
<connect gate="G$1" pin="SDI" pad="9"/>
<connect gate="G$1" pin="SDO" pad="8"/>
<connect gate="G$1" pin="VDD" pad="2"/>
<connect gate="G$1" pin="VDDIO" pad="10"/>
<connect gate="G$1" pin="VSS" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ITG-3200" prefix="U">
<description>ITG-3200 3-axis gyro, digital output, qfn24 package</description>
<gates>
<gate name="G$1" symbol="ITG-3200"/>
</gates>
<devices>
<device name="" package="QFN-24">
<connects>
<connect gate="G$1" pin="AD0" pad="9"/>
<connect gate="G$1" pin="CLKIN" pad="1"/>
<connect gate="G$1" pin="CPOUT" pad="20"/>
<connect gate="G$1" pin="GND" pad="18"/>
<connect gate="G$1" pin="INT" pad="12"/>
<connect gate="G$1" pin="REGOUT" pad="10"/>
<connect gate="G$1" pin="RESV-G" pad="11"/>
<connect gate="G$1" pin="SCL" pad="23"/>
<connect gate="G$1" pin="SDA" pad="24"/>
<connect gate="G$1" pin="VDD" pad="13"/>
<connect gate="G$1" pin="VLOGIC" pad="8"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="OSHW-LOGO">
<description>&lt;b&gt;Open Source Hardware Logo&lt;/b&gt; This logo indicates the piece of hardware it is found on incorporates a OSHW license and/or adheres to the definition of open source hardware found here: http://freedomdefined.org/OSHW</description>
<gates>
<gate name="G$1" symbol="OSHW-LOGO"/>
</gates>
<devices>
<device name="S" package="OSHW-LOGO-S">
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="M" package="OSHW-LOGO-M">
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="L" package="OSHW-LOGO-L">
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="DF13-2P-1.25?">
<gates>
<gate name="-1" symbol="MV"/>
<gate name="-2" symbol="M"/>
</gates>
<devices>
<device name="DSA" package="DF13-2P-1.25DSA">
<connects>
<connect gate="-1" pin="S" pad="1"/>
<connect gate="-2" pin="S" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="H" package="DF13A-2P-1.25H">
<connects>
<connect gate="-1" pin="S" pad="1"/>
<connect gate="-2" pin="S" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="DF13-3P-1.25?">
<gates>
<gate name="-1" symbol="MV"/>
<gate name="-2" symbol="M"/>
<gate name="-3" symbol="M"/>
</gates>
<devices>
<device name="DSA" package="DF13-3P-1.25DSA">
<connects>
<connect gate="-1" pin="S" pad="1"/>
<connect gate="-2" pin="S" pad="2"/>
<connect gate="-3" pin="S" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="H" package="DF13A-3P-1.25H">
<connects>
<connect gate="-1" pin="S" pad="1"/>
<connect gate="-2" pin="S" pad="2"/>
<connect gate="-3" pin="S" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="DF13-15P-1.25?">
<gates>
<gate name="-1" symbol="MV"/>
<gate name="-2" symbol="M"/>
<gate name="-3" symbol="M"/>
<gate name="-4" symbol="M"/>
<gate name="-5" symbol="M"/>
<gate name="-6" symbol="M"/>
<gate name="-7" symbol="M"/>
<gate name="-8" symbol="M"/>
<gate name="-9" symbol="M"/>
<gate name="-10" symbol="M"/>
<gate name="-11" symbol="M"/>
<gate name="-12" symbol="M"/>
<gate name="-13" symbol="M"/>
<gate name="-14" symbol="M"/>
<gate name="-15" symbol="M"/>
</gates>
<devices>
<device name="DSA" package="DF13-15P-1.25DSA">
<connects>
<connect gate="-1" pin="S" pad="1"/>
<connect gate="-10" pin="S" pad="10"/>
<connect gate="-11" pin="S" pad="11"/>
<connect gate="-12" pin="S" pad="12"/>
<connect gate="-13" pin="S" pad="13"/>
<connect gate="-14" pin="S" pad="14"/>
<connect gate="-15" pin="S" pad="15"/>
<connect gate="-2" pin="S" pad="2"/>
<connect gate="-3" pin="S" pad="3"/>
<connect gate="-4" pin="S" pad="4"/>
<connect gate="-5" pin="S" pad="5"/>
<connect gate="-6" pin="S" pad="6"/>
<connect gate="-7" pin="S" pad="7"/>
<connect gate="-8" pin="S" pad="8"/>
<connect gate="-9" pin="S" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="H" package="DF13A-15P-1.25H">
<connects>
<connect gate="-1" pin="S" pad="1"/>
<connect gate="-10" pin="S" pad="10"/>
<connect gate="-11" pin="S" pad="11"/>
<connect gate="-12" pin="S" pad="12"/>
<connect gate="-13" pin="S" pad="13"/>
<connect gate="-14" pin="S" pad="14"/>
<connect gate="-15" pin="S" pad="15"/>
<connect gate="-2" pin="S" pad="2"/>
<connect gate="-3" pin="S" pad="3"/>
<connect gate="-4" pin="S" pad="4"/>
<connect gate="-5" pin="S" pad="5"/>
<connect gate="-6" pin="S" pad="6"/>
<connect gate="-7" pin="S" pad="7"/>
<connect gate="-8" pin="S" pad="8"/>
<connect gate="-9" pin="S" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="DF13-4P-1.25?">
<gates>
<gate name="-1" symbol="MV"/>
<gate name="-2" symbol="M"/>
<gate name="-3" symbol="M"/>
<gate name="-4" symbol="M"/>
</gates>
<devices>
<device name="H" package="DF13A-4P-1.25H">
<connects>
<connect gate="-1" pin="S" pad="1"/>
<connect gate="-2" pin="S" pad="2"/>
<connect gate="-3" pin="S" pad="3"/>
<connect gate="-4" pin="S" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="DSA" package="DF13-4P-1.25DSA">
<connects>
<connect gate="-1" pin="S" pad="1"/>
<connect gate="-2" pin="S" pad="2"/>
<connect gate="-3" pin="S" pad="3"/>
<connect gate="-4" pin="S" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="DF13-5P-1.25?">
<gates>
<gate name="-1" symbol="MV"/>
<gate name="-2" symbol="M"/>
<gate name="-3" symbol="M"/>
<gate name="-4" symbol="M"/>
<gate name="-5" symbol="M"/>
</gates>
<devices>
<device name="DSA" package="DF13-5P-1.25DSA">
<connects>
<connect gate="-1" pin="S" pad="1"/>
<connect gate="-2" pin="S" pad="2"/>
<connect gate="-3" pin="S" pad="3"/>
<connect gate="-4" pin="S" pad="4"/>
<connect gate="-5" pin="S" pad="5"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="H" package="DF13A-5P-1.25H">
<connects>
<connect gate="-1" pin="S" pad="1"/>
<connect gate="-2" pin="S" pad="2"/>
<connect gate="-3" pin="S" pad="3"/>
<connect gate="-4" pin="S" pad="4"/>
<connect gate="-5" pin="S" pad="5"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="DF13-6P-1.25?">
<gates>
<gate name="-1" symbol="MV"/>
<gate name="-2" symbol="M"/>
<gate name="-3" symbol="M"/>
<gate name="-4" symbol="M"/>
<gate name="-5" symbol="M"/>
<gate name="-6" symbol="M"/>
</gates>
<devices>
<device name="DSA" package="DF13-6P-1.25DSA">
<connects>
<connect gate="-1" pin="S" pad="1"/>
<connect gate="-2" pin="S" pad="2"/>
<connect gate="-3" pin="S" pad="3"/>
<connect gate="-4" pin="S" pad="4"/>
<connect gate="-5" pin="S" pad="5"/>
<connect gate="-6" pin="S" pad="6"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="H" package="DF13A-6P-1.25H">
<connects>
<connect gate="-1" pin="S" pad="1"/>
<connect gate="-2" pin="S" pad="2"/>
<connect gate="-3" pin="S" pad="3"/>
<connect gate="-4" pin="S" pad="4"/>
<connect gate="-5" pin="S" pad="5"/>
<connect gate="-6" pin="S" pad="6"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="HEADER_1X6_FTDI">
<gates>
<gate name="-GND" symbol="MV"/>
<gate name="-RTS" symbol="M"/>
<gate name="-+5V" symbol="M"/>
<gate name="-TX" symbol="M"/>
<gate name="-RX" symbol="M"/>
<gate name="-CTS" symbol="M"/>
</gates>
<devices>
<device name="LABELED" package="HEADER_1X06-FTDI">
<connects>
<connect gate="-+5V" pin="S" pad="+5V"/>
<connect gate="-CTS" pin="S" pad="CTS"/>
<connect gate="-GND" pin="S" pad="GND"/>
<connect gate="-RTS" pin="S" pad="RTS"/>
<connect gate="-RX" pin="S" pad="RX"/>
<connect gate="-TX" pin="S" pad="TX"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="" package="HEADER_1X06-SIP_LOCK">
<connects>
<connect gate="-+5V" pin="S" pad="3"/>
<connect gate="-CTS" pin="S" pad="6"/>
<connect gate="-GND" pin="S" pad="1"/>
<connect gate="-RTS" pin="S" pad="2"/>
<connect gate="-RX" pin="S" pad="4"/>
<connect gate="-TX" pin="S" pad="5"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MS5611-01BA">
<description>&lt;b&gt;MS5611-01BA&lt;/b&gt;
&lt;p&gt;The MS5611-01BA is a new generation of high resolution altimeter sensors from MEAS Switzerland with SPI 
and I
2
C bus interface. It is optimized for altimeters and  variometers with an altitude resolution of 10 cm. The 
sensor module includes a high linearity pressure sensor and an ultra low power 24 bit ?? ADC with internal 
factory calibrated coefficients. It provides a precise digital 24 Bit pressure and temperature value and different 
operation modes that allow the user to optimize for conversion speed and current consumption. A high 
resolution temperature output allows the implementation of an altimeter/thermometer function without any 
additional sensor. The MS5611-01BA can be interfaced to virtually any microcontroller. The communication 
protocol is simple, without the need of programming internal registers in the device. Small dimensions of only 
5.0 mm x 3.0 mm and a height of 1.7 mm allow for integration in mobile devices. This new sensor module 
generation is based on leading MEMS technology and latest benefits from  MEAS Switzerland proven 
experience and know-how in high volume manufacturing of altimeter modules, which have been widely used for 
over a decade. The sensing principle employed leads to very low hysteresis and high stability of both pressure 
and temperature signal.&lt;/p&gt;
&lt;ul&gt;
&lt;li&gt;High resolution module, 10 cm &lt;/li&gt;
&lt;li&gt;Fast conversion down to 1 ms &lt;/li&gt;
&lt;li&gt;Low power, 1 µA (standby &lt; 0.15 µA) &lt;/li&gt;
&lt;li&gt;QFN package 5.0 x 3.0 x 1.7 mm3&lt;/li&gt;
&lt;li&gt;Supply voltage 1.8 to 3.6 V &lt;/li&gt;
&lt;li&gt;Integrated digital pressure sensor (24 bit ?? ADC) &lt;/li&gt;
&lt;li&gt;Operating range: 10 to 1200 mbar, -40 to +85 °C &lt;/li&gt;
&lt;li&gt;I2C and SPI interface up to 20 MHz &lt;/li&gt;
&lt;li&gt;No external components (Internal oscillator) &lt;/li&gt;
&lt;li&gt;Excellent long term stability&lt;/li&gt;
&lt;/ul&gt;</description>
<gates>
<gate name="G$1" symbol="MS5611-01BA"/>
</gates>
<devices>
<device name="" package="MS5611-01BA">
<connects>
<connect gate="G$1" pin="CSB1" pad="4"/>
<connect gate="G$1" pin="CSB2" pad="5"/>
<connect gate="G$1" pin="GND" pad="3"/>
<connect gate="G$1" pin="PS" pad="2"/>
<connect gate="G$1" pin="SCLK" pad="8"/>
<connect gate="G$1" pin="SDI/SDA" pad="7"/>
<connect gate="G$1" pin="SDO" pad="6"/>
<connect gate="G$1" pin="VDD" pad="1"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET" value="http://www.meas-spec.com/downloads/MS5611-01BA01.pdf"/>
<attribute name="LINK" value="http://www.meas-spec.com/product/t_product.aspx?id=8503#"/>
<attribute name="MFGPN" value="MS5611-01BA"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="TRANSISTOR_PNP" prefix="Q">
<gates>
<gate name="G$1" symbol="PNP"/>
</gates>
<devices>
<device name="SMD" package="SOT23-3">
<connects>
<connect gate="G$1" pin="B" pad="1"/>
<connect gate="G$1" pin="C" pad="3"/>
<connect gate="G$1" pin="E" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="TO92" package="TO-92">
<connects>
<connect gate="G$1" pin="B" pad="2"/>
<connect gate="G$1" pin="C" pad="3"/>
<connect gate="G$1" pin="E" pad="1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="" package="SOT89">
<connects>
<connect gate="G$1" pin="B" pad="1"/>
<connect gate="G$1" pin="C" pad="2"/>
<connect gate="G$1" pin="E" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="TRANSISTOR_NPN" prefix="Q" uservalue="yes">
<description>&lt;b&gt;Transistor NPN&lt;/b&gt;
BJT configuration in SOT23 package. MMBT2222 is the common NPN we use. Double check BCE configuration again layout.</description>
<gates>
<gate name="G$1" symbol="NPN"/>
</gates>
<devices>
<device name="SOT23" package="SOT23">
<connects>
<connect gate="G$1" pin="B" pad="1"/>
<connect gate="G$1" pin="C" pad="3"/>
<connect gate="G$1" pin="E" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="SOT23-3" package="SOT23-3">
<connects>
<connect gate="G$1" pin="B" pad="1"/>
<connect gate="G$1" pin="C" pad="3"/>
<connect gate="G$1" pin="E" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="TO92" package="TO-92">
<connects>
<connect gate="G$1" pin="B" pad="2"/>
<connect gate="G$1" pin="C" pad="3"/>
<connect gate="G$1" pin="E" pad="1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="&quot;" package="SOT223">
<connects>
<connect gate="G$1" pin="B" pad="1"/>
<connect gate="G$1" pin="C" pad="2"/>
<connect gate="G$1" pin="E" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="SOT89" package="SOT89">
<connects>
<connect gate="G$1" pin="B" pad="1"/>
<connect gate="G$1" pin="C" pad="2"/>
<connect gate="G$1" pin="E" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="TO-92-AMMO" package="TO-92-AMMO">
<connects>
<connect gate="G$1" pin="B" pad="2"/>
<connect gate="G$1" pin="C" pad="3"/>
<connect gate="G$1" pin="E" pad="1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="V_REG_LD1117VXX">
<description>LD1117VXX voltage regulator. We carry the 3.3V version (COM-00526) in TO-220 package.</description>
<gates>
<gate name="G$1" symbol="78XX"/>
</gates>
<devices>
<device name="_TO220_H" package="78XXL">
<connects>
<connect gate="G$1" pin="GND" pad="IN"/>
<connect gate="G$1" pin="IN" pad="OUT"/>
<connect gate="G$1" pin="OUT" pad="GND"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_TO220_V" package="TO220">
<connects>
<connect gate="G$1" pin="GND" pad="2"/>
<connect gate="G$1" pin="IN" pad="1"/>
<connect gate="G$1" pin="OUT" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MT9V034">
<gates>
<gate name="G$1" symbol="MT9V032"/>
</gates>
<devices>
<device name="" package="CLCC-48">
<connects>
<connect gate="G$1" pin="!RESET" pad="32"/>
<connect gate="G$1" pin="AGND@34" pad="34"/>
<connect gate="G$1" pin="AGND@38" pad="38"/>
<connect gate="G$1" pin="BYPASS_CLKIN_N" pad="8"/>
<connect gate="G$1" pin="BYPASS_CLKIN_P" pad="9"/>
<connect gate="G$1" pin="DGND@13" pad="13"/>
<connect gate="G$1" pin="DGND@48" pad="48"/>
<connect gate="G$1" pin="DOUT0" pad="45"/>
<connect gate="G$1" pin="DOUT1" pad="44"/>
<connect gate="G$1" pin="DOUT2" pad="43"/>
<connect gate="G$1" pin="DOUT3" pad="42"/>
<connect gate="G$1" pin="DOUT4" pad="41"/>
<connect gate="G$1" pin="DOUT5" pad="15"/>
<connect gate="G$1" pin="DOUT6" pad="16"/>
<connect gate="G$1" pin="DOUT7" pad="17"/>
<connect gate="G$1" pin="DOUT8" pad="18"/>
<connect gate="G$1" pin="DOUT9" pad="19"/>
<connect gate="G$1" pin="EXPOSURE" pad="23"/>
<connect gate="G$1" pin="FRAME_VALID" pad="21"/>
<connect gate="G$1" pin="LED_OUT" pad="27"/>
<connect gate="G$1" pin="LINE_VALID" pad="20"/>
<connect gate="G$1" pin="LVDS_GND@12" pad="12"/>
<connect gate="G$1" pin="LVDS_GND@7" pad="7"/>
<connect gate="G$1" pin="NC@36" pad="36"/>
<connect gate="G$1" pin="NC@37" pad="37"/>
<connect gate="G$1" pin="OE" pad="28"/>
<connect gate="G$1" pin="PIXCLK" pad="46"/>
<connect gate="G$1" pin="RSVD" pad="29"/>
<connect gate="G$1" pin="SCLK" pad="25"/>
<connect gate="G$1" pin="SCTRL_ADR0" pad="30"/>
<connect gate="G$1" pin="SCTRL_ADR1" pad="31"/>
<connect gate="G$1" pin="SDATA" pad="24"/>
<connect gate="G$1" pin="SER_DATAIN_N" pad="10"/>
<connect gate="G$1" pin="SER_DATAIN_P" pad="11"/>
<connect gate="G$1" pin="SER_DATAOUT_N" pad="4"/>
<connect gate="G$1" pin="SER_DATAOUT_P" pad="5"/>
<connect gate="G$1" pin="SHFT_CLKOUT_N" pad="2"/>
<connect gate="G$1" pin="SHFT_CLKOUT_P" pad="3"/>
<connect gate="G$1" pin="STANDBY" pad="33"/>
<connect gate="G$1" pin="STFRM_OUT" pad="26"/>
<connect gate="G$1" pin="STLN_OUT" pad="22"/>
<connect gate="G$1" pin="SYSCLK" pad="47"/>
<connect gate="G$1" pin="VAA@35" pad="35"/>
<connect gate="G$1" pin="VAA@39" pad="39"/>
<connect gate="G$1" pin="VAA_PIX" pad="40"/>
<connect gate="G$1" pin="VDD@1" pad="1"/>
<connect gate="G$1" pin="VDD@14" pad="14"/>
<connect gate="G$1" pin="VDD_LVDS" pad="6"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="STM32F4X7VX" prefix="IC">
<description>STM32F4X7VX 100 pin LQFP

STM32F407VE - 512 KB flash, no crypto
STM32F407VG - 1 MB flash, no crypto
STM32F417VE - 512 KB flash, with crypto
STM32F417VG - 1 MB flash, with crypto</description>
<gates>
<gate name="PORTA_L" symbol="PORT_A_L-1"/>
<gate name="PORTA_H" symbol="PORT_A_H-1"/>
<gate name="PORTB_L" symbol="PORT_B_L-1"/>
<gate name="PORTB_H" symbol="PORT_B_H-1"/>
<gate name="PORTC_L" symbol="PORT_C_L-1"/>
<gate name="PORTC_H" symbol="PORT_C_H-1"/>
<gate name="PORTD_L" symbol="PORT_D_L"/>
<gate name="PORTD_H" symbol="PORT_D_H"/>
<gate name="PORTE_L" symbol="PORT_E_L"/>
<gate name="PORTE_H" symbol="PORT_E_H"/>
<gate name="OSC" symbol="OSC"/>
<gate name="RESET" symbol="BOOT_RST-1"/>
<gate name="BAT" symbol="STM32F4X_BAT_AN_L"/>
<gate name="G$2" symbol="STM32F4X_VCC_VSS_L"/>
</gates>
<devices>
<device name="" package="TQFP100">
<connects>
<connect gate="BAT" pin="VBAT" pad="6"/>
<connect gate="BAT" pin="VDDA" pad="22"/>
<connect gate="BAT" pin="VREF+" pad="21"/>
<connect gate="BAT" pin="VSSA" pad="20"/>
<connect gate="G$2" pin="VCAP_1" pad="49"/>
<connect gate="G$2" pin="VCAP_2" pad="73"/>
<connect gate="G$2" pin="VDD" pad="11 19 28 50 75 100"/>
<connect gate="G$2" pin="VSS" pad="10 27 74 99"/>
<connect gate="OSC" pin="OSC_IN" pad="12"/>
<connect gate="OSC" pin="OSC_OUT" pad="13"/>
<connect gate="PORTA_H" pin="PA10" pad="69"/>
<connect gate="PORTA_H" pin="PA11" pad="70"/>
<connect gate="PORTA_H" pin="PA12" pad="71"/>
<connect gate="PORTA_H" pin="PA13" pad="72"/>
<connect gate="PORTA_H" pin="PA14" pad="76"/>
<connect gate="PORTA_H" pin="PA15" pad="77"/>
<connect gate="PORTA_H" pin="PA8" pad="67"/>
<connect gate="PORTA_H" pin="PA9" pad="68"/>
<connect gate="PORTA_L" pin="PA0" pad="23"/>
<connect gate="PORTA_L" pin="PA1" pad="24"/>
<connect gate="PORTA_L" pin="PA2" pad="25"/>
<connect gate="PORTA_L" pin="PA3" pad="26"/>
<connect gate="PORTA_L" pin="PA4" pad="29"/>
<connect gate="PORTA_L" pin="PA5" pad="30"/>
<connect gate="PORTA_L" pin="PA6" pad="31"/>
<connect gate="PORTA_L" pin="PA7" pad="32"/>
<connect gate="PORTB_H" pin="PB10" pad="47"/>
<connect gate="PORTB_H" pin="PB11" pad="48"/>
<connect gate="PORTB_H" pin="PB12" pad="51"/>
<connect gate="PORTB_H" pin="PB13" pad="52"/>
<connect gate="PORTB_H" pin="PB14" pad="53"/>
<connect gate="PORTB_H" pin="PB15" pad="54"/>
<connect gate="PORTB_H" pin="PB8" pad="95"/>
<connect gate="PORTB_H" pin="PB9" pad="96"/>
<connect gate="PORTB_L" pin="PB0" pad="35"/>
<connect gate="PORTB_L" pin="PB1" pad="36"/>
<connect gate="PORTB_L" pin="PB2" pad="37"/>
<connect gate="PORTB_L" pin="PB3" pad="89"/>
<connect gate="PORTB_L" pin="PB4" pad="90"/>
<connect gate="PORTB_L" pin="PB5" pad="91"/>
<connect gate="PORTB_L" pin="PB6" pad="92"/>
<connect gate="PORTB_L" pin="PB7" pad="93"/>
<connect gate="PORTC_H" pin="PC10" pad="78"/>
<connect gate="PORTC_H" pin="PC11" pad="79"/>
<connect gate="PORTC_H" pin="PC12" pad="80"/>
<connect gate="PORTC_H" pin="PC13" pad="7"/>
<connect gate="PORTC_H" pin="PC14" pad="8"/>
<connect gate="PORTC_H" pin="PC15" pad="9"/>
<connect gate="PORTC_H" pin="PC8" pad="65"/>
<connect gate="PORTC_H" pin="PC9" pad="66"/>
<connect gate="PORTC_L" pin="PC0" pad="15"/>
<connect gate="PORTC_L" pin="PC1" pad="16"/>
<connect gate="PORTC_L" pin="PC2" pad="17"/>
<connect gate="PORTC_L" pin="PC3" pad="18"/>
<connect gate="PORTC_L" pin="PC4" pad="33"/>
<connect gate="PORTC_L" pin="PC5" pad="34"/>
<connect gate="PORTC_L" pin="PC6" pad="63"/>
<connect gate="PORTC_L" pin="PC7" pad="64"/>
<connect gate="PORTD_H" pin="PD10" pad="57"/>
<connect gate="PORTD_H" pin="PD11" pad="58"/>
<connect gate="PORTD_H" pin="PD12" pad="59"/>
<connect gate="PORTD_H" pin="PD13" pad="60"/>
<connect gate="PORTD_H" pin="PD14" pad="61"/>
<connect gate="PORTD_H" pin="PD15" pad="62"/>
<connect gate="PORTD_H" pin="PD8" pad="55"/>
<connect gate="PORTD_H" pin="PD9" pad="56"/>
<connect gate="PORTD_L" pin="PD0" pad="81"/>
<connect gate="PORTD_L" pin="PD1" pad="82"/>
<connect gate="PORTD_L" pin="PD2" pad="83"/>
<connect gate="PORTD_L" pin="PD3" pad="84"/>
<connect gate="PORTD_L" pin="PD4" pad="85"/>
<connect gate="PORTD_L" pin="PD5" pad="86"/>
<connect gate="PORTD_L" pin="PD6" pad="87"/>
<connect gate="PORTD_L" pin="PD7" pad="88"/>
<connect gate="PORTE_H" pin="PE10" pad="41"/>
<connect gate="PORTE_H" pin="PE11" pad="42"/>
<connect gate="PORTE_H" pin="PE12" pad="43"/>
<connect gate="PORTE_H" pin="PE13" pad="44"/>
<connect gate="PORTE_H" pin="PE14" pad="45"/>
<connect gate="PORTE_H" pin="PE15" pad="46"/>
<connect gate="PORTE_H" pin="PE8" pad="39"/>
<connect gate="PORTE_H" pin="PE9" pad="40"/>
<connect gate="PORTE_L" pin="PE0" pad="97"/>
<connect gate="PORTE_L" pin="PE1" pad="98"/>
<connect gate="PORTE_L" pin="PE2" pad="1"/>
<connect gate="PORTE_L" pin="PE3" pad="2"/>
<connect gate="PORTE_L" pin="PE4" pad="3"/>
<connect gate="PORTE_L" pin="PE5" pad="4"/>
<connect gate="PORTE_L" pin="PE6" pad="5"/>
<connect gate="PORTE_L" pin="PE7" pad="38"/>
<connect gate="RESET" pin="BOOT0" pad="94"/>
<connect gate="RESET" pin="NRST" pad="14"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MAXSONAR">
<gates>
<gate name="-GND" symbol="MV"/>
<gate name="-VDD" symbol="M"/>
<gate name="-TX" symbol="M"/>
<gate name="-RX" symbol="M"/>
<gate name="-AN" symbol="M"/>
<gate name="-PW" symbol="M"/>
<gate name="-BW" symbol="M"/>
</gates>
<devices>
<device name="" package="MAXSONAR">
<connects>
<connect gate="-AN" pin="S" pad="AN"/>
<connect gate="-BW" pin="S" pad="BW"/>
<connect gate="-GND" pin="S" pad="GND"/>
<connect gate="-PW" pin="S" pad="PW"/>
<connect gate="-RX" pin="S" pad="RX"/>
<connect gate="-TX" pin="S" pad="TX"/>
<connect gate="-VDD" pin="S" pad="VDD"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MPU-6000">
<description>&lt;b&gt;Invensense MPU-6000: 3-axis gyro, 3-axis accel &amp; 9-axis MotionFusion&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;
The MPU-60X0 Motion Processing Unit (MPU?) is the world?s first motion processing solution with 
integrated 9-axis sensor fusion for handset and tablet applications, game controllers, motion pointer remote 
controls, and other consumer devices. The MPU-60X0 has an embedded 3-axis MEMS gyroscope, 3-axis 
MEMS accelerometer and Digital Motion Processor? (DMP) hardware accelerator engine with an auxiliary 
I
2
C port that interfaces to third party digital sensors, such as magnetometers. Interfacing with a 3-axis 
magnetometer delivers a complete 9-axis sensor fusion output to the MPU?s primary I
2
C or SPI port. (SPI is 
available on MPU-6000 only). This combines acceleration and rotational motion plus heading information into 
a single data stream for the application</description>
<gates>
<gate name="G$1" symbol="MPU-6000"/>
</gates>
<devices>
<device name="" package="QFN-24">
<connects>
<connect gate="G$1" pin="/CS" pad="8"/>
<connect gate="G$1" pin="AD0/SDO" pad="9"/>
<connect gate="G$1" pin="AUX_CL" pad="7"/>
<connect gate="G$1" pin="AUX_DA" pad="6"/>
<connect gate="G$1" pin="CLKIN" pad="1"/>
<connect gate="G$1" pin="CLKOUT" pad="22"/>
<connect gate="G$1" pin="CPOUT" pad="20"/>
<connect gate="G$1" pin="FSYNC" pad="11"/>
<connect gate="G$1" pin="GND" pad="18"/>
<connect gate="G$1" pin="INT" pad="12"/>
<connect gate="G$1" pin="NC1" pad="2"/>
<connect gate="G$1" pin="NC2" pad="3"/>
<connect gate="G$1" pin="NC3" pad="4"/>
<connect gate="G$1" pin="NC4" pad="5"/>
<connect gate="G$1" pin="NC5" pad="14"/>
<connect gate="G$1" pin="NC6" pad="15"/>
<connect gate="G$1" pin="NC7" pad="16"/>
<connect gate="G$1" pin="NC8" pad="17"/>
<connect gate="G$1" pin="REGOUT" pad="10"/>
<connect gate="G$1" pin="RESV1" pad="19"/>
<connect gate="G$1" pin="RESV2" pad="21"/>
<connect gate="G$1" pin="SCL/SCLK" pad="23"/>
<connect gate="G$1" pin="SDA/SDI" pad="24"/>
<connect gate="G$1" pin="VDD" pad="13"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET" value="http://invensense.com/mems/gyro/documents/PS-MPU-6000A-00_v1.0.pdf"/>
<attribute name="LINK" value="http://invensense.com/mems/gyro/mpu6000.html"/>
<attribute name="MFGPN" value="MPU-6000"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MAX4634">
<gates>
<gate name="G$1" symbol="MAX4634EUB+"/>
</gates>
<devices>
<device name="" package="TI-DGS">
<connects>
<connect gate="G$1" pin="A0" pad="1"/>
<connect gate="G$1" pin="A1" pad="10"/>
<connect gate="G$1" pin="COM" pad="8"/>
<connect gate="G$1" pin="EN" pad="5"/>
<connect gate="G$1" pin="GND" pad="3"/>
<connect gate="G$1" pin="NO1" pad="2"/>
<connect gate="G$1" pin="NO2" pad="9"/>
<connect gate="G$1" pin="NO3" pad="4"/>
<connect gate="G$1" pin="NO4" pad="7"/>
<connect gate="G$1" pin="V+" pad="6"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="QUALIFIED_1_OVERO">
<gates>
<gate name="G$1" symbol="QUALIFIED_1_OVERO"/>
</gates>
<devices>
<device name="" package="QUALIFIED_1_OVERO">
<connects>
<connect gate="G$1" pin="ADCIN2" pad="ADCIN2"/>
<connect gate="G$1" pin="ADCIN3" pad="ADCIN3"/>
<connect gate="G$1" pin="ADCIN4" pad="ADCIN4"/>
<connect gate="G$1" pin="ADCIN5" pad="ADCIN5"/>
<connect gate="G$1" pin="ADCIN6" pad="ADCIN6"/>
<connect gate="G$1" pin="ADCIN7" pad="ADCIN7"/>
<connect gate="G$1" pin="AGND" pad="AGND"/>
<connect gate="G$1" pin="AUXLF" pad="AUXLF"/>
<connect gate="G$1" pin="AUXRF" pad="AUXRF"/>
<connect gate="G$1" pin="EM_A1" pad="EM_A1"/>
<connect gate="G$1" pin="EM_A10" pad="EM_A10"/>
<connect gate="G$1" pin="EM_A2" pad="EM_A2"/>
<connect gate="G$1" pin="EM_A3" pad="EM_A3"/>
<connect gate="G$1" pin="EM_A4" pad="EM_A4"/>
<connect gate="G$1" pin="EM_A5" pad="EM_A5"/>
<connect gate="G$1" pin="EM_A6" pad="EM_A6"/>
<connect gate="G$1" pin="EM_A7" pad="EM_A7"/>
<connect gate="G$1" pin="EM_A8" pad="EM_A8"/>
<connect gate="G$1" pin="EM_A9" pad="EM_A9"/>
<connect gate="G$1" pin="EM_CLK" pad="EM_CLK"/>
<connect gate="G$1" pin="EM_D0" pad="EM_D0"/>
<connect gate="G$1" pin="EM_D1" pad="EM_D1"/>
<connect gate="G$1" pin="EM_D10" pad="EM_D10"/>
<connect gate="G$1" pin="EM_D11" pad="EM_D11"/>
<connect gate="G$1" pin="EM_D12" pad="EM_D12"/>
<connect gate="G$1" pin="EM_D13" pad="EM_D13"/>
<connect gate="G$1" pin="EM_D14" pad="EM_D14"/>
<connect gate="G$1" pin="EM_D15" pad="EM_D15"/>
<connect gate="G$1" pin="EM_D2" pad="EM_D2"/>
<connect gate="G$1" pin="EM_D3" pad="EM_D3"/>
<connect gate="G$1" pin="EM_D4" pad="EM_D4"/>
<connect gate="G$1" pin="EM_D5" pad="EM_D5"/>
<connect gate="G$1" pin="EM_D6" pad="EM_D6"/>
<connect gate="G$1" pin="EM_D7" pad="EM_D7"/>
<connect gate="G$1" pin="EM_D8" pad="EM_D8"/>
<connect gate="G$1" pin="EM_D9" pad="EM_D9"/>
<connect gate="G$1" pin="EM_NADV_ALE" pad="EM_NADV_ALE"/>
<connect gate="G$1" pin="EM_NBE0" pad="EM_NBE0"/>
<connect gate="G$1" pin="EM_NBE1" pad="EM_NBE1"/>
<connect gate="G$1" pin="EM_NCS0" pad="EM_NCS0"/>
<connect gate="G$1" pin="EM_NCS1" pad="EM_NCS1"/>
<connect gate="G$1" pin="EM_NCS4" pad="EM_NCS4"/>
<connect gate="G$1" pin="EM_NCS5_ETH0" pad="EM_NCS5_ETH0"/>
<connect gate="G$1" pin="EM_NCS6" pad="EM_NCS6"/>
<connect gate="G$1" pin="EM_NOE" pad="EM_NOE"/>
<connect gate="G$1" pin="EM_NWE" pad="EM_NWE"/>
<connect gate="G$1" pin="EM_NWP" pad="EM_NWP"/>
<connect gate="G$1" pin="EM_WAIT0" pad="EM_WAIT0"/>
<connect gate="G$1" pin="GND" pad="GND"/>
<connect gate="G$1" pin="GND@33" pad="GND@33"/>
<connect gate="G$1" pin="GND@56" pad="GND@56"/>
<connect gate="G$1" pin="GND@70" pad="GND@70"/>
<connect gate="G$1" pin="GPIO0_WAKEUP" pad="GPIO0_WAKEUP"/>
<connect gate="G$1" pin="GPIO114_SPI1_NIRQ" pad="GPIO114_SPI1_NIRQ"/>
<connect gate="G$1" pin="GPIO127_TS_IRQ" pad="GPIO127_TS_IRQ"/>
<connect gate="G$1" pin="GPIO128_GPS_PPS" pad="GPIO128_GPS_PPS"/>
<connect gate="G$1" pin="GPIO12_MMC3_CLK" pad="GPIO12_MMC3_CLK"/>
<connect gate="G$1" pin="GPIO13_MMC3_CMD" pad="GPIO13_MMC3_CMD"/>
<connect gate="G$1" pin="GPIO144_GPT9_PWM" pad="GPIO144_GPT9_PWM"/>
<connect gate="G$1" pin="GPIO145_GPT10_PWM" pad="GPIO145_GPT10_PWM"/>
<connect gate="G$1" pin="GPIO146_GPT11_PWM" pad="GPIO146_GPT11_PWM"/>
<connect gate="G$1" pin="GPIO147_GPT8_PWM" pad="GPIO147_GPT8_PWM"/>
<connect gate="G$1" pin="GPIO148_TXD1" pad="GPIO148_TXD1"/>
<connect gate="G$1" pin="GPIO149_MMC3_CD" pad="GPIO149_MMC3_CD"/>
<connect gate="G$1" pin="GPIO14_MMC3_DAT4" pad="GPIO14_MMC3_DAT4"/>
<connect gate="G$1" pin="GPIO150_MMC3_WP" pad="GPIO150_MMC3_WP"/>
<connect gate="G$1" pin="GPIO151_RXD1" pad="GPIO151_RXD1"/>
<connect gate="G$1" pin="GPIO163_IR_CTS3" pad="GPIO163_IR_CTS3"/>
<connect gate="G$1" pin="GPIO165_IR_RXD3" pad="GPIO165_IR_RXD3"/>
<connect gate="G$1" pin="GPIO166_IR_TXD3" pad="GPIO166_IR_TXD3"/>
<connect gate="G$1" pin="GPIO168_USBH_CPEN" pad="GPIO168_USBH_CPEN"/>
<connect gate="G$1" pin="GPIO170_HDQ_1WIRE" pad="GPIO170_HDQ_1WIRE"/>
<connect gate="G$1" pin="GPIO171_SPI1_CLK" pad="GPIO171_SPI1_CLK"/>
<connect gate="G$1" pin="GPIO172_SPI1_MOSI" pad="GPIO172_SPI1_MOSI"/>
<connect gate="G$1" pin="GPIO173_SPI1_MISO" pad="GPIO173_SPI1_MISO"/>
<connect gate="G$1" pin="GPIO174_SPI1_CS0" pad="GPIO174_SPI1_CS0"/>
<connect gate="G$1" pin="GPIO175_SPI1_CS1" pad="GPIO175_SPI1_CS1"/>
<connect gate="G$1" pin="GPIO176_ETH0_IRQ" pad="GPIO176_ETH0_IRQ"/>
<connect gate="G$1" pin="GPIO17_MMC3_D3" pad="GPIO17_MMC3_D3"/>
<connect gate="G$1" pin="GPIO184_I2C3_SCL" pad="GPIO184_I2C3_SCL"/>
<connect gate="G$1" pin="GPIO185_I2C3_SDA" pad="GPIO185_I2C3_SDA"/>
<connect gate="G$1" pin="GPIO18_MMC3_D0" pad="GPIO18_MMC3_D0"/>
<connect gate="G$1" pin="GPIO19_MMC3_D1" pad="GPIO19_MMC3_D1"/>
<connect gate="G$1" pin="GPIO20_MMC3_D2" pad="GPIO20_MMC3_D2"/>
<connect gate="G$1" pin="GPIO21_MMC3_DAT7" pad="GPIO21_MMC3_DAT7"/>
<connect gate="G$1" pin="GPIO22_MMC3_DAT6" pad="GPIO22_MMC3_DAT6"/>
<connect gate="G$1" pin="GPIO23_MMC3_DAT5" pad="GPIO23_MMC3_DAT5"/>
<connect gate="G$1" pin="GPIO64_ETH0_NRESET" pad="GPIO64_ETH0_NRESET"/>
<connect gate="G$1" pin="GPIO65_ETH1_IRQ1" pad="GPIO65_ETH1_IRQ1"/>
<connect gate="G$1" pin="GPIO66_L_PCLK" pad="GPIO66_L_PCLK"/>
<connect gate="G$1" pin="GPIO67_L_LCLK" pad="GPIO67_L_LCLK"/>
<connect gate="G$1" pin="GPIO68_L_FCLK" pad="GPIO68_L_FCLK"/>
<connect gate="G$1" pin="GPIO69_L_BIAS" pad="GPIO69_L_BIAS"/>
<connect gate="G$1" pin="GPIO70_L_DD00" pad="GPIO70_L_DD00"/>
<connect gate="G$1" pin="GPIO71_L_DD01" pad="GPIO71_L_DD01"/>
<connect gate="G$1" pin="GPIO72_L_DD02" pad="GPIO72_L_DD02"/>
<connect gate="G$1" pin="GPIO73_L_DD03" pad="GPIO73_L_DD03"/>
<connect gate="G$1" pin="GPIO74_L_DD04" pad="GPIO74_L_DD04"/>
<connect gate="G$1" pin="GPIO75_L_DD05" pad="GPIO75_L_DD05"/>
<connect gate="G$1" pin="GPIO76_L_DD06" pad="GPIO76_L_DD06"/>
<connect gate="G$1" pin="GPIO77_L_DD07" pad="GPIO77_L_DD07"/>
<connect gate="G$1" pin="GPIO78_L_DD08" pad="GPIO78_L_DD08"/>
<connect gate="G$1" pin="GPIO79_L_DD09" pad="GPIO79_L_DD09"/>
<connect gate="G$1" pin="GPIO80_L_DD10" pad="GPIO80_L_DD10"/>
<connect gate="G$1" pin="GPIO81_L_DD11" pad="GPIO81_L_DD11"/>
<connect gate="G$1" pin="GPIO82_L_DD12" pad="GPIO82_L_DD12"/>
<connect gate="G$1" pin="GPIO83_L_DD13" pad="GPIO83_L_DD13"/>
<connect gate="G$1" pin="GPIO84_L_DD14" pad="GPIO84_L_DD14"/>
<connect gate="G$1" pin="GPIO85_L_DD15" pad="GPIO85_L_DD15"/>
<connect gate="G$1" pin="GPIO86_L_DD16" pad="GPIO86_L_DD16"/>
<connect gate="G$1" pin="GPIO87_L_DD17" pad="GPIO87_L_DD17"/>
<connect gate="G$1" pin="GPIO88_L_DD18" pad="GPIO88_L_DD18"/>
<connect gate="G$1" pin="GPIO89_L_DD19" pad="GPIO89_L_DD19"/>
<connect gate="G$1" pin="GPIO90_L_DD20" pad="GPIO90_L_DD20"/>
<connect gate="G$1" pin="GPIO91_L_DD21" pad="GPIO91_L_DD21"/>
<connect gate="G$1" pin="GPIO92_L_DD22" pad="GPIO92_L_DD22"/>
<connect gate="G$1" pin="GPIO93_L_DD23" pad="GPIO93_L_DD23"/>
<connect gate="G$1" pin="HSOLF" pad="HSOLF"/>
<connect gate="G$1" pin="HSORF" pad="HSORF"/>
<connect gate="G$1" pin="MIC_MAIN_MF" pad="MIC_MAIN_MF"/>
<connect gate="G$1" pin="MIC_SUB_MF" pad="MIC_SUB_MF"/>
<connect gate="G$1" pin="NC@62" pad="NC@62"/>
<connect gate="G$1" pin="NC@63" pad="NC@63"/>
<connect gate="G$1" pin="N_MANUAL_RESET" pad="N_MANUAL_RESET"/>
<connect gate="G$1" pin="POWERON" pad="POWERON"/>
<connect gate="G$1" pin="PWM0" pad="PWM0"/>
<connect gate="G$1" pin="PWM1" pad="PWM1"/>
<connect gate="G$1" pin="SYSEN" pad="SYSEN"/>
<connect gate="G$1" pin="USBH_DM" pad="USBH_DM"/>
<connect gate="G$1" pin="USBH_DP" pad="USBH_DP"/>
<connect gate="G$1" pin="USBH_VBUS" pad="USBH_VBUS"/>
<connect gate="G$1" pin="USBOTG_DM" pad="USBOTG_DM"/>
<connect gate="G$1" pin="USBOTG_DP" pad="USBOTG_DP"/>
<connect gate="G$1" pin="USBOTG_ID" pad="USBOTG_ID"/>
<connect gate="G$1" pin="USBOTG_VBUS" pad="USBOTG_VBUS"/>
<connect gate="G$1" pin="VBACKUP" pad="VBACKUP"/>
<connect gate="G$1" pin="VSYSTEM@1" pad="VSYSTEM@1"/>
<connect gate="G$1" pin="VSYSTEM@2" pad="VSYSTEM@2"/>
<connect gate="G$1" pin="VSYSTEM@66" pad="VSYSTEM@66"/>
<connect gate="G$1" pin="VSYSTEM@67" pad="VSYSTEM@67"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="JST-PH-08">
<gates>
<gate name="-1" symbol="MV"/>
<gate name="-2" symbol="M"/>
<gate name="-3" symbol="M"/>
<gate name="-4" symbol="M"/>
<gate name="-5" symbol="M"/>
<gate name="-6" symbol="M"/>
<gate name="-7" symbol="M"/>
<gate name="-8" symbol="M"/>
</gates>
<devices>
<device name="" package="B8B-PH-K-S">
<connects>
<connect gate="-1" pin="S" pad="1"/>
<connect gate="-2" pin="S" pad="2"/>
<connect gate="-3" pin="S" pad="3"/>
<connect gate="-4" pin="S" pad="4"/>
<connect gate="-5" pin="S" pad="5"/>
<connect gate="-6" pin="S" pad="6"/>
<connect gate="-7" pin="S" pad="7"/>
<connect gate="-8" pin="S" pad="8"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="JST-SH-12">
<gates>
<gate name="-1" symbol="MV"/>
<gate name="-2" symbol="M"/>
<gate name="-3" symbol="M"/>
<gate name="-4" symbol="M"/>
<gate name="-5" symbol="M"/>
<gate name="-6" symbol="M"/>
<gate name="-7" symbol="M"/>
<gate name="-8" symbol="M"/>
<gate name="-9" symbol="M"/>
<gate name="-10" symbol="M"/>
<gate name="-11" symbol="M"/>
<gate name="-12" symbol="M"/>
</gates>
<devices>
<device name="BM" package="BM12B-SRSS-TB">
<connects>
<connect gate="-1" pin="S" pad="1"/>
<connect gate="-10" pin="S" pad="10"/>
<connect gate="-11" pin="S" pad="11"/>
<connect gate="-12" pin="S" pad="12"/>
<connect gate="-2" pin="S" pad="2"/>
<connect gate="-3" pin="S" pad="3"/>
<connect gate="-4" pin="S" pad="4"/>
<connect gate="-5" pin="S" pad="6"/>
<connect gate="-6" pin="S" pad="7"/>
<connect gate="-7" pin="S" pad="5"/>
<connect gate="-8" pin="S" pad="8"/>
<connect gate="-9" pin="S" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="" package="SM12B-SRSS-TB">
<connects>
<connect gate="-1" pin="S" pad="1"/>
<connect gate="-10" pin="S" pad="10"/>
<connect gate="-11" pin="S" pad="11"/>
<connect gate="-12" pin="S" pad="12"/>
<connect gate="-2" pin="S" pad="2"/>
<connect gate="-3" pin="S" pad="3"/>
<connect gate="-4" pin="S" pad="4"/>
<connect gate="-5" pin="S" pad="5"/>
<connect gate="-6" pin="S" pad="6"/>
<connect gate="-7" pin="S" pad="7"/>
<connect gate="-8" pin="S" pad="8"/>
<connect gate="-9" pin="S" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="HEADER_2X4">
<gates>
<gate name="-1" symbol="MV"/>
<gate name="-2" symbol="M"/>
<gate name="-3" symbol="M"/>
<gate name="-4" symbol="M"/>
<gate name="-5" symbol="M"/>
<gate name="-6" symbol="M"/>
<gate name="-7" symbol="M"/>
<gate name="-8" symbol="M"/>
</gates>
<devices>
<device name="TH" package="HEADER_2MM_2X4_TH">
<connects>
<connect gate="-1" pin="S" pad="1"/>
<connect gate="-2" pin="S" pad="2"/>
<connect gate="-3" pin="S" pad="3"/>
<connect gate="-4" pin="S" pad="4"/>
<connect gate="-5" pin="S" pad="5"/>
<connect gate="-6" pin="S" pad="6"/>
<connect gate="-7" pin="S" pad="7"/>
<connect gate="-8" pin="S" pad="8"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="TH_REV" package="HEADER_2MM_2X4_TH_REVERSE">
<connects>
<connect gate="-1" pin="S" pad="1"/>
<connect gate="-2" pin="S" pad="2"/>
<connect gate="-3" pin="S" pad="3"/>
<connect gate="-4" pin="S" pad="4"/>
<connect gate="-5" pin="S" pad="5"/>
<connect gate="-6" pin="S" pad="6"/>
<connect gate="-7" pin="S" pad="7"/>
<connect gate="-8" pin="S" pad="8"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="DF13-7P-1.25?">
<gates>
<gate name="-1" symbol="MV"/>
<gate name="-2" symbol="M"/>
<gate name="-3" symbol="M"/>
<gate name="-4" symbol="M"/>
<gate name="-5" symbol="M"/>
<gate name="-6" symbol="M"/>
<gate name="-7" symbol="M"/>
</gates>
<devices>
<device name="H" package="DF13A-7P-1.25H">
<connects>
<connect gate="-1" pin="S" pad="1"/>
<connect gate="-2" pin="S" pad="2"/>
<connect gate="-3" pin="S" pad="3"/>
<connect gate="-4" pin="S" pad="4"/>
<connect gate="-5" pin="S" pad="5"/>
<connect gate="-6" pin="S" pad="6"/>
<connect gate="-7" pin="S" pad="7"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="DSA" package="DF13-7P-1.25DSA">
<connects>
<connect gate="-1" pin="S" pad="1"/>
<connect gate="-2" pin="S" pad="2"/>
<connect gate="-3" pin="S" pad="3"/>
<connect gate="-4" pin="S" pad="4"/>
<connect gate="-5" pin="S" pad="5"/>
<connect gate="-6" pin="S" pad="6"/>
<connect gate="-7" pin="S" pad="7"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="3DROBOTICS_2X6_EXPANSION" prefix="X">
<description>&lt;b&gt;1.27mm SINGLE ROW FEMALE SOCKET&lt;/b&gt;&lt;p&gt;
Source: http://www.leotronics.co.uk/Conexcon/Data%20Sheets/sec.%20A/1296ing.pdf</description>
<gates>
<gate name="-1" symbol="3DROBOTICS_FVAL"/>
<gate name="-2" symbol="3DROBOTICS_FVAL"/>
<gate name="-3" symbol="3DROBOTICS_F"/>
<gate name="-4" symbol="3DROBOTICS_F"/>
<gate name="-5" symbol="3DROBOTICS_F"/>
<gate name="-6" symbol="3DROBOTICS_F"/>
<gate name="-7" symbol="3DROBOTICS_F"/>
<gate name="-8" symbol="3DROBOTICS_F"/>
<gate name="-9" symbol="3DROBOTICS_F"/>
<gate name="-10" symbol="3DROBOTICS_F"/>
<gate name="-11" symbol="3DROBOTICS_F"/>
<gate name="-12" symbol="3DROBOTICS_F"/>
</gates>
<devices>
<device name="" package="3DROBOTICS_1296-12">
<connects>
<connect gate="-1" pin="B" pad="1"/>
<connect gate="-10" pin="B" pad="10"/>
<connect gate="-11" pin="B" pad="11"/>
<connect gate="-12" pin="B" pad="12"/>
<connect gate="-2" pin="B" pad="2"/>
<connect gate="-3" pin="B" pad="3"/>
<connect gate="-4" pin="B" pad="4"/>
<connect gate="-5" pin="B" pad="5"/>
<connect gate="-6" pin="B" pad="6"/>
<connect gate="-7" pin="B" pad="7"/>
<connect gate="-8" pin="B" pad="8"/>
<connect gate="-9" pin="B" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="2MM-2X6" package="3DROBOTICS_2MM-DUAL-ROW-MALE-HEADER-SMT-2X6">
<connects>
<connect gate="-1" pin="B" pad="1"/>
<connect gate="-10" pin="B" pad="10"/>
<connect gate="-11" pin="B" pad="11"/>
<connect gate="-12" pin="B" pad="12"/>
<connect gate="-2" pin="B" pad="2"/>
<connect gate="-3" pin="B" pad="3"/>
<connect gate="-4" pin="B" pad="4"/>
<connect gate="-5" pin="B" pad="5"/>
<connect gate="-6" pin="B" pad="6"/>
<connect gate="-7" pin="B" pad="7"/>
<connect gate="-8" pin="B" pad="8"/>
<connect gate="-9" pin="B" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="HEADER_1X4">
<gates>
<gate name="-1" symbol="MV"/>
<gate name="-2" symbol="M"/>
<gate name="-3" symbol="M"/>
<gate name="-4" symbol="M"/>
</gates>
<devices>
<device name="" package="HEADER_2.54MM-1X04">
<connects>
<connect gate="-1" pin="S" pad="1"/>
<connect gate="-2" pin="S" pad="2"/>
<connect gate="-3" pin="S" pad="3"/>
<connect gate="-4" pin="S" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MOSFET-DUAL-NCHANNEL">
<gates>
<gate name="-NMOS1" symbol="MOSFET-NCHANNEL"/>
<gate name="-NMOS2" symbol="MOSFET-NCHANNEL"/>
</gates>
<devices>
<device name="-SOT363" package="SOT363_PHILIPS">
<connects>
<connect gate="-NMOS1" pin="D" pad="6"/>
<connect gate="-NMOS1" pin="G" pad="2"/>
<connect gate="-NMOS1" pin="S" pad="1"/>
<connect gate="-NMOS2" pin="D" pad="3"/>
<connect gate="-NMOS2" pin="G" pad="5"/>
<connect gate="-NMOS2" pin="S" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MOSFET-PCHANNEL" prefix="Q">
<gates>
<gate name="G$1" symbol="MOSFET-PCHANNEL"/>
</gates>
<devices>
<device name="-SOT23-3" package="SOT23-3">
<connects>
<connect gate="G$1" pin="D" pad="3"/>
<connect gate="G$1" pin="G" pad="1"/>
<connect gate="G$1" pin="S" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-DPAK" package="DPAK">
<connects>
<connect gate="G$1" pin="D" pad="4"/>
<connect gate="G$1" pin="G" pad="1"/>
<connect gate="G$1" pin="S" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MOSFET-DUAL-PCHANNEL">
<gates>
<gate name="-PMOS1" symbol="MOSFET-PCHANNEL"/>
<gate name="-PMOS2" symbol="MOSFET-PCHANNEL"/>
</gates>
<devices>
<device name="-SOT363" package="SOT363_PHILIPS">
<connects>
<connect gate="-PMOS1" pin="D" pad="3"/>
<connect gate="-PMOS1" pin="G" pad="5"/>
<connect gate="-PMOS1" pin="S" pad="4"/>
<connect gate="-PMOS2" pin="D" pad="6"/>
<connect gate="-PMOS2" pin="G" pad="2"/>
<connect gate="-PMOS2" pin="S" pad="1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-CHIPFET" package="1206-8">
<connects>
<connect gate="-PMOS1" pin="D" pad="P$7 P$8"/>
<connect gate="-PMOS1" pin="G" pad="P$2"/>
<connect gate="-PMOS1" pin="S" pad="P$1"/>
<connect gate="-PMOS2" pin="D" pad="P$5 P$6"/>
<connect gate="-PMOS2" pin="G" pad="P$4"/>
<connect gate="-PMOS2" pin="S" pad="P$3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="BUZZER" prefix="SG">
<description>&lt;b&gt;BUZZER&lt;/b&gt;&lt;p&gt; Source: Buerklin</description>
<gates>
<gate name="1" symbol="B"/>
</gates>
<devices>
<device name="" package="F/TMB">
<connects>
<connect gate="1" pin="+" pad="+"/>
<connect gate="1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="INA139">
<gates>
<gate name="G$1" symbol="INA169"/>
</gates>
<devices>
<device name="" package="SC70">
<connects>
<connect gate="G$1" pin="GND" pad="2"/>
<connect gate="G$1" pin="OUT" pad="1"/>
<connect gate="G$1" pin="V+" pad="5"/>
<connect gate="G$1" pin="VIN+" pad="3"/>
<connect gate="G$1" pin="VIN-" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LVK24?">
<gates>
<gate name="G$1" symbol="CURRENT-SENSE-KELVIN"/>
</gates>
<devices>
<device name="" package="LVK24-CURRENT-SENSE">
<connects>
<connect gate="G$1" pin="I_IN" pad="I_1"/>
<connect gate="G$1" pin="I_OUT" pad="I_2"/>
<connect gate="G$1" pin="V+" pad="V1"/>
<connect gate="G$1" pin="V-" pad="V2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="EEPROM-I2C-?">
<gates>
<gate name="G$1" symbol="EEPROM-I2C-5PIN"/>
</gates>
<devices>
<device name="SOT23-5" package="SOT23-5">
<connects>
<connect gate="G$1" pin="SCL" pad="1"/>
<connect gate="G$1" pin="SDA" pad="3"/>
<connect gate="G$1" pin="VCC" pad="4"/>
<connect gate="G$1" pin="VSS" pad="2"/>
<connect gate="G$1" pin="WP" pad="5"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MECH-SERVO-?">
<gates>
<gate name="G$1" symbol="MECH-SERVO"/>
</gates>
<devices>
<device name="MINI" package="MECH-MINI-SERVO">
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="QUALIFIED_1_DUOVERO">
<gates>
<gate name="G$1" symbol="DUOVERO"/>
</gates>
<devices>
<device name="" package="QUALIFIED_1_DUOVERO">
<connects>
<connect gate="G$1" pin="ABE_BSP2_CLKX" pad="J9_54"/>
<connect gate="G$1" pin="ABE_BSP2_DR" pad="J9_55"/>
<connect gate="G$1" pin="ABE_BSP2_DX" pad="J9_53"/>
<connect gate="G$1" pin="ABE_BSP2_FSX" pad="J9_52"/>
<connect gate="G$1" pin="ADCIN2" pad="J8_46"/>
<connect gate="G$1" pin="ADCIN3" pad="J8_48"/>
<connect gate="G$1" pin="ADCIN4" pad="J8_49"/>
<connect gate="G$1" pin="ADCIN5" pad="J8_47"/>
<connect gate="G$1" pin="ADCIN6" pad="J8_45"/>
<connect gate="G$1" pin="AGND" pad="J9_3"/>
<connect gate="G$1" pin="AUXLF" pad="J9_4"/>
<connect gate="G$1" pin="AUXRF" pad="J9_5"/>
<connect gate="G$1" pin="BT_EN" pad="J8_56"/>
<connect gate="G$1" pin="CAM2_DX0" pad="J9_34"/>
<connect gate="G$1" pin="CAM2_DX1" pad="J9_33"/>
<connect gate="G$1" pin="CAM2_DY0" pad="J9_35"/>
<connect gate="G$1" pin="CAM2_DY1" pad="J9_32"/>
<connect gate="G$1" pin="CAM_DX0" pad="J9_31"/>
<connect gate="G$1" pin="CAM_DX1" pad="J9_37"/>
<connect gate="G$1" pin="CAM_DX2" pad="J9_39"/>
<connect gate="G$1" pin="CAM_DX3" pad="J9_40"/>
<connect gate="G$1" pin="CAM_DX4" pad="J9_42"/>
<connect gate="G$1" pin="CAM_DY0" pad="J9_30"/>
<connect gate="G$1" pin="CAM_DY1" pad="J9_36"/>
<connect gate="G$1" pin="CAM_DY2" pad="J9_38"/>
<connect gate="G$1" pin="CAM_DY3" pad="J9_41"/>
<connect gate="G$1" pin="CAM_DY4" pad="J9_43"/>
<connect gate="G$1" pin="CAM_RESET" pad="J9_47"/>
<connect gate="G$1" pin="CAM_SHUTTER" pad="J9_45"/>
<connect gate="G$1" pin="CAM_STROBE" pad="J9_46"/>
<connect gate="G$1" pin="DMIC_CLK1" pad="J9_51"/>
<connect gate="G$1" pin="DMIC_IN1" pad="J9_58"/>
<connect gate="G$1" pin="DMIC_IN2" pad="J9_57"/>
<connect gate="G$1" pin="DMIC_IN3" pad="J9_56"/>
<connect gate="G$1" pin="EM_CLK" pad="J8_59"/>
<connect gate="G$1" pin="EM_D0" pad="J8_19"/>
<connect gate="G$1" pin="EM_D1" pad="J8_16"/>
<connect gate="G$1" pin="EM_D10" pad="J8_8"/>
<connect gate="G$1" pin="EM_D11" pad="J8_9"/>
<connect gate="G$1" pin="EM_D12" pad="J8_7"/>
<connect gate="G$1" pin="EM_D13" pad="J8_6"/>
<connect gate="G$1" pin="EM_D14" pad="J8_4"/>
<connect gate="G$1" pin="EM_D15" pad="J8_5"/>
<connect gate="G$1" pin="EM_D2" pad="J8_18"/>
<connect gate="G$1" pin="EM_D3" pad="J8_17"/>
<connect gate="G$1" pin="EM_D4" pad="J8_15"/>
<connect gate="G$1" pin="EM_D5" pad="J8_14"/>
<connect gate="G$1" pin="EM_D6" pad="J8_13"/>
<connect gate="G$1" pin="EM_D7" pad="J8_12"/>
<connect gate="G$1" pin="EM_D8" pad="J8_10"/>
<connect gate="G$1" pin="EM_D9" pad="J8_11"/>
<connect gate="G$1" pin="EM_NADV_ALE" pad="J8_67"/>
<connect gate="G$1" pin="EM_NBE0" pad="J8_60"/>
<connect gate="G$1" pin="EM_NBE1" pad="J8_64"/>
<connect gate="G$1" pin="EM_NCS0" pad="J8_68"/>
<connect gate="G$1" pin="EM_NCS1" pad="J8_63"/>
<connect gate="G$1" pin="EM_NCS4" pad="J8_66"/>
<connect gate="G$1" pin="EM_NCS5_ETH0" pad="J8_1"/>
<connect gate="G$1" pin="EM_NCS6" pad="J8_65"/>
<connect gate="G$1" pin="EM_NOE" pad="J8_21"/>
<connect gate="G$1" pin="EM_NWE" pad="J8_20"/>
<connect gate="G$1" pin="EM_NWP" pad="J8_2"/>
<connect gate="G$1" pin="EM_WAIT0" pad="J8_69"/>
<connect gate="G$1" pin="GND@22" pad="J8_22"/>
<connect gate="G$1" pin="GND@24" pad="J9_24"/>
<connect gate="G$1" pin="GND@31" pad="J8_31"/>
<connect gate="G$1" pin="GND@44" pad="J9_44"/>
<connect gate="G$1" pin="GP40" pad="J8_50"/>
<connect gate="G$1" pin="GP42" pad="J8_51"/>
<connect gate="G$1" pin="GP44" pad="J8_52"/>
<connect gate="G$1" pin="GP45" pad="J8_53"/>
<connect gate="G$1" pin="GP47" pad="J8_58"/>
<connect gate="G$1" pin="GP48" pad="J8_54"/>
<connect gate="G$1" pin="GPIO114_SPI1_NIRQ" pad="J9_61"/>
<connect gate="G$1" pin="GPIO127_TS_IRQ" pad="J9_62"/>
<connect gate="G$1" pin="GPIO128_GPS_PPS" pad="J9_63"/>
<connect gate="G$1" pin="GPIO144_GPT9_PWM" pad="J9_67"/>
<connect gate="G$1" pin="GPIO145_GPT10_PWM" pad="J9_68"/>
<connect gate="G$1" pin="GPIO146_GPT11_PWM" pad="J9_69"/>
<connect gate="G$1" pin="GPIO147_GPT8_PWM" pad="J9_70"/>
<connect gate="G$1" pin="GPIO148_TXD1" pad="J9_19"/>
<connect gate="G$1" pin="GPIO151_RXD1" pad="J9_18"/>
<connect gate="G$1" pin="GPIO163_IR_CTS3" pad="J9_20"/>
<connect gate="G$1" pin="GPIO165_IR_RXD3" pad="J9_23"/>
<connect gate="G$1" pin="GPIO166_IR_TXD3" pad="J9_22"/>
<connect gate="G$1" pin="GPIO170_HDQ_1WIRE" pad="J9_50"/>
<connect gate="G$1" pin="GPIO171_SPI1_CLK" pad="J9_11"/>
<connect gate="G$1" pin="GPIO172_SPI1_MOSI" pad="J9_12"/>
<connect gate="G$1" pin="GPIO173_SPI1_MISO" pad="J9_14"/>
<connect gate="G$1" pin="GPIO174_SPI1_CS0" pad="J9_13"/>
<connect gate="G$1" pin="GPIO175_SPI1_CS1" pad="J9_10"/>
<connect gate="G$1" pin="GPIO176_ETH0_IRQ" pad="J9_59"/>
<connect gate="G$1" pin="GPIO184_I2C3_SCL" pad="J9_48"/>
<connect gate="G$1" pin="GPIO185_I2C3_SDA" pad="J9_49"/>
<connect gate="G$1" pin="GPIO31_WAKEUP" pad="J9_65"/>
<connect gate="G$1" pin="GPIO64_ETH0_NRESET" pad="J9_60"/>
<connect gate="G$1" pin="GPIO65_ETH1_IRQ1" pad="J9_64"/>
<connect gate="G$1" pin="HDMI_CEC" pad="J8_39"/>
<connect gate="G$1" pin="HDMI_CLOCKX" pad="J8_30"/>
<connect gate="G$1" pin="HDMI_CLOCKY" pad="J8_29"/>
<connect gate="G$1" pin="HDMI_D0X" pad="J8_28"/>
<connect gate="G$1" pin="HDMI_D0Y" pad="J8_27"/>
<connect gate="G$1" pin="HDMI_D1X" pad="J8_25"/>
<connect gate="G$1" pin="HDMI_D1Y" pad="J8_26"/>
<connect gate="G$1" pin="HDMI_D2X" pad="J8_24"/>
<connect gate="G$1" pin="HDMI_D2Y" pad="J8_23"/>
<connect gate="G$1" pin="HDMI_DDC_SCL" pad="J8_36"/>
<connect gate="G$1" pin="HDMI_DDC_SDA" pad="J8_37"/>
<connect gate="G$1" pin="HDMI_HPD" pad="J8_38"/>
<connect gate="G$1" pin="HDMI_LS_OE" pad="J8_40"/>
<connect gate="G$1" pin="HSMIC_PF" pad="J9_9"/>
<connect gate="G$1" pin="HSOLF" pad="J9_6"/>
<connect gate="G$1" pin="HSORF" pad="J9_7"/>
<connect gate="G$1" pin="I2C2_SCL" pad="J8_3"/>
<connect gate="G$1" pin="I2C2_SDA" pad="J8_70"/>
<connect gate="G$1" pin="I2C4_SCL" pad="J9_17"/>
<connect gate="G$1" pin="I2C4_SDA" pad="J9_16"/>
<connect gate="G$1" pin="IR_RTS3" pad="J9_21"/>
<connect gate="G$1" pin="MIC_MAIN_MF" pad="J9_8"/>
<connect gate="G$1" pin="NRESPWRON" pad="J9_66"/>
<connect gate="G$1" pin="POWERON" pad="J8_57"/>
<connect gate="G$1" pin="PWM1" pad="J8_43"/>
<connect gate="G$1" pin="PWM2" pad="J8_44"/>
<connect gate="G$1" pin="SYSEN" pad="J8_61"/>
<connect gate="G$1" pin="USBH_CPEN" pad="J9_25"/>
<connect gate="G$1" pin="USBH_DM" pad="J9_29"/>
<connect gate="G$1" pin="USBH_DP" pad="J9_28"/>
<connect gate="G$1" pin="USBH_RESET" pad="J9_26"/>
<connect gate="G$1" pin="USBH_VBUS" pad="J9_27"/>
<connect gate="G$1" pin="USBOTG_CE" pad="J8_35"/>
<connect gate="G$1" pin="USBOTG_DM" pad="J8_34"/>
<connect gate="G$1" pin="USBOTG_DP" pad="J8_33"/>
<connect gate="G$1" pin="USBOTG_ID" pad="J8_32"/>
<connect gate="G$1" pin="USBOTG_VBUS_IN" pad="J8_62"/>
<connect gate="G$1" pin="VBACKUP" pad="J8_55"/>
<connect gate="G$1" pin="VSYSTEM@1" pad="J9_1"/>
<connect gate="G$1" pin="VSYSTEM@2" pad="J9_2"/>
<connect gate="G$1" pin="VSYSTEM@41" pad="J8_41"/>
<connect gate="G$1" pin="VSYSTEM@42" pad="J8_42"/>
<connect gate="G$1" pin="WIFI_EN" pad="J9_15"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="USB-B-AB">
<gates>
<gate name="G$1" symbol="QUALIFIED_1_USB"/>
<gate name="G$2" symbol="QUALIFIED_1_M"/>
<gate name="G$3" symbol="QUALIFIED_1_M"/>
<gate name="G$4" symbol="QUALIFIED_1_M"/>
<gate name="G$5" symbol="QUALIFIED_1_M"/>
</gates>
<devices>
<device name="-MINI-SMT-LOCK" package="QUALIFIED_1_USB-B-SMT">
<connects>
<connect gate="G$1" pin="1_VBUS" pad="VBUS"/>
<connect gate="G$1" pin="2_D-" pad="D-"/>
<connect gate="G$1" pin="3_D+" pad="D+"/>
<connect gate="G$1" pin="4_ID" pad="ID"/>
<connect gate="G$1" pin="5_GND" pad="GND"/>
<connect gate="G$2" pin="S" pad="P1"/>
<connect gate="G$3" pin="S" pad="P2"/>
<connect gate="G$4" pin="S" pad="P3"/>
<connect gate="G$5" pin="S" pad="P4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-MINI-AB-SMT" package="QUALIFIED_1_USB-MINI-AB-SMT">
<connects>
<connect gate="G$1" pin="1_VBUS" pad="VBUS"/>
<connect gate="G$1" pin="2_D-" pad="D-"/>
<connect gate="G$1" pin="3_D+" pad="D+"/>
<connect gate="G$1" pin="4_ID" pad="ID"/>
<connect gate="G$1" pin="5_GND" pad="GND"/>
<connect gate="G$2" pin="S" pad="P1"/>
<connect gate="G$3" pin="S" pad="P2"/>
<connect gate="G$4" pin="S" pad="P3"/>
<connect gate="G$5" pin="S" pad="P4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-MINI-SMT" package="USB-MINI-B-SMT">
<connects>
<connect gate="G$1" pin="1_VBUS" pad="VBUS"/>
<connect gate="G$1" pin="2_D-" pad="D-"/>
<connect gate="G$1" pin="3_D+" pad="D+"/>
<connect gate="G$1" pin="4_ID" pad="ID"/>
<connect gate="G$1" pin="5_GND" pad="GND"/>
<connect gate="G$2" pin="S" pad="P1"/>
<connect gate="G$3" pin="S" pad="P2"/>
<connect gate="G$4" pin="S" pad="P3"/>
<connect gate="G$5" pin="S" pad="P4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-MICRO-B-SMT" package="MOLEX-47346-0001">
<connects>
<connect gate="G$1" pin="1_VBUS" pad="VBUS"/>
<connect gate="G$1" pin="2_D-" pad="D-"/>
<connect gate="G$1" pin="3_D+" pad="D+"/>
<connect gate="G$1" pin="4_ID" pad="ID"/>
<connect gate="G$1" pin="5_GND" pad="GND"/>
<connect gate="G$2" pin="S" pad="GND1"/>
<connect gate="G$3" pin="S" pad="GND2"/>
<connect gate="G$4" pin="S" pad="GND3"/>
<connect gate="G$5" pin="S" pad="GND4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="TXS0108">
<gates>
<gate name="G$1" symbol="TX?0108"/>
</gates>
<devices>
<device name="TSSOP-20" package="R-PDSO-G20">
<connects>
<connect gate="G$1" pin="A1" pad="1"/>
<connect gate="G$1" pin="A2" pad="3"/>
<connect gate="G$1" pin="A3" pad="4"/>
<connect gate="G$1" pin="A4" pad="5"/>
<connect gate="G$1" pin="A5" pad="6"/>
<connect gate="G$1" pin="A6" pad="7"/>
<connect gate="G$1" pin="A7" pad="8"/>
<connect gate="G$1" pin="A8" pad="9"/>
<connect gate="G$1" pin="B1" pad="20"/>
<connect gate="G$1" pin="B2" pad="18"/>
<connect gate="G$1" pin="B3" pad="17"/>
<connect gate="G$1" pin="B4" pad="16"/>
<connect gate="G$1" pin="B5" pad="15"/>
<connect gate="G$1" pin="B6" pad="14"/>
<connect gate="G$1" pin="B7" pad="13"/>
<connect gate="G$1" pin="B8" pad="12"/>
<connect gate="G$1" pin="GND" pad="11"/>
<connect gate="G$1" pin="OE" pad="10"/>
<connect gate="G$1" pin="VCCA" pad="2"/>
<connect gate="G$1" pin="VCCB" pad="19"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="QFN20" package="QFN20-RGY">
<connects>
<connect gate="G$1" pin="A1" pad="1"/>
<connect gate="G$1" pin="A2" pad="3"/>
<connect gate="G$1" pin="A3" pad="4"/>
<connect gate="G$1" pin="A4" pad="5"/>
<connect gate="G$1" pin="A5" pad="6"/>
<connect gate="G$1" pin="A6" pad="7"/>
<connect gate="G$1" pin="A7" pad="8"/>
<connect gate="G$1" pin="A8" pad="9"/>
<connect gate="G$1" pin="B1" pad="20"/>
<connect gate="G$1" pin="B2" pad="18"/>
<connect gate="G$1" pin="B3" pad="17"/>
<connect gate="G$1" pin="B4" pad="16"/>
<connect gate="G$1" pin="B5" pad="15"/>
<connect gate="G$1" pin="B6" pad="14"/>
<connect gate="G$1" pin="B7" pad="13"/>
<connect gate="G$1" pin="B8" pad="12"/>
<connect gate="G$1" pin="GND" pad="11"/>
<connect gate="G$1" pin="OE" pad="10"/>
<connect gate="G$1" pin="VCCA" pad="2"/>
<connect gate="G$1" pin="VCCB" pad="19"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="KRUBERG_IP4786CZ32">
<gates>
<gate name="G$1" symbol="IP4786CZ32"/>
</gates>
<devices>
<device name="" package="KRUBERG_HVQFN32">
<connects>
<connect gate="G$1" pin="CEC_A" pad="29"/>
<connect gate="G$1" pin="CEC_B" pad="25"/>
<connect gate="G$1" pin="CON_5V0" pad="13"/>
<connect gate="G$1" pin="ESD_BYP\" pad="26"/>
<connect gate="G$1" pin="HPD_A" pad="32"/>
<connect gate="G$1" pin="HPD_B" pad="12"/>
<connect gate="G$1" pin="LS_OE" pad="28"/>
<connect gate="G$1" pin="NC@30" pad="30"/>
<connect gate="G$1" pin="NC@31" pad="31"/>
<connect gate="G$1" pin="PGND@PAD" pad="PGND"/>
<connect gate="G$1" pin="SCL_A" pad="9"/>
<connect gate="G$1" pin="SCL_B" pad="15"/>
<connect gate="G$1" pin="SDA_A" pad="10"/>
<connect gate="G$1" pin="SDA_B" pad="14"/>
<connect gate="G$1" pin="SYS_TXC+" pad="7"/>
<connect gate="G$1" pin="SYS_TXC-" pad="8"/>
<connect gate="G$1" pin="SYS_TXD0+" pad="5"/>
<connect gate="G$1" pin="SYS_TXD0-" pad="6"/>
<connect gate="G$1" pin="SYS_TXD1+" pad="3"/>
<connect gate="G$1" pin="SYS_TXD1-\" pad="4"/>
<connect gate="G$1" pin="SYS_TXD2+" pad="1"/>
<connect gate="G$1" pin="SYS_TXD2-" pad="2"/>
<connect gate="G$1" pin="TXC+" pad="18"/>
<connect gate="G$1" pin="TXC-" pad="17"/>
<connect gate="G$1" pin="TXD0+" pad="20"/>
<connect gate="G$1" pin="TXD0-" pad="19"/>
<connect gate="G$1" pin="TXD1+" pad="22"/>
<connect gate="G$1" pin="TXD1-" pad="21"/>
<connect gate="G$1" pin="TXD2+" pad="24"/>
<connect gate="G$1" pin="TXD2-" pad="23"/>
<connect gate="G$1" pin="UTILITY" pad="16"/>
<connect gate="G$1" pin="VCC_1.8" pad="27"/>
<connect gate="G$1" pin="VCC_5.0" pad="11"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MOLEX-HDMI_HDMI">
<gates>
<gate name="G$1" symbol="MOLEX-HDMI"/>
</gates>
<devices>
<device name="_FULLSIZE" package="MOLEX-HDMI_47151-001">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="17" pad="17"/>
<connect gate="G$1" pin="18" pad="18"/>
<connect gate="G$1" pin="19" pad="19"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="20" pad="G1"/>
<connect gate="G$1" pin="21" pad="G2"/>
<connect gate="G$1" pin="22" pad="G3"/>
<connect gate="G$1" pin="23" pad="G4"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_MICRO" package="MOLEX-HDMI-46765-0001">
<connects>
<connect gate="G$1" pin="1" pad="3"/>
<connect gate="G$1" pin="10" pad="12"/>
<connect gate="G$1" pin="11" pad="13"/>
<connect gate="G$1" pin="12" pad="14"/>
<connect gate="G$1" pin="13" pad="15"/>
<connect gate="G$1" pin="14" pad="2"/>
<connect gate="G$1" pin="15" pad="17"/>
<connect gate="G$1" pin="16" pad="18"/>
<connect gate="G$1" pin="17" pad="16"/>
<connect gate="G$1" pin="18" pad="19"/>
<connect gate="G$1" pin="19" pad="1"/>
<connect gate="G$1" pin="2" pad="4"/>
<connect gate="G$1" pin="20" pad="S1"/>
<connect gate="G$1" pin="21" pad="S2"/>
<connect gate="G$1" pin="22" pad="S3"/>
<connect gate="G$1" pin="23" pad="S4"/>
<connect gate="G$1" pin="3" pad="5"/>
<connect gate="G$1" pin="4" pad="6"/>
<connect gate="G$1" pin="5" pad="7"/>
<connect gate="G$1" pin="6" pad="8"/>
<connect gate="G$1" pin="7" pad="9"/>
<connect gate="G$1" pin="8" pad="10"/>
<connect gate="G$1" pin="9" pad="11"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="SWITCH-DIP-4POS">
<gates>
<gate name="G$1" symbol="SWITCH-SPST-4POS"/>
</gates>
<devices>
<device name="-219-4MST" package="CTS-219-4MST">
<connects>
<connect gate="G$1" pin="S1A" pad="S1A"/>
<connect gate="G$1" pin="S1B" pad="S1B"/>
<connect gate="G$1" pin="S2A" pad="S2A"/>
<connect gate="G$1" pin="S2B" pad="S2B"/>
<connect gate="G$1" pin="S3A" pad="S3A"/>
<connect gate="G$1" pin="S3B" pad="S3B"/>
<connect gate="G$1" pin="S4A" pad="S4A"/>
<connect gate="G$1" pin="S4B" pad="S4B"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-CHS-04TA" package="COPAL-CHS-04TA">
<connects>
<connect gate="G$1" pin="S1A" pad="S1A"/>
<connect gate="G$1" pin="S1B" pad="S1B"/>
<connect gate="G$1" pin="S2A" pad="S2A"/>
<connect gate="G$1" pin="S2B" pad="S2B"/>
<connect gate="G$1" pin="S3A" pad="S3A"/>
<connect gate="G$1" pin="S3B" pad="S3B"/>
<connect gate="G$1" pin="S4A" pad="S4A"/>
<connect gate="G$1" pin="S4B" pad="S4B"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="PX4-LOGO">
<gates>
<gate name="G$1" symbol="PX4-LOGO"/>
</gates>
<devices>
<device name="-10MM" package="PX4-LOGO-10MM">
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-15MM" package="PX4-LOGO-15MM">
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-20MM" package="PX4-LOGO-20MM">
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-30MM" package="PX4-LOGO-30MM">
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="BAT54A" prefix="D">
<description>&lt;b&gt;Schottky Diodes&lt;/b&gt;&lt;p&gt;
Source: Fairchild .. BAT54.pdf</description>
<gates>
<gate name="G$1" symbol="SDD_KAAK"/>
</gates>
<devices>
<device name="" package="SOT23-3">
<connects>
<connect gate="G$1" pin="AA" pad="3"/>
<connect gate="G$1" pin="K1" pad="1"/>
<connect gate="G$1" pin="K2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="BAT54C" prefix="D">
<description>&lt;b&gt;Schottky Diodes&lt;/b&gt;&lt;p&gt;
Source: Fairchild .. BAT54.pdf</description>
<gates>
<gate name="G$1" symbol="SDD_AKKA"/>
</gates>
<devices>
<device name="" package="SOT23-3">
<connects>
<connect gate="G$1" pin="A1" pad="1"/>
<connect gate="G$1" pin="A2" pad="2"/>
<connect gate="G$1" pin="CC" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="BAT54" prefix="D">
<description>&lt;b&gt;Schottky Diodes&lt;/b&gt;&lt;p&gt;
Source: Fairchild .. BAT54.pdf</description>
<gates>
<gate name="G$1" symbol="SCHOTTKY"/>
</gates>
<devices>
<device name="" package="SOT23-3">
<connects>
<connect gate="G$1" pin="A" pad="1"/>
<connect gate="G$1" pin="C" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="BAT54S" prefix="D">
<description>&lt;b&gt;Schottky Diodes&lt;/b&gt;&lt;p&gt;
Source: Fairchild .. BAT54.pdf</description>
<gates>
<gate name="G$1" symbol="SDD_AKAK"/>
</gates>
<devices>
<device name="" package="SOT23-3">
<connects>
<connect gate="G$1" pin="A1" pad="1"/>
<connect gate="G$1" pin="C1A2" pad="2"/>
<connect gate="G$1" pin="C2" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="DMS-20LCD">
<description>Murata DMS-20LCD

Datasheet: &lt;a href="http://www.murata-ps.com/data/meters/20lcd.pdf"&gt;Murata Link&lt;/a&gt;</description>
<gates>
<gate name="G$1" symbol="DMS-20LCD"/>
</gates>
<devices>
<device name="" package="DMS-20LCD">
<connects>
<connect gate="G$1" pin="!BACKLIGHT" pad="9"/>
<connect gate="G$1" pin="!DP1" pad="6"/>
<connect gate="G$1" pin="!DP2" pad="5"/>
<connect gate="G$1" pin="!DP3" pad="4"/>
<connect gate="G$1" pin="(+)INPUT_HI" pad="11"/>
<connect gate="G$1" pin="(-)INPUT_LO" pad="12"/>
<connect gate="G$1" pin="+5V/+BATTERY" pad="1"/>
<connect gate="G$1" pin="-5V/-BATTERY" pad="3"/>
<connect gate="G$1" pin="AN_COMMON" pad="10"/>
<connect gate="G$1" pin="REF_IN" pad="7"/>
<connect gate="G$1" pin="REF_OUT" pad="8"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="BMA280">
<gates>
<gate name="G$1" symbol="BMA280"/>
</gates>
<devices>
<device name="" package="BMA280">
<connects>
<connect gate="G$1" pin="CSB" pad="10"/>
<connect gate="G$1" pin="GND" pad="9"/>
<connect gate="G$1" pin="GNDIO" pad="8"/>
<connect gate="G$1" pin="INT1" pad="5"/>
<connect gate="G$1" pin="INT2" pad="6"/>
<connect gate="G$1" pin="PS" pad="11"/>
<connect gate="G$1" pin="SCK/SCL" pad="12"/>
<connect gate="G$1" pin="SDI/SDA" pad="2"/>
<connect gate="G$1" pin="SDO" pad="1"/>
<connect gate="G$1" pin="VDD" pad="7"/>
<connect gate="G$1" pin="VDDIO" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="CD4017B">
<gates>
<gate name="G$1" symbol="CD4017"/>
</gates>
<devices>
<device name="" package="TSSOP-16">
<connects>
<connect gate="G$1" pin="!CLK_EN" pad="13"/>
<connect gate="G$1" pin="CLK" pad="14"/>
<connect gate="G$1" pin="GND" pad="8"/>
<connect gate="G$1" pin="Q0" pad="3"/>
<connect gate="G$1" pin="Q1" pad="2"/>
<connect gate="G$1" pin="Q2" pad="4"/>
<connect gate="G$1" pin="Q3" pad="7"/>
<connect gate="G$1" pin="Q4" pad="10"/>
<connect gate="G$1" pin="Q5" pad="1"/>
<connect gate="G$1" pin="Q6" pad="5"/>
<connect gate="G$1" pin="Q7" pad="6"/>
<connect gate="G$1" pin="Q8" pad="9"/>
<connect gate="G$1" pin="Q9" pad="11"/>
<connect gate="G$1" pin="RST" pad="15"/>
<connect gate="G$1" pin="TC" pad="12"/>
<connect gate="G$1" pin="VCC" pad="16"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="V_REG_RECOM">
<gates>
<gate name="G$1" symbol="78XX"/>
</gates>
<devices>
<device name="" package="R-78X.0-1.0">
<connects>
<connect gate="G$1" pin="GND" pad="2"/>
<connect gate="G$1" pin="IN" pad="1"/>
<connect gate="G$1" pin="OUT" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="HEADER-3X4">
<gates>
<gate name="G$1" symbol="SERVO4"/>
</gates>
<devices>
<device name="" package="3X4RA">
<connects>
<connect gate="G$1" pin="GND2@2" pad="6"/>
<connect gate="G$1" pin="GND@1" pad="3"/>
<connect gate="G$1" pin="GND@3" pad="9"/>
<connect gate="G$1" pin="GND@4" pad="12"/>
<connect gate="G$1" pin="PPM1" pad="1"/>
<connect gate="G$1" pin="PPM2" pad="4"/>
<connect gate="G$1" pin="PPM3" pad="7"/>
<connect gate="G$1" pin="PPM4" pad="10"/>
<connect gate="G$1" pin="VCC_5V@1" pad="2"/>
<connect gate="G$1" pin="VCC_5V@2" pad="5"/>
<connect gate="G$1" pin="VCC_5V@3" pad="8"/>
<connect gate="G$1" pin="VCC_5V@4" pad="11"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="FM25V01">
<description>&lt;b&gt;FM25V01 128Kb Serial 3V F-RAM Memory&lt;/b&gt;</description>
<gates>
<gate name="G$1" symbol="FM25V01"/>
</gates>
<devices>
<device name="" package="SO08">
<connects>
<connect gate="G$1" pin="!HOLD" pad="7"/>
<connect gate="G$1" pin="!S" pad="1"/>
<connect gate="G$1" pin="!W" pad="3"/>
<connect gate="G$1" pin="C" pad="6"/>
<connect gate="G$1" pin="D" pad="5"/>
<connect gate="G$1" pin="Q" pad="2"/>
<connect gate="G$1" pin="VDD" pad="8"/>
<connect gate="G$1" pin="VSS" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET" value="http://www.ramtron.com/files/datasheets/FM25V01_ds.pdf"/>
<attribute name="LINK" value="http://www.digikey.com/product-detail/en/FM25V01-GTR/1140-1026-1-ND/2809832"/>
<attribute name="MFGPN" value="FM25V01"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="L3GD20H">
<description>&lt;b&gt;L3GD20H MEMS motion sensor: 3-axis digital output gyroscope&lt;/b&gt;</description>
<gates>
<gate name="G$1" symbol="L3GD20H"/>
</gates>
<devices>
<device name="" package="LGA-16L">
<connects>
<connect gate="G$1" pin="CAP" pad="14"/>
<connect gate="G$1" pin="CS" pad="5"/>
<connect gate="G$1" pin="DEN" pad="8"/>
<connect gate="G$1" pin="DRDY/INT2" pad="6"/>
<connect gate="G$1" pin="GND" pad="9 10 11 12 13"/>
<connect gate="G$1" pin="INT1" pad="7"/>
<connect gate="G$1" pin="SCL/SPC" pad="2"/>
<connect gate="G$1" pin="SDA/SDI/SDO" pad="3"/>
<connect gate="G$1" pin="SDO/SA0" pad="4"/>
<connect gate="G$1" pin="VDD" pad="15 16"/>
<connect gate="G$1" pin="VDD_IO" pad="1"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET" value="http://www.st.com/internet/com/TECHNICAL_RESOURCES/TECHNICAL_LITERATURE/DATASHEET/DM00060659.pdf"/>
<attribute name="LINK" value="http://www.st.com/internet/analog/product/254039.jsp"/>
<attribute name="MFGPN" value="L3GD20H"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LPS331AP">
<description>&lt;b&gt;LPS331AP MEMS pressure sensor, 260-1260 mbar absolute digital output barometer&lt;/b&gt;</description>
<gates>
<gate name="G$1" symbol="LPS331AP"/>
</gates>
<devices>
<device name="" package="LGA-16L">
<connects>
<connect gate="G$1" pin="CS" pad="8"/>
<connect gate="G$1" pin="GND1" pad="5"/>
<connect gate="G$1" pin="GND2" pad="12"/>
<connect gate="G$1" pin="GND3" pad="13"/>
<connect gate="G$1" pin="GND4" pad="16"/>
<connect gate="G$1" pin="INT1" pad="11"/>
<connect gate="G$1" pin="INT2" pad="9"/>
<connect gate="G$1" pin="RSRV" pad="10"/>
<connect gate="G$1" pin="SCL/SPC" pad="4"/>
<connect gate="G$1" pin="SDA/SDI/SDO" pad="6"/>
<connect gate="G$1" pin="SDO/SA0" pad="7"/>
<connect gate="G$1" pin="VCCA" pad="15"/>
<connect gate="G$1" pin="VDD" pad="14"/>
<connect gate="G$1" pin="VDD_IO" pad="1"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET" value="http://www.st.com/internet/com/TECHNICAL_RESOURCES/TECHNICAL_LITERATURE/DATASHEET/DM00036196.pdf"/>
<attribute name="LINK" value="http://www.st.com/jp/analog/product/251601.jsp"/>
<attribute name="MFGPN" value="LPS331AP"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LSM303D">
<description>&lt;b&gt;LSM303D Ultra compact high performance e-compass: 3D accelerometer and 3D magnetometer module&lt;/b&gt;</description>
<gates>
<gate name="G$1" symbol="LSM303D"/>
</gates>
<devices>
<device name="" package="LGA-16L">
<connects>
<connect gate="G$1" pin="C1" pad="15"/>
<connect gate="G$1" pin="CS" pad="8"/>
<connect gate="G$1" pin="GND@1" pad="5"/>
<connect gate="G$1" pin="GND@2" pad="12"/>
<connect gate="G$1" pin="GND@3" pad="13"/>
<connect gate="G$1" pin="GND@4" pad="16"/>
<connect gate="G$1" pin="INT1" pad="11"/>
<connect gate="G$1" pin="INT2" pad="9"/>
<connect gate="G$1" pin="RSRV" pad="10"/>
<connect gate="G$1" pin="SCL/SPC" pad="4"/>
<connect gate="G$1" pin="SDA/SDI/SDO" pad="6"/>
<connect gate="G$1" pin="SDO/SA0" pad="7"/>
<connect gate="G$1" pin="SETC" pad="2"/>
<connect gate="G$1" pin="SETP" pad="3"/>
<connect gate="G$1" pin="VDD" pad="14"/>
<connect gate="G$1" pin="VDD_IO" pad="1"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET" value="http://www.st.com/internet/com/TECHNICAL_RESOURCES/TECHNICAL_LITERATURE/DATASHEET/DM00057547.pdf"/>
<attribute name="LINK" value="http://www.st.com/internet/analog/product/253884.jsp"/>
<attribute name="MFGPN" value="LSM303D"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LT3028" prefix="U" uservalue="yes">
<description>LT3028 100mA/500mA low-dropout regulator</description>
<gates>
<gate name="G$1" symbol="LT3028"/>
</gates>
<devices>
<device name="DFN16" package="DFN16+GND_5X3">
<connects>
<connect gate="G$1" pin="!SHDN1" pad="P$15"/>
<connect gate="G$1" pin="!SHDN2" pad="P$10"/>
<connect gate="G$1" pin="ADJ1" pad="P$16"/>
<connect gate="G$1" pin="ADJ2" pad="P$9"/>
<connect gate="G$1" pin="BYP1" pad="P$1"/>
<connect gate="G$1" pin="BYP2" pad="P$8"/>
<connect gate="G$1" pin="GND" pad="P$5 P$17"/>
<connect gate="G$1" pin="IN1" pad="P$13 P$14"/>
<connect gate="G$1" pin="IN2" pad="P$11 P$12"/>
<connect gate="G$1" pin="OUT1" pad="P$3 P$4"/>
<connect gate="G$1" pin="OUT2" pad="P$6 P$7"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="TPS76701Q">
<description>TPS76701Q 1A Adjustable LDO</description>
<gates>
<gate name="G$1" symbol="TPS76701Q"/>
</gates>
<devices>
<device name="SO08" package="SO08">
<connects>
<connect gate="G$1" pin="!EN" pad="2"/>
<connect gate="G$1" pin="!RESET" pad="8"/>
<connect gate="G$1" pin="FB" pad="7"/>
<connect gate="G$1" pin="GND" pad="1"/>
<connect gate="G$1" pin="IN" pad="3 4"/>
<connect gate="G$1" pin="OUT" pad="5 6"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="SERVO-3X6">
<gates>
<gate name="G$1" symbol="SERVO6"/>
</gates>
<devices>
<device name="" package="3X6RA">
<connects>
<connect gate="G$1" pin="+5V@1" pad="2"/>
<connect gate="G$1" pin="+5V@2" pad="5"/>
<connect gate="G$1" pin="+5V@3" pad="8"/>
<connect gate="G$1" pin="+5V@4" pad="11"/>
<connect gate="G$1" pin="+5V@5" pad="14"/>
<connect gate="G$1" pin="+5V@6" pad="17"/>
<connect gate="G$1" pin="GND@1" pad="3"/>
<connect gate="G$1" pin="GND@2" pad="6"/>
<connect gate="G$1" pin="GND@3" pad="9"/>
<connect gate="G$1" pin="GND@4" pad="12"/>
<connect gate="G$1" pin="GND@5" pad="15"/>
<connect gate="G$1" pin="GND@6" pad="18"/>
<connect gate="G$1" pin="PPM1" pad="16"/>
<connect gate="G$1" pin="PPM2" pad="13"/>
<connect gate="G$1" pin="PPM3" pad="10"/>
<connect gate="G$1" pin="PPM4" pad="7"/>
<connect gate="G$1" pin="PPM5" pad="4"/>
<connect gate="G$1" pin="PPM6" pad="1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MS621FE">
<description>&lt;b&gt;SEIKO 6.8mm Rechargeable 3V lithium battery&lt;b&gt;
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;If discontinued or not available, similar devices are available from Panasonic and Sanyo, usually direct replacements.&lt;b&gt;</description>
<gates>
<gate name="G$1" symbol="BATTERY"/>
</gates>
<devices>
<device name="" package="MS621FE">
<connects>
<connect gate="G$1" pin="NEG" pad="2"/>
<connect gate="G$1" pin="POS" pad="1"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET" value="http://speed.sii.co.jp/data/file_PRODUCT_MASTER_50112_TITLE_IMAGESP.pdf"/>
<attribute name="LINK" value="http://search.digikey.com/us/en/products/MS621FE-FL11E/728-1057-ND/1889208"/>
<attribute name="MFGPN" value="MS621FE"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LTC4411">
<description>LTC4411 2.6A low loss ideal diode</description>
<gates>
<gate name="G$1" symbol="LTC4411"/>
</gates>
<devices>
<device name="SOT23" package="SOT23-5">
<connects>
<connect gate="G$1" pin="CTL" pad="3"/>
<connect gate="G$1" pin="GND" pad="2"/>
<connect gate="G$1" pin="IN" pad="1"/>
<connect gate="G$1" pin="OUT" pad="5"/>
<connect gate="G$1" pin="STAT" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MIC5357" prefix="U" uservalue="yes">
<description>MIC5357 low-noise dual 500mA LDO</description>
<gates>
<gate name="G$1" symbol="MIC5357"/>
</gates>
<devices>
<device name="" package="MSOP-8-EPAD">
<connects>
<connect gate="G$1" pin="BYP" pad="3"/>
<connect gate="G$1" pin="EN1" pad="5"/>
<connect gate="G$1" pin="EN2" pad="4"/>
<connect gate="G$1" pin="GND" pad="2 9"/>
<connect gate="G$1" pin="IN" pad="1"/>
<connect gate="G$1" pin="OUT1" pad="8"/>
<connect gate="G$1" pin="OUT2" pad="7"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="RGB-LED" prefix="U">
<description>RGB LED with separate anode/cathode terminals</description>
<gates>
<gate name="BLUE" symbol="LED"/>
<gate name="GREEN" symbol="LED"/>
<gate name="RED" symbol="LED"/>
</gates>
<devices>
<device name="6-PLCC" package="6-PLCC">
<connects>
<connect gate="BLUE" pin="A" pad="A1"/>
<connect gate="BLUE" pin="C" pad="C1"/>
<connect gate="GREEN" pin="A" pad="A2"/>
<connect gate="GREEN" pin="C" pad="C2"/>
<connect gate="RED" pin="A" pad="A3"/>
<connect gate="RED" pin="C" pad="C3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MC14504B">
<description>Hex level shifter</description>
<gates>
<gate name="G$1" symbol="MC14504B"/>
</gates>
<devices>
<device name="TSSOP16" package="TSSOP-16">
<connects>
<connect gate="G$1" pin="AIN" pad="3"/>
<connect gate="G$1" pin="AOUT" pad="2"/>
<connect gate="G$1" pin="BIN" pad="5"/>
<connect gate="G$1" pin="BOUT" pad="4"/>
<connect gate="G$1" pin="CIN" pad="7"/>
<connect gate="G$1" pin="COUT" pad="6"/>
<connect gate="G$1" pin="DIN" pad="9"/>
<connect gate="G$1" pin="DOUT" pad="10"/>
<connect gate="G$1" pin="EIN" pad="11"/>
<connect gate="G$1" pin="EOUT" pad="12"/>
<connect gate="G$1" pin="FIN" pad="14"/>
<connect gate="G$1" pin="FOUT" pad="15"/>
<connect gate="G$1" pin="GND" pad="8"/>
<connect gate="G$1" pin="MODE" pad="13"/>
<connect gate="G$1" pin="VCC" pad="1"/>
<connect gate="G$1" pin="VDD" pad="16"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LT3469" prefix="U" uservalue="yes">
<description>LT3469 Piezo microactuator driver with boost regulator</description>
<gates>
<gate name="G$1" symbol="LT3469"/>
</gates>
<devices>
<device name="" package="SOT23-8">
<connects>
<connect gate="G$1" pin="+IN" pad="7"/>
<connect gate="G$1" pin="-IN" pad="8"/>
<connect gate="G$1" pin="FB" pad="2"/>
<connect gate="G$1" pin="GND" pad="4"/>
<connect gate="G$1" pin="OUT" pad="1"/>
<connect gate="G$1" pin="SW" pad="5"/>
<connect gate="G$1" pin="VCC" pad="6"/>
<connect gate="G$1" pin="VIN" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="74LVC1G125">
<gates>
<gate name="G$1" symbol="74LVC1G125"/>
</gates>
<devices>
<device name="-SOT353" package="SOT353">
<connects>
<connect gate="G$1" pin="!OE" pad="1"/>
<connect gate="G$1" pin="A" pad="2"/>
<connect gate="G$1" pin="GND" pad="3"/>
<connect gate="G$1" pin="VCC" pad="5"/>
<connect gate="G$1" pin="Y" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="TCA62724FMG" prefix="U">
<description>Toshiba TCA62724FMG I2C RGB LED driver</description>
<gates>
<gate name="G$1" symbol="TCA62724"/>
</gates>
<devices>
<device name="" package="SON10">
<connects>
<connect gate="G$1" pin="!RESET" pad="4"/>
<connect gate="G$1" pin="!SHDN" pad="1"/>
<connect gate="G$1" pin="GND" pad="5"/>
<connect gate="G$1" pin="OUT0" pad="9"/>
<connect gate="G$1" pin="OUT1" pad="8"/>
<connect gate="G$1" pin="OUT2" pad="7"/>
<connect gate="G$1" pin="REXT" pad="6"/>
<connect gate="G$1" pin="SCL" pad="3"/>
<connect gate="G$1" pin="SDA" pad="2"/>
<connect gate="G$1" pin="VIN" pad="10"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="KNH16C104DA5TS" prefix="L">
<description>Kyocera KNH16C104DA5TS EMI filter</description>
<gates>
<gate name="G$1" symbol="CAP-FEEDTHROUGH"/>
</gates>
<devices>
<device name="" package="KYOCERA-KNH16-DA">
<connects>
<connect gate="G$1" pin="P$1" pad="P$1"/>
<connect gate="G$1" pin="P$2" pad="P$2"/>
<connect gate="G$1" pin="P$3" pad="P$3 P$4 P$5"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="IR2301">
<gates>
<gate name="G$1" symbol="IR2301"/>
</gates>
<devices>
<device name="SOIC" package="SO08">
<connects>
<connect gate="G$1" pin="COM" pad="4"/>
<connect gate="G$1" pin="HIN" pad="2"/>
<connect gate="G$1" pin="HO" pad="7"/>
<connect gate="G$1" pin="LIN" pad="3"/>
<connect gate="G$1" pin="LO" pad="5"/>
<connect gate="G$1" pin="VB" pad="8"/>
<connect gate="G$1" pin="VCC" pad="1"/>
<connect gate="G$1" pin="VS" pad="6"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="INA169">
<gates>
<gate name="G$1" symbol="INA169-1"/>
</gates>
<devices>
<device name="" package="SOT23-5">
<connects>
<connect gate="G$1" pin="GND" pad="2"/>
<connect gate="G$1" pin="OUT" pad="1"/>
<connect gate="G$1" pin="V+" pad="5"/>
<connect gate="G$1" pin="VIN+" pad="3"/>
<connect gate="G$1" pin="VIN-" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="DIODE" prefix="D" uservalue="yes">
<gates>
<gate name="G$1" symbol="DIODE"/>
</gates>
<devices>
<device name="-B" package="3528/B-DIO">
<connects>
<connect gate="G$1" pin="A" pad="A"/>
<connect gate="G$1" pin="C" pad="C"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-MELF" package="MELF-MLL41">
<connects>
<connect gate="G$1" pin="A" pad="A"/>
<connect gate="G$1" pin="C" pad="C"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-SOD-123" package="SOD-123-DIO">
<connects>
<connect gate="G$1" pin="A" pad="A"/>
<connect gate="G$1" pin="C" pad="C"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-0603" package="0603-DIO">
<connects>
<connect gate="G$1" pin="A" pad="A"/>
<connect gate="G$1" pin="C" pad="C"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MIC5332">
<gates>
<gate name="G$1" symbol="MIC5332"/>
</gates>
<devices>
<device name="" package="MLF-8-EPAD">
<connects>
<connect gate="G$1" pin="CSET" pad="6"/>
<connect gate="G$1" pin="EN1" pad="5"/>
<connect gate="G$1" pin="EN2" pad="4"/>
<connect gate="G$1" pin="GND" pad="2 GND"/>
<connect gate="G$1" pin="POR2" pad="3"/>
<connect gate="G$1" pin="VIN" pad="1"/>
<connect gate="G$1" pin="VOUT1" pad="8"/>
<connect gate="G$1" pin="VOUT2" pad="7"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="NUF2042XV6">
<gates>
<gate name="G$1" symbol="NUF20X0XV6"/>
</gates>
<devices>
<device name="" package="SOT563-6">
<connects>
<connect gate="G$1" pin="D1I" pad="1"/>
<connect gate="G$1" pin="D1O" pad="6"/>
<connect gate="G$1" pin="D2I" pad="3"/>
<connect gate="G$1" pin="D2O" pad="4"/>
<connect gate="G$1" pin="GND" pad="2"/>
<connect gate="G$1" pin="VBUS" pad="5"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="BQ24313">
<gates>
<gate name="G$1" symbol="BQ24313"/>
</gates>
<devices>
<device name="" package="QFN8-DSG">
<connects>
<connect gate="G$1" pin="!CE" pad="5"/>
<connect gate="G$1" pin="!FAULT" pad="4"/>
<connect gate="G$1" pin="ILIM" pad="7"/>
<connect gate="G$1" pin="IN" pad="1"/>
<connect gate="G$1" pin="OUT" pad="8"/>
<connect gate="G$1" pin="VBAT" pad="6"/>
<connect gate="G$1" pin="VSS" pad="2 GND P$2 P$3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="FR014H5JZ">
<gates>
<gate name="G$1" symbol="FR014H5JZ"/>
</gates>
<devices>
<device name="" package="MLP08W">
<connects>
<connect gate="G$1" pin="CTL" pad="4"/>
<connect gate="G$1" pin="NEG" pad="1 2 3"/>
<connect gate="G$1" pin="POS" pad="5 6 7 8"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="BQ24315">
<gates>
<gate name="G$1" symbol="BQ24313"/>
</gates>
<devices>
<device name="" package="QFN8-DSG">
<connects>
<connect gate="G$1" pin="!CE" pad="5"/>
<connect gate="G$1" pin="!FAULT" pad="4"/>
<connect gate="G$1" pin="ILIM" pad="7"/>
<connect gate="G$1" pin="IN" pad="1"/>
<connect gate="G$1" pin="OUT" pad="8"/>
<connect gate="G$1" pin="VBAT" pad="6"/>
<connect gate="G$1" pin="VSS" pad="2 GND P$2 P$3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="DIODE-TVS">
<gates>
<gate name="G$1" symbol="DIODE-TVS"/>
</gates>
<devices>
<device name="" package="0402-TVS">
<connects>
<connect gate="G$1" pin="A" pad="A"/>
<connect gate="G$1" pin="C" pad="C"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ZXCT1051">
<gates>
<gate name="G$1" symbol="ZXCT1051"/>
</gates>
<devices>
<device name="" package="SOT23-5L">
<connects>
<connect gate="G$1" pin="GND" pad="2"/>
<connect gate="G$1" pin="VCC" pad="1"/>
<connect gate="G$1" pin="VOUT" pad="3"/>
<connect gate="G$1" pin="VSENSE+" pad="4"/>
<connect gate="G$1" pin="VSENSE-" pad="5"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="TPS54332">
<gates>
<gate name="G$1" symbol="TPS54332"/>
</gates>
<devices>
<device name="" package="SO08-DDA-EPAD">
<connects>
<connect gate="G$1" pin="BOOT" pad="1"/>
<connect gate="G$1" pin="COMP" pad="6"/>
<connect gate="G$1" pin="EN" pad="3"/>
<connect gate="G$1" pin="GND" pad="7 EPAD TH1 TH2 TH3 TH4 TH5 TH6"/>
<connect gate="G$1" pin="PH" pad="8"/>
<connect gate="G$1" pin="SS" pad="4"/>
<connect gate="G$1" pin="VIN" pad="2"/>
<connect gate="G$1" pin="VSENSE" pad="5"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="CONN_FPC_10">
<description>10-pin FPC connector for PX4 sensor board</description>
<gates>
<gate name="G$1" symbol="KV"/>
<gate name="G$2" symbol="K"/>
<gate name="G$3" symbol="K"/>
<gate name="G$4" symbol="K"/>
<gate name="G$5" symbol="K"/>
<gate name="G$6" symbol="K"/>
<gate name="G$7" symbol="K"/>
<gate name="G$8" symbol="K"/>
<gate name="G$9" symbol="K"/>
<gate name="G$10" symbol="K"/>
</gates>
<devices>
<device name="RA" package="51281-1094">
<connects>
<connect gate="G$1" pin="S" pad="1"/>
<connect gate="G$10" pin="S" pad="10"/>
<connect gate="G$2" pin="S" pad="2"/>
<connect gate="G$3" pin="S" pad="3"/>
<connect gate="G$4" pin="S" pad="4"/>
<connect gate="G$5" pin="S" pad="5"/>
<connect gate="G$6" pin="S" pad="6"/>
<connect gate="G$7" pin="S" pad="7"/>
<connect gate="G$8" pin="S" pad="8"/>
<connect gate="G$9" pin="S" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="VERT" package="78119-0108">
<connects>
<connect gate="G$1" pin="S" pad="1"/>
<connect gate="G$10" pin="S" pad="10"/>
<connect gate="G$2" pin="S" pad="2"/>
<connect gate="G$3" pin="S" pad="3"/>
<connect gate="G$4" pin="S" pad="4"/>
<connect gate="G$5" pin="S" pad="5"/>
<connect gate="G$6" pin="S" pad="6"/>
<connect gate="G$7" pin="S" pad="7"/>
<connect gate="G$8" pin="S" pad="8"/>
<connect gate="G$9" pin="S" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="FIDUCIAL" prefix="JP">
<description>&lt;b&gt;Fiducial Alignment Points&lt;/b&gt;
Various fiducial points for machine vision alignment.</description>
<gates>
<gate name="G$1" symbol="FIDUCIAL"/>
</gates>
<devices>
<device name="1.5X3" package="FIDUCIAL-1.5X3">
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="1X2" package="FIDUCIAL-1X2">
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="1X2.5" package="FIDUCIAL-1X2.5">
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="UFIDUCIAL" package="MICRO-FIDUCIAL">
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LTC4117">
<gates>
<gate name="G$1" symbol="LTC4417"/>
</gates>
<devices>
<device name="" package="MO-220">
<connects>
<connect gate="G$1" pin="!SHDN" pad="P$23"/>
<connect gate="G$1" pin="!VALID1" pad="P$7"/>
<connect gate="G$1" pin="!VALID2" pad="P$8"/>
<connect gate="G$1" pin="!VALID3" pad="P$9"/>
<connect gate="G$1" pin="CAS" pad="P$11"/>
<connect gate="G$1" pin="EN" pad="P$22"/>
<connect gate="G$1" pin="G1" pad="P$17"/>
<connect gate="G$1" pin="G2" pad="P$15"/>
<connect gate="G$1" pin="G3" pad="P$13"/>
<connect gate="G$1" pin="GND" pad="P$10 P$25"/>
<connect gate="G$1" pin="HYS" pad="P$24"/>
<connect gate="G$1" pin="OV1" pad="P$2"/>
<connect gate="G$1" pin="OV2" pad="P$4"/>
<connect gate="G$1" pin="OV3" pad="P$6"/>
<connect gate="G$1" pin="UV1" pad="P$1"/>
<connect gate="G$1" pin="UV2" pad="P$3"/>
<connect gate="G$1" pin="UV3" pad="P$5"/>
<connect gate="G$1" pin="V1" pad="P$21"/>
<connect gate="G$1" pin="V2" pad="P$20"/>
<connect gate="G$1" pin="V3" pad="P$19"/>
<connect gate="G$1" pin="VOUT" pad="P$12"/>
<connect gate="G$1" pin="VS1" pad="P$18"/>
<connect gate="G$1" pin="VS2" pad="P$16"/>
<connect gate="G$1" pin="VS3" pad="P$14"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="4525DO-DSXAIYYYD">
<gates>
<gate name="G$1" symbol="4525DO"/>
</gates>
<devices>
<device name="P" package="4525DO-DS5AI001DP">
<connects>
<connect gate="G$1" pin="GND" pad="1"/>
<connect gate="G$1" pin="INT/SS" pad="5"/>
<connect gate="G$1" pin="SCL/SCLK" pad="4"/>
<connect gate="G$1" pin="SDA/MISO" pad="3"/>
<connect gate="G$1" pin="VCC" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="S" package="4525DO-DSXAI001DS">
<connects>
<connect gate="G$1" pin="GND" pad="1"/>
<connect gate="G$1" pin="INT/SS" pad="5"/>
<connect gate="G$1" pin="SCL/SCLK" pad="4"/>
<connect gate="G$1" pin="SDA/MISO" pad="3"/>
<connect gate="G$1" pin="VCC" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="PMEG2005CT">
<description>&lt;b&gt;500 mA low VF dual MEGA Schottky barrier rectifier&lt;/b&gt;

&lt;p&gt;http://www.nxp.com/documents/data_sheet/PMEG2005CT.pdf&lt;/p&gt;</description>
<gates>
<gate name="G$1" symbol="SDD_AKKA"/>
</gates>
<devices>
<device name="" package="SOT23-3">
<connects>
<connect gate="G$1" pin="A1" pad="1"/>
<connect gate="G$1" pin="A2" pad="2"/>
<connect gate="G$1" pin="CC" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="HEADER-3X16" prefix="J">
<description>3x16 servo header</description>
<gates>
<gate name="-1" symbol="MV-1"/>
<gate name="-2" symbol="MV-1"/>
<gate name="-4" symbol="MV-1"/>
<gate name="-7" symbol="MV-1"/>
<gate name="-10" symbol="MV-1"/>
<gate name="-13" symbol="MV-1"/>
<gate name="-16" symbol="MV-1"/>
<gate name="-19" symbol="MV-1"/>
<gate name="-22" symbol="MV-1"/>
<gate name="-25" symbol="MV-1"/>
<gate name="-28" symbol="MV-1"/>
<gate name="-31" symbol="MV-1"/>
<gate name="-34" symbol="MV-1"/>
<gate name="-37" symbol="MV-1"/>
<gate name="-40" symbol="MV-1"/>
<gate name="-43" symbol="MV-1"/>
<gate name="-46" symbol="MV-1"/>
<gate name="-GND" symbol="MV-1"/>
<gate name="-VCC" symbol="MV-1"/>
</gates>
<devices>
<device name="3X16RA" package="3X16RA">
<connects>
<connect gate="-1" pin="S" pad="1"/>
<connect gate="-10" pin="S" pad="10"/>
<connect gate="-13" pin="S" pad="13"/>
<connect gate="-16" pin="S" pad="16"/>
<connect gate="-19" pin="S" pad="19"/>
<connect gate="-2" pin="S" pad="2"/>
<connect gate="-22" pin="S" pad="22"/>
<connect gate="-25" pin="S" pad="25"/>
<connect gate="-28" pin="S" pad="28"/>
<connect gate="-31" pin="S" pad="31"/>
<connect gate="-34" pin="S" pad="34"/>
<connect gate="-37" pin="S" pad="37"/>
<connect gate="-4" pin="S" pad="4"/>
<connect gate="-40" pin="S" pad="40"/>
<connect gate="-43" pin="S" pad="43"/>
<connect gate="-46" pin="S" pad="46"/>
<connect gate="-7" pin="S" pad="7"/>
<connect gate="-GND" pin="S" pad="3 6 9 12 15 18 21 24 27 30 33 36 39 42 45 48"/>
<connect gate="-VCC" pin="S" pad="5 8 11 14 17 20 23 26 29 32 35 38 41 44 47"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="STM32F10XRXT6" prefix="IC">
<description>ST STM32F101/103/105 64pin LQFP</description>
<gates>
<gate name="PORTA_L" symbol="PORT_A_L"/>
<gate name="PORTA_H" symbol="PORT_A_H"/>
<gate name="PORTB_L" symbol="PORT_B_L"/>
<gate name="PORTB_H" symbol="PORT_B_H"/>
<gate name="AN_POWER" symbol="BAT_AN_M"/>
<gate name="RESET" symbol="BOOT_RST"/>
<gate name="G$1" symbol="PORT_C_H"/>
<gate name="G$2" symbol="PORT_C_L"/>
<gate name="G$3" symbol="VDD_VSS_M_F1X"/>
<gate name="G$4" symbol="PORT_D_3"/>
</gates>
<devices>
<device name="L" package="TQFP64">
<connects>
<connect gate="AN_POWER" pin="VBAT" pad="1"/>
<connect gate="AN_POWER" pin="VDDA" pad="13"/>
<connect gate="AN_POWER" pin="VSSA" pad="12"/>
<connect gate="G$1" pin="PC10" pad="51"/>
<connect gate="G$1" pin="PC11" pad="52"/>
<connect gate="G$1" pin="PC12" pad="53"/>
<connect gate="G$1" pin="PC13" pad="2"/>
<connect gate="G$1" pin="PC14" pad="3"/>
<connect gate="G$1" pin="PC15" pad="4"/>
<connect gate="G$1" pin="PC8" pad="39"/>
<connect gate="G$1" pin="PC9" pad="40"/>
<connect gate="G$2" pin="PC0" pad="8"/>
<connect gate="G$2" pin="PC1" pad="9"/>
<connect gate="G$2" pin="PC2" pad="10"/>
<connect gate="G$2" pin="PC3" pad="11"/>
<connect gate="G$2" pin="PC4" pad="24"/>
<connect gate="G$2" pin="PC5" pad="25"/>
<connect gate="G$2" pin="PC6" pad="37"/>
<connect gate="G$2" pin="PC7" pad="38"/>
<connect gate="G$3" pin="VDD@1" pad="32"/>
<connect gate="G$3" pin="VDD@2" pad="48"/>
<connect gate="G$3" pin="VDD@3" pad="64"/>
<connect gate="G$3" pin="VDD@4" pad="19"/>
<connect gate="G$3" pin="VSS@1" pad="31"/>
<connect gate="G$3" pin="VSS@2" pad="47"/>
<connect gate="G$3" pin="VSS@3" pad="63"/>
<connect gate="G$3" pin="VSS@4" pad="18"/>
<connect gate="G$4" pin="PD2" pad="54"/>
<connect gate="G$4" pin="PH0/OSC&lt;=" pad="5"/>
<connect gate="G$4" pin="PH1/OSC=&gt;" pad="6"/>
<connect gate="PORTA_H" pin="PA10" pad="43"/>
<connect gate="PORTA_H" pin="PA11" pad="44"/>
<connect gate="PORTA_H" pin="PA12" pad="45"/>
<connect gate="PORTA_H" pin="PA13" pad="46"/>
<connect gate="PORTA_H" pin="PA14" pad="49"/>
<connect gate="PORTA_H" pin="PA15" pad="50"/>
<connect gate="PORTA_H" pin="PA8" pad="41"/>
<connect gate="PORTA_H" pin="PA9" pad="42"/>
<connect gate="PORTA_L" pin="PA0" pad="14"/>
<connect gate="PORTA_L" pin="PA1" pad="15"/>
<connect gate="PORTA_L" pin="PA2" pad="16"/>
<connect gate="PORTA_L" pin="PA3" pad="17"/>
<connect gate="PORTA_L" pin="PA4" pad="20"/>
<connect gate="PORTA_L" pin="PA5" pad="21"/>
<connect gate="PORTA_L" pin="PA6" pad="22"/>
<connect gate="PORTA_L" pin="PA7" pad="23"/>
<connect gate="PORTB_H" pin="PB10" pad="29"/>
<connect gate="PORTB_H" pin="PB11" pad="30"/>
<connect gate="PORTB_H" pin="PB12" pad="33"/>
<connect gate="PORTB_H" pin="PB13" pad="34"/>
<connect gate="PORTB_H" pin="PB14" pad="35"/>
<connect gate="PORTB_H" pin="PB15" pad="36"/>
<connect gate="PORTB_H" pin="PB8" pad="61"/>
<connect gate="PORTB_H" pin="PB9" pad="62"/>
<connect gate="PORTB_L" pin="PB0" pad="26"/>
<connect gate="PORTB_L" pin="PB1" pad="27"/>
<connect gate="PORTB_L" pin="PB2" pad="28"/>
<connect gate="PORTB_L" pin="PB3" pad="55"/>
<connect gate="PORTB_L" pin="PB4" pad="56"/>
<connect gate="PORTB_L" pin="PB5" pad="57"/>
<connect gate="PORTB_L" pin="PB6" pad="58"/>
<connect gate="PORTB_L" pin="PB7" pad="59"/>
<connect gate="RESET" pin="BOOT0" pad="60"/>
<connect gate="RESET" pin="NRST" pad="7"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="HEADER_2.54MM_2X23">
<description>Header for BBB</description>
<gates>
<gate name="G$1" symbol="BBB_PLUG_8"/>
</gates>
<devices>
<device name="" package="HEADER_2.54MM_2X23_TH">
<connects>
<connect gate="G$1" pin="P$1" pad="1"/>
<connect gate="G$1" pin="P$10" pad="10"/>
<connect gate="G$1" pin="P$11" pad="11"/>
<connect gate="G$1" pin="P$12" pad="12"/>
<connect gate="G$1" pin="P$13" pad="13"/>
<connect gate="G$1" pin="P$14" pad="14"/>
<connect gate="G$1" pin="P$15" pad="15"/>
<connect gate="G$1" pin="P$16" pad="16"/>
<connect gate="G$1" pin="P$17" pad="17"/>
<connect gate="G$1" pin="P$18" pad="18"/>
<connect gate="G$1" pin="P$19" pad="19"/>
<connect gate="G$1" pin="P$2" pad="2"/>
<connect gate="G$1" pin="P$20" pad="20"/>
<connect gate="G$1" pin="P$21" pad="21"/>
<connect gate="G$1" pin="P$22" pad="22"/>
<connect gate="G$1" pin="P$23" pad="23"/>
<connect gate="G$1" pin="P$24" pad="24"/>
<connect gate="G$1" pin="P$25" pad="25"/>
<connect gate="G$1" pin="P$26" pad="26"/>
<connect gate="G$1" pin="P$27" pad="27"/>
<connect gate="G$1" pin="P$28" pad="28"/>
<connect gate="G$1" pin="P$29" pad="29"/>
<connect gate="G$1" pin="P$3" pad="3"/>
<connect gate="G$1" pin="P$30" pad="30"/>
<connect gate="G$1" pin="P$31" pad="31"/>
<connect gate="G$1" pin="P$32" pad="32"/>
<connect gate="G$1" pin="P$33" pad="33"/>
<connect gate="G$1" pin="P$34" pad="34"/>
<connect gate="G$1" pin="P$35" pad="35"/>
<connect gate="G$1" pin="P$36" pad="36"/>
<connect gate="G$1" pin="P$37" pad="37"/>
<connect gate="G$1" pin="P$38" pad="38"/>
<connect gate="G$1" pin="P$39" pad="39"/>
<connect gate="G$1" pin="P$4" pad="4"/>
<connect gate="G$1" pin="P$40" pad="40"/>
<connect gate="G$1" pin="P$41" pad="41"/>
<connect gate="G$1" pin="P$42" pad="42"/>
<connect gate="G$1" pin="P$43" pad="43"/>
<connect gate="G$1" pin="P$44" pad="44"/>
<connect gate="G$1" pin="P$45" pad="45"/>
<connect gate="G$1" pin="P$46" pad="46"/>
<connect gate="G$1" pin="P$5" pad="5"/>
<connect gate="G$1" pin="P$6" pad="6"/>
<connect gate="G$1" pin="P$7" pad="7"/>
<connect gate="G$1" pin="P$8" pad="8"/>
<connect gate="G$1" pin="P$9" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="HEAD_2.54_6">
<gates>
<gate name="G$1" symbol="HEAD_10"/>
</gates>
<devices>
<device name="" package="HEADER_2.54MM-1X10">
<connects>
<connect gate="G$1" pin="P$1" pad="P$1"/>
<connect gate="G$1" pin="P$2" pad="P$2"/>
<connect gate="G$1" pin="P$3" pad="P$3"/>
<connect gate="G$1" pin="P$4" pad="P$4"/>
<connect gate="G$1" pin="P$5" pad="P$5"/>
<connect gate="G$1" pin="P$6" pad="P$6"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LSM9DS0">
<description>LSM9DS0 Accel compass gyro</description>
<gates>
<gate name="G$1" symbol="LSM9DS0"/>
</gates>
<devices>
<device name="" package="LGA-24">
<connects>
<connect gate="G$1" pin="C1_XM" pad="7"/>
<connect gate="G$1" pin="CS_G" pad="19"/>
<connect gate="G$1" pin="CS_XM" pad="20"/>
<connect gate="G$1" pin="DEN_G" pad="10"/>
<connect gate="G$1" pin="DRDY_G" pad="12"/>
<connect gate="G$1" pin="GND@1" pad="2"/>
<connect gate="G$1" pin="GND@2" pad="3"/>
<connect gate="G$1" pin="GND@3" pad="4"/>
<connect gate="G$1" pin="GND@4" pad="5"/>
<connect gate="G$1" pin="GND@5" pad="6"/>
<connect gate="G$1" pin="INT1_XM" pad="13"/>
<connect gate="G$1" pin="INT2_XM" pad="14"/>
<connect gate="G$1" pin="INT_G" pad="11"/>
<connect gate="G$1" pin="NC" pad="1"/>
<connect gate="G$1" pin="SDA" pad="24"/>
<connect gate="G$1" pin="SDO_G" pad="22"/>
<connect gate="G$1" pin="SDO_XM" pad="23"/>
<connect gate="G$1" pin="SETC_XM" pad="8"/>
<connect gate="G$1" pin="SETP_XM" pad="9"/>
<connect gate="G$1" pin="SPC" pad="21"/>
<connect gate="G$1" pin="VDD@1" pad="15"/>
<connect gate="G$1" pin="VDD@2" pad="16"/>
<connect gate="G$1" pin="VDD@3" pad="17"/>
<connect gate="G$1" pin="VDD_IO" pad="18"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="BEAGLEBONE_OUTLINE">
<description>Should match A3 pinout - but not completely tested</description>
<gates>
<gate name="G$1" symbol="BEAGLEBONE-1"/>
</gates>
<devices>
<device name="" package="BEAGLEBONE_SHIELD">
<connects>
<connect gate="G$1" pin="AIN0" pad="85"/>
<connect gate="G$1" pin="AIN1" pad="86"/>
<connect gate="G$1" pin="AIN2" pad="83"/>
<connect gate="G$1" pin="AIN3" pad="84"/>
<connect gate="G$1" pin="AIN4" pad="79"/>
<connect gate="G$1" pin="AIN5" pad="82"/>
<connect gate="G$1" pin="AIN6" pad="81"/>
<connect gate="G$1" pin="BATT_GND" pad="TP8"/>
<connect gate="G$1" pin="BAT_+_LIPO_1_S" pad="TP5"/>
<connect gate="G$1" pin="BAT_SENSE" pad="TP6"/>
<connect gate="G$1" pin="CLKOUT2" pad="87"/>
<connect gate="G$1" pin="EHRPWM1A" pad="60"/>
<connect gate="G$1" pin="EHRPWM1B" pad="62"/>
<connect gate="G$1" pin="EHRPWM2A" pad="19"/>
<connect gate="G$1" pin="EHRPWM2B" pad="13"/>
<connect gate="G$1" pin="GND@1" pad="47"/>
<connect gate="G$1" pin="GND@2" pad="48"/>
<connect gate="G$1" pin="GND@3" pad="89"/>
<connect gate="G$1" pin="GND@4" pad="91"/>
<connect gate="G$1" pin="GND@5" pad="90"/>
<connect gate="G$1" pin="GND@6" pad="92"/>
<connect gate="G$1" pin="GND@7" pad="1"/>
<connect gate="G$1" pin="GND@8" pad="2"/>
<connect gate="G$1" pin="GND@9" pad="93"/>
<connect gate="G$1" pin="GNDA_ADC" pad="80"/>
<connect gate="G$1" pin="GPIO0_26" pad="14"/>
<connect gate="G$1" pin="GPIO0_27" pad="17"/>
<connect gate="G$1" pin="GPIO0_7" pad="88"/>
<connect gate="G$1" pin="GPIO1_0" pad="25"/>
<connect gate="G$1" pin="GPIO1_1" pad="24"/>
<connect gate="G$1" pin="GPIO1_12" pad="12"/>
<connect gate="G$1" pin="GPIO1_13" pad="11"/>
<connect gate="G$1" pin="GPIO1_14" pad="16"/>
<connect gate="G$1" pin="GPIO1_15" pad="15"/>
<connect gate="G$1" pin="GPIO1_16" pad="61"/>
<connect gate="G$1" pin="GPIO1_17" pad="69"/>
<connect gate="G$1" pin="GPIO1_2" pad="5"/>
<connect gate="G$1" pin="GPIO1_28" pad="58"/>
<connect gate="G$1" pin="GPIO1_29" pad="26"/>
<connect gate="G$1" pin="GPIO1_3" pad="6"/>
<connect gate="G$1" pin="GPIO1_30" pad="21"/>
<connect gate="G$1" pin="GPIO1_31" pad="20"/>
<connect gate="G$1" pin="GPIO1_4" pad="23"/>
<connect gate="G$1" pin="GPIO1_5" pad="22"/>
<connect gate="G$1" pin="GPIO1_6" pad="3"/>
<connect gate="G$1" pin="GPIO1_7" pad="4"/>
<connect gate="G$1" pin="GPIO2_1" pad="18"/>
<connect gate="G$1" pin="GPIO2_10" pad="41"/>
<connect gate="G$1" pin="GPIO2_11" pad="42"/>
<connect gate="G$1" pin="GPIO2_12" pad="39"/>
<connect gate="G$1" pin="GPIO2_13" pad="40"/>
<connect gate="G$1" pin="GPIO2_22" pad="27"/>
<connect gate="G$1" pin="GPIO2_23" pad="29"/>
<connect gate="G$1" pin="GPIO2_24" pad="28"/>
<connect gate="G$1" pin="GPIO2_25" pad="30"/>
<connect gate="G$1" pin="GPIO2_6" pad="45"/>
<connect gate="G$1" pin="GPIO2_7" pad="46"/>
<connect gate="G$1" pin="GPIO2_8" pad="43"/>
<connect gate="G$1" pin="GPIO2_9" pad="44"/>
<connect gate="G$1" pin="GPIO3_19" pad="73"/>
<connect gate="G$1" pin="GPIO3_21" pad="71"/>
<connect gate="G$1" pin="I2C1_SCL" pad="63"/>
<connect gate="G$1" pin="I2C1_SDA" pad="64"/>
<connect gate="G$1" pin="I2C2_SCL" pad="65"/>
<connect gate="G$1" pin="I2C2_SDA" pad="66"/>
<connect gate="G$1" pin="NC@1" pad="94"/>
<connect gate="G$1" pin="NC@2" pad="95"/>
<connect gate="G$1" pin="NC@3" pad="98"/>
<connect gate="G$1" pin="PWR_BUT" pad="55"/>
<connect gate="G$1" pin="SCREW$1" pad="P$1"/>
<connect gate="G$1" pin="SCREW$2" pad="P$2"/>
<connect gate="G$1" pin="SCREW$3" pad="P$3"/>
<connect gate="G$1" pin="SCREW$4" pad="P$4"/>
<connect gate="G$1" pin="SPI1_CS0" pad="74"/>
<connect gate="G$1" pin="SPI1_DI" pad="76"/>
<connect gate="G$1" pin="SPI1_DO" pad="75"/>
<connect gate="G$1" pin="SPI1_SCLK" pad="77"/>
<connect gate="G$1" pin="SYS_5V@1" pad="53"/>
<connect gate="G$1" pin="SYS_5V@2" pad="54"/>
<connect gate="G$1" pin="SYS_RESETN" pad="56"/>
<connect gate="G$1" pin="TEMP_SENSE" pad="TP7"/>
<connect gate="G$1" pin="TIMER4" pad="7"/>
<connect gate="G$1" pin="TIMER5" pad="9"/>
<connect gate="G$1" pin="TIMER6" pad="10"/>
<connect gate="G$1" pin="TIMER7" pad="8"/>
<connect gate="G$1" pin="UART0_RXD" pad="97"/>
<connect gate="G$1" pin="UART0_TXD" pad="96"/>
<connect gate="G$1" pin="UART1_RXD" pad="72"/>
<connect gate="G$1" pin="UART1_TXD" pad="70"/>
<connect gate="G$1" pin="UART2_RXD" pad="68"/>
<connect gate="G$1" pin="UART2_TXD" pad="67"/>
<connect gate="G$1" pin="UART3_CTSN" pad="36"/>
<connect gate="G$1" pin="UART3_RTSN" pad="34"/>
<connect gate="G$1" pin="UART4_CTSN" pad="35"/>
<connect gate="G$1" pin="UART4_RTSN" pad="33"/>
<connect gate="G$1" pin="UART4_RXD" pad="57"/>
<connect gate="G$1" pin="UART4_TXD" pad="59"/>
<connect gate="G$1" pin="UART5_CTSN" pad="31"/>
<connect gate="G$1" pin="UART5_RTSN" pad="32"/>
<connect gate="G$1" pin="UART5_RXD" pad="38"/>
<connect gate="G$1" pin="UART5_TXD" pad="37"/>
<connect gate="G$1" pin="VDD_3V3EXP@1" pad="49"/>
<connect gate="G$1" pin="VDD_3V3EXP@2" pad="50"/>
<connect gate="G$1" pin="VDD_5V@1" pad="51"/>
<connect gate="G$1" pin="VDD_5V@2" pad="52"/>
<connect gate="G$1" pin="VDD_ADC" pad="78"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="BBB_3X14_RA">
<gates>
<gate name="G$1" symbol="3X14RA_SERVO"/>
</gates>
<devices>
<device name="" package="3X14RA">
<connects>
<connect gate="G$1" pin="5V@1" pad="2"/>
<connect gate="G$1" pin="5V@10" pad="29"/>
<connect gate="G$1" pin="5V@11" pad="32"/>
<connect gate="G$1" pin="5V@12" pad="35"/>
<connect gate="G$1" pin="5V@13" pad="38"/>
<connect gate="G$1" pin="5V@14" pad="41"/>
<connect gate="G$1" pin="5V@2" pad="5"/>
<connect gate="G$1" pin="5V@3" pad="8"/>
<connect gate="G$1" pin="5V@4" pad="11"/>
<connect gate="G$1" pin="5V@5" pad="14"/>
<connect gate="G$1" pin="5V@6" pad="17"/>
<connect gate="G$1" pin="5V@7" pad="20"/>
<connect gate="G$1" pin="5V@8" pad="23"/>
<connect gate="G$1" pin="5V@9" pad="26"/>
<connect gate="G$1" pin="CH11" pad="4"/>
<connect gate="G$1" pin="CH12" pad="1"/>
<connect gate="G$1" pin="CH_1" pad="34"/>
<connect gate="G$1" pin="CH_10" pad="7"/>
<connect gate="G$1" pin="CH_2" pad="31"/>
<connect gate="G$1" pin="CH_3" pad="28"/>
<connect gate="G$1" pin="CH_4" pad="25"/>
<connect gate="G$1" pin="CH_5" pad="22"/>
<connect gate="G$1" pin="CH_6" pad="19"/>
<connect gate="G$1" pin="CH_7" pad="16"/>
<connect gate="G$1" pin="CH_8" pad="13"/>
<connect gate="G$1" pin="CH_9" pad="10"/>
<connect gate="G$1" pin="GND@1" pad="3"/>
<connect gate="G$1" pin="GND@10" pad="30"/>
<connect gate="G$1" pin="GND@11" pad="33"/>
<connect gate="G$1" pin="GND@12" pad="36"/>
<connect gate="G$1" pin="GND@13" pad="39"/>
<connect gate="G$1" pin="GND@14" pad="42"/>
<connect gate="G$1" pin="GND@2" pad="6"/>
<connect gate="G$1" pin="GND@3" pad="9"/>
<connect gate="G$1" pin="GND@4" pad="12"/>
<connect gate="G$1" pin="GND@5" pad="15"/>
<connect gate="G$1" pin="GND@6" pad="18"/>
<connect gate="G$1" pin="GND@7" pad="21"/>
<connect gate="G$1" pin="GND@8" pad="24"/>
<connect gate="G$1" pin="GND@9" pad="27"/>
<connect gate="G$1" pin="PPM/S.BUS_IN" pad="40"/>
<connect gate="G$1" pin="PPM/S.BUS_OUT" pad="37"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MPU-6500">
<gates>
<gate name="G$1" symbol="MPU-6500"/>
</gates>
<devices>
<device name="" package="MPU-6500">
<connects>
<connect gate="G$1" pin="!CS" pad="22"/>
<connect gate="G$1" pin="AD0/SDO" pad="9"/>
<connect gate="G$1" pin="AUX_CL" pad="7"/>
<connect gate="G$1" pin="AUX_DA" pad="21"/>
<connect gate="G$1" pin="FSYNC" pad="11"/>
<connect gate="G$1" pin="GND" pad="18"/>
<connect gate="G$1" pin="INT" pad="12"/>
<connect gate="G$1" pin="NC@1" pad="1"/>
<connect gate="G$1" pin="NC@10" pad="17"/>
<connect gate="G$1" pin="NC@2" pad="2"/>
<connect gate="G$1" pin="NC@3" pad="3"/>
<connect gate="G$1" pin="NC@4" pad="4"/>
<connect gate="G$1" pin="NC@5" pad="5"/>
<connect gate="G$1" pin="NC@6" pad="6"/>
<connect gate="G$1" pin="NC@7" pad="14"/>
<connect gate="G$1" pin="NC@8" pad="15"/>
<connect gate="G$1" pin="NC@9" pad="16"/>
<connect gate="G$1" pin="REGOUT" pad="10"/>
<connect gate="G$1" pin="RESV@1" pad="20"/>
<connect gate="G$1" pin="RESV@2" pad="19"/>
<connect gate="G$1" pin="SCL/SCLK" pad="23"/>
<connect gate="G$1" pin="SDA/SDI" pad="24"/>
<connect gate="G$1" pin="VDD" pad="13"/>
<connect gate="G$1" pin="VDDIO" pad="8"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LTC3080">
<description>LTC3080 250mA LDO

Input: 1.2V to 36V, Output: 0V to 36V, 1.1A


&lt;a href="http://cds.linear.com/docs/en/datasheet/3080fc.pdf"&gt;PDF Datasheet&lt;/a&gt;</description>
<gates>
<gate name="G$1" symbol="LTC3080"/>
</gates>
<devices>
<device name="" package="DFN8+OUT_3X3MM">
<connects>
<connect gate="G$1" pin="IN" pad="7 8"/>
<connect gate="G$1" pin="OUT" pad="1 2 3 OUT"/>
<connect gate="G$1" pin="SET" pad="4"/>
<connect gate="G$1" pin="VCONTROL" pad="5 6"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MCP14700">
<description>MCP14700

Asynchronous MOSFET driver, 5V

&lt;a href="http://ww1.microchip.com/downloads/en/DeviceDoc/22201B.pdf"&gt;PDF datasheet&lt;/a&gt;</description>
<gates>
<gate name="G$1" symbol="MCP14700"/>
</gates>
<devices>
<device name="" package="DFN8+OUT_3X3MM">
<connects>
<connect gate="G$1" pin="BOOT" pad="7"/>
<connect gate="G$1" pin="GND" pad="4 OUT"/>
<connect gate="G$1" pin="HI" pad="2"/>
<connect gate="G$1" pin="HIGHDR" pad="8"/>
<connect gate="G$1" pin="LO" pad="3"/>
<connect gate="G$1" pin="LOWDR" pad="5"/>
<connect gate="G$1" pin="PHASE" pad="1"/>
<connect gate="G$1" pin="VCC" pad="6"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
</devicesets>
</library>
</drawing>
</eagle>
