{"text_format":"3","workbook":"xls","n_sheets":3,"sheets":["Sheet1","Sheet2","Sheet3"],"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Sheet1","index":0,"n_rows":14,"n_cols":7,"rows_kept":14,"flags":["formulas_cached_only"]}
["Part","RS partno","Manufacturer partno","Value","Device","Package","Remarks"]
["724-3175","724-3175","RS 724-3175",{"$nulls":3},"buzzer"]
["DS1","532-6818","Displaytech 204A-CC-BC-3LP",{"$nulls":3},"lcd screen Blue/White, soldered with header 2.54 mm"]
["EC11E15244B2","729-5609","ALPS EC11E15244B2",{"$nulls":3},"20mm Vertical encoder 15 Pulses 30 DET"]
["EXP1","473-8349","TE connectivity 1-1634689-0",{"$nulls":3},"right angle!"]
["EXP2","473-8349","TE connectivity 1-1634689-0",{"$nulls":3},"right angle!"]
["HRS163_REVERSE","685-0788","Hirose DM1B-DSF-PEJ(82)"]
["R3","731-2883","Panasonic EVM3YSX50B14","10K"]
["RBEEP","708-6014",null,"440R",null,"0805"]
["RLED","721-9725 ",null,"68R",null,"1206"]
["SHIFT","483-6544P","NXP 74HC4050D","4050D",null,null,"levelshifter"]
["T4","294-312","Magnatec 2N3904","2N3904"]
[]
["JP1","not used"]

{"sheet":"Sheet2","index":1,"n_rows":0,"n_cols":0,"rows_kept":0,"flags":["formulas_cached_only"]}

{"sheet":"Sheet3","index":2,"n_rows":0,"n_cols":0,"rows_kept":0,"flags":["formulas_cached_only"]}