IFC building model
Schema: "IFC2X3"
Description: "ViewDefinition [CoordinationView]"
File name: "0001"
Time stamp: "2011-10-24T08:49:50"
Preprocessor: "Autodesk Revit MEP 2011 - 1.0"
Originating system: "20100903_2115(x64)"
Application: "Autodesk Revit MEP 2011" version "2011" identifier "Revit" by Organization "Autodesk Revit MEP 2011"

People and organizations
  Person "mjt" of Organization (no name given)
  Owner history of Person "mjt" of Organization (no name given) | application "Autodesk Revit MEP 2011" version "2011" identifier "Revit" by Organization "Autodesk Revit MEP 2011" | change NOCHANGE | created 0 (1970-01-01T00:00:00Z)

Units
  LENGTHUNIT: METRE
  AREAUNIT: SQUARE_METRE
  VOLUMEUNIT: CUBIC_METRE
  PLANEANGLEUNIT: DEGREE (conversion based)
  TIMEUNIT: SECOND

Spatial structure
IFCPROJECT "0001" | long name "Duplex Apartment" | phase "Designed"
  IFCSITE "Default" | latitude 41° 52′ 41.206054″ | longitude -87° 37′ 47.276″ | elevation above sea level -0.
    IFCBUILDING | postal address: "Enter address here", "Chicago", "IL", "USA"
      IFCBUILDINGSTOREY "Level 1" | elevation 0.
        contains 203 elements
          71 x IFCFLOWFITTING | type IFCPIPEFITTINGTYPE "Standard" | object type "Standard" | names: "M_Elbow - Generic:Standard:Standard:545367", "M_Elbow - Generic:Standard:Standard:546380", "M_Elbow - Generic:Standard:Standard:546395" (+68 more) | property sets: PSet_Revit_Dimensions, PSet_Revit_Mechanical, PSet_Revit_Other, PSet_Revit_Constraints, PSet_Revit_Graphics, PSet_Revit_Identity Data
          35 x IFCFLOWFITTING | type IFCPIPEFITTINGTYPE "Standard" | object type "Standard" | names: "M_Tee - Generic:Standard:Standard:546905", "M_Tee - Generic:Standard:Standard:547149", "M_Tee - Generic:Standard:Standard:547619" (+32 more) | property sets: PSet_Revit_Dimensions, PSet_Revit_Other, PSet_Revit_Mechanical, PSet_Revit_Constraints, PSet_Revit_Graphics, PSet_Revit_Identity Data
          73 x IFCFLOWSEGMENT | type IFCPIPESEGMENTTYPE "Pipe Types:Mechanical Pipe:540160" | object type "Pipe Types:Mechanical Pipe" | names: "Pipe Types:Mechanical Pipe:547487", "Pipe Types:Mechanical Pipe:547595", "Pipe Types:Mechanical Pipe:547742" (+70 more) | property sets: PSet_Revit_Mechanical, PSet_Revit_Dimensions, PSet_Revit_Identity Data, PSet_Revit_Other, PSet_Revit_Phasing, PSet_Revit_Constraints
          2 x IFCFLOWFITTING | type IFCPIPEFITTINGTYPE "Standard" | object type "Standard" | names: "M_Tee - Generic:Standard:Standard:547884", "M_Tee - Generic:Standard:Standard:557602" | property sets: PSet_Revit_Dimensions, PSet_Revit_Other, PSet_Revit_Mechanical, PSet_Revit_Constraints, PSet_Revit_Graphics, PSet_Revit_Identity Data
          1 x IFCFLOWFITTING | type IFCPIPEFITTINGTYPE "Standard" | object type "Standard" | names: "M_Elbow - Generic:Standard:Standard:550223" | property sets: PSet_Revit_Dimensions, PSet_Revit_Mechanical, PSet_Revit_Other, PSet_Revit_Constraints, PSet_Revit_Graphics, PSet_Revit_Identity Data
          1 x IFCFLOWFITTING | type IFCPIPEFITTINGTYPE "Standard" | object type "Standard" | names: "M_Tee - Generic:Standard:Standard:577990" | property sets: PSet_Revit_Dimensions, PSet_Revit_Other, PSet_Revit_Mechanical, PSet_Revit_Constraints, PSet_Revit_Graphics, PSet_Revit_Identity Data
          1 x IFCFLOWFITTING | type IFCPIPEFITTINGTYPE "Standard" | object type "Standard" | names: "M_Tee - Generic:Standard:Standard:578774" | property sets: PSet_Revit_Dimensions, PSet_Revit_Other, PSet_Revit_Mechanical, PSet_Revit_Constraints, PSet_Revit_Graphics, PSet_Revit_Identity Data
          1 x IFCFLOWFITTING | type IFCPIPEFITTINGTYPE "Standard" | object type "Standard" | names: "M_Elbow - Generic:Standard:Standard:580429" | property sets: PSet_Revit_Dimensions, PSet_Revit_Mechanical, PSet_Revit_Other, PSet_Revit_Constraints, PSet_Revit_Graphics, PSet_Revit_Identity Data
          1 x IFCFLOWFITTING | type IFCPIPEFITTINGTYPE "Standard" | object type "Standard" | names: "M_Elbow - Generic:Standard:Standard:600269" | property sets: PSet_Revit_Dimensions, PSet_Revit_Mechanical, PSet_Revit_Other, PSet_Revit_Constraints, PSet_Revit_Graphics, PSet_Revit_Identity Data
          1 x IFCFLOWFITTING | type IFCPIPEFITTINGTYPE "Standard" | object type "Standard" | names: "M_Elbow - Generic:Standard:Standard:600282" | property sets: PSet_Revit_Dimensions, PSet_Revit_Mechanical, PSet_Revit_Other, PSet_Revit_Constraints, PSet_Revit_Graphics, PSet_Revit_Identity Data
          1 x IFCFLOWFITTING | type IFCPIPEFITTINGTYPE "Standard" | object type "Standard" | names: "M_Elbow - Generic:Standard:Standard:600493" | property sets: PSet_Revit_Dimensions, PSet_Revit_Mechanical, PSet_Revit_Other, PSet_Revit_Constraints, PSet_Revit_Graphics, PSet_Revit_Identity Data
          1 x IFCFLOWFITTING | type IFCPIPEFITTINGTYPE "Standard" | object type "Standard" | names: "M_Elbow - Generic:Standard:Standard:600509" | property sets: PSet_Revit_Dimensions, PSet_Revit_Mechanical, PSet_Revit_Other, PSet_Revit_Constraints, PSet_Revit_Graphics, PSet_Revit_Identity Data
          1 x IFCFLOWFITTING | type IFCPIPEFITTINGTYPE "Standard" | object type "Standard" | names: "M_Elbow - Generic:Standard:Standard:600581" | property sets: PSet_Revit_Dimensions, PSet_Revit_Mechanical, PSet_Revit_Other, PSet_Revit_Constraints, PSet_Revit_Graphics, PSet_Revit_Identity Data
          2 x IFCFLOWFITTING | type IFCPIPEFITTINGTYPE "Standard" | object type "Standard" | names: "M_Elbow - Generic:Standard:Standard:600907", "M_Elbow - Generic:Standard:Standard:600922" | property sets: PSet_Revit_Dimensions, PSet_Revit_Mechanical, PSet_Revit_Other, PSet_Revit_Constraints, PSet_Revit_Graphics, PSet_Revit_Identity Data
          2 x IFCFLOWFITTING | type IFCPIPEFITTINGTYPE "Standard" | object type "Standard" | names: "M_Elbow - Generic:Standard:Standard:601021", "M_Elbow - Generic:Standard:Standard:601037" | property sets: PSet_Revit_Dimensions, PSet_Revit_Mechanical, PSet_Revit_Other, PSet_Revit_Constraints, PSet_Revit_Graphics, PSet_Revit_Identity Data
          1 x IFCFLOWFITTING | type IFCPIPEFITTINGTYPE "Standard" | object type "Standard" | names: "M_Elbow - Generic:Standard:Standard:601157" | property sets: PSet_Revit_Dimensions, PSet_Revit_Mechanical, PSet_Revit_Other, PSet_Revit_Constraints, PSet_Revit_Graphics, PSet_Revit_Identity Data
          1 x IFCFLOWFITTING | type IFCPIPEFITTINGTYPE "Standard" | object type "Standard" | names: "M_Tee - Generic:Standard:Standard:601285" | property sets: PSet_Revit_Dimensions, PSet_Revit_Other, PSet_Revit_Mechanical, PSet_Revit_Constraints, PSet_Revit_Graphics, PSet_Revit_Identity Data
          1 x IFCFLOWFITTING | type IFCPIPEFITTINGTYPE "Standard" | object type "Standard" | names: "M_Elbow - Generic:Standard:Standard:613017" | property sets: PSet_Revit_Dimensions, PSet_Revit_Mechanical, PSet_Revit_Other, PSet_Revit_Constraints, PSet_Revit_Graphics, PSet_Revit_Identity Data
          1 x IFCFLOWFITTING | type IFCPIPEFITTINGTYPE "Standard" | object type "Standard" | names: "M_Elbow - Generic:Standard:Standard:631338" | property sets: PSet_Revit_Dimensions, PSet_Revit_Mechanical, PSet_Revit_Other, PSet_Revit_Constraints, PSet_Revit_Graphics, PSet_Revit_Identity Data
          1 x IFCFLOWFITTING | type IFCPIPEFITTINGTYPE "Standard" | object type "Standard" | names: "M_Elbow - Generic:Standard:Standard:631971" | property sets: PSet_Revit_Dimensions, PSet_Revit_Mechanical, PSet_Revit_Other, PSet_Revit_Constraints, PSet_Revit_Graphics, PSet_Revit_Identity Data
          2 x IFCFLOWFITTING | type IFCPIPEFITTINGTYPE "Standard" | object type "Standard" | names: "M_Tee - Generic:Standard:Standard:632424", "M_Tee - Generic:Standard:Standard:632455" | property sets: PSet_Revit_Dimensions, PSet_Revit_Other, PSet_Revit_Mechanical, PSet_Revit_Constraints, PSet_Revit_Graphics, PSet_Revit_Identity Data
          1 x IFCFLOWFITTING | type IFCPIPEFITTINGTYPE "Standard" | object type "Standard" | names: "M_Elbow - Generic:Standard:Standard:632824" | property sets: PSet_Revit_Dimensions, PSet_Revit_Mechanical, PSet_Revit_Other, PSet_Revit_Constraints, PSet_Revit_Graphics, PSet_Revit_Identity Data
          1 x IFCFLOWFITTING | type IFCPIPEFITTINGTYPE "Standard" | object type "Standard" | names: "M_Elbow - Generic:Standard:Standard:633375" | property sets: PSet_Revit_Dimensions, PSet_Revit_Mechanical, PSet_Revit_Other, PSet_Revit_Constraints, PSet_Revit_Graphics, PSet_Revit_Identity Data
        IFCSPACE "A101" | long name "Foyer" | INTERNAL
        IFCSPACE "A102" | long name "Living Room" | INTERNAL
        IFCSPACE "A103" | long name "Kitchen" | INTERNAL
        IFCSPACE "B101" | long name "Foyer" | INTERNAL
        IFCSPACE "B102" | long name "Living Room" | INTERNAL
        IFCSPACE "B103" | long name "Kitchen" | INTERNAL
        IFCSPACE "B104" | long name "Bathroom 1" | INTERNAL
        IFCSPACE "B101" | long name "Foyer" | INTERNAL
          contains 6 elements
            2 x IFCENERGYCONVERSIONDEVICE | type IFCSPACEHEATERTYPE "25" | object type "25" | names: "M_Radiator - Hosted:25:25:557524", "M_Radiator - Hosted:25:25:632215" | property sets: PSet_Revit_Mechanical, PSet_Revit_Mechanical - Loads, PSet_Revit_Dimensions, PSet_Revit_Other, PSet_Revit_Constraints, PSet_Revit_Identity Data
            1 x IFCFLOWFITTING | type IFCPIPEFITTINGTYPE "Standard" | object type "Standard" | names: "M_Elbow - Generic:Standard:Standard:601051" | property sets: PSet_Revit_Dimensions, PSet_Revit_Mechanical, PSet_Revit_Other, PSet_Revit_Constraints, PSet_Revit_Graphics, PSet_Revit_Identity Data
            1 x IFCFLOWFITTING | type IFCPIPEFITTINGTYPE "Standard" | object type "Standard" | names: "M_Elbow - Generic:Standard:Standard:606628" | property sets: PSet_Revit_Dimensions, PSet_Revit_Mechanical, PSet_Revit_Other, PSet_Revit_Constraints, PSet_Revit_Graphics, PSet_Revit_Identity Data
            2 x IFCFLOWFITTING | type IFCPIPEFITTINGTYPE "Standard" | object type "Standard" | names: "M_Elbow - Generic:Standard:Standard:632430", "M_Elbow - Generic:Standard:Standard:632460" | property sets: PSet_Revit_Dimensions, PSet_Revit_Mechanical, PSet_Revit_Other, PSet_Revit_Constraints, PSet_Revit_Graphics, PSet_Revit_Identity Data
        IFCSPACE "B102" | long name "Living Room" | INTERNAL
          contains 6 elements
            2 x IFCENERGYCONVERSIONDEVICE | type IFCSPACEHEATERTYPE "25" | object type "25" | names: "M_Radiator - Hosted:25:25:557520", "M_Radiator - Hosted:25:25:632515" | property sets: PSet_Revit_Mechanical, PSet_Revit_Mechanical - Loads, PSet_Revit_Dimensions, PSet_Revit_Other, PSet_Revit_Constraints, PSet_Revit_Identity Data
            3 x IFCFLOWFITTING | type IFCPIPEFITTINGTYPE "Standard" | object type "Standard" | names: "M_Elbow - Generic:Standard:Standard:601283", "M_Elbow - Generic:Standard:Standard:632634", "M_Elbow - Generic:Standard:Standard:632768" | property sets: PSet_Revit_Dimensions, PSet_Revit_Mechanical, PSet_Revit_Other, PSet_Revit_Constraints, PSet_Revit_Graphics, PSet_Revit_Identity Data
            1 x IFCFLOWFITTING | type IFCPIPEFITTINGTYPE "Standard" | object type "Standard" | names: "M_Elbow - Generic:Standard:Standard:606592" | property sets: PSet_Revit_Dimensions, PSet_Revit_Mechanical, PSet_Revit_Other, PSet_Revit_Constraints, PSet_Revit_Graphics, PSet_Revit_Identity Data
        IFCSPACE "B103" | long name "Kitchen" | INTERNAL
        IFCSPACE "B104" | long name "Bathroom 1" | INTERNAL
          contains 1 element
            1 x IFCENERGYCONVERSIONDEVICE | type IFCSPACEHEATERTYPE "25" | object type "25" | names: "M_Radiator - Hosted:25:25:557620" | property sets: PSet_Revit_Mechanical, PSet_Revit_Mechanical - Loads, PSet_Revit_Dimensions, PSet_Revit_Other, PSet_Revit_Constraints, PSet_Revit_Identity Data
        IFCSPACE "A101" | long name "Foyer" | INTERNAL
          contains 4 elements
            2 x IFCENERGYCONVERSIONDEVICE | type IFCSPACEHEATERTYPE "25" | object type "25" | names: "M_Radiator - Hosted:25:25:538847", "M_Radiator - Hosted:25:25:629670" | property sets: PSet_Revit_Mechanical, PSet_Revit_Mechanical - Loads, PSet_Revit_Dimensions, PSet_Revit_Other, PSet_Revit_Constraints, PSet_Revit_Identity Data
            2 x IFCFLOWFITTING | type IFCPIPEFITTINGTYPE "Standard" | object type "Standard" | names: "M_Elbow - Generic:Standard:Standard:649438", "M_Elbow - Generic:Standard:Standard:649468" | property sets: PSet_Revit_Dimensions, PSet_Revit_Mechanical, PSet_Revit_Other, PSet_Revit_Constraints, PSet_Revit_Graphics, PSet_Revit_Identity Data
        IFCSPACE "A103" | long name "Kitchen" | INTERNAL
        IFCSPACE "A102" | long name "Living Room" | INTERNAL
          contains 4 elements
            2 x IFCENERGYCONVERSIONDEVICE | type IFCSPACEHEATERTYPE "25" | object type "25" | names: "M_Radiator - Hosted:25:25:536919", "M_Radiator - Hosted:25:25:630326" | property sets: PSet_Revit_Mechanical, PSet_Revit_Mechanical - Loads, PSet_Revit_Dimensions, PSet_Revit_Other, PSet_Revit_Constraints, PSet_Revit_Identity Data
            2 x IFCFLOWFITTING | type IFCPIPEFITTINGTYPE "Standard" | object type "Standard" | names: "M_Elbow - Generic:Standard:Standard:630850", "M_Elbow - Generic:Standard:Standard:631197" | property sets: PSet_Revit_Dimensions, PSet_Revit_Mechanical, PSet_Revit_Other, PSet_Revit_Constraints, PSet_Revit_Graphics, PSet_Revit_Identity Data
        IFCSPACE "A104" | long name "Bathroom 1" | INTERNAL
          contains 1 element
            1 x IFCENERGYCONVERSIONDEVICE | type IFCSPACEHEATERTYPE "25" | object type "25" | names: "M_Radiator - Hosted:25:25:548240" | property sets: PSet_Revit_Mechanical, PSet_Revit_Mechanical - Loads, PSet_Revit_Dimensions, PSet_Revit_Other, PSet_Revit_Constraints, PSet_Revit_Identity Data
      IFCBUILDINGSTOREY "Level 2" | elevation 3.100000000000205
        contains 204 elements
          167 x IFCFLOWSEGMENT | type IFCPIPESEGMENTTYPE "Pipe Types:Mechanical Pipe:540160" | object type "Pipe Types:Mechanical Pipe" | names: "Pipe Types:Mechanical Pipe:540160", "Pipe Types:Mechanical Pipe:540175", "Pipe Types:Mechanical Pipe:540182" (+164 more) | property sets: PSet_Revit_Mechanical, PSet_Revit_Dimensions, PSet_Revit_Identity Data, PSet_Revit_Other, PSet_Revit_Phasing, PSet_Revit_Constraints
          19 x IFCFLOWFITTING | type IFCPIPEFITTINGTYPE "Standard" | object type "Standard" | names: "M_Elbow - Generic:Standard:Standard:549664", "M_Elbow - Generic:Standard:Standard:549943", "M_Elbow - Generic:Standard:Standard:577810" (+16 more) | property sets: PSet_Revit_Dimensions, PSet_Revit_Mechanical, PSet_Revit_Other, PSet_Revit_Constraints, PSet_Revit_Graphics, PSet_Revit_Identity Data
          1 x IFCFLOWFITTING | type IFCPIPEFITTINGTYPE "Standard" | object type "Standard" | names: "M_Transition - Generic:Standard:Standard:550098" | property sets: PSet_Revit_Other, PSet_Revit_Dimensions, PSet_Revit_Mechanical, PSet_Revit_Constraints, PSet_Revit_Graphics, PSet_Revit_Identity Data
          1 x IFCFLOWFITTING | type IFCPIPEFITTINGTYPE "Standard" | object type "Standard" | names: "M_Transition - Generic:Standard:Standard:554027" | property sets: PSet_Revit_Other, PSet_Revit_Dimensions, PSet_Revit_Mechanical, PSet_Revit_Constraints, PSet_Revit_Graphics, PSet_Revit_Identity Data
          1 x IFCFLOWSEGMENT | type IFCDUCTSEGMENTTYPE "Round Duct:Taps:557534" | object type "Round Duct:Taps" | names: "Round Duct:Taps:557534" | property sets: PSet_Revit_Mechanical, PSet_Revit_Dimensions, PSet_Revit_Identity Data, PSet_Revit_Other, PSet_Revit_Phasing, PSet_Revit_Mechanical - Airflow
          1 x IFCFLOWFITTING | type IFCPIPEFITTINGTYPE "Standard" | object type "Standard" | names: "M_Tee - Generic:Standard:Standard:578229" | property sets: PSet_Revit_Dimensions, PSet_Revit_Other, PSet_Revit_Mechanical, PSet_Revit_Constraints, PSet_Revit_Graphics, PSet_Revit_Identity Data
          1 x IFCFLOWFITTING | type IFCPIPEFITTINGTYPE "Standard" | object type "Standard" | names: "M_Elbow - Generic:Standard:Standard:580397" | property sets: PSet_Revit_Dimensions, PSet_Revit_Mechanical, PSet_Revit_Other, PSet_Revit_Constraints, PSet_Revit_Graphics, PSet_Revit_Identity Data
          1 x IFCFLOWFITTING | type IFCPIPEFITTINGTYPE "Standard" | object type "Standard" | names: "M_Tee - Generic:Standard:Standard:580417" | property sets: PSet_Revit_Dimensions, PSet_Revit_Other, PSet_Revit_Mechanical, PSet_Revit_Constraints, PSet_Revit_Graphics, PSet_Revit_Identity Data
          1 x IFCFLOWFITTING | type IFCPIPEFITTINGTYPE "Standard" | object type "Standard" | names: "M_Transition - Generic:Standard:Standard:581027" | property sets: PSet_Revit_Other, PSet_Revit_Dimensions, PSet_Revit_Mechanical, PSet_Revit_Constraints, PSet_Revit_Graphics, PSet_Revit_Identity Data
          1 x IFCFLOWFITTING | type IFCPIPEFITTINGTYPE "Standard" | object type "Standard" | names: "M_Elbow - Generic:Standard:Standard:581029" | property sets: PSet_Revit_Dimensions, PSet_Revit_Mechanical, PSet_Revit_Other, PSet_Revit_Constraints, PSet_Revit_Graphics, PSet_Revit_Identity Data
          1 x IFCFLOWFITTING | type IFCPIPEFITTINGTYPE "Standard" | object type "Standard" | names: "M_Transition - Generic:Standard:Standard:581046" | property sets: PSet_Revit_Other, PSet_Revit_Dimensions, PSet_Revit_Mechanical, PSet_Revit_Constraints, PSet_Revit_Graphics, PSet_Revit_Identity Data
          4 x IFCFLOWSEGMENT | type IFCPIPESEGMENTTYPE "Pipe Types:Hot Water:583610" | object type "Pipe Types:Hot Water" | names: "Pipe Types:Hot Water:583610", "Pipe Types:Hot Water:583768", "Pipe Types:Hot Water:593619" (+1 more) | property sets: PSet_Revit_Mechanical, PSet_Revit_Dimensions, PSet_Revit_Identity Data, PSet_Revit_Other, PSet_Revit_Phasing, PSet_Revit_Constraints
          1 x IFCFLOWFITTING | type IFCPIPEFITTINGTYPE "Standard" | object type "Standard" | names: "M_Elbow - Generic:Standard:Standard:606821" | property sets: PSet_Revit_Dimensions, PSet_Revit_Mechanical, PSet_Revit_Other, PSet_Revit_Constraints, PSet_Revit_Graphics, PSet_Revit_Identity Data
          2 x IFCFLOWFITTING | type IFCPIPEFITTINGTYPE "Standard" | object type "Standard" | names: "M_Transition - Generic:Standard:Standard:661150", "M_Transition - Generic:Standard:Standard:661183" | property sets: PSet_Revit_Other, PSet_Revit_Dimensions, PSet_Revit_Mechanical, PSet_Revit_Constraints, PSet_Revit_Graphics, PSet_Revit_Identity Data
          1 x IFCFLOWFITTING | type IFCPIPEFITTINGTYPE "Standard" | object type "Standard" | names: "M_Transition - Generic:Standard:Standard:663179" | property sets: PSet_Revit_Other, PSet_Revit_Dimensions, PSet_Revit_Mechanical, PSet_Revit_Constraints, PSet_Revit_Graphics, PSet_Revit_Identity Data
          1 x IFCFLOWFITTING | type IFCPIPEFITTINGTYPE "Standard" | object type "Standard" | names: "M_Transition - Generic:Standard:Standard:663237" | property sets: PSet_Revit_Other, PSet_Revit_Dimensions, PSet_Revit_Mechanical, PSet_Revit_Constraints, PSet_Revit_Graphics, PSet_Revit_Identity Data
        IFCSPACE "A203" | long name "Bedroom 2" | INTERNAL
        IFCSPACE "B202" | long name "Bedroom 1" | INTERNAL
        IFCSPACE "A201" | long name "Hallway" | INTERNAL
        IFCSPACE "A202" | long name "Bedroom 1" | INTERNAL
        IFCSPACE "B203" | long name "Bedroom 2" | INTERNAL
        IFCSPACE "B201" | long name "Hallyway" | INTERNAL
        IFCSPACE "B204" | long name "Bathroom 2" | INTERNAL
        IFCSPACE "B205" | long name "Utility" | INTERNAL
        IFCSPACE "A204" | long name "Bathroom 2" | INTERNAL
        IFCSPACE "A205" | long name "Utility" | INTERNAL
        IFCSPACE "B203" | long name "Bedroom 2" | INTERNAL
          contains 6 elements
            2 x IFCENERGYCONVERSIONDEVICE | type IFCSPACEHEATERTYPE "25" | object type "25" | names: "M_Radiator - Hosted:25:25:557517", "M_Radiator - Hosted:25:25:633263" | property sets: PSet_Revit_Mechanical, PSet_Revit_Mechanical - Loads, PSet_Revit_Dimensions, PSet_Revit_Other, PSet_Revit_Constraints, PSet_Revit_Identity Data
            4 x IFCFLOWFITTING | type IFCPIPEFITTINGTYPE "Standard" | object type "Standard" | names: "M_Elbow - Generic:Standard:Standard:579415", "M_Elbow - Generic:Standard:Standard:606680", "M_Elbow - Generic:Standard:Standard:633346" (+1 more) | property sets: PSet_Revit_Dimensions, PSet_Revit_Mechanical, PSet_Revit_Other, PSet_Revit_Constraints, PSet_Revit_Graphics, PSet_Revit_Identity Data
        IFCSPACE "A202" | long name "Bedroom 1" | INTERNAL
          contains 3 elements
            1 x IFCENERGYCONVERSIONDEVICE | type IFCSPACEHEATERTYPE "25" | object type "25" | names: "M_Radiator - Hosted:25:25:538562" | property sets: PSet_Revit_Mechanical, PSet_Revit_Mechanical - Loads, PSet_Revit_Dimensions, PSet_Revit_Other, PSet_Revit_Constraints, PSet_Revit_Identity Data
            2 x IFCFLOWFITTING | type IFCPIPEFITTINGTYPE "Standard" | object type "Standard" | names: "M_Elbow - Generic:Standard:Standard:549727", "M_Elbow - Generic:Standard:Standard:606552" | property sets: PSet_Revit_Dimensions, PSet_Revit_Mechanical, PSet_Revit_Other, PSet_Revit_Constraints, PSet_Revit_Graphics, PSet_Revit_Identity Data
        IFCSPACE "B201" | long name "Hallway" | INTERNAL
          contains 1 element
            1 x IFCENERGYCONVERSIONDEVICE | type IFCSPACEHEATERTYPE "25" | object type "25" | names: "M_Radiator - Hosted:25:25:557519" | property sets: PSet_Revit_Mechanical, PSet_Revit_Mechanical - Loads, PSet_Revit_Dimensions, PSet_Revit_Other, PSet_Revit_Constraints, PSet_Revit_Identity Data
        IFCSPACE "B204" | long name "Bathroom 2" | INTERNAL
          contains 1 element
            1 x IFCENERGYCONVERSIONDEVICE | type IFCSPACEHEATERTYPE "25" | object type "25" | names: "M_Radiator - Hosted:25:25:557628" | property sets: PSet_Revit_Mechanical, PSet_Revit_Mechanical - Loads, PSet_Revit_Dimensions, PSet_Revit_Other, PSet_Revit_Constraints, PSet_Revit_Identity Data
        IFCSPACE "B205" | long name "Utility" | INTERNAL
          contains 17 elements
            1 x IFCENERGYCONVERSIONDEVICE | type IFCBOILERTYPE "147 kW" | object type "147 kW" | names: "M_Hot Water Boiler - 59-440 kW:147 kW:147 kW:557516" | property sets: PSet_Revit_Mechanical, PSet_Revit_Constraints, PSet_Revit_Electrical - Loads, PSet_Revit_Identity Data, PSet_Revit_Other, PSet_Revit_Phasing
            2 x IFCFLOWFITTING | type IFCPIPEFITTINGTYPE "Standard" | object type "Standard" | names: "M_Transition - Generic:Standard:Standard:579165", "M_Transition - Generic:Standard:Standard:584241" | property sets: PSet_Revit_Other, PSet_Revit_Dimensions, PSet_Revit_Mechanical, PSet_Revit_Constraints, PSet_Revit_Graphics, PSet_Revit_Identity Data
            2 x IFCFLOWCONTROLLER | type IFCVALVETYPE "50 mm" | object type "50 mm" | names: "M_Ball Valve - 50-150 mm:50 mm:50 mm:579237", "M_Ball Valve - 50-150 mm:50 mm:50 mm:579260" | property sets: PSet_Revit_Constraints, PSet_Revit_Mechanical, PSet_Revit_Graphics, PSet_Revit_Dimensions, PSet_Revit_Identity Data, PSet_Revit_Other
            2 x IFCFLOWFITTING | type IFCPIPEFITTINGTYPE "Standard" | object type "Standard" | names: "M_Transition - Generic:Standard:Standard:579263", "M_Transition - Generic:Standard:Standard:584239" | property sets: PSet_Revit_Other, PSet_Revit_Dimensions, PSet_Revit_Mechanical, PSet_Revit_Constraints, PSet_Revit_Graphics, PSet_Revit_Identity Data
            1 x IFCFLOWMOVINGDEVICE | type IFCPUMPTYPE "3.9 LPS - 0.8 Meter Head" | object type "3.9 LPS - 0.8 Meter Head" | names: "M_Inline Pump - Circulator:3.9 LPS - 0.8 Meter Head:3.9 LPS - 0.8 Meter Head:580717" | property sets: PSet_Revit_Mechanical, PSet_Revit_Constraints, PSet_Revit_Electrical - Loads, PSet_Revit_Identity Data, PSet_Revit_Other, PSet_Revit_Phasing
            1 x IFCFLOWFITTING | type IFCPIPEFITTINGTYPE "Standard" | object type "Standard" | names: "M_Elbow - Generic:Standard:Standard:581164" | property sets: PSet_Revit_Dimensions, PSet_Revit_Mechanical, PSet_Revit_Other, PSet_Revit_Constraints, PSet_Revit_Graphics, PSet_Revit_Identity Data
            3 x IFCFLOWFITTING | type IFCPIPEFITTINGTYPE "Standard" | object type "Standard" | names: "M_Elbow - Generic:Standard:Standard:584240", "M_Elbow - Generic:Standard:Standard:593346", "M_Elbow - Generic:Standard:Standard:696231" | property sets: PSet_Revit_Dimensions, PSet_Revit_Mechanical, PSet_Revit_Other, PSet_Revit_Constraints, PSet_Revit_Graphics, PSet_Revit_Identity Data
            2 x IFCFLOWCONTROLLER | type IFCVALVETYPE "25 mm" | object type "25 mm" | names: "M_Backflow Preventer_ DCW to Hydronic Supply_15-50 mm_:25 mm:25 mm:591225", "M_Backflow Preventer_ DCW to Hydronic Supply_15-50 mm_:25 mm:25 mm:593194" | property sets: PSet_Revit_Mechanical, PSet_Revit_Constraints, PSet_Revit_Graphics, PSet_Revit_Dimensions, PSet_Revit_Identity Data, PSet_Revit_Other
            2 x IFCFLOWFITTING | type IFCPIPEFITTINGTYPE "Standard" | object type "Standard" | names: "M_Tee - Generic:Standard:Standard:593348", "M_Tee - Generic:Standard:Standard:658559" | property sets: PSet_Revit_Dimensions, PSet_Revit_Other, PSet_Revit_Mechanical, PSet_Revit_Constraints, PSet_Revit_Graphics, PSet_Revit_Identity Data
            1 x IFCFLOWFITTING | type IFCPIPEFITTINGTYPE "Standard" | object type "Standard" | names: "M_Elbow - Generic:Standard:Standard:696282" | property sets: PSet_Revit_Dimensions, PSet_Revit_Mechanical, PSet_Revit_Other, PSet_Revit_Constraints, PSet_Revit_Graphics, PSet_Revit_Identity Data
        IFCSPACE "A204" | long name "Bathroom 2" | INTERNAL
          contains 1 element
            1 x IFCENERGYCONVERSIONDEVICE | type IFCSPACEHEATERTYPE "25" | object type "25" | names: "M_Radiator - Hosted:25:25:549304" | property sets: PSet_Revit_Mechanical, PSet_Revit_Mechanical - Loads, PSet_Revit_Dimensions, PSet_Revit_Other, PSet_Revit_Constraints, PSet_Revit_Identity Data
        IFCSPACE "A205" | long name "Utility" | INTERNAL
          contains 16 elements
            1 x IFCENERGYCONVERSIONDEVICE | type IFCBOILERTYPE "147 kW" | object type "147 kW" | names: "M_Hot Water Boiler - 59-440 kW:147 kW:147 kW:530072" | property sets: PSet_Revit_Mechanical, PSet_Revit_Constraints, PSet_Revit_Electrical - Loads, PSet_Revit_Identity Data, PSet_Revit_Other, PSet_Revit_Phasing
            1 x IFCFLOWMOVINGDEVICE | type IFCPUMPTYPE "3.9 LPS - 0.8 Meter Head" | object type "3.9 LPS - 0.8 Meter Head" | names: "M_Inline Pump - Circulator:3.9 LPS - 0.8 Meter Head:3.9 LPS - 0.8 Meter Head:550094" | property sets: PSet_Revit_Mechanical, PSet_Revit_Constraints, PSet_Revit_Electrical - Loads, PSet_Revit_Identity Data, PSet_Revit_Other, PSet_Revit_Phasing
            2 x IFCFLOWFITTING | type IFCPIPEFITTINGTYPE "Standard" | object type "Standard" | names: "M_Transition - Generic:Standard:Standard:578414", "M_Transition - Generic:Standard:Standard:578599" | property sets: PSet_Revit_Other, PSet_Revit_Dimensions, PSet_Revit_Mechanical, PSet_Revit_Constraints, PSet_Revit_Graphics, PSet_Revit_Identity Data
            2 x IFCFLOWCONTROLLER | type IFCVALVETYPE "50 mm" | object type "50 mm" | names: "M_Ball Valve - 50-150 mm:50 mm:50 mm:578433", "M_Ball Valve - 50-150 mm:50 mm:50 mm:578607" | property sets: PSet_Revit_Constraints, PSet_Revit_Mechanical, PSet_Revit_Graphics, PSet_Revit_Dimensions, PSet_Revit_Identity Data, PSet_Revit_Other
            4 x IFCFLOWFITTING | type IFCPIPEFITTINGTYPE "Standard" | object type "Standard" | names: "M_Elbow - Generic:Standard:Standard:578596", "M_Elbow - Generic:Standard:Standard:578598", "M_Elbow - Generic:Standard:Standard:594163" (+1 more) | property sets: PSet_Revit_Dimensions, PSet_Revit_Mechanical, PSet_Revit_Other, PSet_Revit_Constraints, PSet_Revit_Graphics, PSet_Revit_Identity Data
            2 x IFCFLOWFITTING | type IFCPIPEFITTINGTYPE "Standard" | object type "Standard" | names: "M_Transition - Generic:Standard:Standard:578610", "M_Transition - Generic:Standard:Standard:578611" | property sets: PSet_Revit_Other, PSet_Revit_Dimensions, PSet_Revit_Mechanical, PSet_Revit_Constraints, PSet_Revit_Graphics, PSet_Revit_Identity Data
            2 x IFCFLOWFITTING | type IFCPIPEFITTINGTYPE "Standard" | object type "Standard" | names: "M_Tee - Generic:Standard:Standard:593705", "M_Tee - Generic:Standard:Standard:661546" | property sets: PSet_Revit_Dimensions, PSet_Revit_Other, PSet_Revit_Mechanical, PSet_Revit_Constraints, PSet_Revit_Graphics, PSet_Revit_Identity Data
            2 x IFCFLOWCONTROLLER | type IFCVALVETYPE "25 mm" | object type "25 mm" | names: "M_Backflow Preventer_ DCW to Hydronic Supply_15-50 mm_:25 mm:25 mm:593973", "M_Backflow Preventer_ DCW to Hydronic Supply_15-50 mm_:25 mm:25 mm:594130" | property sets: PSet_Revit_Mechanical, PSet_Revit_Constraints, PSet_Revit_Graphics, PSet_Revit_Dimensions, PSet_Revit_Identity Data, PSet_Revit_Other
        IFCSPACE "A201" | long name "Hallway" | INTERNAL
          contains 3 elements
            1 x IFCENERGYCONVERSIONDEVICE | type IFCSPACEHEATERTYPE "25" | object type "25" | names: "M_Radiator - Hosted:25:25:536357" | property sets: PSet_Revit_Mechanical, PSet_Revit_Mechanical - Loads, PSet_Revit_Dimensions, PSet_Revit_Other, PSet_Revit_Constraints, PSet_Revit_Identity Data
            2 x IFCFLOWFITTING | type IFCPIPEFITTINGTYPE "Standard" | object type "Standard" | names: "M_Elbow - Generic:Standard:Standard:577875", "M_Elbow - Generic:Standard:Standard:606523" | property sets: PSet_Revit_Dimensions, PSet_Revit_Mechanical, PSet_Revit_Other, PSet_Revit_Constraints, PSet_Revit_Graphics, PSet_Revit_Identity Data
        IFCSPACE "A203" | long name "Bedroom 2" | INTERNAL
          contains 4 elements
            2 x IFCENERGYCONVERSIONDEVICE | type IFCSPACEHEATERTYPE "25" | object type "25" | names: "M_Radiator - Hosted:25:25:535063", "M_Radiator - Hosted:25:25:631726" | property sets: PSet_Revit_Mechanical, PSet_Revit_Mechanical - Loads, PSet_Revit_Dimensions, PSet_Revit_Other, PSet_Revit_Constraints, PSet_Revit_Identity Data
            2 x IFCFLOWFITTING | type IFCPIPEFITTINGTYPE "Standard" | object type "Standard" | names: "M_Elbow - Generic:Standard:Standard:631907", "M_Elbow - Generic:Standard:Standard:631992" | property sets: PSet_Revit_Dimensions, PSet_Revit_Mechanical, PSet_Revit_Other, PSet_Revit_Constraints, PSet_Revit_Graphics, PSet_Revit_Identity Data
        IFCSPACE "B202" | long name "Bedroom 1" | INTERNAL
          contains 1 element
            1 x IFCENERGYCONVERSIONDEVICE | type IFCSPACEHEATERTYPE "25" | object type "25" | names: "M_Radiator - Hosted:25:25:557522" | property sets: PSet_Revit_Mechanical, PSet_Revit_Mechanical - Loads, PSet_Revit_Dimensions, PSet_Revit_Other, PSet_Revit_Constraints, PSet_Revit_Identity Data
      IFCBUILDINGSTOREY "Roof" | elevation 6.000000000000207
        contains 3 elements
          2 x IFCFLOWFITTING | type IFCDUCTFITTINGTYPE "45 Degree" | object type "45 Degree" | names: "M_Rectangular to Round Transition - Angle:45 Degree:45 Degree:602990", "M_Rectangular to Round Transition - Angle:45 Degree:45 Degree:603490" | property sets: PSet_Revit_Other, PSet_Revit_Dimensions, PSet_Revit_Mechanical, PSet_Revit_Constraints, PSet_Revit_Graphics, PSet_Revit_Identity Data
          1 x IFCFLOWSEGMENT | type IFCDUCTSEGMENTTYPE "Round Duct:Taps:557534" | object type "Round Duct:Taps" | names: "Round Duct:Taps:603399" | property sets: PSet_Revit_Mechanical, PSet_Revit_Dimensions, PSet_Revit_Identity Data, PSet_Revit_Other, PSet_Revit_Phasing, PSet_Revit_Mechanical - Airflow
        IFCSPACE "A/B" | long name "Roof" | INTERNAL
          contains 2 elements
            2 x IFCFLOWMOVINGDEVICE | type IFCFANTYPE "991-1905 LPS" | object type "991-1905 LPS" | names: "M_Centrifugal Fan - Rooftop - Upblast:991-1905 LPS:991-1905 LPS:602113", "M_Centrifugal Fan - Rooftop - Upblast:991-1905 LPS:991-1905 LPS:602396" | property sets: PSet_Revit_Mechanical, PSet_Revit_Mechanical - Airflow, PSet_Revit_Other, PSet_Revit_Constraints, PSet_Revit_Electrical - Loads, PSet_Revit_Identity Data
        IFCSPACE "A/B" | long name "Roof" | INTERNAL

Types
  IFCPIPEFITTINGTYPE "Standard" | element type "Standard" | 116 occurrences
  IFCPIPEFITTINGTYPE "Standard" | element type "Standard" | 40 occurrences
  IFCPIPESEGMENTTYPE "Pipe Types:Mechanical Pipe:540160" | element type "Pipe Types:Mechanical Pipe:540160" | 240 occurrences
  IFCPIPEFITTINGTYPE "Standard" | element type "Standard" | 2 occurrences
  IFCPIPEFITTINGTYPE "Standard" | element type "Standard" | 1 occurrence
  IFCPIPEFITTINGTYPE "Standard" | element type "Standard" | 1 occurrence
  IFCPIPEFITTINGTYPE "Standard" | element type "Standard" | 1 occurrence
  IFCPIPEFITTINGTYPE "Standard" | element type "Standard" | 1 occurrence
  IFCPIPEFITTINGTYPE "Standard" | element type "Standard" | 1 occurrence
  IFCPIPEFITTINGTYPE "Standard" | element type "Standard" | 1 occurrence
  IFCPIPEFITTINGTYPE "Standard" | element type "Standard" | 1 occurrence
  IFCPIPEFITTINGTYPE "Standard" | element type "Standard" | 1 occurrence
  IFCPIPEFITTINGTYPE "Standard" | element type "Standard" | 1 occurrence
  IFCPIPEFITTINGTYPE "Standard" | element type "Standard" | 2 occurrences
  IFCPIPEFITTINGTYPE "Standard" | element type "Standard" | 2 occurrences
  IFCPIPEFITTINGTYPE "Standard" | element type "Standard" | 1 occurrence
  IFCPIPEFITTINGTYPE "Standard" | element type "Standard" | 1 occurrence
  IFCPIPEFITTINGTYPE "Standard" | element type "Standard" | 1 occurrence
  IFCPIPEFITTINGTYPE "Standard" | element type "Standard" | 1 occurrence
  IFCPIPEFITTINGTYPE "Standard" | element type "Standard" | 1 occurrence
  IFCPIPEFITTINGTYPE "Standard" | element type "Standard" | 2 occurrences
  IFCPIPEFITTINGTYPE "Standard" | element type "Standard" | 1 occurrence
  IFCPIPEFITTINGTYPE "Standard" | element type "Standard" | 1 occurrence
  IFCSPACEHEATERTYPE "25" | element type "25" | USERDEFINED | 6 occurrences
  IFCPIPEFITTINGTYPE "Standard" | element type "Standard" | 1 occurrence
  IFCPIPEFITTINGTYPE "Standard" | element type "Standard" | 1 occurrence
  IFCSPACEHEATERTYPE "25" | element type "25" | USERDEFINED | 4 occurrences
  IFCPIPEFITTINGTYPE "Standard" | element type "Standard" | 1 occurrence
  IFCSPACEHEATERTYPE "25" | element type "25" | USERDEFINED | 1 occurrence
  IFCSPACEHEATERTYPE "25" | element type "25" | USERDEFINED | 1 occurrence
  IFCPIPEFITTINGTYPE "Standard" | element type "Standard" | 1 occurrence
  IFCPIPEFITTINGTYPE "Standard" | element type "Standard" | 1 occurrence
  IFCDUCTSEGMENTTYPE "Round Duct:Taps:557534" | element type "Round Duct:Taps:557534" | 2 occurrences
  IFCPIPEFITTINGTYPE "Standard" | element type "Standard" | 1 occurrence
  IFCPIPEFITTINGTYPE "Standard" | element type "Standard" | 1 occurrence
  IFCPIPEFITTINGTYPE "Standard" | element type "Standard" | 1 occurrence
  IFCPIPEFITTINGTYPE "Standard" | element type "Standard" | 1 occurrence
  IFCPIPEFITTINGTYPE "Standard" | element type "Standard" | 5 occurrences
  IFCPIPESEGMENTTYPE "Pipe Types:Hot Water:583610" | element type "Pipe Types:Hot Water:583610" | 4 occurrences
  IFCPIPEFITTINGTYPE "Standard" | element type "Standard" | 1 occurrence
  IFCPIPEFITTINGTYPE "Standard" | element type "Standard" | 2 occurrences
  IFCPIPEFITTINGTYPE "Standard" | element type "Standard" | 5 occurrences
  IFCPIPEFITTINGTYPE "Standard" | element type "Standard" | 1 occurrence
  IFCSPACEHEATERTYPE "25" | element type "25" | USERDEFINED | 4 occurrences
  IFCSPACEHEATERTYPE "25" | element type "25" | USERDEFINED | 2 occurrences
  IFCSPACEHEATERTYPE "25" | element type "25" | USERDEFINED | 1 occurrence
  IFCBOILERTYPE "147 kW" | element type "147 kW" | WATER | 2 occurrences
  IFCVALVETYPE "50 mm" | element type "50 mm" | ISOLATING | 4 occurrences
  IFCPUMPTYPE "3.9 LPS - 0.8 Meter Head" | element type "3.9 LPS - 0.8 Meter Head" | CIRCULATOR | 2 occurrences
  IFCPIPEFITTINGTYPE "Standard" | element type "Standard" | 1 occurrence
  IFCVALVETYPE "25 mm" | element type "25 mm" | DOUBLECHECK | 4 occurrences
  IFCPIPEFITTINGTYPE "Standard" | element type "Standard" | 1 occurrence
  IFCSPACEHEATERTYPE "25" | element type "25" | USERDEFINED | 1 occurrence
  IFCDUCTFITTINGTYPE "45 Degree" | element type "45 Degree" | 2 occurrences
  IFCFANTYPE "991-1905 LPS" | element type "991-1905 LPS" | VANEAXIAL | 2 occurrences

Property sets
  GSA Space Areas | quantities | on 2 objects (2 IFCSPACE)
    GSA BIM Area = 22.04323199999996 [SQUARE_METRE]
  GSA Space Areas | quantities | on 2 objects (2 IFCSPACE)
    GSA BIM Area = 26.17799424999996 [SQUARE_METRE]
  GSA Space Areas | quantities | on 2 objects (2 IFCSPACE)
    GSA BIM Area = 135.1511559999993 [SQUARE_METRE]
  GSA Space Areas | quantities | on 1 object (1 IFCSPACE)
    GSA BIM Area = 22.04323199999979 [SQUARE_METRE]
  GSA Space Areas | quantities | on 1 object (1 IFCSPACE)
    GSA BIM Area = 10.41449999999989 [SQUARE_METRE]
  GSA Space Areas | quantities | on 1 object (1 IFCSPACE)
    GSA BIM Area = 22.04323199999995 [SQUARE_METRE]
  GSA Space Areas | quantities | on 1 object (1 IFCSPACE)
    GSA BIM Area = 10.41449999999997 [SQUARE_METRE]
  GSA Space Areas | quantities | on 1 object (1 IFCSPACE)
    GSA BIM Area = 4.754957996050097 [SQUARE_METRE]
  GSA Space Areas: 26 more contents on 26 objects not shown
  Pset_SpaceCommon | properties | on 37 objects (37 IFCSPACE)
    Reference = "" (IFCLABEL)
  PSet_Revit_Identity Data | properties | on 2 objects (2 IFCFLOWSEGMENT)
    Mark = "5" (IFCLABEL)
  PSet_Revit_Identity Data | properties | on 2 objects (2 IFCFLOWSEGMENT)
    Mark = "8" (IFCLABEL)
  PSet_Revit_Identity Data | properties | on 2 objects (1 IFCFLOWFITTING, 1 IFCFLOWSEGMENT)
    Mark = "351" (IFCLABEL)
  PSet_Revit_Identity Data | properties | on 2 objects (1 IFCFLOWFITTING, 1 IFCFLOWSEGMENT)
    Mark = "372" (IFCLABEL)
  PSet_Revit_Identity Data | properties | on 2 objects (1 IFCFLOWFITTING, 1 IFCFLOWSEGMENT)
    Mark = "483" (IFCLABEL)
  PSet_Revit_Identity Data | properties | on 2 objects (1 IFCFLOWFITTING, 1 IFCFLOWSEGMENT)
    Mark = "521" (IFCLABEL)
  PSet_Revit_Identity Data | properties | on 2 objects (1 IFCFLOWFITTING, 1 IFCFLOWSEGMENT)
    Mark = "540" (IFCLABEL)
  PSet_Revit_Identity Data | properties | on 2 objects (1 IFCFLOWFITTING, 1 IFCFLOWSEGMENT)
    Mark = "544" (IFCLABEL)
  PSet_Revit_Identity Data: 502 more contents on 511 objects not shown
  PSet_Revit_Constraints | properties | on 12 objects (12 IFCFLOWSEGMENT)
    End Offset = 0.1778 (IFCLENGTHMEASURE) [METRE]
    Horizontal Justification = 0 (IFCINTEGER)
    Offset = 0.1778 (IFCLENGTHMEASURE) [METRE]
    Reference Level = "Level 1" (IFCLABEL)
    Slope = 0. (IFCREAL)
    Start Offset = 0.1778 (IFCLENGTHMEASURE) [METRE]
    Vertical Justification = 0 (IFCINTEGER)
  PSet_Revit_Constraints | properties | on 11 objects (11 IFCFLOWSEGMENT)
    End Offset = 0.1777999999999764 (IFCLENGTHMEASURE) [METRE]
    Horizontal Justification = 0 (IFCINTEGER)
    Offset = 0.1777999999999764 (IFCLENGTHMEASURE) [METRE]
    Reference Level = "Level 2" (IFCLABEL)
    Slope = 0. (IFCREAL)
    Start Offset = 0.1777999999999764 (IFCLENGTHMEASURE) [METRE]
    Vertical Justification = 0 (IFCINTEGER)
  PSet_Revit_Constraints | properties | on 11 objects (11 IFCFLOWSEGMENT)
    End Offset = -0.4412404168723878 (IFCLENGTHMEASURE) [METRE]
    Horizontal Justification = 0 (IFCINTEGER)
    Offset = -0.4412404168723878 (IFCLENGTHMEASURE) [METRE]
    Reference Level = "Level 2" (IFCLABEL)
    Slope = 0. (IFCREAL)
    Start Offset = -0.4412404168723878 (IFCLENGTHMEASURE) [METRE]
    Vertical Justification = 0 (IFCINTEGER)
  PSet_Revit_Constraints | properties | on 10 objects (10 IFCSPACE)
    Base Offset = 0. (IFCLENGTHMEASURE) [METRE]
    Level = "Level 2" (IFCLABEL)
    Limit Offset = 4.000000000000001 (IFCLENGTHMEASURE) [METRE]
    Upper Limit = "Level 2" (IFCLABEL)
  PSet_Revit_Constraints | properties | on 10 objects (10 IFCSPACE)
    Base Offset = 0. (IFCLENGTHMEASURE) [METRE]
    Level = "Level 2" (IFCLABEL)
    Limit Offset = 0. (IFCLENGTHMEASURE) [METRE]
    Upper Limit = "Roof" (IFCLABEL)
  PSet_Revit_Constraints | properties | on 10 objects (10 IFCFLOWFITTING)
    Host = "Level : Level 1" (IFCLABEL)
    Level = "Level 1" (IFCLABEL)
    Offset = 0.1778 (IFCLENGTHMEASURE) [METRE]
  PSet_Revit_Constraints | properties | on 8 objects (8 IFCSPACE)
    Base Offset = 0. (IFCLENGTHMEASURE) [METRE]
    Level = "Level 1" (IFCLABEL)
    Limit Offset = 2.530131081845663 (IFCLENGTHMEASURE) [METRE]
    Upper Limit = "Level 1" (IFCLABEL)
  PSet_Revit_Constraints | properties | on 7 objects (7 IFCSPACE)
    Base Offset = 0. (IFCLENGTHMEASURE) [METRE]
    Level = "Level 1" (IFCLABEL)
    Limit Offset = 4.000000000000001 (IFCLENGTHMEASURE) [METRE]
    Upper Limit = "Level 1" (IFCLABEL)
  PSet_Revit_Constraints: 353 more contents on 448 objects not shown
  PSet_Revit_Dimensions | properties | on 116 objects (116 IFCFLOWFITTING)
    Angle = 90. (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
    Center to End = 0.06770833333333323 (IFCREAL)
    Fitting Outside Diameter = 0.09375000000000001 (IFCREAL)
    Insulation Radius = 0.04687500000000001 (IFCREAL)
    Nominal Diameter = 0.08202099737532809 (IFCREAL)
    Nominal Radius = 0.04101049868766404 (IFCREAL)
    Size = "25 mmø-25 mmø" (IFCLABEL)
    Tick Size = 0.03749999999999994 (IFCREAL)
  PSet_Revit_Dimensions | properties | on 40 objects (40 IFCFLOWFITTING)
    Angle = 90. (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
    Center to End = 0.08854166666666667 (IFCREAL)
    Fitting Outside Diameter = 0.09375000000000001 (IFCREAL)
    Insulation Radius = 0.04687500000000001 (IFCREAL)
    Nominal Diameter = 0.08202099737532809 (IFCREAL)
    Nominal Radius = 0.04101049868766404 (IFCREAL)
    Size = "25 mmø-25 mmø-25 mmø" (IFCLABEL)
    Tick Size = 0.03750000000000001 (IFCREAL)
  PSet_Revit_Dimensions | properties | on 6 objects (6 IFCENERGYCONVERSIONDEVICE)
    Length = 1. (IFCLENGTHMEASURE) [METRE]
  PSet_Revit_Dimensions | properties | on 6 objects (6 IFCFLOWFITTING)
    Fitting Outside Diameter 1 = 0.1770833333333333 (IFCREAL)
    Fitting Outside Diameter 2 = 0.09375000000000001 (IFCREAL)
    Insulation Radius 1 = 0.08854166666666667 (IFCREAL)
    Insulation Radius 2 = 0.04687500000000001 (IFCREAL)
    Length = 0.04427083333333334 (IFCREAL)
    Nominal Diameter 1 = 0.1640419947506562 (IFCREAL)
    Nominal Diameter 2 = 0.08202099737532809 (IFCREAL)
    Nominal Radius 1 = 0.08202099737532809 (IFCREAL)
    Nominal Radius 2 = 0.04101049868766404 (IFCREAL)
    OffsetHeight = 0.08202099737532809 (IFCREAL)
    OffsetWidth = 0.08202099737532809 (IFCREAL)
    Size = "50 mmø-25 mmø" (IFCLABEL)
    Tick Size 1 = 0.07083333333333335 (IFCREAL)
    Tick Size 2 = 0.03750000000000001 (IFCREAL)
  PSet_Revit_Dimensions | properties | on 4 objects (4 IFCENERGYCONVERSIONDEVICE)
    Length = 1.15 (IFCLENGTHMEASURE) [METRE]
  PSet_Revit_Dimensions | properties | on 4 objects (4 IFCENERGYCONVERSIONDEVICE)
    Length = 1.36 (IFCLENGTHMEASURE) [METRE]
  PSet_Revit_Dimensions | properties | on 4 objects (4 IFCENERGYCONVERSIONDEVICE)
    Length = 0.4999999999999999 (IFCLENGTHMEASURE) [METRE]
  PSet_Revit_Dimensions | properties | on 4 objects (4 IFCFLOWFITTING)
    Fitting Outside Diameter 1 = 0.1770833333333333 (IFCREAL)
    Fitting Outside Diameter 2 = 0.09375000000000001 (IFCREAL)
    Insulation Radius 1 = 0.08854166666666667 (IFCREAL)
    Insulation Radius 2 = 0.04687500000000001 (IFCREAL)
    Length = 0.04427083333333334 (IFCREAL)
    Nominal Diameter 1 = 0.1312335958005249 (IFCREAL)
    Nominal Diameter 2 = 0.08202099737532809 (IFCREAL)
    Nominal Radius 1 = 0.06561679790026247 (IFCREAL)
    Nominal Radius 2 = 0.04101049868766404 (IFCREAL)
    OffsetHeight = 0.06561679790026247 (IFCREAL)
    OffsetWidth = 0.06561679790026247 (IFCREAL)
    Size = "40 mmø-25 mmø" (IFCLABEL)
    Tick Size 1 = 0.07083333333333335 (IFCREAL)
    Tick Size 2 = 0.03750000000000001 (IFCREAL)
  PSet_Revit_Dimensions: 317 more contents on 334 objects not shown
  PSet_Revit_Phasing | properties | on 487 objects (246 IFCFLOWSEGMENT, 207 IFCFLOWFITTING, 22 IFCENERGYCONVERSIONDEVICE, 8 IFCFLOWCONTROLLER)
    Phase Created = "New Construction" (IFCLABEL)
  PSet_Revit_Phasing | properties | on 37 objects (37 IFCSPACE)
    Phase = "New Construction" (IFCLABEL)
  PSet_Revit_Energy Analysis | properties | on 2 objects (2 IFCSPACE)
    Condition Type = 2 (IFCINTEGER)
    Design Cooling Load = 0. (IFCREAL)
    Design Heating Load = 0. (IFCREAL)
    Occupiable = TRUE (IFCBOOLEAN)
    Plenum = FALSE (IFCBOOLEAN)
    Space Type = -1 (IFCINTEGER)
    Zone = "4" (IFCLABEL)
  PSet_Revit_Energy Analysis | properties | on 1 object (1 IFCSPACE)
    Calculated Cooling Load = 16389.14694919201 (IFCREAL)
    Calculated Heating Load = 36276.034800122 (IFCREAL)
    Condition Type = 2 (IFCINTEGER)
    Design Cooling Load = 16389.14694919201 (IFCREAL)
    Design Heating Load = 36276.034800122 (IFCREAL)
    Occupiable = TRUE (IFCBOOLEAN)
    Plenum = FALSE (IFCBOOLEAN)
    Space Type = -1 (IFCINTEGER)
    Zone = "4" (IFCLABEL)
  PSet_Revit_Energy Analysis | properties | on 1 object (1 IFCSPACE)
    Calculated Cooling Load = 19390.84917587349 (IFCREAL)
    Calculated Heating Load = 34898.28105790762 (IFCREAL)
    Condition Type = 2 (IFCINTEGER)
    Design Cooling Load = 19390.84917587349 (IFCREAL)
    Design Heating Load = 34898.28105790762 (IFCREAL)
    Occupiable = TRUE (IFCBOOLEAN)
    Plenum = FALSE (IFCBOOLEAN)
    Space Type = -1 (IFCINTEGER)
    Zone = "3" (IFCLABEL)
  PSet_Revit_Energy Analysis | properties | on 1 object (1 IFCSPACE)
    Calculated Cooling Load = 6091.152056153079 (IFCREAL)
    Calculated Heating Load = 12084.35857815326 (IFCREAL)
    Condition Type = 2 (IFCINTEGER)
    Design Cooling Load = 6091.152056153079 (IFCREAL)
    Design Heating Load = 12084.35857815326 (IFCREAL)
    Occupiable = TRUE (IFCBOOLEAN)
    Plenum = FALSE (IFCBOOLEAN)
    Space Type = -1 (IFCINTEGER)
    Zone = "4" (IFCLABEL)
  PSet_Revit_Energy Analysis | properties | on 1 object (1 IFCSPACE)
    Calculated Cooling Load = 14770.5344334791 (IFCREAL)
    Calculated Heating Load = 34898.28105790775 (IFCREAL)
    Condition Type = 2 (IFCINTEGER)
    Design Cooling Load = 14770.5344334791 (IFCREAL)
    Design Heating Load = 34898.28105790775 (IFCREAL)
    Occupiable = TRUE (IFCBOOLEAN)
    Plenum = FALSE (IFCBOOLEAN)
    Space Type = -1 (IFCINTEGER)
    Zone = "4" (IFCLABEL)
  PSet_Revit_Energy Analysis | properties | on 1 object (1 IFCSPACE)
    Calculated Cooling Load = 15885.35419707831 (IFCREAL)
    Calculated Heating Load = 36280.93042062399 (IFCREAL)
    Condition Type = 2 (IFCINTEGER)
    Design Cooling Load = 15885.35419707831 (IFCREAL)
    Design Heating Load = 36280.93042062399 (IFCREAL)
    Occupiable = TRUE (IFCBOOLEAN)
    Plenum = FALSE (IFCBOOLEAN)
    Space Type = -1 (IFCINTEGER)
    Zone = "3" (IFCLABEL)
  PSet_Revit_Energy Analysis | properties | on 1 object (1 IFCSPACE)
    Calculated Cooling Load = 5726.726275379966 (IFCREAL)
    Calculated Heating Load = 12084.35857815329 (IFCREAL)
    Condition Type = 2 (IFCINTEGER)
    Design Cooling Load = 5726.726275379966 (IFCREAL)
    Design Heating Load = 12084.35857815329 (IFCREAL)
    Occupiable = TRUE (IFCBOOLEAN)
    Plenum = FALSE (IFCBOOLEAN)
    Space Type = -1 (IFCINTEGER)
    Zone = "3" (IFCLABEL)
  PSet_Revit_Energy Analysis | properties | on 1 object (1 IFCSPACE)
    Calculated Cooling Load = 1888.976817960332 (IFCREAL)
    Calculated Heating Load = 3020.338669750679 (IFCREAL)
    Condition Type = 2 (IFCINTEGER)
    Design Cooling Load = 1888.976817960332 (IFCREAL)
    Design Heating Load = 3020.338669750679 (IFCREAL)
    Occupiable = TRUE (IFCBOOLEAN)
    Plenum = FALSE (IFCBOOLEAN)
    Space Type = -1 (IFCINTEGER)
    Zone = "3" (IFCLABEL)
  PSet_Revit_Energy Analysis: 9 more contents on 9 objects not shown
  PSet_Revit_Mechanical - Airflow | properties | on 3 objects (3 IFCSPACE)
    Actual Exhaust Airflow = 0. (IFCREAL)
    Actual Return Airflow = 0. (IFCREAL)
    Actual Supply Airflow = 0. (IFCREAL)
    Return Airflow = 0 (IFCINTEGER)
    Specified Exhaust Airflow = 0. (IFCREAL)
    Specified Return Airflow = 0. (IFCREAL)
    Specified Supply Airflow = 0. (IFCREAL)
  PSet_Revit_Mechanical - Airflow | properties | on 2 objects (2 IFCFLOWSEGMENT)
    Additional Flow = 0. (IFCREAL)
    Flow = 0.1412586668859543 (IFCREAL)
    Friction = 7.721539245935043E-005 (IFCREAL)
    Pressure Drop = 0.0005433957244924869 (IFCREAL)
    Reynolds number = 1357.404684647311 (IFCREAL)
    Velocity = 0.2673468860336302 (IFCREAL)
    Velocity Pressure = 0.001216988156416308 (IFCREAL)
  PSet_Revit_Mechanical - Airflow | properties | on 2 objects (2 IFCFLOWMOVINGDEVICE)
    Air Flow = 1.341957335416566 (IFCREAL)
  PSet_Revit_Mechanical - Airflow | properties | on 1 object (1 IFCSPACE)
    Actual Exhaust Airflow = 0. (IFCREAL)
    Actual Return Airflow = 0. (IFCREAL)
    Actual Supply Airflow = 0. (IFCREAL)
    Calculated Supply Airflow = 2.785395577453438 (IFCREAL)
    Return Airflow = 0 (IFCINTEGER)
    Specified Exhaust Airflow = 0. (IFCREAL)
    Specified Return Airflow = 0. (IFCREAL)
    Specified Supply Airflow = 2.785395577453438 (IFCREAL)
  PSet_Revit_Mechanical - Airflow | properties | on 1 object (1 IFCSPACE)
    Actual Exhaust Airflow = 0. (IFCREAL)
    Actual Return Airflow = 0. (IFCREAL)
    Actual Supply Airflow = 0. (IFCREAL)
    Calculated Supply Airflow = 3.295545869774962 (IFCREAL)
    Return Airflow = 0 (IFCINTEGER)
    Specified Exhaust Airflow = 0. (IFCREAL)
    Specified Return Airflow = 0. (IFCREAL)
    Specified Supply Airflow = 3.295545869774962 (IFCREAL)
  PSet_Revit_Mechanical - Airflow | properties | on 1 object (1 IFCSPACE)
    Actual Exhaust Airflow = 0. (IFCREAL)
    Actual Return Airflow = 0. (IFCREAL)
    Actual Supply Airflow = 0. (IFCREAL)
    Calculated Supply Airflow = 1.035213611263742 (IFCREAL)
    Return Airflow = 0 (IFCINTEGER)
    Specified Exhaust Airflow = 0. (IFCREAL)
    Specified Return Airflow = 0. (IFCREAL)
    Specified Supply Airflow = 1.035213611263742 (IFCREAL)
  PSet_Revit_Mechanical - Airflow | properties | on 1 object (1 IFCSPACE)
    Actual Exhaust Airflow = 0. (IFCREAL)
    Actual Return Airflow = 0. (IFCREAL)
    Actual Supply Airflow = 0. (IFCREAL)
    Calculated Supply Airflow = 2.510306449455852 (IFCREAL)
    Return Airflow = 0 (IFCINTEGER)
    Specified Exhaust Airflow = 0. (IFCREAL)
    Specified Return Airflow = 0. (IFCREAL)
    Specified Supply Airflow = 2.510306449455852 (IFCREAL)
  PSet_Revit_Mechanical - Airflow | properties | on 1 object (1 IFCSPACE)
    Actual Exhaust Airflow = 0. (IFCREAL)
    Actual Return Airflow = 0. (IFCREAL)
    Actual Supply Airflow = 0. (IFCREAL)
    Calculated Supply Airflow = 2.699774153224291 (IFCREAL)
    Return Airflow = 0 (IFCINTEGER)
    Specified Exhaust Airflow = 0. (IFCREAL)
    Specified Return Airflow = 0. (IFCREAL)
    Specified Supply Airflow = 2.699774153224291 (IFCREAL)
  PSet_Revit_Mechanical - Airflow: 10 more contents on 10 objects not shown
  PSet_Revit_Electrical - Loads | properties | on 18 objects (18 IFCSPACE)
    Design HVAC Load per area = 0. (IFCREAL)
    Design Other Load per area = 0. (IFCREAL)
  PSet_Revit_Electrical - Loads | properties | on 6 objects (4 IFCFLOWMOVINGDEVICE, 2 IFCENERGYCONVERSIONDEVICE)
    Circuit Number = "<unnamed>" (IFCLABEL)
    Panel = "" (IFCLABEL)
  PSet_Revit_Electrical - Lighting | properties | on 18 objects (18 IFCSPACE)
    Average Estimated Illumination = 0. (IFCREAL)
    Ceiling Reflectance = 0.75 (IFCREAL)
    Floor Reflectance = 0.2 (IFCREAL)
    Lighting Calculation Workplane = 0.762 (IFCLENGTHMEASURE) [METRE]
    Room Cavity Ratio = 0. (IFCREAL)
    Wall Reflectance = 0.5 (IFCREAL)
  PSet_Revit_Mechanical | properties | on 71 objects (71 IFCFLOWFITTING)
    Insulation Thickness = 0. (IFCREAL)
    K Coefficient Table = "Regular 45, 90 and 180 Elbow" (IFCLABEL)
    Loss Method = 5 (IFCINTEGER)
    System Name = "Hydronic Return Unit A" (IFCLABEL)
    System Type = "Hydronic Supply" (IFCLABEL)
  PSet_Revit_Mechanical | properties | on 70 objects (70 IFCFLOWFITTING)
    Insulation Thickness = 0. (IFCREAL)
    K Coefficient Table = "Regular 45, 90 and 180 Elbow" (IFCLABEL)
    Loss Method = 5 (IFCINTEGER)
    System Name = "Hydronic Supply Unit B" (IFCLABEL)
    System Type = "Hydronic Supply" (IFCLABEL)
  PSet_Revit_Mechanical | properties | on 24 objects (24 IFCFLOWFITTING)
    Insulation Thickness = 0. (IFCREAL)
    K Coefficient Table = "Tee" (IFCLABEL)
    Loss Method = 5 (IFCINTEGER)
    System Name = "Hydronic Return Unit A" (IFCLABEL)
    System Type = "Hydronic Supply" (IFCLABEL)
  PSet_Revit_Mechanical | properties | on 24 objects (24 IFCFLOWFITTING)
    Insulation Thickness = 0. (IFCREAL)
    K Coefficient Table = "Tee" (IFCLABEL)
    Loss Method = 5 (IFCINTEGER)
    System Name = "Hydronic Supply Unit B" (IFCLABEL)
    System Type = "Hydronic Supply" (IFCLABEL)
  PSet_Revit_Mechanical | properties | on 8 objects (8 IFCFLOWFITTING)
    Insulation Thickness = 0. (IFCREAL)
    K Coefficient Table = "Reducer/Coupling/Union/Increaser" (IFCLABEL)
    Loss Method = 5 (IFCINTEGER)
    System Name = "Hydronic Return Unit A" (IFCLABEL)
    System Type = "Hydronic Supply" (IFCLABEL)
  PSet_Revit_Mechanical | properties | on 8 objects (8 IFCFLOWFITTING)
    Insulation Thickness = 0. (IFCREAL)
    K Coefficient Table = "Reducer/Coupling/Union/Increaser" (IFCLABEL)
    Loss Method = 5 (IFCINTEGER)
    System Name = "Hydronic Supply Unit B" (IFCLABEL)
    System Type = "Hydronic Supply" (IFCLABEL)
  PSet_Revit_Mechanical | properties | on 3 objects (3 IFCENERGYCONVERSIONDEVICE)
    Flow = 0.002118880003289315 (IFCREAL)
    Pressure Drop = 275.804376 (IFCREAL)
    System Name = "Hydronic Supply Unit A,Hydronic Return Unit A" (IFCLABEL)
    System Type = "Hydronic Supply" (IFCLABEL)
  PSet_Revit_Mechanical | properties | on 3 objects (3 IFCENERGYCONVERSIONDEVICE)
    Flow = 0.002118880003289315 (IFCREAL)
    Pressure Drop = 275.804376 (IFCREAL)
    System Name = "Hydronic Supply Unit B,Hydronic Return Unit B" (IFCLABEL)
    System Type = "Hydronic Supply" (IFCLABEL)
  PSet_Revit_Mechanical: 268 more contents on 276 objects not shown
  PSet_Revit_Other | properties | on 184 objects (184 IFCFLOWSEGMENT)
    AssetIdentifier = "AssetIdentifier" (IFCLABEL)
    BarCode = "BarCode" (IFCLABEL)
    InstallationDate = "InstallationDate" (IFCLABEL)
    SerialNumber = "SerialNumber" (IFCLABEL)
    TagNumber = "TagNumber" (IFCLABEL)
    WarrantyStartDate = "WarrantyStartDate" (IFCLABEL)
  PSet_Revit_Other | properties | on 95 objects (95 IFCFLOWFITTING)
    AssetIdentifier = "AssetIdentifier" (IFCLABEL)
    BarCode = "BarCode" (IFCLABEL)
    Center Radius = 0.06770833333333334 (IFCREAL)
    Fitting Outside Radius = 0.04687500000000001 (IFCREAL)
    InstallationDate = "InstallationDate" (IFCLABEL)
    SerialNumber = "SerialNumber" (IFCLABEL)
    TagNumber = "TagNumber" (IFCLABEL)
    WarrantyStartDate = "WarrantyStartDate" (IFCLABEL)
  PSet_Revit_Other | properties | on 46 objects (46 IFCFLOWFITTING)
    Center Radius = 0.06770833333333334 (IFCREAL)
    Fitting Outside Radius = 0.04687500000000001 (IFCREAL)
  PSet_Revit_Other | properties | on 31 objects (31 IFCFLOWFITTING)
    Angle 1 = 90. (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
    AssetIdentifier = "AssetIdentifier" (IFCLABEL)
    BarCode = "BarCode" (IFCLABEL)
    Center to End Label = 0.08854166666666667 (IFCREAL)
    Fitting Outside Radius = 0.04687500000000001 (IFCREAL)
    InstallationDate = "InstallationDate" (IFCLABEL)
    SerialNumber = "SerialNumber" (IFCLABEL)
    TagNumber = "TagNumber" (IFCLABEL)
    WarrantyStartDate = "WarrantyStartDate" (IFCLABEL)
  PSet_Revit_Other | properties | on 13 objects (13 IFCFLOWFITTING)
    Angle 1 = 90. (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
    Center to End Label = 0.08854166666666667 (IFCREAL)
    Fitting Outside Radius = 0.04687500000000001 (IFCREAL)
  PSet_Revit_Other | properties | on 10 objects (10 IFCFLOWFITTING)
    AssetIdentifier = "AssetIdentifier" (IFCLABEL)
    BarCode = "BarCode" (IFCLABEL)
    Fitting Outside Radius 1 = 0.08854166666666667 (IFCREAL)
    Fitting Outside Radius 2 = 0.04687500000000001 (IFCREAL)
    Height Offset = 10. (IFCREAL)
    InstallationDate = "InstallationDate" (IFCLABEL)
    Max Fitting Outside Diameter 12 = 0.1770833333333333 (IFCREAL)
    SerialNumber = "SerialNumber" (IFCLABEL)
    TagNumber = "TagNumber" (IFCLABEL)
    Visibility 1 = FALSE (IFCBOOLEAN)
    Visibility 2 = TRUE (IFCBOOLEAN)
    Visibility 3 = FALSE (IFCBOOLEAN)
    WarrantyStartDate = "WarrantyStartDate" (IFCLABEL)
    Width Offset = 10. (IFCREAL)
  PSet_Revit_Other | properties | on 2 objects (2 IFCFLOWFITTING)
    AssetIdentifier = "AssetIdentifier" (IFCLABEL)
    BarCode = "BarCode" (IFCLABEL)
    Fitting Outside Radius 1 = 0.06770833333333334 (IFCREAL)
    Fitting Outside Radius 2 = 0.04687500000000001 (IFCREAL)
    Height Offset = 10. (IFCREAL)
    InstallationDate = "InstallationDate" (IFCLABEL)
    Max Fitting Outside Diameter 12 = 0.1354166666666667 (IFCREAL)
    SerialNumber = "SerialNumber" (IFCLABEL)
    TagNumber = "TagNumber" (IFCLABEL)
    Visibility 1 = FALSE (IFCBOOLEAN)
    Visibility 2 = TRUE (IFCBOOLEAN)
    Visibility 3 = FALSE (IFCBOOLEAN)
    WarrantyStartDate = "WarrantyStartDate" (IFCLABEL)
    Width Offset = 10. (IFCREAL)
  PSet_Revit_Other | properties | on 2 objects (2 IFCFLOWFITTING)
    Fitting Outside Radius 1 = 0.04687500000000001 (IFCREAL)
    Fitting Outside Radius 2 = 0.08854166666666667 (IFCREAL)
    Height Offset = 10. (IFCREAL)
    Max Fitting Outside Diameter 12 = 0.1770833333333333 (IFCREAL)
    Visibility 1 = FALSE (IFCBOOLEAN)
    Visibility 2 = FALSE (IFCBOOLEAN)
    Visibility 3 = TRUE (IFCBOOLEAN)
    Width Offset = 10. (IFCREAL)
  PSet_Revit_Other: 42 more contents on 43 objects not shown
  PSet_Revit_Mechanical - Loads | properties | on 4 objects (4 IFCENERGYCONVERSIONDEVICE)
    Power = 62136.15609645916 (IFCREAL)
  PSet_Revit_Mechanical - Loads | properties | on 4 objects (4 IFCENERGYCONVERSIONDEVICE)
    Power = 73482.75851407345 (IFCREAL)
  PSet_Revit_Mechanical - Loads | properties | on 4 objects (4 IFCENERGYCONVERSIONDEVICE)
    Power = 54031.44008387754 (IFCREAL)
  PSet_Revit_Mechanical - Loads | properties | on 4 objects (4 IFCENERGYCONVERSIONDEVICE)
    Power = 27015.72004193877 (IFCREAL)
  PSet_Revit_Mechanical - Loads | properties | on 2 objects (2 IFCENERGYCONVERSIONDEVICE)
    Power = 54031.44008387753 (IFCREAL)
  PSet_Revit_Mechanical - Loads | properties | on 2 objects (2 IFCENERGYCONVERSIONDEVICE)
    Power = 119409.4825853693 (IFCREAL)
  PSet_Revit_Graphics | properties | on 133 objects (125 IFCFLOWFITTING, 8 IFCFLOWCONTROLLER)
    Use Annotation Scale = TRUE (IFCBOOLEAN)
  PSet_Revit_Graphics | properties | on 82 objects (82 IFCFLOWFITTING)
    Use Annotation Scale = FALSE (IFCBOOLEAN)
  Pset_BuildingCommon | properties | on 1 object (1 IFCBUILDING)
    NumberOfStoreys = 3 (IFCINTEGER)
  PSet_Revit_Type_Graphics | properties | on 3 objects (3 IFCBUILDINGSTOREY)
    Color = 0 (IFCINTEGER)
    Line Pattern = "Centre" (IFCLABEL)
    Line Weight = 1 (IFCINTEGER)
    Symbol at End 1 Default = FALSE (IFCBOOLEAN)
    Symbol at End 2 Default = TRUE (IFCBOOLEAN)
  PSet_Revit_Type_Constraints | properties | on 20 objects (20 IFCENERGYCONVERSIONDEVICE)
    Default Elevation = 0.1016 (IFCLENGTHMEASURE) [METRE]
  PSet_Revit_Type_Constraints | properties | on 3 objects (3 IFCBUILDINGSTOREY)
    Elevation Base = 0 (IFCINTEGER)
  PSet_Revit_Type_Constraints | properties | on 2 objects (2 IFCFLOWFITTING)
    Angle = 45. (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
  PSet_Revit_Type_Constraints | properties | on 2 objects (2 IFCFLOWMOVINGDEVICE)
    Default Elevation = 1.2 (IFCLENGTHMEASURE) [METRE]
  PSet_Revit_Type_Dimensions | properties | on 20 objects (20 IFCENERGYCONVERSIONDEVICE)
    Connector = 0.04101049868766404 (IFCREAL)
    Height = 0.3556 (IFCLENGTHMEASURE) [METRE]
  PSet_Revit_Type_Dimensions | properties | on 4 objects (4 IFCFLOWCONTROLLER)
    Adapter Diameter = 0.08 (IFCLENGTHMEASURE) [METRE]
    Adapter Length = 0.0178 (IFCLENGTHMEASURE) [METRE]
    Adapter Radius = 0.04 (IFCLENGTHMEASURE) [METRE]
    Body Diameter = 0.05500000000000001 (IFCLENGTHMEASURE) [METRE]
    Body Height = 0.07150000000000001 (IFCLENGTHMEASURE) [METRE]
    Body Length = 0.178 (IFCLENGTHMEASURE) [METRE]
    Body Radius = 0.0275 (IFCLENGTHMEASURE) [METRE]
    Handle Height = 0.229 (IFCLENGTHMEASURE) [METRE]
    Handle Length = 0.127 (IFCLENGTHMEASURE) [METRE]
    Handle Width = 0.025 (IFCLENGTHMEASURE) [METRE]
    Nominal Diameter = 0.1640419947506562 (IFCREAL)
    Nominal Radius = 0.08202099737532809 (IFCREAL)
    Nut Diameter = 0.015 (IFCLENGTHMEASURE) [METRE]
    Nut Height = 0.0165 (IFCLENGTHMEASURE) [METRE]
    Nut Radius = 0.007500000000000001 (IFCLENGTHMEASURE) [METRE]
    Seal Length = 0.04450000000000001 (IFCLENGTHMEASURE) [METRE]
    Stem Diameter = 0.01 (IFCLENGTHMEASURE) [METRE]
    Stem Height = 0.0275 (IFCLENGTHMEASURE) [METRE]
    Stem Radius = 0.005 (IFCLENGTHMEASURE) [METRE]
  PSet_Revit_Type_Dimensions | properties | on 4 objects (4 IFCFLOWCONTROLLER)
    Body Length = 0.245 (IFCLENGTHMEASURE) [METRE]
    C1 Offset 1 = 0.098 (IFCLENGTHMEASURE) [METRE]
    C1 Offset 2 = 0.062 (IFCLENGTHMEASURE) [METRE]
    Nominal Diameter = 0.08202099737532809 (IFCREAL)
    Nominal Radius = 0.04101049868766404 (IFCREAL)
    Open Height = 0.116 (IFCLENGTHMEASURE) [METRE]
    Outside Diameter = 0.03 (IFCLENGTHMEASURE) [METRE]
    Valve Length = 0.36 (IFCLENGTHMEASURE) [METRE]
    Width 1 = 0.033 (IFCLENGTHMEASURE) [METRE]
  PSet_Revit_Type_Dimensions | properties | on 3 objects (3 IFCBUILDINGSTOREY)
    Automatic Room Computation Height = FALSE (IFCBOOLEAN)
    Computation Height = 1.2 (IFCLENGTHMEASURE) [METRE]
  PSet_Revit_Type_Dimensions | properties | on 2 objects (2 IFCFLOWMOVINGDEVICE)
    Discharge Nominal Diameter = 0.1312335958005249 (IFCREAL)
    Discharge Nominal Radius = 0.06561679790026247 (IFCREAL)
    Flange Diameter = 0.102 (IFCLENGTHMEASURE) [METRE]
    Flange Height = 0.13 (IFCLENGTHMEASURE) [METRE]
    Housing Width = 0.152 (IFCLENGTHMEASURE) [METRE]
    Length 1 = 0.4310000000000001 (IFCLENGTHMEASURE) [METRE]
    Length 2 = 0.3448000000000001 (IFCLENGTHMEASURE) [METRE]
    Length 3 = 0.06206400000000001 (IFCLENGTHMEASURE) [METRE]
    Outside Diameter 1 = 0.184 (IFCLENGTHMEASURE) [METRE]
    Outside Diameter 2 = 0.171 (IFCLENGTHMEASURE) [METRE]
    Outside Diameter 4 = 0.06206400000000001 (IFCLENGTHMEASURE) [METRE]
    Suction Nominal Diameter = 0.1312335958005249 (IFCREAL)
    Suction Nominal Radius = 0.06561679790026247 (IFCREAL)
    Suction Outside Diameter = 0.172244094488189 (IFCREAL)
    Suction Outside Radius = 0.08612204724409449 (IFCREAL)
  PSet_Revit_Type_Dimensions | properties | on 2 objects (2 IFCENERGYCONVERSIONDEVICE)
    Boiler Diameter = 0.6100000000000001 (IFCLENGTHMEASURE) [METRE]
    Boiler Height = 0.9650000000000001 (IFCLENGTHMEASURE) [METRE]
    Boiler Top Diameter = 0.5600000000000001 (IFCLENGTHMEASURE) [METRE]
    Cold Water Diameter = 0.1312335958005249 (IFCREAL)
    Cold Water Radius = 0.06561679790026247 (IFCREAL)
    Electrical Box Height = 0.203 (IFCLENGTHMEASURE) [METRE]
    Electrical Box Length = 0.203 (IFCLENGTHMEASURE) [METRE]
    Electrical Box Width = 0.094 (IFCLENGTHMEASURE) [METRE]
    Gas Diameter = 0.08202099737532809 (IFCREAL)
    Gas Radius = 0.04101049868766404 (IFCREAL)
    Hot Water Diameter = 0.1312335958005249 (IFCREAL)
    Hot Water Radius = 0.06561679790026247 (IFCREAL)
    Vent Box Diameter = 0.254 (IFCLENGTHMEASURE) [METRE]
    Vent Box Height = 0.102 (IFCLENGTHMEASURE) [METRE]
    Vent Diameter = 0.8202099737532809 (IFCREAL)
    Vent Radius = 0.4101049868766404 (IFCREAL)
  PSet_Revit_Type_Dimensions | properties | on 2 objects (2 IFCFLOWMOVINGDEVICE)
    Base Width = 0.4 (IFCLENGTHMEASURE) [METRE]
    Cap Diameter = 0.28 (IFCLENGTHMEASURE) [METRE]
    Cap Radius = 0.14 (IFCLENGTHMEASURE) [METRE]
    Fan Diameter = 0.4 (IFCLENGTHMEASURE) [METRE]
    Fan Height = 0.2 (IFCLENGTHMEASURE) [METRE]
    Fan Radius = 0.2 (IFCLENGTHMEASURE) [METRE]
    Outlet Height = 0.8202099737532809 (IFCREAL)
    Outlet Width = 0.8202099737532809 (IFCREAL)
    Overall Height = 0.2999999999999999 (IFCLENGTHMEASURE) [METRE]
  PSet_Revit_Type_Mechanical | properties | on 240 objects (240 IFCFLOWSEGMENT)
    Class = "Schedule 40" (IFCLABEL)
    Connection Type = "Threaded" (IFCLABEL)
    Material = "Carbon Steel" (IFCLABEL)
    Roughness = 0.04572 (IFCREAL)
  PSet_Revit_Type_Mechanical | properties | on 141 objects (141 IFCFLOWFITTING)
    K Coefficient Table = "Regular 45, 90 and 180 Elbow" (IFCLABEL)
    Loss Method = 1 (IFCINTEGER)
  PSet_Revit_Type_Mechanical | properties | on 48 objects (48 IFCFLOWFITTING)
    K Coefficient Table = "Tee" (IFCLABEL)
    Loss Method = 1 (IFCINTEGER)
  PSet_Revit_Type_Mechanical | properties | on 16 objects (16 IFCFLOWFITTING)
    K Coefficient Table = "Reducer/Coupling/Union/Increaser" (IFCLABEL)
    Loss Method = 1 (IFCINTEGER)
  PSet_Revit_Type_Mechanical | properties | on 4 objects (4 IFCFLOWCONTROLLER)
    K Coefficient = 0.35 (IFCREAL)
    K Coefficient Table = "Ball Valve Full Port Full Open" (IFCLABEL)
    Loss Method = 0 (IFCINTEGER)
  PSet_Revit_Type_Mechanical | properties | on 4 objects (4 IFCFLOWSEGMENT)
    Class = "A" (IFCLABEL)
    Connection Type = "Soldered" (IFCLABEL)
    Material = "Copper" (IFCLABEL)
    Roughness = 0.00254 (IFCREAL)
  PSet_Revit_Type_Mechanical | properties | on 4 objects (4 IFCFLOWCONTROLLER)
    K Coefficient Table = "Swing Check Valve Threaded" (IFCLABEL)
    Loss Method = 0 (IFCINTEGER)
  PSet_Revit_Type_Mechanical | properties | on 2 objects (2 IFCFLOWMOVINGDEVICE)
    RPM = 1050. (IFCREAL)
  PSet_Revit_Type_Other | properties | on 248 objects (246 IFCFLOWSEGMENT, 2 IFCFLOWFITTING)
    AccessibilityPerformance = "AccessibilityPerformance" (IFCLABEL)
    AssetAccountingType = "FIXED" (IFCLABEL)
    CodePerformance = "CodePerformance" (IFCLABEL)
    Color = "Color" (IFCLABEL)
    Constituents = "Constituents" (IFCLABEL)
    ExpectedLife = "ExpectedLife" (IFCLABEL)
    Features = "Features" (IFCLABEL)
    Finish = "Finish" (IFCLABEL)
    Grade = "Grade" (IFCLABEL)
    Material = "Material" (IFCLABEL)
    ModelNumber = "ModelNumber" (IFCLABEL)
    ModelReference = "ModelReference" (IFCLABEL)
    NominalHeight = "NominalHeight" (IFCLABEL)
    NominalLength = "NominalLength" (IFCLABEL)
    NominalWidth = "NominalWidth" (IFCLABEL)
    ProductionYear = "ProductionYear" (IFCLABEL)
    Reference = "Reference" (IFCLABEL)
    ReplacementCost = "ReplacementCost" (IFCLABEL)
    Shape = "Shape" (IFCLABEL)
    Size = "Size" (IFCLABEL)
    SustainabilityPerformance = "SustainabilityPerformance" (IFCLABEL)
    WarrantyDescription = "WarrantyDescription" (IFCLABEL)
    WarrantyDurationLabor = "WarrantyDurationLabor" (IFCLABEL)
    WarrantyDurationParts = "WarrantyDurationParts" (IFCLABEL)
    WarrantyGuarantorLabor = "WarrantyGuarantorLabor" (IFCLABEL)
    WarrantyGuarantorParts = "WarrantyGuarantorParts" (IFCLABEL)
  PSet_Revit_Type_Other | properties | on 205 objects (205 IFCFLOWFITTING)
    AccessibilityPerformance = "AccessibilityPerformance" (IFCLABEL)
    AssetAccountingType = "FIXED" (IFCLABEL)
    CodePerformance = "CodePerformance" (IFCLABEL)
    Color = "Color" (IFCLABEL)
    Constituents = "Constituents" (IFCLABEL)
    ExpectedLife = "ExpectedLife" (IFCLABEL)
    Features = "Features" (IFCLABEL)
    Finish = "Finish" (IFCLABEL)
    Grade = "Grade" (IFCLABEL)
    Lookup Table Name = "M_Pipe Fitting - Generic.csv" (IFCLABEL)
    Material = "Material" (IFCLABEL)
    ModelNumber = "ModelNumber" (IFCLABEL)
    ModelReference = "ModelReference" (IFCLABEL)
    NominalHeight = "NominalHeight" (IFCLABEL)
    NominalLength = "NominalLength" (IFCLABEL)
    NominalWidth = "NominalWidth" (IFCLABEL)
    ProductionYear = "ProductionYear" (IFCLABEL)
    Reference = "Reference" (IFCLABEL)
    ReplacementCost = "ReplacementCost" (IFCLABEL)
    Shape = "Shape" (IFCLABEL)
    Size = "Size" (IFCLABEL)
    SustainabilityPerformance = "SustainabilityPerformance" (IFCLABEL)
    WarrantyDescription = "WarrantyDescription" (IFCLABEL)
    WarrantyDurationLabor = "WarrantyDurationLabor" (IFCLABEL)
    WarrantyDurationParts = "WarrantyDurationParts" (IFCLABEL)
    WarrantyGuarantorLabor = "WarrantyGuarantorLabor" (IFCLABEL)
    WarrantyGuarantorParts = "WarrantyGuarantorParts" (IFCLABEL)
  PSet_Revit_Type_Other | properties | on 20 objects (20 IFCENERGYCONVERSIONDEVICE)
    AccessibilityPerformance = "n/a" (IFCLABEL)
    AssetAccountingType = "FIXED" (IFCLABEL)
    CodePerformance = "15700" (IFCLABEL)
    Color = "White" (IFCLABEL)
    Constituents = "n/a" (IFCLABEL)
    ExpectedLife = "5 years" (IFCLABEL)
    Features = "2.67 fins per inch" (IFCLABEL)
    Finish = "Baked Enamel" (IFCLABEL)
    Grade = "A" (IFCLABEL)
    Material = "Aluminum" (IFCLABEL)
    ModelNumber = "JVB" (IFCLABEL)
    ModelReference = "JVB" (IFCLABEL)
    NominalHeight = "14 inches" (IFCLABEL)
    NominalLength = "see plans" (IFCLABEL)
    NominalWidth = "5-5/16"" (IFCLABEL)
    ProductionYear = "2011" (IFCLABEL)
    Reference = "Internet" (IFCLABEL)
    ReplacementCost = "$30/foot" (IFCLABEL)
    Shape = "Rectangular" (IFCLABEL)
    Size = "25mm" (IFCLABEL)
    SustainabilityPerformance = "n/a" (IFCLABEL)
    WarrantyDescription = "tbd" (IFCLABEL)
    WarrantyDurationLabor = "tbd" (IFCLABEL)
    WarrantyDurationParts = "tbd" (IFCLABEL)
    WarrantyGuarantorLabor = "tbd" (IFCLABEL)
    WarrantyGuarantorParts = "tbd" (IFCLABEL)
  PSet_Revit_Type_Other | properties | on 4 objects (4 IFCFLOWCONTROLLER)
    AccessibilityPerformance = "n/a" (IFCLABEL)
    AssetAccountingType = "FIXED" (IFCLABEL)
    CodePerformance = "15200" (IFCLABEL)
    Color = "Bronze" (IFCLABEL)
    Constituents = "n/a" (IFCLABEL)
    ExpectedLife = "20 years" (IFCLABEL)
    Features = "Chromium Plated Ball" (IFCLABEL)
    Finish = "Bronze Body" (IFCLABEL)
    Grade = "A" (IFCLABEL)
    Half Nut Height = 0.008250000000000002 (IFCLENGTHMEASURE) [METRE]
    Length 1 = 0.1424 (IFCLENGTHMEASURE) [METRE]
    Length 2 = 0.04450000000000001 (IFCLENGTHMEASURE) [METRE]
    Material = "Bronze" (IFCLABEL)
    ModelNumber = "32-208" (IFCLABEL)
    ModelReference = "32-208" (IFCLABEL)
    NominalHeight = "89 mm" (IFCLABEL)
    NominalLength = "165 mm" (IFCLABEL)
    NominalWidth = "63.5 mm" (IFCLABEL)
    ProductionYear = "2011" (IFCLABEL)
    Radius = 0.092 (IFCLENGTHMEASURE) [METRE]
    Reference = "Internet" (IFCLABEL)
    ReplacementCost = "$50" (IFCLABEL)
    Shape = "Odd" (IFCLABEL)
    Size = "50 mm" (IFCLABEL)
    SustainabilityPerformance = "n/a" (IFCLABEL)
    WarrantyDescription = "tbd" (IFCLABEL)
    WarrantyDurationLabor = "tbd" (IFCLABEL)
    WarrantyDurationParts = "tbd" (IFCLABEL)
    WarrantyGuarantorLabor = "tbd" (IFCLABEL)
    WarrantyGuarantorParts = "tbd" (IFCLABEL)
  PSet_Revit_Type_Other | properties | on 4 objects (4 IFCFLOWCONTROLLER)
    AccessibilityPerformance = "n/a" (IFCLABEL)
    Angle 1 = 45. (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
    Angle 2 = 45. (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
    AssetAccountingType = "FIXED" (IFCLABEL)
    CodePerformance = "15520" (IFCLABEL)
    Color = "Bronze" (IFCLABEL)
    Constituents = "n/a" (IFCLABEL)
    ExpectedLife = "20 years" (IFCLABEL)
    Features = "top-mounted test cocks" (IFCLABEL)
    Finish = "Bronze Body" (IFCLABEL)
    Grade = "A" (IFCLABEL)
    Height 1 = 0.04500000000000001 (IFCLENGTHMEASURE) [METRE]
    Height 2 = 0.06000000000000001 (IFCLENGTHMEASURE) [METRE]
    Height 3 = 0.02025 (IFCLENGTHMEASURE) [METRE]
    Height 4 = 0.00225 (IFCLENGTHMEASURE) [METRE]
    Height 5 = 0.015 (IFCLENGTHMEASURE) [METRE]
    Height 6 = 0.007500000000000001 (IFCLENGTHMEASURE) [METRE]
    Length 1 = 0.0254 (IFCLENGTHMEASURE) [METRE]
    Length 2 = 0.0254 (IFCLENGTHMEASURE) [METRE]
    Length 3 = 0.00635 (IFCLENGTHMEASURE) [METRE]
    Length 4 = 0.00640359523141434 (IFCLENGTHMEASURE) [METRE]
    Length 5 = 0.05122876185131472 (IFCLENGTHMEASURE) [METRE]
    Length 6 = 0.01280719046282868 (IFCLENGTHMEASURE) [METRE]
    Length 7 = 0.01921078569424302 (IFCLENGTHMEASURE) [METRE]
    Length 8 = 0.001600898807853585 (IFCLENGTHMEASURE) [METRE]
    Length 9 = 0.01120629165497509 (IFCLENGTHMEASURE) [METRE]
    Length = 0.1280719046282868 (IFCLENGTHMEASURE) [METRE]
    Material = "Bronze" (IFCLABEL)
    ModelNumber = "DCLF40" (IFCLABEL)
    ModelReference = "DCLF40" (IFCLABEL)
    NominalHeight = "146 mm" (IFCLABEL)
    NominalLength = "356 mm" (IFCLABEL)
    NominalWidth = "79.4 mm" (IFCLABEL)
    Outside Radius = 0.015 (IFCLENGTHMEASURE) [METRE]
    ProductionYear = "2011" (IFCLABEL)
    Radius 1 = 0.0254 (IFCLENGTHMEASURE) [METRE]
    Radius 10 = 0.02475 (IFCLENGTHMEASURE) [METRE]
    Radius 2 = 0.0381 (IFCLENGTHMEASURE) [METRE]
    Radius 3 = 0.0135 (IFCLENGTHMEASURE) [METRE]
    Radius 4 = 0.01125 (IFCLENGTHMEASURE) [METRE]
    Radius 5 = 0.03135 (IFCLENGTHMEASURE) [METRE]
    Radius 6 = 0.033 (IFCLENGTHMEASURE) [METRE]
    Radius 7 = 0.009000000000000001 (IFCLENGTHMEASURE) [METRE]
    Radius 8 = 0.00375 (IFCLENGTHMEASURE) [METRE]
    Radius 9 = 0.006000000000000001 (IFCLENGTHMEASURE) [METRE]
    Reference = "Internet" (IFCLABEL)
    ReplacementCost = "$150" (IFCLABEL)
    Shape = "Odd" (IFCLABEL)
    Size = "25 mm" (IFCLABEL)
    SustainabilityPerformance = "n/a" (IFCLABEL)
    Thickness 1 = 0.00375 (IFCLENGTHMEASURE) [METRE]
    WarrantyDescription = "tbd" (IFCLABEL)
    WarrantyDurationLabor = "tbd" (IFCLABEL)
    WarrantyDurationParts = "tbd" (IFCLABEL)
    WarrantyGuarantorLabor = "tbd" (IFCLABEL)
    WarrantyGuarantorParts = "tbd" (IFCLABEL)
    Width 2 = 0.006750000000000001 (IFCLENGTHMEASURE) [METRE]
  PSet_Revit_Type_Other | properties | on 2 objects (2 IFCFLOWMOVINGDEVICE)
    AccessibilityPerformance = "n/a" (IFCLABEL)
    AssetAccountingType = "FIXED" (IFCLABEL)
    CodePerformance = "15700" (IFCLABEL)
    Color = "Green" (IFCLABEL)
    Constituents = "n/a" (IFCLABEL)
    ExpectedLife = "10 years" (IFCLABEL)
    Features = "Compact, self-lubricating" (IFCLABEL)
    Finish = "Cast Iron" (IFCLABEL)
    Flange Radius = 0.051 (IFCLENGTHMEASURE) [METRE]
    Grade = "A" (IFCLABEL)
    Length 4 = 0.02134819455806278 (IFCLENGTHMEASURE) [METRE]
    Material = "Cast Iron" (IFCLABEL)
    ModelNumber = "0014" (IFCLABEL)
    ModelReference = "0014" (IFCLABEL)
    NominalHeight = "184 mm" (IFCLABEL)
    NominalLength = "165 mm" (IFCLABEL)
    NominalWidth = "137 mm" (IFCLABEL)
    Outside Radius 1 = 0.092 (IFCLENGTHMEASURE) [METRE]
    Outside Radius 2 = 0.08550000000000001 (IFCLENGTHMEASURE) [METRE]
    Outside Radius 4 = 0.031032 (IFCLENGTHMEASURE) [METRE]
    ProductionYear = "2011" (IFCLABEL)
    Radius 1 = 0.07915000000000001 (IFCLENGTHMEASURE) [METRE]
    Radius 2 = 0.0728 (IFCLENGTHMEASURE) [METRE]
    Radius 3 = 0.056432 (IFCLENGTHMEASURE) [METRE]
    Reference = "Internet" (IFCLABEL)
    ReplacementCost = "$300" (IFCLABEL)
    Shape = "Odd" (IFCLABEL)
    Size = "0014" (IFCLABEL)
    SustainabilityPerformance = "n/a" (IFCLABEL)
    WarrantyDescription = "tbd" (IFCLABEL)
    WarrantyDurationLabor = "tbd" (IFCLABEL)
    WarrantyDurationParts = "tbd" (IFCLABEL)
    WarrantyGuarantorLabor = "tbd" (IFCLABEL)
    WarrantyGuarantorParts = "tbd" (IFCLABEL)
  PSet_Revit_Type_Other | properties | on 2 objects (2 IFCENERGYCONVERSIONDEVICE)
    AccessibilityPerformance = "n/a" (IFCLABEL)
    AssetAccountingType = "FIXED" (IFCLABEL)
    Boiler Radius = 0.3050000000000001 (IFCLENGTHMEASURE) [METRE]
    Boiler Top Radius = 0.28 (IFCLENGTHMEASURE) [METRE]
    CodePerformance = "15500" (IFCLABEL)
    Color = "White" (IFCLABEL)
    Constituents = "n/a" (IFCLABEL)
    ExpectedLife = "20 years" (IFCLABEL)
    Features = "Cast Aluminum Block" (IFCLABEL)
    Finish = "Shell" (IFCLABEL)
    Grade = "A" (IFCLABEL)
    Material = "Various" (IFCLABEL)
    ModelNumber = "Ultra 155" (IFCLABEL)
    ModelReference = "Ultra 155" (IFCLABEL)
    NominalHeight = "1092 mm" (IFCLABEL)
    NominalLength = "584 mm" (IFCLABEL)
    NominalWidth = "559 mm" (IFCLABEL)
    ProductionYear = "2011" (IFCLABEL)
    Radius 1 = 0.2288 (IFCLENGTHMEASURE) [METRE]
    Reference = "Internet" (IFCLABEL)
    ReplacementCost = "$4000" (IFCLABEL)
    Shape = "Rectangular" (IFCLABEL)
    Size = "155" (IFCLABEL)
    SustainabilityPerformance = "n/a" (IFCLABEL)
    Vent Box Radius = 0.127 (IFCLENGTHMEASURE) [METRE]
    WarrantyDescription = "tbd" (IFCLABEL)
    WarrantyDurationLabor = "tbd" (IFCLABEL)
    WarrantyDurationParts = "tbd" (IFCLABEL)
    WarrantyGuarantorLabor = "tbd" (IFCLABEL)
    WarrantyGuarantorParts = "tbd" (IFCLABEL)
  PSet_Revit_Type_Other | properties | on 2 objects (2 IFCFLOWMOVINGDEVICE)
    AccessibilityPerformance = "n/a" (IFCLABEL)
    AssetAccountingType = "FIXED" (IFCLABEL)
    CodePerformance = "15700" (IFCLABEL)
    Color = "Grey" (IFCLABEL)
    Constituents = "n/a" (IFCLABEL)
    Diameter 1 = 0.2999999999999999 (IFCLENGTHMEASURE) [METRE]
    Diameter 2 = 0.32 (IFCLENGTHMEASURE) [METRE]
    ExpectedLife = "10 years" (IFCLABEL)
    Features = "Backdraft Damper" (IFCLABEL)
    Finish = "Milled" (IFCLABEL)
    Grade = "A" (IFCLABEL)
    Half Exhaust Inlet Height = 0.125 (IFCLENGTHMEASURE) [METRE]
    Half Outlet Radius = 0.125 (IFCLENGTHMEASURE) [METRE]
    Material = "Aluminum" (IFCLABEL)
    ModelNumber = "CUE 060-E" (IFCLABEL)
    ModelReference = "CUE 060-E" (IFCLABEL)
    NominalHeight = "387 mm" (IFCLABEL)
    NominalLength = "467 mm" (IFCLABEL)
    NominalWidth = "467 mm" (IFCLABEL)
    ProductionYear = "2011" (IFCLABEL)
    Radius 1 = 0.15 (IFCLENGTHMEASURE) [METRE]
    Radius 2 = 0.16 (IFCLENGTHMEASURE) [METRE]
    Reference = "Internet" (IFCLABEL)
    ReplacementCost = "$1500" (IFCLABEL)
    Shape = "Odd" (IFCLABEL)
    Size = "060-E" (IFCLABEL)
    SustainabilityPerformance = "n/a" (IFCLABEL)
    WarrantyDescription = "tbd" (IFCLABEL)
    WarrantyDurationLabor = "tbd" (IFCLABEL)
    WarrantyDurationParts = "tbd" (IFCLABEL)
    WarrantyGuarantorLabor = "tbd" (IFCLABEL)
    WarrantyGuarantorParts = "tbd" (IFCLABEL)
  PSet_Revit_Type_Identity Data | properties | on 246 objects (246 IFCFLOWSEGMENT)
    Assembly Code = "" (IFCLABEL)
    Assembly Description = "" (IFCLABEL)
    Manufacturer = "Manufacturer" (IFCLABEL)
  PSet_Revit_Type_Identity Data | properties | on 205 objects (205 IFCFLOWFITTING)
    Assembly Code = "" (IFCLABEL)
    Assembly Description = "" (IFCLABEL)
    Manufacturer = "Manufacturer" (IFCLABEL)
    OmniClass Number = "23.60.30.11.14" (IFCLABEL)
    OmniClass Title = "Pipework Fittings" (IFCLABEL)
  PSet_Revit_Type_Identity Data | properties | on 20 objects (20 IFCENERGYCONVERSIONDEVICE)
    Assembly Code = "D3090900" (IFCLABEL)
    Assembly Description = "Misc. Other HVAC Systems & Equipment" (IFCLABEL)
    Cost = 65. (IFCREAL)
    Description = "Sloped Style FTR" (IFCLABEL)
    Keynote = "15700" (IFCLABEL)
    Manufacturer = "Sterling" (IFCLABEL)
    Model = "JVB" (IFCLABEL)
    OmniClass Number = "23.75.70.17.11" (IFCLABEL)
    OmniClass Title = "Radiators" (IFCLABEL)
    Type Comments = "none" (IFCLABEL)
    Type Mark = "n/a" (IFCLABEL)
    URL = "none" (IFCLABEL)
  PSet_Revit_Type_Identity Data | properties | on 4 objects (4 IFCFLOWCONTROLLER)
    Assembly Code = "D3040400" (IFCLABEL)
    Assembly Description = "Hot Water Distribution" (IFCLABEL)
    Cost = 50. (IFCREAL)
    Description = "Solder End Bronze Ball Valve" (IFCLABEL)
    Keynote = "15200" (IFCLABEL)
    Manufacturer = "Apollo" (IFCLABEL)
    Model = "32-208" (IFCLABEL)
    OmniClass Number = "23.65.55.14.17" (IFCLABEL)
    OmniClass Title = "Adjusting/Controlling Valves for Liquid Services" (IFCLABEL)
    Type Comments = "Solder End Bronze Ball Valve" (IFCLABEL)
    Type Mark = "none" (IFCLABEL)
    URL = "n/a" (IFCLABEL)
  PSet_Revit_Type_Identity Data | properties | on 4 objects (4 IFCFLOWCONTROLLER)
    Assembly Code = "D3040400" (IFCLABEL)
    Assembly Description = "Hot Water Distribution" (IFCLABEL)
    Cost = 150. (IFCREAL)
    Description = "Double Check Valve" (IFCLABEL)
    Keynote = "15200" (IFCLABEL)
    Manufacturer = "Apollo" (IFCLABEL)
    Model = "DCLF40" (IFCLABEL)
    OmniClass Number = "23.65.55.14.21" (IFCLABEL)
    OmniClass Title = "Non-Return Valves for Liquid Services" (IFCLABEL)
    Type Comments = "Corrosion Resistant" (IFCLABEL)
    Type Mark = "none" (IFCLABEL)
    URL = "n/a" (IFCLABEL)
  PSet_Revit_Type_Identity Data | properties | on 2 objects (2 IFCFLOWFITTING)
    Assembly Code = "" (IFCLABEL)
    Assembly Description = "" (IFCLABEL)
    Manufacturer = "Manufacturer" (IFCLABEL)
    OmniClass Number = "23.75.70.14" (IFCLABEL)
    OmniClass Title = "Air Ductwork" (IFCLABEL)
  PSet_Revit_Type_Identity Data | properties | on 2 objects (2 IFCFLOWMOVINGDEVICE)
    Assembly Code = "D3040400" (IFCLABEL)
    Assembly Description = "Hot Water Distribution" (IFCLABEL)
    Cost = 300. (IFCREAL)
    Description = "Medium Flow Circulator" (IFCLABEL)
    Keynote = "15700" (IFCLABEL)
    Manufacturer = "TACO" (IFCLABEL)
    Model = "0014" (IFCLABEL)
    OmniClass Number = "23.60.30.21" (IFCLABEL)
    OmniClass Title = "Pumps" (IFCLABEL)
    Type Comments = "Cartridge Circulator" (IFCLABEL)
    Type Mark = "None" (IFCLABEL)
    URL = "None" (IFCLABEL)
  PSet_Revit_Type_Identity Data | properties | on 2 objects (2 IFCENERGYCONVERSIONDEVICE)
    Assembly Code = "D3020100" (IFCLABEL)
    Assembly Description = "Boilers" (IFCLABEL)
    Cost = 4000. (IFCREAL)
    Description = "Condensing Gas Boiler" (IFCLABEL)
    Keynote = "15500" (IFCLABEL)
    Manufacturer = "Weil-McLain" (IFCLABEL)
    Model = "Ultra 155" (IFCLABEL)
    OmniClass Number = "23.75.10.11.14" (IFCLABEL)
    OmniClass Title = "Hot Water Heat Generators" (IFCLABEL)
    Type Comments = "none" (IFCLABEL)
    Type Mark = "none" (IFCLABEL)
    URL = "n/a" (IFCLABEL)
  PSet_Revit_Type_Identity Data: 1 more content on 2 objects not shown
  PSet_Revit_Type_Construction | properties | on 2 objects (2 IFCFLOWSEGMENT)
    Roughness = 0. (IFCREAL)
  PSet_Revit_Type_Fitting | properties | on 244 objects (244 IFCFLOWSEGMENT)
    Cross = "M_Cross - Generic: Standard" (IFCLABEL)
    Elbow = "M_Elbow - Generic: Standard" (IFCLABEL)
    Preferred Junction Type = 1 (IFCINTEGER)
    Tee = "M_Tee - Generic: Standard" (IFCLABEL)
    Transition = "M_Transition - Generic: Standard" (IFCLABEL)
    Union = "M_Coupling - Generic: Standard" (IFCLABEL)
  PSet_Revit_Type_Fitting | properties | on 2 objects (2 IFCFLOWSEGMENT)
    Cross = "M_Round Cross: Standard" (IFCLABEL)
    Elbow = "M_Round Elbow: 1.5 D" (IFCLABEL)
    Multi Shape Transition Oval to Round = "M_Oval to Round Transition - Length: Standard" (IFCLABEL)
    Multi Shape Transition Rect to Round = "M_Rectangular to Round Transition - Angle: 45 Degree" (IFCLABEL)
    Preferred Junction Type = 0 (IFCINTEGER)
    Tap = "M_Round Takeoff: Standard" (IFCLABEL)
    Tee = "M_Round Tee: Standard" (IFCLABEL)
    Transition = "M_Round Transition - Angle: 45 Degree" (IFCLABEL)
    Union = "M_Round Union: Standard" (IFCLABEL)
  PSet_Revit_Type_Electrical | properties | on 2 objects (2 IFCFLOWMOVINGDEVICE)
    Load Classification = "Appliance - Dwelling Unit" (IFCLABEL)
    Number of Poles = 1 (IFCINTEGER)
    Voltage = 1237.849697921618 (IFCREAL)
  PSet_Revit_Type_Electrical | properties | on 2 objects (2 IFCENERGYCONVERSIONDEVICE)
    Load Classification = "Heating" (IFCLABEL)
    Number of Poles = 3 (IFCINTEGER)
    Voltage = 2238.893366675622 (IFCREAL)
  PSet_Revit_Type_Electrical | properties | on 2 objects (2 IFCFLOWMOVINGDEVICE)
    Load Classification = "HVAC" (IFCLABEL)
    Number of Poles = 3 (IFCINTEGER)
    Voltage = 2238.893366675622 (IFCREAL)
  PSet_Revit_Type_Electrical - Loads | properties | on 2 objects (2 IFCFLOWMOVINGDEVICE)
    Apparent Load = 5834.039445856669 (IFCREAL)
  PSet_Revit_Type_Electrical - Loads | properties | on 2 objects (2 IFCENERGYCONVERSIONDEVICE)
    Apparent Load = 1571530.920839619 (IFCREAL)
  PSet_Revit_Type_Electrical - Loads | properties | on 2 objects (2 IFCFLOWMOVINGDEVICE)
    Apparent Load = 5166.677000020666 (IFCREAL)
  PSet_Revit_Type_Mechanical - Loads | properties | on 20 objects (20 IFCENERGYCONVERSIONDEVICE)
    BtuPerFt = 16468.78293756587 (IFCREAL)