<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="7.4.0">
<drawing>
<board>
<plain>
<wire x1="0" y1="-0.47" x2="25" y2="-0.47" width="0.2" layer="20"/>
<wire x1="25" y1="-0.47" x2="25" y2="99.53" width="0.2" layer="20"/>
<wire x1="25" y1="99.53" x2="0" y2="99.53" width="0.2" layer="20"/>
<wire x1="0" y1="99.53" x2="0" y2="-0.47" width="0.2" layer="20"/>
<text>Rev 2019/05
(c) Peter Müller</text>
<text>HomePi
Adapter-Board</text>
<text>1</text>
<text>BOT</text>
<text>TOP</text>
</plain>
<libraries>
<library name="64-pol-verbinder">
<packages>
<package name="1X31">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="con-vg">
<description>&lt;b&gt;VG Connectors (DIN 41612/DIN 41617)&lt;/b&gt;&lt;p&gt;
The library contains devices which allow to place the contacts individually or 
in one or several blocks.&lt;p&gt;
This behavior is indicated by the key words &lt;i&gt;single&lt;/i&gt; and &lt;i&gt;block&lt;/i&gt; in
the respective device descriptions.&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="MAC64L">
<description>&lt;b&gt;CONNECTOR&lt;/b&gt;&lt;p&gt;
male, 64 pins, type C, rows AC, grid 5.08 mm</description>
</package>
</packages>
</library>
<library name="cryCode-Logo">
<packages>
<package name="30MM">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="SV1" library="64-pol-verbinder" package="1X31" value="">
<attribute name="VALUE"/>
</element>
<element name="X1" library="con-vg" package="MAC64L" value="MAC64L">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="U$2" library="cryCode-Logo" package="30MM" value=""/>
</elements>
<signals>
<signal name="+5V_EXT">
<contactref element="SV1" pad="31"/>
<contactref element="X1" pad="A31"/>
<contactref element="X1" pad="C31"/>
</signal>
<signal name="GND">
<contactref element="SV1" pad="29"/>
<contactref element="SV1" pad="8"/>
<contactref element="SV1" pad="6"/>
<contactref element="SV1" pad="3"/>
<contactref element="X1" pad="C3"/>
<contactref element="X1" pad="A3"/>
<contactref element="X1" pad="A6"/>
<contactref element="X1" pad="A8"/>
<contactref element="X1" pad="A29"/>
<contactref element="X1" pad="C6"/>
<contactref element="X1" pad="C8"/>
<contactref element="X1" pad="C29"/>
<contactref element="X1" pad="A11"/>
<contactref element="X1" pad="A13"/>
<contactref element="X1" pad="C13"/>
<contactref element="X1" pad="A27"/>
</signal>
<signal name="+5V_INT">
<contactref element="SV1" pad="1"/>
<contactref element="X1" pad="A1"/>
<contactref element="X1" pad="C1"/>
</signal>
<signal name="GPIO.25">
<contactref element="SV1" pad="27"/>
<contactref element="X1" pad="C27"/>
</signal>
<signal name="GPIO.24">
<contactref element="SV1" pad="26"/>
<contactref element="X1" pad="C26"/>
</signal>
<signal name="GPIO.23">
<contactref element="SV1" pad="25"/>
<contactref element="X1" pad="C25"/>
</signal>
<signal name="GPIO.22">
<contactref element="SV1" pad="24"/>
<contactref element="X1" pad="C24"/>
</signal>
<signal name="GPIO.21">
<contactref element="SV1" pad="23"/>
<contactref element="X1" pad="C23"/>
</signal>
<signal name="GPIO.20">
<contactref element="SV1" pad="22"/>
<contactref element="X1" pad="C22"/>
</signal>
<signal name="GPIO.19">
<contactref element="SV1" pad="21"/>
<contactref element="X1" pad="C21"/>
</signal>
<signal name="GPIO.18">
<contactref element="SV1" pad="20"/>
<contactref element="X1" pad="C20"/>
</signal>
<signal name="GPIO.17">
<contactref element="SV1" pad="19"/>
<contactref element="X1" pad="C19"/>
</signal>
<signal name="GPIO.16">
<contactref element="SV1" pad="18"/>
<contactref element="X1" pad="C18"/>
</signal>
<signal name="GPIO.13">
<contactref element="SV1" pad="17"/>
<contactref element="X1" pad="C17"/>
</signal>
<signal name="GPIO.12">
<contactref element="SV1" pad="16"/>
<contactref element="X1" pad="C16"/>
</signal>
<signal name="GPIO.06">
<contactref element="SV1" pad="15"/>
<contactref element="X1" pad="C15"/>
</signal>
<signal name="GPIO.05">
<contactref element="SV1" pad="14"/>
<contactref element="X1" pad="C14"/>
</signal>
<signal name="SPI_CE1">
<contactref element="SV1" pad="13"/>
<contactref element="X1" pad="C11"/>
</signal>
<signal name="SPI_SCLK">
<contactref element="SV1" pad="11"/>
<contactref element="X1" pad="C10"/>
</signal>
<signal name="SPI_MOSI">
<contactref element="SV1" pad="9"/>
<contactref element="X1" pad="C9"/>
</signal>
<signal name="1WIRE">
<contactref element="SV1" pad="7"/>
<contactref element="X1" pad="A7"/>
<contactref element="X1" pad="C7"/>
</signal>
<signal name="I2C_SCL">
<contactref element="SV1" pad="5"/>
<contactref element="X1" pad="A5"/>
<contactref element="X1" pad="C5"/>
</signal>
<signal name="I2C_SDA">
<contactref element="SV1" pad="4"/>
<contactref element="X1" pad="A4"/>
<contactref element="X1" pad="C4"/>
</signal>
<signal name="+3,3V">
<contactref element="SV1" pad="2"/>
<contactref element="X1" pad="A2"/>
<contactref element="X1" pad="C2"/>
</signal>
<signal name="GND_EXT">
<contactref element="SV1" pad="30"/>
<contactref element="X1" pad="A30"/>
<contactref element="X1" pad="C30"/>
</signal>
<signal name="+24V">
<contactref element="X1" pad="A32"/>
<contactref element="X1" pad="C32"/>
</signal>
<signal name="+5V_INT2">
<contactref element="SV1" pad="28"/>
<contactref element="X1" pad="A28"/>
<contactref element="X1" pad="C28"/>
</signal>
<signal name="PI_RXD">
<contactref element="X1" pad="C12"/>
</signal>
<signal name="SPI_MISO">
<contactref element="SV1" pad="10"/>
<contactref element="X1" pad="A9"/>
</signal>
<signal name="SPI_CE0">
<contactref element="SV1" pad="12"/>
<contactref element="X1" pad="A10"/>
</signal>
<signal name="PI_TXD">
<contactref element="X1" pad="A12"/>
</signal>
<signal name="!PI_RESET">
<contactref element="X1" pad="A26"/>
</signal>
<signal name="TOP">
</signal>
<signal name="BOT">
</signal>
</signals>
</board>
</drawing>
</eagle>
