|  |  |
| --- | --- |
|  | Aviation Incident Report |
|  |  |
| **Overview** | British Airways B772 at London, rejected take-off due to unreliable speed |
| **Flight No** | BA-81 |
| **Incident ICAO** | B772 |
| **Incident Date** | 11/06/21 |
|  |  |
| **Captain’s Report** | |
| British Airways Boeing 777-200, registration G-YMMR performing flight BA-81 from London Heathrow, EN (UK) to Accra (Ghana), was accelerating for take-off from Heathrow's runway 27L when the crew rejected take-off at about 80 KIAS due to unreliable air speed indications on all three pilot systems. The aircraft slowed safely and returned to the apron.  A replacement Boeing 777-200 registration G-YMMA reached Accra with a delay of about 5:15 hours.  The AAIB reported the occurrence was rated a serious incident and is being investigated, all three pitot systems provided unreliable air speed indications. In addition, British Airways had two more unreliable air speed events involving an A320-200 with 2 blocked pitot tubes and an A320-200N with one blocked pitot tube in about the same time frame.  Flight was short of capacity with 79 passengers and 7 flight crew. | |