Par Statistics
Total Non-vccgnd Signals=4081
Total Non-vccgnd Design Pins=17011
Total Non-vccgnd Conns=17011
Total Non-vccgnd Timing Constrained Conns=16075
Phase 1 CPU=6.7 sec
Phase 2 CPU=7.3 sec
Phase 3 CPU=16.7 sec
Phase 4 CPU=18.0 sec
Phase 5 CPU=26.2 sec
Phase 6 CPU=26.2 sec
Phase 7 CPU=26.2 sec
Phase 8 CPU=26.2 sec
Phase 9 CPU=26.5 sec
Phase 10 CPU=27.6 sec
AvgWirelenPerPin Fanout 1=4.0
AvgWirelenPerPin Fanout 2=3.5
AvgWirelenPerPin Fanout 3=3.7
AvgWirelenPerPin Fanout 4=6.5
AvgWirelenPerPin Fanout 10=3.9
AvgWirelenPerPin Fanout 50=3.7
AvgWirelenPerPin Fanout 100=9.1
AvgWirelenPerPin Fanout 500=7.6
AvgWirelenPerPin Fanout 5000=3.7
AvgWirelenPerPin Fanout 20000=0.0
AvgWirelenPerPin Fanout 50000=0.0
AvgWirelenPerPin Fanout 100000=0.0
IRR Gamma=12.9674