<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="9.6.2">
<drawing>
<board>
<plain>
<wire x1="2.54" y1="0" x2="48.26" y2="0" width="0" layer="20"/>
<wire x1="48.26" y1="22.86" x2="2.54" y2="22.86" width="0" layer="20"/>
<wire x1="0" y1="20.32" x2="2.54" y2="22.86" width="0" layer="20" curve="-90"/>
<wire x1="0" y1="2.54" x2="2.54" y2="0" width="0" layer="20" curve="90"/>
<wire x1="0" y1="2.54" x2="0" y2="20.32" width="0" layer="20"/>
<wire x1="50.8" y1="20.32" x2="48.26" y2="22.86" width="0" layer="20" curve="90"/>
<wire x1="50.8" y1="20.32" x2="50.8" y2="2.54" width="0" layer="20"/>
<wire x1="50.8" y1="2.54" x2="48.26" y2="0" width="0" layer="20" curve="-90"/>
<text>Multiplexer</text>
<text>A</text>
<text>B</text>
<text>C</text>
<text>D</text>
<text>https://github.com/milador/FAIO_Multiplexer</text>
<text>F</text>
<text>A</text>
<text>I</text>
<text>O</text>
<text>GND</text>
<text>+3v3</text>
<text>Multiplexer</text>
</plain>
<libraries>
<library name="milador">
<packages>
<package name="NEOPIXELS-5MM">
</package>
<package name="CONN_1X16">
<description>Single-row, 16-pin Receptacle Header (Female) Straight, 2.54 mm (0.10 in) col pitch, 8.50 mm insulator length, 41.14 X 2.54 X 8.50 mm body
&lt;p&gt;Single-row (1X16), 16-pin Receptacle Header (Female) Straight package with 2.54 mm (0.10 in) col pitch, 0.64 mm lead width, 3.00 mm tail length and 8.50 mm insulator length with overall size 41.14 X 2.54 X 8.50 mm, pin pattern - clockwise from top left&lt;/p&gt;</description>
</package>
<package name="CONN_1X12">
<description>Single-row, 12-pin Receptacle Header (Female) Straight, 2.54 mm (0.10 in) col pitch, 8.50 mm insulator length, 30.98 X 2.54 X 8.50 mm body
&lt;p&gt;Single-row (1X12), 12-pin Receptacle Header (Female) Straight package with 2.54 mm (0.10 in) col pitch, 0.64 mm lead width, 3.00 mm tail length and 8.50 mm insulator length with overall size 30.98 X 2.54 X 8.50 mm, pin pattern - clockwise from top left&lt;/p&gt;</description>
</package>
<package name="CONN_1X5">
<description>Single-row, 5-pin Pin Header (Male) Straight, 2.54 mm (0.10 in) col pitch, 5.84 mm mating length, 12.70 X 2.14 X 8.38 mm body
&lt;p&gt;Single-row (1X5), 5-pin Pin Header (Male) Straight package with 2.54 mm (0.10 in) col pitch, 0.64 mm lead width, 3.00 mm tail length and 5.84 mm mating length with overall size 12.70 X 2.14 X 8.38 mm, pin pattern - clockwise from top left&lt;/p&gt;</description>
</package>
<package name="CUI_SJ1-3535NG">
</package>
<package name="0204/7">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
type 0204, grid 7.5 mm</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="R1" library="milador" package="0204/7" value="470">
<attribute name="NAME"/>
</element>
<element name="J1" library="milador" package="CUI_SJ1-3535NG" value="SJ1-3535NG">
<attribute name="MANUFACTURER" value="CUI"/>
<attribute name="NAME"/>
<attribute name="PARTREV" value="1.02"/>
<attribute name="STANDARD" value="Manufacturer recommendation"/>
</element>
<element name="J2" library="milador" package="CUI_SJ1-3535NG" value="SJ1-3535NG">
<attribute name="MANUFACTURER" value="CUI"/>
<attribute name="NAME"/>
<attribute name="PARTREV" value="1.02"/>
<attribute name="STANDARD" value="Manufacturer recommendation"/>
</element>
<element name="J3" library="milador" package="CUI_SJ1-3535NG" value="SJ1-3535NG">
<attribute name="MANUFACTURER" value="CUI"/>
<attribute name="NAME"/>
<attribute name="PARTREV" value="1.02"/>
<attribute name="STANDARD" value="Manufacturer recommendation"/>
</element>
<element name="J4" library="milador" package="CUI_SJ1-3535NG" value="SJ1-3535NG">
<attribute name="MANUFACTURER" value="CUI"/>
<attribute name="NAME"/>
<attribute name="PARTREV" value="1.02"/>
<attribute name="STANDARD" value="Manufacturer recommendation"/>
</element>
<element name="LED1" library="milador" package="NEOPIXELS-5MM" value="LED">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="U2" library="milador" package="CONN_1X12" value="CONN_1X12_FEMALECONN_1X12_FEMALE"/>
<element name="U3" library="milador" package="CONN_1X16" value="">
<attribute name="VALUE"/>
</element>
<element name="U1" library="milador" package="CONN_1X5" value="CONN_1X5_MALE"/>
</elements>
<signals>
<signal name="GND">
<contactref element="J1" pad="1"/>
<contactref element="J3" pad="1"/>
<contactref element="J4" pad="1"/>
<contactref element="LED1" pad="4"/>
<contactref element="LED1" pad="3"/>
<contactref element="U3" pad="4"/>
<contactref element="U1" pad="1"/>
<contactref element="J2" pad="1"/>
</signal>
<signal name="+3V3">
<contactref element="LED1" pad="2"/>
<contactref element="U3" pad="2"/>
<contactref element="U1" pad="5"/>
</signal>
<signal name="N$5">
<contactref element="J4" pad="3"/>
<contactref element="U2" pad="3"/>
</signal>
<signal name="N$4">
<contactref element="R1" pad="1"/>
<contactref element="LED1" pad="1"/>
</signal>
<signal name="N$8">
</signal>
<signal name="N$12">
</signal>
<signal name="N$13">
<contactref element="U1" pad="3"/>
<contactref element="U3" pad="10"/>
</signal>
<signal name="N$7">
<contactref element="U3" pad="9"/>
<contactref element="U1" pad="4"/>
</signal>
<signal name="N$9">
<contactref element="U3" pad="5"/>
<contactref element="J1" pad="2"/>
</signal>
<signal name="N$10">
<contactref element="U3" pad="6"/>
<contactref element="J1" pad="3"/>
</signal>
<signal name="N$11">
<contactref element="J2" pad="2"/>
<contactref element="U3" pad="7"/>
</signal>
<signal name="N$14">
<contactref element="J2" pad="3"/>
<contactref element="U3" pad="8"/>
</signal>
<signal name="N$3">
<contactref element="U2" pad="4"/>
<contactref element="J4" pad="2"/>
</signal>
<signal name="N$1">
<contactref element="U2" pad="6"/>
<contactref element="J3" pad="3"/>
</signal>
<signal name="N$2">
<contactref element="J3" pad="2"/>
<contactref element="U2" pad="7"/>
</signal>
<signal name="N$6">
<contactref element="R1" pad="2"/>
<contactref element="U2" pad="8"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
