<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="9.4.2">
<drawing>
<board>
<plain>
<wire x1="0" y1="90" x2="4.5" y2="94" width="0.4064" layer="20" curve="-90"/>
<wire x1="4.5" y1="94" x2="95.5" y2="94" width="0.4064" layer="20"/>
<wire x1="95.5" y1="94" x2="100" y2="90" width="0.4064" layer="20" curve="-90"/>
<wire x1="100" y1="90" x2="100" y2="64.5" width="0.4064" layer="20"/>
<wire x1="100" y1="64.5" x2="97.5" y2="62" width="0.4064" layer="20" curve="-90"/>
<wire x1="97.5" y1="62" x2="81.5" y2="62" width="0.4064" layer="20"/>
<wire x1="81.5" y1="62" x2="81.5" y2="32" width="0.4064" layer="20"/>
<wire x1="81.5" y1="32" x2="97.5" y2="32" width="0.4064" layer="20"/>
<wire x1="97.5" y1="32" x2="100" y2="29.5" width="0.4064" layer="20" curve="-90"/>
<wire x1="100" y1="29.5" x2="100" y2="4.5" width="0.4064" layer="20"/>
<wire x1="100" y1="4.5" x2="95.5" y2="0" width="0.4064" layer="20" curve="-90"/>
<wire x1="95.5" y1="0" x2="4.5" y2="0" width="0.4064" layer="20"/>
<wire x1="4.5" y1="0" x2="0" y2="4.5" width="0.4064" layer="20" curve="-90"/>
<wire x1="0" y1="4.5" x2="0" y2="90" width="0.4064" layer="20"/>
<text>LEFT</text>
<text>https://github.com/milador/Open-GCI</text>
<text>DOWN</text>
<text>UP</text>
<text>RIGHT</text>
<text>SELECT</text>
<text>START</text>
<text>L1</text>
<text>HOME</text>
<text>SQUARE</text>
<text>CIRCLE</text>
<text>X</text>
<text>R1</text>
<text>L2</text>
<text>R2</text>
<text>USB Powered</text>
<text>TRIANGLE</text>
<text>V 1.1</text>
</plain>
<libraries>
<library name="holes">
<description>&lt;b&gt;Mounting Holes and Pads&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="3,2-PAD">
<description>&lt;b&gt;MOUNTING PAD&lt;/b&gt; 3.2 mm, round</description>
</package>
</packages>
</library>
<library name="pinhead">
<description>&lt;b&gt;Pin Header Connectors&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="1X02">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="milador">
<packages>
<package name="CUI_SJ1-3535NG">
</package>
<package name="NEOPIXELS-5MM">
</package>
<package name="0204/7">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
type 0204, grid 7.5 mm</description>
</package>
<package name="CONN_2X10">
<description>Double-row, 20-pin Receptacle Header (Female) Straight, 2.54 mm (0.10 in) row pitch, 2.54 mm (0.10 in) col pitch, 8.50 mm insulator length, 25.90 X 5.08 X 8.50 mm body
&lt;p&gt;Double-row (2X10), 20-pin Receptacle Header (Female) Straight package with 2.54 mm (0.10 in) row pitch, 2.54 mm (0.10 in) col pitch, 0.64 mm lead width, 3.00 mm tail length and 8.50 mm insulator length with overall size 25.90 X 5.08 X 8.50 mm, pin pattern - clockwise from top left&lt;/p&gt;</description>
</package>
<package name="SIL9">
<description>&lt;b&gt;Single In Line&lt;/b&gt;</description>
</package>
<package name="SN74HCT245">
<description>20-DIP, 2.54 mm (0.10 in) pitch, 7.62 mm (0.30 in) span, 25.91 X 6.35 X 5.08 mm body
&lt;p&gt;20-pin DIP package with 2.54 mm (0.10 in) pitch, 7.62 mm (0.30 in) span with body size 25.91 X 6.35 X 5.08 mm&lt;/p&gt;</description>
</package>
<package name="RASPBERRYPI_ZERO">
<description>Raspberry Pi board model B+, full outline with position of big connectors &amp;amp; drill holes</description>
</package>
</packages>
</library>
<library name="SparkFun-Hardware">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
This library contains board components that are not electrical in nature, such as stand-offs, magnets, and Actobotics. 
&lt;br&gt;
&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is &lt;b&gt; the end user's responsibility&lt;/b&gt; to ensure correctness and suitablity for a given componet or application. 
&lt;br&gt;
&lt;br&gt;If you enjoy using this library, please buy one of our products at &lt;a href=" www.sparkfun.com"&gt;SparkFun.com&lt;/a&gt;.
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;
&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="STAND-OFF">
<description>&lt;h3&gt;Standoff (#4 Screw)&lt;/h3&gt;
&lt;p&gt;This is the mechanical footprint for a #4 phillips button head screw. Use the keepout ring to avoid running the screw head into surrounding components.&lt;/p&gt;
&lt;h4&gt;Devices Using&lt;/h4&gt;
&lt;ul&gt;&lt;li&gt;STAND-OFF&lt;/li&gt;&lt;/ul&gt;</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="IC1" library="milador" package="SN74HCT245" value="SN74HCT245">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="IC2" library="milador" package="SN74HCT245" value="SN74HCT245">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="JP2" library="milador" package="RASPBERRYPI_ZERO" value="RASPBERRYPI ZERO">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="H1" library="holes" package="3,2-PAD" value="MOUNT-PAD-ROUND3.2"/>
<element name="H2" library="holes" package="3,2-PAD" value="MOUNT-PAD-ROUND3.2"/>
<element name="H3" library="holes" package="3,2-PAD" value="MOUNT-PAD-ROUND3.2"/>
<element name="H4" library="holes" package="3,2-PAD" value="MOUNT-PAD-ROUND3.2"/>
<element name="RN1" library="milador" package="SIL9" value="9SIP">
<attribute name="NAME"/>
</element>
<element name="RN2" library="milador" package="SIL9" value="9SIP">
<attribute name="NAME"/>
</element>
<element name="R1" library="milador" package="0204/7" value="470">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="JP1" library="pinhead" package="1X02" value="No Rpi">
<attribute name="NAME"/>
</element>
<element name="J_L2" library="milador" package="CUI_SJ1-3535NG" value="SJ1-3535NG">
<attribute name="MANUFACTURER" value="CUI"/>
<attribute name="NAME"/>
<attribute name="PARTREV" value="1.02"/>
<attribute name="STANDARD" value="Manufacturer recommendation"/>
</element>
<element name="J_CIRCLE" library="milador" package="CUI_SJ1-3535NG" value="SJ1-3535NG">
<attribute name="MANUFACTURER" value="CUI"/>
<attribute name="NAME"/>
<attribute name="PARTREV" value="1.02"/>
<attribute name="STANDARD" value="Manufacturer recommendation"/>
</element>
<element name="J_R1" library="milador" package="CUI_SJ1-3535NG" value="SJ1-3535NG">
<attribute name="MANUFACTURER" value="CUI"/>
<attribute name="NAME"/>
<attribute name="PARTREV" value="1.02"/>
<attribute name="STANDARD" value="Manufacturer recommendation"/>
</element>
<element name="J_SQUARE" library="milador" package="CUI_SJ1-3535NG" value="SJ1-3535NG">
<attribute name="MANUFACTURER" value="CUI"/>
<attribute name="NAME"/>
<attribute name="PARTREV" value="1.02"/>
<attribute name="STANDARD" value="Manufacturer recommendation"/>
</element>
<element name="J_HOME" library="milador" package="CUI_SJ1-3535NG" value="SJ1-3535NG">
<attribute name="MANUFACTURER" value="CUI"/>
<attribute name="NAME"/>
<attribute name="PARTREV" value="1.02"/>
<attribute name="STANDARD" value="Manufacturer recommendation"/>
</element>
<element name="J_LEFT" library="milador" package="CUI_SJ1-3535NG" value="SJ1-3535NG">
<attribute name="MANUFACTURER" value="CUI"/>
<attribute name="NAME"/>
<attribute name="PARTREV" value="1.02"/>
<attribute name="STANDARD" value="Manufacturer recommendation"/>
</element>
<element name="J_DOWN" library="milador" package="CUI_SJ1-3535NG" value="SJ1-3535NG">
<attribute name="MANUFACTURER" value="CUI"/>
<attribute name="NAME"/>
<attribute name="PARTREV" value="1.02"/>
<attribute name="STANDARD" value="Manufacturer recommendation"/>
</element>
<element name="J_R2" library="milador" package="CUI_SJ1-3535NG" value="SJ1-3535NG">
<attribute name="MANUFACTURER" value="CUI"/>
<attribute name="NAME"/>
<attribute name="PARTREV" value="1.02"/>
<attribute name="STANDARD" value="Manufacturer recommendation"/>
</element>
<element name="J_X" library="milador" package="CUI_SJ1-3535NG" value="SJ1-3535NG">
<attribute name="MANUFACTURER" value="CUI"/>
<attribute name="NAME"/>
<attribute name="PARTREV" value="1.02"/>
<attribute name="STANDARD" value="Manufacturer recommendation"/>
</element>
<element name="J_L1" library="milador" package="CUI_SJ1-3535NG" value="SJ1-3535NG">
<attribute name="MANUFACTURER" value="CUI"/>
<attribute name="NAME"/>
<attribute name="PARTREV" value="1.02"/>
<attribute name="STANDARD" value="Manufacturer recommendation"/>
</element>
<element name="J_TRIANGLE" library="milador" package="CUI_SJ1-3535NG" value="SJ1-3535NG">
<attribute name="MANUFACTURER" value="CUI"/>
<attribute name="NAME"/>
<attribute name="PARTREV" value="1.02"/>
<attribute name="STANDARD" value="Manufacturer recommendation"/>
</element>
<element name="J_START" library="milador" package="CUI_SJ1-3535NG" value="SJ1-3535NG">
<attribute name="MANUFACTURER" value="CUI"/>
<attribute name="NAME"/>
<attribute name="PARTREV" value="1.02"/>
<attribute name="STANDARD" value="Manufacturer recommendation"/>
</element>
<element name="J_SELECT" library="milador" package="CUI_SJ1-3535NG" value="SJ1-3535NG">
<attribute name="MANUFACTURER" value="CUI"/>
<attribute name="NAME"/>
<attribute name="PARTREV" value="1.02"/>
<attribute name="STANDARD" value="Manufacturer recommendation"/>
</element>
<element name="J_RIGHT" library="milador" package="CUI_SJ1-3535NG" value="SJ1-3535NG">
<attribute name="MANUFACTURER" value="CUI"/>
<attribute name="NAME"/>
<attribute name="PARTREV" value="1.02"/>
<attribute name="STANDARD" value="Manufacturer recommendation"/>
</element>
<element name="J_UP" library="milador" package="CUI_SJ1-3535NG" value="SJ1-3535NG">
<attribute name="MANUFACTURER" value="CUI"/>
<attribute name="NAME"/>
<attribute name="PARTREV" value="1.02"/>
<attribute name="STANDARD" value="Manufacturer recommendation"/>
</element>
<element name="L1" library="milador" package="NEOPIXELS-5MM" value="NEOPIXELS">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="H8" library="SparkFun-Hardware" package="STAND-OFF" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="H7" library="SparkFun-Hardware" package="STAND-OFF" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="JP3" library="milador" package="CONN_2X10" value="BROOK">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="H5" library="SparkFun-Hardware" package="STAND-OFF" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="H6" library="SparkFun-Hardware" package="STAND-OFF" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
</elements>
<signals>
<signal name="GND">
<contactref element="JP2" pad="6"/>
<contactref element="JP2" pad="9"/>
<contactref element="JP2" pad="25"/>
<contactref element="JP2" pad="14"/>
<contactref element="JP2" pad="20"/>
<contactref element="JP2" pad="30"/>
<contactref element="JP2" pad="34"/>
<contactref element="IC1" pad="10"/>
<contactref element="IC1" pad="1"/>
<contactref element="IC1" pad="19"/>
<contactref element="IC2" pad="1"/>
<contactref element="IC2" pad="10"/>
<contactref element="IC2" pad="19"/>
<contactref element="JP2" pad="39"/>
<contactref element="H1" pad="B3,2"/>
<contactref element="H2" pad="B3,2"/>
<contactref element="H3" pad="B3,2"/>
<contactref element="H4" pad="B3,2"/>
<contactref element="J_L2" pad="1"/>
<contactref element="J_CIRCLE" pad="1"/>
<contactref element="J_R1" pad="1"/>
<contactref element="J_SQUARE" pad="1"/>
<contactref element="J_HOME" pad="1"/>
<contactref element="J_LEFT" pad="1"/>
<contactref element="J_DOWN" pad="1"/>
<contactref element="J_R2" pad="1"/>
<contactref element="J_X" pad="1"/>
<contactref element="J_L1" pad="1"/>
<contactref element="J_TRIANGLE" pad="1"/>
<contactref element="J_START" pad="1"/>
<contactref element="J_SELECT" pad="1"/>
<contactref element="J_RIGHT" pad="1"/>
<contactref element="J_UP" pad="1"/>
<contactref element="L1" pad="4"/>
<contactref element="L1" pad="3"/>
<contactref element="JP3" pad="GND1"/>
<contactref element="JP3" pad="GND2"/>
<contactref element="JP3" pad="GND3"/>
</signal>
<signal name="NJ_L2">
<contactref element="IC1" pad="2"/>
<contactref element="J_L2" pad="2"/>
<contactref element="JP3" pad="L2"/>
</signal>
<signal name="NJ_CIR">
<contactref element="IC1" pad="3"/>
<contactref element="J_CIRCLE" pad="2"/>
<contactref element="JP3" pad="CIRCLE"/>
</signal>
<signal name="NJ_R1">
<contactref element="IC1" pad="4"/>
<contactref element="J_R1" pad="2"/>
<contactref element="JP3" pad="R1"/>
</signal>
<signal name="NJ_SQU">
<contactref element="IC1" pad="5"/>
<contactref element="J_SQUARE" pad="2"/>
<contactref element="JP3" pad="SQUARE"/>
</signal>
<signal name="NJ_HOME">
<contactref element="IC1" pad="6"/>
<contactref element="J_HOME" pad="2"/>
<contactref element="JP3" pad="HOME"/>
</signal>
<signal name="NJ_LEFT">
<contactref element="IC1" pad="7"/>
<contactref element="J_LEFT" pad="2"/>
<contactref element="JP3" pad="LEFT"/>
</signal>
<signal name="NJ_DOWN">
<contactref element="IC1" pad="8"/>
<contactref element="J_DOWN" pad="2"/>
<contactref element="JP3" pad="DOWN"/>
</signal>
<signal name="NJ_R2">
<contactref element="IC2" pad="2"/>
<contactref element="J_R2" pad="2"/>
<contactref element="JP3" pad="R2"/>
</signal>
<signal name="NJ_X">
<contactref element="IC2" pad="3"/>
<contactref element="J_X" pad="2"/>
<contactref element="JP3" pad="X"/>
</signal>
<signal name="NJ_L1">
<contactref element="IC2" pad="4"/>
<contactref element="J_L1" pad="2"/>
<contactref element="JP3" pad="L1"/>
</signal>
<signal name="NJ_TRI">
<contactref element="IC2" pad="5"/>
<contactref element="J_TRIANGLE" pad="2"/>
<contactref element="JP3" pad="TRIANGLE"/>
</signal>
<signal name="NJ_START">
<contactref element="IC2" pad="6"/>
<contactref element="J_START" pad="2"/>
<contactref element="JP3" pad="START"/>
</signal>
<signal name="+5V">
<contactref element="IC1" pad="20"/>
<contactref element="IC2" pad="20"/>
<contactref element="RN1" pad="1"/>
<contactref element="RN2" pad="1"/>
<contactref element="JP2" pad="2"/>
<contactref element="JP2" pad="4"/>
<contactref element="JP1" pad="2"/>
<contactref element="L1" pad="2"/>
</signal>
<signal name="NGP7">
<contactref element="IC1" pad="18"/>
<contactref element="JP2" pad="7"/>
<contactref element="RN1" pad="2"/>
</signal>
<signal name="NGP11">
<contactref element="JP2" pad="11"/>
<contactref element="IC1" pad="17"/>
<contactref element="RN1" pad="3"/>
</signal>
<signal name="NGP13">
<contactref element="IC1" pad="16"/>
<contactref element="JP2" pad="13"/>
<contactref element="RN1" pad="4"/>
</signal>
<signal name="NGP15">
<contactref element="JP2" pad="15"/>
<contactref element="IC1" pad="15"/>
<contactref element="RN1" pad="5"/>
</signal>
<signal name="NGP19">
<contactref element="IC1" pad="14"/>
<contactref element="JP2" pad="19"/>
<contactref element="RN1" pad="6"/>
</signal>
<signal name="NGP21">
<contactref element="JP2" pad="21"/>
<contactref element="IC1" pad="13"/>
<contactref element="RN1" pad="7"/>
</signal>
<signal name="NGP23">
<contactref element="IC1" pad="12"/>
<contactref element="JP2" pad="23"/>
<contactref element="RN1" pad="8"/>
</signal>
<signal name="NGP31">
<contactref element="IC2" pad="18"/>
<contactref element="JP2" pad="31"/>
<contactref element="RN2" pad="2"/>
</signal>
<signal name="NGP33">
<contactref element="IC2" pad="17"/>
<contactref element="JP2" pad="33"/>
<contactref element="RN2" pad="3"/>
</signal>
<signal name="NGP35">
<contactref element="IC2" pad="16"/>
<contactref element="JP2" pad="35"/>
<contactref element="RN2" pad="4"/>
</signal>
<signal name="NGP37">
<contactref element="IC2" pad="15"/>
<contactref element="JP2" pad="37"/>
<contactref element="RN2" pad="5"/>
</signal>
<signal name="NGP40">
<contactref element="IC2" pad="14"/>
<contactref element="JP2" pad="40"/>
<contactref element="RN2" pad="6"/>
</signal>
<signal name="NGP38">
<contactref element="IC2" pad="13"/>
<contactref element="JP2" pad="38"/>
<contactref element="RN2" pad="7"/>
</signal>
<signal name="NGP36">
<contactref element="IC2" pad="12"/>
<contactref element="JP2" pad="36"/>
<contactref element="RN2" pad="8"/>
</signal>
<signal name="NGP32">
<contactref element="IC2" pad="11"/>
<contactref element="JP2" pad="32"/>
<contactref element="RN2" pad="9"/>
</signal>
<signal name="+3V3">
<contactref element="JP2" pad="1"/>
<contactref element="JP2" pad="17"/>
</signal>
<signal name="N$33">
<contactref element="R1" pad="1"/>
<contactref element="L1" pad="1"/>
</signal>
<signal name="NGP12">
<contactref element="IC1" pad="11"/>
<contactref element="JP2" pad="12"/>
</signal>
<signal name="+5V/2">
<contactref element="JP1" pad="1"/>
<contactref element="JP3" pad="VCC1"/>
<contactref element="JP3" pad="VCC2"/>
</signal>
<signal name="N$32">
<contactref element="IC1" pad="9"/>
<contactref element="R1" pad="2"/>
</signal>
<signal name="NJ_UP">
<contactref element="IC2" pad="9"/>
<contactref element="J_UP" pad="2"/>
<contactref element="JP3" pad="UP"/>
</signal>
<signal name="NJ_RIGHT">
<contactref element="IC2" pad="8"/>
<contactref element="J_RIGHT" pad="2"/>
<contactref element="JP3" pad="RIGHT"/>
</signal>
<signal name="NJ_SELECT">
<contactref element="IC2" pad="7"/>
<contactref element="J_SELECT" pad="2"/>
<contactref element="JP3" pad="SELECT"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
