{"text_format":"3","workbook":"xls","n_sheets":1,"sheets":["BOC"],"not_rendered":{"external_links":1,"defined_names":1},"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"BOC","index":0,"n_rows":94,"n_cols":13,"rows_kept":94,"flags":["formulas_cached_only"]}
["Item #","Comment","Quantity","Designator","Footprint","Manufacturer","Manufacturer Part Number 1","Supplier 1","Supplier Part Number 1","Part Description","Assembly Info","Number of NF parts in row","Number of fitted parts in row"]
[1,"10pF, 25V",1,"C1","CAP0402","AVX","04023A100JAT2A","Farnell","2332478RL","10pF ±5% 25V C0G, NP0 Ceramic Capacitor -55°C ~ 125°C Surface Mount, MLCC 0402 (1005 Metric) 0.039\" L x 0.020\" W (1.00mm x 0.50mm)","",null,1]
[2,"1uF, 10V",6,"C2, C159, C164, C165, C186, C194","CAP0402","TDK","C1005X5R1E105K050BC","Digi-Key","445-9066-1-ND","1µF ±10% 10V X5R Ceramic Capacitor -55°C ~ 85°C Surface Mount, MLCC 0402 (1005 Metric) 0.039\" L x 0.020\" W (1.00mm x 0.50mm)","NF(C186 C194)",2,4]
[3,"100pF, 50V",18,"C3, C5, C7, C16, C17, C19, C20, C22, C23, C71, C84, C167, C168, C169, C170, C172, C173, C192","CAP0402","Yageo","CC0402JRNPO9BN101","Digi-Key","311-1024-1-ND","100pF ±5% 50V C0G, NP0 Ceramic Capacitor -55°C ~ 125°C Surface Mount, MLCC 0402 (1005 Metric) 0.039\" L x 0.020\" W (1.00mm x 0.50mm)","NF(C7 C19 C20 C22 C71 C84 C192)",7,11]
[4,"100nF, 16V",28,"C4, C6, C8, C15, C18, C21, C97, C129, C132, C133, C153, C154, C155, C156, C161, C162, C163, C166, C171, C174, C175, C176, C181, C182, C185, C195, MN12, MN15","CAP0402","Murata Electronics","GRM155R71C104KA88D","Mouser","81-GRM155R71C104KA88","0.10µF ±10% 16V X7R Ceramic Capacitor -55°C ~ 125°C Surface Mount, MLCC 0402 (1005 Metric) 0.039\" L x 0.020\" W (1.00mm x 0.50mm)","NF(C6 C21 C174 C176 C182 C185)",6,22]
[5,"47pF, 50V",4,"C9, C12, C24, C27","CAP0402","TDK Corporation","GRM1555C1H470FA01D","Digi-Key","490-6241-1-ND","47pF ±1% 50V C0G, NP0 Ceramic Capacitor -55°C ~ 125°C Surface Mount, MLCC 0402 (1005 Metric) 0.039\" L x 0.020\" W (1.00mm x 0.50mm)","",null,4]
[6,"510pF",6,"C10, C11, C25, C26, MN21, MN24","CAP0402","Murata Electronics North America","GRM1555C1H511JA01D","Digi-Key","490-3237-1-ND","510pF ±5% 50V C0G, NP0 Ceramic Capacitor -55°C ~ 125°C Surface Mount, MLCC 0402 (1005 Metric) 0.039\" L x 0.020\" W (1.00mm x 0.50mm)","",null,6]
[7,"10nF, 50V",14,"C13, C14, C28, C29, C102, C104, C109, C113, C115, C119, C124, C146, C148, C150","CAP0402","Murata","GRM155R71H103KA88D","Digi-Key","490-4516-1-ND","10000pF ±10% 50V Ceramic Capacitor X7R 0402 (1005 Metric)","",null,14]
[8,"1uF, 6.3V",59,"C30, C32, C33, C34, C35, C36, C37, C39, C41, C43, C44, C45, C46, C48, C49, C50, C51, C52, C53, C54, C55, C56, C57, C58, C59, C60, C62, C63, C64, C65, C66, C67, C73, C75, C77, C79, C81, C85, C86, C87, C88, C89, C90, C91, C92, C93, C94, C95, C96, C100, C111, C117, C122, C135, C137, C139, C141, C144, C152","CAP0201","TDK Corporation","JMK063ABJ105MP-F","Digi-Key","587-5864-2-ND","1µF ±20% 6.3V X5R Ceramic Capacitor -55°C ~ 85°C Surface Mount, MLCC 0201 (0603 Metric) 0.024\" L x 0.012\" W (0.60mm x 0.30mm)","",null,59]
[9,"1nF, 10%",11,"C31, C38, C40, C42, C47, C61, C72, C74, C76, C78, C80","CAP0201","TDK Corporation","C0603X7R1E102K030BA","Digi-Key","445-7275-1-ND","1000pF ±10% 25V X7R Ceramic Capacitor -55°C ~ 125°C Surface Mount, MLCC 0201 (0603 Metric) 0.024\" L x 0.012\" W (0.60mm x 0.30mm)","",null,11]
[10,"4.7uF, 6.3V",10,"C68, C69, C82, C83, C179, C180, C187, C190, C191, C197","CAP0402","Murata Electronics North America","GRM155R60J475ME87D","Digi-Key","490-5408-1-ND","4.7µF ±20% 6.3V X5R Ceramic Capacitor -55°C ~ 85°C Surface Mount, MLCC 0402 (1005 Metric) 0.039\" L x 0.020\" W (1.00mm x 0.50mm)","NF(C187)",1,9]
[11,"10uF, 6.3V",9,"C70, C99, C116, C121, C134, C143, C151, C196, C198","CAP0603","Yageo","CC0603MRX5R5BB106","Digi-Key","311-1448-2-ND","10µF ±20% 6.3V X5R Ceramic Capacitor -55°C ~ 85°C Surface Mount, MLCC 0603 (1608 Metric) 0.063\" L x 0.031\" W (1.60mm x 0.80mm)","",null,9]
[12,"100nF, 6.3V",24,"C98, C101, C103, C105, C106, C107, C108, C110, C112, C114, C118, C120, C123, C125, C126, C127, C128, C136, C138, C140, C142, C145, C147, C149","CAP0201","Murata","GRT033C81A104KE01D","Digi-Key","490-12232-1-ND","0.10µF ±10% 6.3V X6S Ceramic Capacitor -55°C ~ 105°C Surface Mount, MLCC 0201 (0603 Metric) 0.024\" L x 0.012\" W (0.60mm x 0.30mm)","",null,24]
[13,"10pF, 5%",2,"C130, C131","CAP0402","AVX","04023A100JAT2A","Farnell","2332478RL","10pF ±5% 25V C0G, NP0 Ceramic Capacitor -55°C ~ 125°C Surface Mount, MLCC 0402 (1005 Metric) 0.039\" L x 0.020\" W (1.00mm x 0.50mm)","",null,2]
[14,"18nF, 16V",1,"C157","CAP0402","Yageo","CC0402KRX7R7BB183","Digi-Key","311-1706-1-ND","CAP CER 0.018UF 16V X7R 0402","NF(C157)",1,0]
[15,"47pF",2,"C158, C160","CAP0402","TDK Corporation","GRM1555C1H470FA01D","Digi-Key","490-6241-1-ND","47pF ±1% 50V C0G, NP0 Ceramic Capacitor -55°C ~ 125°C Surface Mount, MLCC 0402 (1005 Metric) 0.039\" L x 0.020\" W (1.00mm x 0.50mm)","NF(C158 C160)",2,0]
[16,"22uF, 10V",4,"C177, C178, C188, C189","CAP0603","TDK Corporation","C1608X5R1A226M080AC","Mouser","810-C1608X5R1A226M","22µF ±20% 10V X5R Ceramic Capacitor -55°C ~ 85°C Surface Mount, MLCC 0603 (1608 Metric) 0.063\" L x 0.031\" W (1.60mm x 0.80mm)","",null,4]
[17,"1nF, 50V",1,"C183","CAP0402","Murata Electronics","GCM155R71H102KA37D","Mouser","81-GCM155R71H102KA7D","1000pF ±10% 50V X7R Ceramic Capacitor -55°C ~ 125°C Surface Mount, MLCC 0402 (1005 Metric) 0.039\" L x 0.020\" W (1.00mm x 0.50mm)","NF(C183)",1,0]
[18,"470pF, 50V",2,"C184, C193","CAP0402","TDK Corporation","C1005C0G1H471J050BA","Digi-Key","445-2656-6-ND","470pF ±5% 50V Ceramic Capacitor C0G, NP0 0402 (1005 Metric)","",null,2]
[19,"ESD8472",2,"ESD1, ESD2","ESD8472_X3DFN2","ON Semiconductor","ESD8472MUT5G","Digi-Key","ESD8472MUT5GOSCT-ND","TVS DIODE 5.3VWM 14VC X3DFN2","NF(ESD1 ESD2)",2,0]
[20,"ESD7016",1,"ESD3","ESD7016","ON Semiconductor","ESD7016MUTAG","Digi-Key","ESD7016MUTAGOSDKR-ND","TVS DIODE 5VWM 10VC 8UDFN","",null,1]
[21,"5V DC FAN",1,"FAN1","","Sunon Fans","MC30060V2-000U-A99","Digi-Key","259-1572-ND","FAN AXIAL 30X6.9MM 5VDC WIRE","NF(FAN1)",1,0]
[22,"Fiducial",1,"FL1","Fiducial_local","","","","","","",null,1]
[23,"600R, 0.27A",37,"FR1, FR2, FR3, FR4, FR5, FR6, FR7, FR8, FR9, FR10, FR11, FR12, FR13, FR14, FR15, FR16, FR17, FR18, FR19, FR20, FR21, FR24, FR26, FR27, FR28, FR29, FR30, FR31, FR32, FR33, FR34, FR38, FR39, FR40, FR41, FR42, FR43","RES0201","Taiyo Yuden","BK0603TS601-T","Digi-Key","587-3277-1-ND","FERRITE BEAD 600 OHM 0201 1LN","NF(FR42 FR43)",2,35]
[24,"220R, 0.9A",6,"FR22, FR25, FR35, FR37, FR44, FR45","RES0402","TDK Corporation","MPZ1005S221ET000","Digi-Key","445-9329-2-ND","FERRITE BEAD 220 OHM 0402 1LN","",null,6]
[25,"600R, 2A",2,"FR23, FR36","RES0805","TDK Corporation","MPZ2012S601AT000","Digi-Key","445-2206-2-ND","FERRITE BEAD 600 OHM 0805 1LN","",null,2]
[26,"LMS7002M",1,"IC1","LMS7002M_v5","Lime Microsystems","LMS7002M","Lime Microsystems","LMS7002M","IC FPRF Transceiver LMS7002M; 261 pin aQFN","",null,1]
[27,"M24128",2,"IC2, IC12","M24128-DFMC6TG","STMicroelectronics","M24128-DFMC6TG","Digi-Key","497-15739-1-ND","EEPROM Memory IC 128Kb (16K x 8) I²C 1MHz 450ns 8-UFDFPN (2x3)","NF(IC2 IC12)",2,0]
[28,"SKY13411-374LF",2,"IC3, IC4","SKY13411-374LF","Skyworks Solutions Inc.","SKY13411-374LF","Digi-Key","863-1455-1-ND","RF Switch IC 802.11a/b/g/n DPDT 50 Ohm 6-MLPD (1.5x1.5)","",null,2]
[29,"LD39100PUR",4,"IC5, IC6, IC13, IC18","LD39100PUR","STMicroelectronics","LD39100PUR","Digi-Key","497-11013-1-ND","Linear Voltage Regulator IC Positive Adjustable Output 0.8 V ~ 4.5 V 1A 6-DFN (3x3)","",null,4]
[30,"LFE5U-25F-MG285",1,"IC7","LFE5U-25F-8MG285C_LATTICE_FPGA","Lattice Semiconductor","LFE5U-25F-8MG285C","Digi-Key","LFE5U-25F-8MG285C-ND","series Field Programmable Gate Array (FPGA) IC 118 1032192 24000 285-LFBGA, CSPBGA","",null,1]
[31,"FT601Q",1,"IC8","FT601Q","FTDI, Future Technology Devices International Ltd","FT601Q-B-T","Digi-Key","768-1311-ND","IC USB3-32BIT SYNC FIFO 76QFN","",null,1]
[32,"LMK00105",1,"IC9","LMK00105SQ","Texas Instruments","LMK00105SQ/NOPB","Digi-Key","LMK00105SQ/NOPBCT-ND","IC CLK BUFFER 2:5 200MHZ 24WQFN","",null,1]
[33,"LM75",1,"IC10","HWSON8_LM75","NXP Semiconductors","LM75BTP,147","Digi-Key","568-9815-2-ND","SENSOR TEMPERATURE I2C 8HWSON","",null,1]
[34,"DAC6311IDCK",1,"IC11","AD5601_SOT23-6","Texas Instruments","DAC6311IDCKT","Digi-Key","296-23716-1-ND","10 Bit Digital to Analog Converter 1 SC-70-6","",null,1]
[35,"LMZ10501",2,"IC14, IC19","LMZ10501","Texas Instruments","LMZ10501SILR","Digi-Key","296-37104-1-ND","n  Non-Isolated PoL Module DC DC Converter 1 Output 0.6 ~ 3.6 V 1A 2.7V - 5.5V Input","",null,2]
[36,"W25Q128JVSIQ",1,"IC15","S25FL164K_WSON8_DFN6","Winbond","W25Q128JVSIQ","Digi-Key","W25Q128JVSIQ-ND","FLASH - NOR Memory IC 128Mb (16M x 8) SPI - Quad I/O, QPI, DTR 133 MHz 8-SOIC","",null,1]
[37,"AD5662",1,"IC16","AD5662_SOT23-8","Analog Devices Inc.","AD5662BRJZ-2REEL7","Digi-Key","AD5662BRJZ-2REEL7CT-ND","IC DAC 16BIT BUFF V-OUT SOT23-8","NF(IC16)",1,0]
[38,"MCP1525T",1,"IC17","SOT23-3_v2","Microchip Technology","MCP1525T-I/TT","Digi-Key","MCP1525T-I/TTDKR-ND","Series Voltage Reference IC ±1% 2mA SOT-23-3","NF(IC17)",1,0]
[39,"SMA board edge",2,"J1, J2","SMA_connector_board_edge_SM","RF Solutions","CON-SMA-EDGE-S","Digi-Key","CON-SMA-EDGE-S-ND","SMA Connector Jack, Female Socket Board Edge, End Launch Solder","",null,2]
[40,"FPGA GPIO",1,"J3","SWD_10_pin","Harwin Inc","M50-3600542","Digi-Key","952-1389-ND","CONN HDR 1.27MM SMD AU 10POS","NF(J3)",1,0]
[41,"FPGA EGPIO (board edge)",1,"J4","Header5x1_TH_v2","Amphenol FCI","69190-405HLF","Digi-Key","609-4726-ND","5 Positions Header Connector 0.100\" (2.54mm) Through Hole Tin","NF(J4)",1,0]
[42,"FPGA JTAG (board edge)",1,"J5","Header7x1_TH_v2","Sullins Connector Solutions","PEC07SAAN","Digi-Key","S1012E-07-ND","7 Positions Header, Unshrouded, Breakaway Connector 0.100\" (2.54mm) Through Hole Tin","NF(J5)",1,0]
[43,"USB3.0_MALE",1,"J6","USB3A_SM","Wurth Electronics Inc.","692112030100","Digi-Key","732-3157-ND","USB - A USB 3.0 (USB 3.1 Gen 1, Superspeed) Plug Connector 9 Position Surface Mount, Right Angle","",null,1]
[44,"U.FL/MMCX",2,"J7, J8","MMCX_UFL_conn_u","Molex, LLC","0734120110","Digi-Key","WM5587CT-ND","Ultra Miniature Coaxial Connector Receptacle, Male Pin 50 Ohm Surface Mount Solder","",null,2]
[45,"FAN",1,"J9","Header2x1_TH_v2","3M","961102-6404-AR","Digi-Key","3M9447-ND","2 Positions Header, Unshrouded Connector 0.100\" (2.54mm) Through Hole Gold","NF(J9)",1,0]
[46,"LED_RG",3,"LED1, LED2, LED3","LED-2x0603","Avago Technologies US Inc.","HSMF-C165","Digi-Key","516-1419-1-ND","LED GREEN/RED DIFFUSED 0603 SMD","",null,3]
[47,"RFI Shield clip",12,"MECH1, MECH2, MECH3, MECH4, MECH12, MECH13, MECH14, MECH15, MECH17, MECH19, MECH20, MECH21","RFI_SHIELD_CLPS_MINI","HARWIN","S0971-46R","Farnell","2361677","RFI SHIELD CLIP MINI TIN SMD","NF(MECH1 MECH2 MECH3 MECH4 MECH17 MECH19 MECH20 MECH21)",8,4]
[48,"RFI Shield",3,"MECH5, MECH16, MECH18","WurthElectronic_RF_shield","WURTH ELEKTRONIK","36003250","Farnell","1909662","Enclosure, Shielding Cabinet Cover, Shielding Cabinet, 25 mm, 25 mm, 3 mm, Tin Plate","NF(MECH5 MECH18)",2,1]
[49,"Spacer M3",2,"MECH6, MECH7","","BOSSARD","TDYSFF-M3/5","TME","TDYSFF-M3/5","Screwed spacer sleeve; Int.thread: M3; 5mm; brass","NF(MECH6 MECH7)",2,0]
[50,"Screws M3 v1",2,"MECH8, MECH9","","KRAFTBERG","M3X3/D7985","TME","M3X3/D7985","Screw; M3x3; DIN:7985; Head: cheese head; Phillips; steel; zinc; PH1","NF(MECH8 MECH9)",2,0]
[51,"Screws M3 v2",2,"MECH10, MECH11","","KRAFTBERG","M3X8/D7985B","TME","M3X8/D7985B","Screw; M3x8; DIN:7985; Head: cheese head; Phillips; black finish","NF(MECH10 MECH11)",2,0]
[52,"8.2nH, 5%",3,"MN1, MN2, MN22","RES0402","COILCRAFT","0402HP-8N2XJLU","Farnell","2285826","Surface Mount High Frequency Inductor, 0402HP Series, 8.2 nH, ± 5%, 0402 [1005 Metric], 5.4 GHz","NF(MN22)",1,2]
[53,"100uH",2,"MN3, MN17","RES0805_0603","TDK Corporation","MLF2012C101KT000","Digi-Key","445-1071-1-ND","FIXED IND 100UH 2MA 3.1 OHM SMD","NF(MN3 MN17)",2,0]
[54,"0.8pF",2,"MN4, MN7","CAP0402","Murata Electronics North America","GRM1555C1HR80BA01D","Digi-Key","490-6269-1-ND","0.80pF ±0.1pF 50V C0G, NP0 Ceramic Capacitor -55°C ~ 125°C Surface Mount, MLCC 0402 (1005 Metric) 0.039\" L x 0.020\" W (1.00mm x 0.50mm)","",null,2]
[55,"1pF",3,"MN5, MN13, MN19","CAP0402","TDK Corporation","C1005C0G1H010B050BA","Digi-Key","445-4854-6-ND","1pF ±0.1pF 50V C0G, NP0 Ceramic Capacitor -55°C ~ 125°C Surface Mount, MLCC 0402 (1005 Metric) 0.039\" L x 0.020\" W (1.00mm x 0.50mm)","NF(MN5 MN13)",2,1]
[56,"0.5pF",2,"MN6, MN18","CAP0402","Yageo","CC0402CRNPO9BNR50","Digi-Key","311-1001-1-ND","0.50pF ±0.25pF 50V C0G, NP0 Ceramic Capacitor -55°C ~ 125°C Surface Mount, MLCC 0402 (1005 Metric) 0.039\" L x 0.020\" W (1.00mm x 0.50mm)","NF(MN18)",1,1]
[57,"100uH",2,"MN8, MN9","RES0805","TDK Corporation","MLF2012C101KT000","Digi-Key","445-1071-1-ND","FIXED IND 100UH 2MA 3.1 OHM SMD","",null,2]
[58,"0R",31,"MN10, MN11, R14, R15, R20, R21, R26, R27, R32, R34, R35, R36, R37, R42, R43, R44, R45, R46, R53, R61, R63, R65, R66, R69, R76, R89, R93, R95, R97, R99, R100","RES0402","Yageo","RC0402JR-070RL","Digi-Key","311-0.0JRTR-ND","RES SMD 0.0OHM JUMPER 1/16W 0402","NF(R14 R15 R20 R21 R26 R43 R66 R76 R95 R99 R100)",11,20]
[59,"2pF",3,"MN14, MN16, MN20","CAP0402","AVX","04025U2R0BAT2A","Farnell","2332536","SMD Multilayer Ceramic Capacitor, U Series, 2 pF, ± 0.1pF, C0G / NP0, 50 V, 0402 [1005 Metric]","",null,3]
[60,"1.2pF",1,"MN23","CAP0402","Murata Electronics North America","GRM1555C1H1R2CA01D","Digi-Key","490-5927-1-ND","'1.2pF ±0.25pF 50V C0G, NP0 Ceramic Capacitor -55°C ~ 125°C Surface Mount, MLCC 0402 (1005 Metric) 0.039\" L x 0.020\" W (1.00mm x 0.50mm)","",null,1]
[61,"10k, 1%",19,"R1, R2, R3, R4, R5, R10, R11, R39, R54, R55, R56, R58, R62, R72, R74, R77, R81, R83, R85","RES0402","Yageo","RC0402FR-0710KL","Digi-Key","311-10.0KLRTR-ND","RES SMD 10K OHM 1% 1/16W 0402","NF(R81)",1,18]
[62,"49.9R, 1%",7,"R6, R7, R8, R9, R22, R23, R67","RES0402","Samsung Electro-Mechanics America, Inc.","RC1005F49R9CS","Digi-Key","1276-3469-6-ND","RES SMD 49.9 OHM 1% 1/16W 0402","",null,7]
[63,"2k2, 1%",2,"R12, R13","RES0402","Stackpole Electronics Inc","RMCF0402FT2K20","Digi-Key","RMCF0402FT2K20CT-ND","RES SMD 2.2K OHM 1% 1/16W 0402","",null,2]
[64,"560R, 1%",1,"R16","RES0402","Vishay Dale","CRCW0402560RFKED","Digi-Key","541-560LCT-ND","RES SMD 560 OHM 1% 1/16W 0402","NF(R16)",1,0]
[65,"100R, 1%",9,"R17, R24, R25, R84, R86, R91, R94, R96, R98","RES0402","Stackpole Electronics Inc.","RMCF0402FT100R","Digi-Key","RMCF0402FT100RDKR-ND","RES SMD 100 OHM 1% 1/16W 0402","NF(R17 R24)",2,7]
[66,"2.49k, 1%",1,"R18","RES0402","Yageo","RC0402FR-072K49L","Digi-Key","311-2.49KLRDKR-ND","RES SMD 2.49K OHM 1% 1/16W 0402","",null,1]
[67,"1k, 1%",5,"R19, R68, R70, R75, R78","RES0402","Stackpole Electronics Inc","RMCF0402FT1K00","Digi-Key","RMCF0402FT1K00TR-ND","RES SMD 1K OHM 1% 1/16W 0402","NF(R19 R78)",2,3]
[68,"10R",4,"R28, R29, R40, R41","RES0201","Panasonic Electronic Components","ERJ-1GEF10R0C","Digi-Key","P10.0ABCT-ND","RES SMD 10 OHM 1% 1/20W 0201","",null,4]
[69,"0R",1,"R30","RES0201","Rohm Semiconductor","RC0201FR-070RL","Digi-Key","311-0.0MCT-ND","RES SMD 0.0OHM JUMPER 1/20W 0201","",null,1]
[70,"8.2k, 1%",1,"R31","RES0402","Yageo","RC0402FR-078K2L","Digi-Key","311-8.20KLRCT-ND","RES SMD 8.2K OHM 1% 1/16W 0402","",null,1]
[71,"15k, 1%",1,"R33","RES0402","Yageo","RC0402FR-0715KL","Digi-Key","311-15.0KLRCT-ND","RES SMD 15K OHM 1% 1/16W 0402","",null,1]
[72,"7.5k, 1%",1,"R38","RES0402","Yageo","RC0402FR-077K5L","Digi-Key","YAG3512CT-ND","±1% 0.063W, 1/16W Chip Resistor 0402 (1005 Metric) Automotive AEC-Q200, Moisture Resistant Thick Film","",null,1]
[73,"4K7, 1%",9,"R47, R48, R49, R50, R51, R52, R57, R88, R92","RES0402","Yageo","RC0402FR-074K7L","Digi-Key","311-4.7KLRCT-ND","±1% 0.063W, 1/16W Chip Resistor 0402 (1005 Metric) Moisture Resistant Thick Film","NF(R92)",1,8]
[74,"22R",2,"R59, R64","RES0402","Yageo","RC0402FR-0722RL","Digi-Key","311-22.0LRTR-ND","RES SMD 22 OHM 1% 1/16W 0402","",null,2]
[75,"1k6, 1%",1,"R60","RES0402","Yageo","RC0402FR-071K6L","Digi-Key","YAG3045CT-ND","RES SMD 1.6K OHM 1% 1/16W 0402","",null,1]
[76,"3k, 1%",2,"R71, R73","RES0402","Vishay Dale","RMCF0402FT3K00","Digi-Key","RMCF0402FT3K00TR-ND","RES SMD 3K OHM 1% 1/16W 0402","NF(R73)",1,1]
[77,"187k, 1%",1,"R79","RES0402","Yageo","RC0402FR-07187KL","Digi-Key","311-187KLRCT-ND","187 kOhms ±1% 0.063W, 1/16W Chip Resistor 0402 (1005 Metric) Moisture Resistant Thick Film","",null,1]
[78,"27k, 1%",1,"R80","RES0402","Yageo","RC0402FR-0727KL","Digi-Key","311-27.0KLRCT-ND","27 kOhms ±1% 0.063W, 1/16W Chip Resistor 0402 (1005 Metric) Moisture Resistant Thick Film","",null,1]
[79,"82.5k, 1%",1,"R82","RES0402","Yageo","RC0402FR-0782K5L","Digi-Key","311-82.5KLRCT-ND","82.5 kOhms ±1% 0.063W, 1/16W Chip Resistor 0402 (1005 Metric) Moisture Resistant Thick Film","",null,1]
[80,"118k, 1%",1,"R87","RES0402","Yageo","RC0402FR-07118KL","Digi-Key","YAG2369CT-ND","118 kOhms ±1% 0.063W, 1/16W Chip Resistor 0402 (1005 Metric) Moisture Resistant Thick Film","",null,1]
[81,"150k, 1%",1,"R90","RES0402","Yageo","RC0402JR-07150KL","Digi-Key","311-150KJRCT-ND","150 kOhms ±5% 0.063W, 1/16W Chip Resistor 0402 (1005 Metric) Moisture Resistant Thick Film","",null,1]
[82,"TC1-1-13M-45+",4,"T1, T2, T3, T4","TC1-1-13MA+_JA4220-AL_","Minicircuits","TC1-1-13M-45+","Minicircuits","TC1-1-13M-45+","RF balun; 1:1 ratio; 3 dB bandwidth: 0.3 MHz to 3.5 GHz; 3.8mm x 3.8mm","",null,4]
[83,"ZVN4525E6TA",3,"VT1, VT2, VT3","ZVN4525E6_NMOS_SOT23-6","Diodes Zetex","ZVN4525E6TA","Digi-Key","31-ZVN4525E6TACT-ND","N-Channel 250 V 230mA (Ta) 1.1W (Ta) Surface Mount SOT-23-6","NF(VT1 VT2)",2,1]
[84,"IRLML6244TRPBF",1,"VT4","SOT23-3","Infineon Technologies","IRLML6244TRPBF","Digi-Key","IRLML6244TRPBFTR-ND","N-Channel 20V 6.3A (Ta) 1.3W (Ta) Surface Mount Micro3™/SOT-23","",null,1]
[85,"E7355LF, 40MHz, w VC",1,"XO1","RAKON_RTX5032A","Rakon","E7355LF","RAKON","E7355LF","E7355LF 40MHz, High performance TCXO, With VC, 6-pin 5mm x 3.2 mm x 2.1 mm package","",null,1]
[86,"30MHz",1,"XT1","CRYSTAL_4-LCC","AVX Corp/Kyocera Corp","CX3225SB30000D0FPLCC","Digi-Key","1253-1368-1-ND","30MHz ±10ppm Crystal 8pF 50 Ohm -40°C ~ 85°C Surface Mount 4-SMD, No Lead (DFN, LCC)","",null,1]
[]
[{"$nulls":10},"Total NF element number: 76"]
[]
[{"$nulls":10},"All NF elements in one row:"]
[{"$nulls":10},"NF(C186 C194 C7 C19 C20 C22 C71 C84 C192 C6 C21 C174 C176 C182 C185 C187 C157 C158 C160 C183 ESD1 ESD2 FAN1 FR42 FR43 IC2 IC12 IC16 IC17 J3 J4 J5 J9 MECH1 MECH2 MECH3 MECH4 MECH17 MECH19 MECH20 MECH21 MECH5 MECH18 MECH6 MECH7 MECH8 MECH9 MECH10 MECH11 MN22 MN3 MN17 MN5 MN13 MN18 R14 R15 R20 R21 R26 R43 R66 R76 R95 R99 R100 R81 R16 R17 R24 R19 R78 R92 R73 VT1 VT2)"]
[]
[{"$nulls":10},"*NOTE: NF(R1 R2) means that elements R1 and R2 are unpopulated (NF)"]