<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="6.4">
<drawing>
<library>
<description>Nonolith Labs Eagle Library</description>
<packages>
<package name="QFN-12">
</package>
<package name="HVQFN33-7X7">
<description>&lt;b&gt;HVQFN33 &lt;/b&gt;&lt;p&gt;Plastic thermal enhanced very thin quad flat package; 33 terminals; body 7x7x0.85 mm;
&lt;p&gt;Thermal pad intentionally smaller than actual pad size to avoid bridges&lt;/p&gt;</description>
</package>
<package name="2512">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
chip</description>
</package>
<package name="MSOP10">
<description>MSOP10 - .5mm</description>
</package>
<package name="SOT23-3">
</package>
<package name="DCU-8">
<description>DCU / MSOP8 - .5</description>
</package>
<package name="0805">
<description>0805 (2012 Metric)</description>
</package>
<package name="1206">
<description>1206 (3216 Metric)</description>
</package>
<package name="0603">
<description>0603 (1608 Metric)</description>
</package>
<package name="0402">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;&lt;p&gt;
chip</description>
</package>
<package name="HC49UP">
<description>&lt;b&gt;SMD CRYSTAL&lt;/b&gt;</description>
</package>
<package name="CRYSTAL32SMT">
<description>32.768KHz Crystal - SMT Cylinder</description>
</package>
<package name="CRYSTAL_3.2X2.5">
<description>3.2mm x 2.5mm Thin SMT Crystal</description>
</package>
<package name="CRYSTAL_4.9X1.8">
<description>&lt;p&gt;4.9mm x 1.8mm Thin SMT Crystal&lt;/p&gt;
Epson Toyocom FCC-255</description>
</package>
<package name="SMA-DIODE">
<description>&lt;B&gt;Diode&lt;/B&gt;&lt;p&gt;
Basic SMA packaged diode. Good for reverse polarization protection. Common part #: MBRA140</description>
</package>
<package name="1X01_OVAL">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
</package>
<package name="1X01_ROUND">
</package>
<package name="1X01_2MM">
</package>
<package name="1X01_2MM_OVAL">
</package>
<package name="1X02_OVAL">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
</package>
<package name="1X02_ROUND">
</package>
<package name="1X02_SMT">
<description>&lt;p&gt;&lt;b&gt;Pin Headers&lt;/b&gt;&lt;br/&gt;
2 Pin, 0.1"/2.54mm pitch, SMT&lt;/p&gt;</description>
</package>
<package name="1X03_OVAL">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
</package>
<package name="1X03_ROUND">
</package>
<package name="1X03_SMT">
<description>&lt;p&gt;&lt;b&gt;Pin Headers&lt;/b&gt;&lt;br/&gt;
2 Pin, 0.1"/2.54mm pitch, SMT&lt;/p&gt;</description>
</package>
<package name="1X04_OVAL">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
</package>
<package name="1X04_ROUND">
</package>
<package name="1X04_SMT">
<description>&lt;p&gt;&lt;b&gt;Pin Headers&lt;/b&gt;&lt;br/&gt;
4 Pin, 0.1"/2.54mm pitch, SMT&lt;/p&gt;</description>
</package>
<package name="1X05_OVAL">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
</package>
<package name="1X05_ROUND">
</package>
<package name="1X05_SMT">
<description>&lt;p&gt;&lt;b&gt;Pin Headers&lt;/b&gt;&lt;br/&gt;
5 Pin, 0.1"/2.54mm pitch, SMT&lt;/p&gt;</description>
</package>
<package name="1X06_OVAL">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
</package>
<package name="1X06_ROUND">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
</package>
<package name="1X06_SMT">
<description>&lt;p&gt;&lt;b&gt;Pin Headers&lt;/b&gt;&lt;br/&gt;
6 Pin, 0.1"/2.54mm pitch, SMT&lt;/p&gt;</description>
</package>
<package name="1X07_OVAL">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
</package>
<package name="1X07_ROUND">
</package>
<package name="1X08_OVAL">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
</package>
<package name="1X08_ROUND">
</package>
<package name="1X09_OVAL">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
</package>
<package name="1X10_OVAL">
<description>&lt;b&gt;1x10 PIN HEADER&lt;/b&gt;</description>
</package>
<package name="1X10_SMT">
<description>&lt;p&gt;&lt;b&gt;Pin Headers&lt;/b&gt;&lt;br/&gt;
10 Pin, 0.1"/2.54mm pitch, SMT&lt;/p&gt;</description>
</package>
<package name="1X10_ROUND">
</package>
<package name="1X10_ROUND_2MM">
<description>1x10 2.0mm Header Pins</description>
</package>
<package name="2X05">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
</package>
<package name="LQFP48">
</package>
<package name="TQFP-44">
<description>&lt;b&gt;TQFP-44&lt;/b&gt;</description>
</package>
<package name="QFN-44">
</package>
<package name="MINI-USBB">
</package>
<package name="SO-20">
<description>SO-20</description>
</package>
<package name="MICROSOIC10">
<description>&lt;b&gt;10-Lead microSOIC&lt;/b&gt;&lt;p&gt;
(RM-10) 10-µSOIC</description>
</package>
<package name="MSOP8">
<description>&lt;b&gt;Micro Small Outline Package&lt;/b&gt;</description>
</package>
<package name="SOT23-5L">
<description>&lt;b&gt;Small Outline Transistor&lt;/b&gt;&lt;p&gt;
package type OT</description>
</package>
<package name="SOT23-6">
<description>&lt;b&gt;Small Outline Transistor&lt;/b&gt; 6 lead</description>
</package>
<package name="TSSOP-16">
<description>&lt;b&gt;Thin Shrink Small Outline Plastic 16&lt;/b&gt;&lt;p&gt;
http://www.maxim-ic.com .. MAX3223-MAX3243.pdf</description>
</package>
<package name="TSSOP-14">
</package>
<package name="SO-08">
</package>
<package name="SO-16">
<description>&lt;b&gt;SMALL OUTLINE INTEGRATED CIRCUIT&lt;/b&gt;&lt;p&gt;
body 3.9 mm/JEDEC MS-012AC</description>
</package>
<package name="STAND-OFF">
<description>&lt;b&gt;Stand Off&lt;/b&gt;&lt;p&gt;
This is the mechanical footprint for a #4 phillips button head screw. Use the keepout ring to avoid running the screw head into surrounding components. SKU : PRT-00447</description>
</package>
<package name="RN8P-4R-CRA06S">
</package>
<package name="LOGO_CEE">
</package>
<package name="LOGO_NONOLITH">
</package>
<package name="LFCSP-16">
<description>&lt;b&gt;16-Terminal Leadless Frame Chip Scale Package [LFCSP] (CP) - Reflow Footprint&lt;/b&gt;&lt;p&gt;
Source: Analog Devices .. 780914713ADD8704_0.pdf</description>
</package>
<package name="TSSOP-28">
<description>TSSOP28</description>
</package>
<package name="PCC-SMP">
<description>OMEGA's PCC-SMP thermocouple connector, speced at
&lt;br&gt;http://www.omega.com/Temperature/pdf/PCC-OST-SMP.pdf</description>
</package>
<package name="NX8045GB">
<description>package for SMD crystal - a'la &lt;a href="http://media.digikey.com/pdf/Data%20Sheets/NDK%20PDFs/NX8045GB.pdf"&gt;644-1018-1-ND&lt;/a&gt;</description>
</package>
<package name="LGA-8">
<description>&lt;h4&gt;LGA8 Package&lt;/h4&gt;
&lt;li&gt; 5.0x3.0x1.2mm&lt;/li&gt;</description>
</package>
<package name="USB-MINIB">
<description>Surface Mount USB Mini-B Connector</description>
</package>
<package name="QFN-20-NOPAD">
</package>
<package name="2X03">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
</package>
<package name="LGA28L">
</package>
<package name="USB-MICROB">
<description>SMD USB Micro-B connector 
&lt;br&gt;
FCI P/N - 10118192-0001LF
&lt;br&gt;
DigiKey P/N - 609-4613-1-ND
&lt;br&gt;
Mouser P/N - 649-10118192-0001LF</description>
</package>
<package name="MOT_RIC_BM_CW">
</package>
<package name="MOT_RIC_BM_CCW">
</package>
<package name="LQFP100">
<description>&lt;b&gt;LQFP100 &lt;/b&gt;&lt;p&gt;Low Profile Quad Flat Package 14x14x1.4 mm&lt;p&gt;</description>
</package>
<package name="LQFP144">
<description>&lt;b&gt;Quad Flat Pack&lt;/b&gt;</description>
</package>
<package name="1X06_ROUND_2MM">
</package>
<package name="VQFN-20">
<description>3x3mm 20 pin QFN &lt;p&gt; AKA Atmel's 20M2</description>
</package>
<package name="QFN-16">
</package>
<package name="RGBLED_PLCC6">
<description>&lt;b&gt;RGB LED PLCC-6&lt;/b&gt;&lt;p&gt;
5.0mm x 5.0mm 1.5mm Pitch</description>
</package>
<package name="SC-70">
<description>tiny sot23</description>
</package>
<package name="TO252">
<description>&lt;b&gt;SMALL OUTLINE TRANSISTOR&lt;/b&gt;&lt;p&gt;
TS-003</description>
</package>
<package name="SOT-223">
<description>&lt;b&gt;SOT-223&lt;/b&gt;</description>
</package>
<package name="SSOP-24">
<description>&lt;b&gt;Shrink Small Outline Package&lt;/b&gt; SSOP-24&lt;p&gt;</description>
</package>
<package name="NXT-FOOTPRINT">
<description>LEGO NXT Board-Mount Connector</description>
</package>
<package name="BGA96_0.33MM">
</package>
<package name="HEADER_PRG_2X03">
</package>
<package name="R-PDSO-N5">
<description>&lt;b&gt;SOT-553&lt;/b&gt;&lt;br/&gt;SOT package for TI ESD protection chip.</description>
</package>
<package name="QRE1113">
</package>
<package name="BGA96">
</package>
<package name="QFN20">
</package>
</packages>
<symbols>
<symbol name="OPA567">
<pin name="VO"/>
<pin name="VIN+" direction="in"/>
<pin name="VIN-" direction="in"/>
<pin name="ENABLE" direction="in"/>
<pin name="IFLAG"/>
<pin name="ISET"/>
<pin name="TFLAG"/>
<pin name="V+" direction="pwr"/>
<pin name="GND" direction="pwr"/>
</symbol>
<symbol name="TS5A21366">
<pin name="V+"/>
<pin name="IN1"/>
<pin name="COM2"/>
<pin name="NO2"/>
<pin name="NO1"/>
<pin name="COM1"/>
<pin name="IN2"/>
<pin name="GND"/>
</symbol>
<symbol name="LPC1343FHN33">
<pin name="PIO2_0/DTR"/>
<pin name="RESET/PIO0_0"/>
<pin name="PIO0_1/CLKOUT/CT32B0_MAT2/USB_FTOGGLE"/>
<pin name="XTALIN" direction="in"/>
<pin name="XTALOUT" direction="out"/>
<pin name="VDD(IO)" direction="pwr"/>
<pin name="PIO1_8/CT16B1_CAP0"/>
<pin name="PIO0_2/SSEL/CT16B0_CAP0"/>
<pin name="PIO0_3/USB_VBUS"/>
<pin name="PIO0_4/SCL"/>
<pin name="PIO0_5/SDA"/>
<pin name="PIO1_9/CT16B1_MAT0"/>
<pin name="USB_DM"/>
<pin name="USB_DP"/>
<pin name="PIO0_6/USB_CONNECT/SCK"/>
<pin name="PIO0_7/CTS"/>
<pin name="PIO0_8/MISO/CT16B0_MAT0"/>
<pin name="PIO0_9/MOSI/CT16B0_MAT1/SWO"/>
<pin name="SWCLK/PIO0_10/SCK/CT16B0_MAT2"/>
<pin name="PIO1_10/AD6/CT16B1_MAT1"/>
<pin name="TDI/PIO0_11/AD0/CT32B0_MAT3"/>
<pin name="TMS/PIO1_0/AD1/CT32B1_CAP0"/>
<pin name="TDO/PIO1_1/AD2/CT32B1_MAT0"/>
<pin name="TRST/PIO1_2/AD3/CT32B1_MAT1"/>
<pin name="SWDIO/PIO1_3/AD4/CT32B1_MAT2"/>
<pin name="PIO1_4/AD5/CT32B1_MAT3/WAKEUP"/>
<pin name="PIO1_11/AD7"/>
<pin name="PIO3_2"/>
<pin name="VDD(3V3)" direction="pwr"/>
<pin name="PIO1_5/RTS/CT32B0_CAP0"/>
<pin name="PIO1_6/RXD/CT32B0_MAT0"/>
<pin name="PIO1_7/TXD/CT32B0_MAT1"/>
<pin name="VSS" direction="pwr"/>
</symbol>
<symbol name="VREF">
<pin name="GND"/>
<pin name="VIN"/>
<pin name="VO"/>
</symbol>
<symbol name="MCP4728">
<pin name="GND"/>
<pin name="VOD"/>
<pin name="VOC"/>
<pin name="VOB"/>
<pin name="VOA"/>
<pin name="V+"/>
<pin name="SCL"/>
<pin name="SDA"/>
<pin name="LDAC"/>
<pin name="RDY"/>
</symbol>
<symbol name="ADS1015">
<pin name="SCL"/>
<pin name="SDA"/>
<pin name="V+"/>
<pin name="VIN4"/>
<pin name="VIN3"/>
<pin name="ADDR"/>
<pin name="RDY"/>
<pin name="GND"/>
<pin name="VIN1"/>
<pin name="VIN2"/>
</symbol>
<symbol name="TS5A23157">
<pin name="COM1"/>
<pin name="NC1"/>
<pin name="V+"/>
<pin name="NC2"/>
<pin name="COM2"/>
<pin name="IN1"/>
<pin name="NO1"/>
<pin name="GND"/>
<pin name="NO2"/>
<pin name="IN2"/>
</symbol>
<symbol name="RESISTOR">
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
</symbol>
<symbol name="CAPACITOR">
<pin name="P$1" direction="pas"/>
<pin name="P$2" direction="pas"/>
</symbol>
<symbol name="CRYSTAL">
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
</symbol>
<symbol name="DIODE-SCHOTTKY">
<pin name="A" direction="pas"/>
<pin name="C" direction="pas"/>
</symbol>
<symbol name="GND">
<pin name="GND" direction="sup"/>
</symbol>
<symbol name="TESTPOINT">
<pin name="P$1"/>
</symbol>
<symbol name="PINHD1">
<pin name="1" direction="pas" function="dot"/>
</symbol>
<symbol name="PINHD2">
<pin name="1" direction="pas" function="dot"/>
<pin name="2" direction="pas" function="dot"/>
</symbol>
<symbol name="PINHD3">
<pin name="1" direction="pas" function="dot"/>
<pin name="2" direction="pas" function="dot"/>
<pin name="3" direction="pas" function="dot"/>
</symbol>
<symbol name="PINHD4">
<pin name="1" direction="pas" function="dot"/>
<pin name="2" direction="pas" function="dot"/>
<pin name="3" direction="pas" function="dot"/>
<pin name="4" direction="pas" function="dot"/>
</symbol>
<symbol name="PINHD5">
<pin name="1" direction="pas" function="dot"/>
<pin name="2" direction="pas" function="dot"/>
<pin name="3" direction="pas" function="dot"/>
<pin name="4" direction="pas" function="dot"/>
<pin name="5" direction="pas" function="dot"/>
</symbol>
<symbol name="PINHD6">
<pin name="1" direction="pas" function="dot"/>
<pin name="2" direction="pas" function="dot"/>
<pin name="3" direction="pas" function="dot"/>
<pin name="4" direction="pas" function="dot"/>
<pin name="5" direction="pas" function="dot"/>
<pin name="6" direction="pas" function="dot"/>
</symbol>
<symbol name="PINHD7">
<pin name="1" direction="pas" function="dot"/>
<pin name="2" direction="pas" function="dot"/>
<pin name="3" direction="pas" function="dot"/>
<pin name="4" direction="pas" function="dot"/>
<pin name="5" direction="pas" function="dot"/>
<pin name="6" direction="pas" function="dot"/>
<pin name="7" direction="pas" function="dot"/>
</symbol>
<symbol name="PINHD8">
<pin name="1" direction="pas" function="dot"/>
<pin name="2" direction="pas" function="dot"/>
<pin name="3" direction="pas" function="dot"/>
<pin name="4" direction="pas" function="dot"/>
<pin name="5" direction="pas" function="dot"/>
<pin name="6" direction="pas" function="dot"/>
<pin name="7" direction="pas" function="dot"/>
<pin name="8" direction="pas" function="dot"/>
</symbol>
<symbol name="PINHD9">
<pin name="1" direction="pas" function="dot"/>
<pin name="2" direction="pas" function="dot"/>
<pin name="3" direction="pas" function="dot"/>
<pin name="4" direction="pas" function="dot"/>
<pin name="5" direction="pas" function="dot"/>
<pin name="6" direction="pas" function="dot"/>
<pin name="7" direction="pas" function="dot"/>
<pin name="8" direction="pas" function="dot"/>
<pin name="9" direction="pas" function="dot"/>
</symbol>
<symbol name="PINHD10">
<pin name="1" direction="pas" function="dot"/>
<pin name="2" direction="pas" function="dot"/>
<pin name="3" direction="pas" function="dot"/>
<pin name="4" direction="pas" function="dot"/>
<pin name="5" direction="pas" function="dot"/>
<pin name="6" direction="pas" function="dot"/>
<pin name="7" direction="pas" function="dot"/>
<pin name="8" direction="pas" function="dot"/>
<pin name="9" direction="pas" function="dot"/>
<pin name="10" direction="pas" function="dot"/>
</symbol>
<symbol name="PINH2X5">
<pin name="1" direction="pas" function="dot"/>
<pin name="2" direction="pas" function="dot"/>
<pin name="3" direction="pas" function="dot"/>
<pin name="4" direction="pas" function="dot"/>
<pin name="5" direction="pas" function="dot"/>
<pin name="6" direction="pas" function="dot"/>
<pin name="7" direction="pas" function="dot"/>
<pin name="8" direction="pas" function="dot"/>
<pin name="9" direction="pas" function="dot"/>
<pin name="10" direction="pas" function="dot"/>
</symbol>
<symbol name="LPC1343FBD48">
<pin name="PIO2_6"/>
<pin name="PIO2_0/DTR"/>
<pin name="RESET/PIO0_0"/>
<pin name="PIO0_1/CLKOUT/CT32B0_MAT2/USB_FTOGGLE"/>
<pin name="VSSIO" direction="pwr"/>
<pin name="XTALIN" direction="in"/>
<pin name="XTALOUT" direction="out"/>
<pin name="VDD(IO)" direction="pwr"/>
<pin name="PIO1_8/CT16B1_CAP0"/>
<pin name="PIO0_2/SSEL/CT16B0_CAP0"/>
<pin name="PIO2_7"/>
<pin name="PIO2_8"/>
<pin name="PIO2_1/DSR"/>
<pin name="PIO0_3/USB_VBUS"/>
<pin name="PIO0_4/SCL"/>
<pin name="PIO0_5/SDA"/>
<pin name="PIO1_9/CT16B1_MAT0"/>
<pin name="PIO2_4"/>
<pin name="USB_DM"/>
<pin name="USB_DP"/>
<pin name="PIO2_5"/>
<pin name="PIO0_6/USB_CONNECT/SCK"/>
<pin name="PIO0_7/CTS"/>
<pin name="PIO2_9"/>
<pin name="PIO2_10"/>
<pin name="PIO2_2/DCD"/>
<pin name="PIO0_8/MISO/CT16B0_MAT0"/>
<pin name="PIO0_9/MOSI/CT16B0_MAT1/SWO"/>
<pin name="SWCLK/PIO0_10/SCK/CT16B0_MAT2"/>
<pin name="PIO1_10/AD6/CT16B1_MAT1"/>
<pin name="PIO2_11/SCK"/>
<pin name="TDI/PIO0_11/AD0/CT32B0_MAT3"/>
<pin name="TMS/PIO1_0/AD1/CT32B1_CAP0"/>
<pin name="TDO/PIO1_1/AD2/CT32B1_MAT0"/>
<pin name="TRST/PIO1_2/AD3/CT32B1_MAT1"/>
<pin name="PIO3_0"/>
<pin name="PIO3_1"/>
<pin name="PIO2_3/RI"/>
<pin name="SWDIO/PIO1_3/AD4/CT32B1_MAT2"/>
<pin name="PIO1_4/AD5/CT32B1_MAT3/WAKEUP"/>
<pin name="VSS" direction="pwr"/>
<pin name="PIO1_11/AD7"/>
<pin name="PIO3_2"/>
<pin name="VDD(3V3)" direction="pwr"/>
<pin name="PIO1_5/RTS/CT32B0_CAP0"/>
<pin name="PIO1_6/RXD/CT32B0_MAT0"/>
<pin name="PIO1_7/TXD/CT32B0_MAT1"/>
<pin name="PIO3_3"/>
</symbol>
<symbol name="XMEGA-A4U">
<pin name="PA3/ADC3"/>
<pin name="PA4/ADC4"/>
<pin name="PA5/ADC5"/>
<pin name="PB1/ADC9"/>
<pin name="GND@1" direction="pwr"/>
<pin name="VCC@1" direction="pwr"/>
<pin name="PC1/OC0B/XCK0/SCL"/>
<pin name="AVCC" direction="pwr"/>
<pin name="PA1/ADC1"/>
<pin name="PA2/ADC2"/>
<pin name="PB2/ADC10/DAC0"/>
<pin name="GND@2" direction="pwr"/>
<pin name="PC0/OC0A/SDA"/>
<pin name="PC2/OC0C/RXD0"/>
<pin name="GND@3" direction="pwr"/>
<pin name="PA0/ADC0/AREFA"/>
<pin name="PA6/ADC6"/>
<pin name="PB3/ADC11/DAC1"/>
<pin name="PC3/OC0D/TXD0"/>
<pin name="PC4/OC1A/#SS"/>
<pin name="PC5/OC1B/MOSI/XCK1"/>
<pin name="PR1/XTAL1"/>
<pin name="GND@4" direction="pwr"/>
<pin name="PA7/ADC7"/>
<pin name="PB0/ADC8/AREFB"/>
<pin name="PC6/MISO/RXD1"/>
<pin name="PC7/SCK/TXD1/CLKO/EVO"/>
<pin name="PR0/XTAL2"/>
<pin name="RESET/PDI-CLK" direction="in"/>
<pin name="SS/PD4"/>
<pin name="OC0A/PD0"/>
<pin name="PDI-DATA"/>
<pin name="RXD0/OC0C/PE2"/>
<pin name="XCK0/OC0B/SCL/PE1"/>
<pin name="TXD1/USB+/PD7"/>
<pin name="XCK1/MOSI/PD5"/>
<pin name="OC0B/XCK0/PD1"/>
<pin name="VCC@2" direction="pwr"/>
<pin name="TXD0/OC0D/PE3"/>
<pin name="VCC@3" direction="pwr"/>
<pin name="OC0A/SDA/PE0"/>
<pin name="RXD1/MISO/USB-/PD6"/>
<pin name="OC0D/TXD0/PD3"/>
<pin name="OC0C/RXD0/PD2"/>
</symbol>
<symbol name="OPAMP">
<pin name="-IN" direction="in"/>
<pin name="+IN" direction="in"/>
<pin name="OUT" direction="out"/>
</symbol>
<symbol name="PWR+-">
<pin name="V+" direction="pwr"/>
<pin name="V-" direction="pwr"/>
</symbol>
<symbol name="MCP4922">
<pin name="LDAC"/>
<pin name="SHDN"/>
<pin name="VOUTB"/>
<pin name="VREFB"/>
<pin name="AVSS"/>
<pin name="VREFA"/>
<pin name="VOUTA"/>
<pin name="VCC"/>
<pin name="NC@2"/>
<pin name="CS"/>
<pin name="SCK"/>
<pin name="MOSI"/>
<pin name="NC@6"/>
<pin name="NC@7"/>
</symbol>
<symbol name="MAX9919">
<pin name="RS+"/>
<pin name="RS-"/>
<pin name="SHDN"/>
<pin name="VCC"/>
<pin name="REFIN"/>
<pin name="FB"/>
<pin name="OUT"/>
<pin name="GND"/>
</symbol>
<symbol name="RESISTOR_B">
<pin name="2" direction="pas"/>
<pin name="1" direction="pas"/>
</symbol>
<symbol name="TS5A3157">
<pin name="NO"/>
<pin name="GND"/>
<pin name="NC"/>
<pin name="COM"/>
<pin name="V+"/>
<pin name="IN"/>
</symbol>
<symbol name="VREG">
<pin name="VIN"/>
<pin name="GND"/>
<pin name="VO"/>
</symbol>
<symbol name="ADXL335">
<pin name="VS1"/>
<pin name="VS2"/>
<pin name="GND1"/>
<pin name="GND2"/>
<pin name="GND3"/>
<pin name="GND4"/>
<pin name="X"/>
<pin name="Y"/>
<pin name="Z"/>
<pin name="TEST"/>
</symbol>
<symbol name="MAX31855">
<pin name="GND"/>
<pin name="T-"/>
<pin name="T+"/>
<pin name="VCC"/>
<pin name="SCK"/>
<pin name="CS"/>
<pin name="SO"/>
<pin name="DNC"/>
</symbol>
<symbol name="MOSFET-P">
<pin name="G"/>
<pin name="S"/>
<pin name="D"/>
</symbol>
<symbol name="ADP3120A">
<pin name="BST"/>
<pin name="IN"/>
<pin name="OD"/>
<pin name="VCC"/>
<pin name="DRVL"/>
<pin name="PGND"/>
<pin name="SW"/>
<pin name="DRVH"/>
</symbol>
<symbol name="LT1999">
<pin name="VCC@1"/>
<pin name="RS+"/>
<pin name="RS-"/>
<pin name="VCC@4"/>
<pin name="GND"/>
<pin name="VREF"/>
<pin name="OUT"/>
<pin name="SHDN"/>
</symbol>
<symbol name="MPL115A">
<pin name="VDD"/>
<pin name="CAP"/>
<pin name="GND"/>
<pin name="SHDN"/>
<pin name="RST"/>
<pin name="NC"/>
<pin name="SDA"/>
<pin name="SCL"/>
</symbol>
<symbol name="USB">
<pin name="D+"/>
<pin name="D-"/>
<pin name="VBUS" direction="pwr"/>
<pin name="GND" direction="pwr"/>
<pin name="ID"/>
<pin name="SHIELD"/>
</symbol>
<symbol name="ATTINY24">
<pin name="VCC"/>
<pin name="PB0"/>
<pin name="PB1"/>
<pin name="PB2"/>
<pin name="PB3/RESET"/>
<pin name="PA7/ADC7"/>
<pin name="PA6/MOSI"/>
<pin name="PA5/MISO"/>
<pin name="PA4/SCL"/>
<pin name="PA3/ADC3"/>
<pin name="PA2/ADC2"/>
<pin name="PA1/ADC1"/>
<pin name="PA0/ADC0"/>
<pin name="GND"/>
</symbol>
<symbol name="PINH2X3">
<pin name="1" direction="pas" function="dot"/>
<pin name="2" direction="pas" function="dot"/>
<pin name="3" direction="pas" function="dot"/>
<pin name="4" direction="pas" function="dot"/>
<pin name="5" direction="pas" function="dot"/>
<pin name="6" direction="pas" function="dot"/>
</symbol>
<symbol name="LSM330DLCTR">
<pin name="VDD"/>
<pin name="INT1_A"/>
<pin name="GND"/>
<pin name="INT2_G"/>
<pin name="INT2_A"/>
<pin name="INT1_G"/>
<pin name="SCL_G"/>
<pin name="SDO_G"/>
<pin name="SDO_A"/>
<pin name="SCL_A"/>
<pin name="CS_G"/>
<pin name="CS_A"/>
<pin name="VCONT"/>
<pin name="SDA/SDI_A"/>
<pin name="SDA/SDI_G"/>
</symbol>
<symbol name="MOT">
<pin name="+"/>
<pin name="-"/>
</symbol>
<symbol name="SAM3U_LQFP100">
<pin name="VDDANA" direction="pwr"/>
<pin name="ADVREF" direction="pwr"/>
<pin name="GNDANA" direction="pwr"/>
<pin name="AD12BVREF" direction="in"/>
<pin name="PA22"/>
<pin name="PA30"/>
<pin name="PB3"/>
<pin name="PB4"/>
<pin name="VDDCORE" direction="pwr"/>
<pin name="PA13"/>
<pin name="PA14"/>
<pin name="PA15"/>
<pin name="PA16"/>
<pin name="PA17"/>
<pin name="PB16"/>
<pin name="PB15"/>
<pin name="PA18"/>
<pin name="PA19"/>
<pin name="PA20"/>
<pin name="PA21"/>
<pin name="PA23"/>
<pin name="VDDIO" direction="pwr"/>
<pin name="PA24"/>
<pin name="PA25"/>
<pin name="PA26"/>
<pin name="PA0"/>
<pin name="PA1"/>
<pin name="PA2"/>
<pin name="PA3"/>
<pin name="PA4"/>
<pin name="PA5"/>
<pin name="PA6"/>
<pin name="PA7"/>
<pin name="VDDCORE@1" direction="pwr"/>
<pin name="GND" direction="pwr"/>
<pin name="VDDIO@1" direction="pwr"/>
<pin name="PA8"/>
<pin name="PA9"/>
<pin name="PA10"/>
<pin name="PA11"/>
<pin name="PA12"/>
<pin name="FWUP" direction="pas"/>
<pin name="ERASE" direction="pas"/>
<pin name="TST" direction="in"/>
<pin name="VDDBU" direction="pwr"/>
<pin name="GNDBU" direction="pwr"/>
<pin name="NRSTB" direction="pas"/>
<pin name="JTAGSEL" direction="in"/>
<pin name="XOUT32" direction="pas"/>
<pin name="XIN32" direction="pas"/>
<pin name="TDI" direction="in"/>
<pin name="VDDOUT" direction="pwr"/>
<pin name="VDDIN" direction="pwr"/>
<pin name="TDO" direction="out"/>
<pin name="TMS" direction="in"/>
<pin name="TCK" direction="in"/>
<pin name="NRST" direction="in"/>
<pin name="PB24"/>
<pin name="VDDCORE@2" direction="pwr"/>
<pin name="VDDIO@2" direction="pwr"/>
<pin name="GND@1" direction="pwr"/>
<pin name="PB23"/>
<pin name="PB22"/>
<pin name="PB21"/>
<pin name="PB20"/>
<pin name="PB19"/>
<pin name="PB18"/>
<pin name="PB17"/>
<pin name="PB14"/>
<pin name="PB10"/>
<pin name="PB9"/>
<pin name="GNDPLL" direction="pwr"/>
<pin name="VDDPLL" direction="pwr"/>
<pin name="XOUT" direction="pas"/>
<pin name="XIN" direction="pas"/>
<pin name="DHSDP" direction="pas"/>
<pin name="DHSDM" direction="pas"/>
<pin name="VBG" direction="pwr"/>
<pin name="VDDUTMI" direction="pwr"/>
<pin name="DFSDM" direction="pas"/>
<pin name="DFSDP" direction="pas"/>
<pin name="GNDUTMI" direction="pwr"/>
<pin name="VDDCORE@3" direction="pwr"/>
<pin name="PA28"/>
<pin name="PA29"/>
<pin name="PA31"/>
<pin name="VDDCORE@4" direction="pwr"/>
<pin name="VDDIO@3" direction="pwr"/>
<pin name="GND@2" direction="pwr"/>
<pin name="PB0"/>
<pin name="PB1"/>
<pin name="PB2"/>
<pin name="PB11"/>
<pin name="PB12"/>
<pin name="PB13"/>
<pin name="PA27"/>
<pin name="PB5"/>
<pin name="PB6"/>
<pin name="PB7"/>
<pin name="PB8"/>
</symbol>
<symbol name="LEDRGB_PLCC6">
<pin name="RED"/>
<pin name="GRN"/>
<pin name="BLUE"/>
<pin name="RGND" direction="pwr"/>
<pin name="GGND" direction="pwr"/>
<pin name="BGND" direction="pwr"/>
</symbol>
<symbol name="LM4764">
<pin name="INR+"/>
<pin name="INR-"/>
<pin name="INL-"/>
<pin name="INL+"/>
<pin name="G1"/>
<pin name="PVDD"/>
<pin name="OUTLA"/>
<pin name="OUTLB"/>
<pin name="SDL"/>
<pin name="SDR"/>
<pin name="PGND"/>
<pin name="GND"/>
<pin name="OUTRB"/>
<pin name="OUTRA"/>
<pin name="VDD"/>
<pin name="G0"/>
</symbol>
<symbol name="INA213">
<pin name="OUT"/>
<pin name="IN-"/>
<pin name="IN+"/>
<pin name="REF"/>
<pin name="GND"/>
<pin name="V+"/>
</symbol>
<symbol name="PCA9306">
<pin name="SDA1"/>
<pin name="SCL1"/>
<pin name="EN"/>
<pin name="VREF1"/>
<pin name="VREF2"/>
<pin name="SCL2"/>
<pin name="SDA2"/>
<pin name="GND"/>
</symbol>
<symbol name="MAX232">
<pin name="C1+"/>
<pin name="C1-"/>
<pin name="C2+"/>
<pin name="C2-"/>
<pin name="T1IN" direction="in"/>
<pin name="T2IN" direction="in"/>
<pin name="R1OUT" direction="out"/>
<pin name="R2OUT" direction="out"/>
<pin name="V+"/>
<pin name="V-"/>
<pin name="T1OUT" direction="out"/>
<pin name="T2OUT" direction="out"/>
<pin name="R1IN" direction="in"/>
<pin name="R2IN" direction="in"/>
<pin name="GND"/>
<pin name="VCC"/>
</symbol>
<symbol name="TB6612FNG">
<pin name="AO1" direction="out"/>
<pin name="AO1'" direction="out"/>
<pin name="PGND1" direction="pwr"/>
<pin name="PGND1'" direction="pwr"/>
<pin name="AO2" direction="out"/>
<pin name="AO2'" direction="out"/>
<pin name="BO1" direction="out"/>
<pin name="BO1'" direction="out"/>
<pin name="PGND2" direction="pwr"/>
<pin name="PGND2'" direction="pwr"/>
<pin name="BO2" direction="out"/>
<pin name="BO2'" direction="out"/>
<pin name="VM2" direction="pwr"/>
<pin name="VM3" direction="pwr"/>
<pin name="PWMB" direction="in"/>
<pin name="BIN2" direction="in"/>
<pin name="BIN1" direction="in"/>
<pin name="GND" direction="pwr"/>
<pin name="STBY" direction="in"/>
<pin name="VCC" direction="pwr"/>
<pin name="AIN1" direction="in"/>
<pin name="AIN2" direction="in"/>
<pin name="PWMA" direction="in"/>
<pin name="VM1" direction="pwr"/>
</symbol>
<symbol name="NXT-CONN">
<pin name="GND"/>
<pin name="9V0"/>
<pin name="4V3"/>
<pin name="SCL"/>
<pin name="SDA"/>
</symbol>
<symbol name="MIC2091">
<pin name="VIN"/>
<pin name="VOUT"/>
<pin name="EN"/>
<pin name="GND"/>
<pin name="FAULT"/>
</symbol>
<symbol name="MCP4013">
<pin name="VDD"/>
<pin name="GND"/>
<pin name="U/~D"/>
<pin name="A"/>
<pin name="W"/>
<pin name="~CS"/>
</symbol>
<symbol name="74LVC1T45">
<pin name="V+A"/>
<pin name="V+B"/>
<pin name="GND"/>
<pin name="B"/>
<pin name="A"/>
<pin name="DIR"/>
</symbol>
<symbol name="VREG-ADJ-EN">
<pin name="VIN"/>
<pin name="GND"/>
<pin name="EN"/>
<pin name="FB"/>
<pin name="VOUT"/>
</symbol>
<symbol name="MCP6N11">
<pin name="VFG"/>
<pin name="VI-"/>
<pin name="VI+"/>
<pin name="GND"/>
<pin name="VREF"/>
<pin name="VOUT"/>
<pin name="VDD"/>
<pin name="EN/CAL"/>
</symbol>
<symbol name="XS1-U8A_I/O">
<pin name="ADC_VREF"/>
<pin name="ADC_IN_0"/>
<pin name="USB_DP"/>
<pin name="USB_DN"/>
<pin name="USB_VBUS"/>
<pin name="USB_ID"/>
<pin name="X0D00"/>
<pin name="X0D01"/>
<pin name="X0D10"/>
<pin name="X0D11"/>
<pin name="X0D12"/>
<pin name="X0D13"/>
<pin name="X0D14"/>
<pin name="X0D15"/>
<pin name="X0D16"/>
<pin name="X0D17"/>
<pin name="X0D18"/>
<pin name="X0D19"/>
<pin name="X0D20"/>
<pin name="X0D21"/>
<pin name="X0D22"/>
<pin name="X0D24"/>
<pin name="X0D35"/>
<pin name="X0D43/WAKE"/>
<pin name="X0D49"/>
<pin name="X0D50"/>
<pin name="X0D51"/>
<pin name="X0D52"/>
<pin name="X0D53"/>
<pin name="X0D54"/>
<pin name="X0D55"/>
<pin name="X0D56"/>
<pin name="X0D57"/>
<pin name="X0D58"/>
<pin name="X0D61"/>
<pin name="X0D62"/>
<pin name="X0D63"/>
<pin name="X0D64"/>
<pin name="X0D65"/>
<pin name="X0D66"/>
<pin name="X0D67"/>
<pin name="X0D68"/>
<pin name="X0D69"/>
<pin name="X0D70"/>
<pin name="ADC_IN_1"/>
<pin name="ADC_IN_2"/>
<pin name="ADC_IN_3"/>
</symbol>
<symbol name="XS1-U8A-FB96_POWER">
<pin name="VSS"/>
<pin name="VDDIO"/>
<pin name="SW1"/>
<pin name="SW2"/>
<pin name="VDDCORE"/>
<pin name="VDD1V8"/>
<pin name="PGND"/>
<pin name="VSUP"/>
</symbol>
<symbol name="XS1-U8A-FB96_CONFIG/JTAG">
<pin name="XI/CLK"/>
<pin name="XO"/>
<pin name="MODE_0"/>
<pin name="MODE_1"/>
<pin name="MODE_2"/>
<pin name="MODE_3"/>
<pin name="OSC_EXT_N"/>
<pin name="TDI"/>
<pin name="TDO"/>
<pin name="TMS"/>
<pin name="TCK"/>
<pin name="DEBUG_N"/>
<pin name="NC"/>
<pin name="RST_N"/>
</symbol>
<symbol name="PRG_ICSP_AVR">
<pin name="+V" direction="pas" function="dot"/>
<pin name="MISO" direction="pas" function="dot"/>
<pin name="SCK" direction="pas" function="dot"/>
<pin name="RST" direction="pas" function="dot"/>
<pin name="MOSI" direction="pas" function="dot"/>
<pin name="GND" direction="pas" function="dot"/>
</symbol>
<symbol name="ATTINY261">
<description>&lt;b&gt;ATTINYx61&lt;/b&gt;&lt;br/&gt; 
8-bit  Microcontroller with 2/4/8K  Bytes In-System Programmable  
Flash</description>
<pin name="PB0"/>
<pin name="PB1"/>
<pin name="PB2"/>
<pin name="PB3"/>
<pin name="VCC"/>
<pin name="GND"/>
<pin name="PB4"/>
<pin name="PB5"/>
<pin name="PB6"/>
<pin name="PB7"/>
<pin name="PA7"/>
<pin name="PA6"/>
<pin name="PA5"/>
<pin name="PA4"/>
<pin name="AVCC"/>
<pin name="AGND"/>
<pin name="PA3"/>
<pin name="PA2"/>
<pin name="PA1"/>
<pin name="PA0"/>
</symbol>
<symbol name="TPD2E001">
<description>&lt;b&gt;TPD2E001&lt;/b&gt;&lt;br/&gt;Two channel ESD protection chip from TI. &lt;br/&gt;&lt;a href="http://www.ti.com/lit/ds/symlink/tpd2e001.pdf"&gt;datasheet&lt;/a&gt;</description>
<pin name="IO1"/>
<pin name="IO2"/>
<pin name="VCC"/>
<pin name="GND"/>
</symbol>
<symbol name="QRE1113">
<pin name="A"/>
<pin name="E"/>
<pin name="C"/>
<pin name="K"/>
</symbol>
<symbol name="MOSFET-N">
<pin name="G"/>
<pin name="S"/>
<pin name="D"/>
</symbol>
<symbol name="IRS2186">
<pin name="HIN"/>
<pin name="LIN"/>
<pin name="COM"/>
<pin name="LO"/>
<pin name="VCC"/>
<pin name="VS"/>
<pin name="HO"/>
<pin name="VB"/>
</symbol>
<symbol name="MOSFET-N-1">
<pin name="G"/>
<pin name="S"/>
<pin name="D"/>
</symbol>
</symbols>
<devicesets>
<deviceset name="OPA567">
<description>OPA567: 2a RRIO CMOS OPA / QFN12</description>
<gates>
<gate name="G$1" symbol="OPA567"/>
</gates>
<devices>
<device name="" package="QFN-12">
<connects>
<connect gate="G$1" pin="ENABLE" pad="11"/>
<connect gate="G$1" pin="GND" pad="4 5 GNDPAD GNDPAD1 GNDPAD2 GNDPAD3 GNDPAD4"/>
<connect gate="G$1" pin="IFLAG" pad="7"/>
<connect gate="G$1" pin="ISET" pad="6"/>
<connect gate="G$1" pin="TFLAG" pad="10"/>
<connect gate="G$1" pin="V+" pad="1 12"/>
<connect gate="G$1" pin="VIN+" pad="9"/>
<connect gate="G$1" pin="VIN-" pad="8"/>
<connect gate="G$1" pin="VO" pad="2 3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="TS5A21366">
<description>200ma digitally controlled switch: TS5A21366</description>
<gates>
<gate name="G$1" symbol="TS5A21366"/>
</gates>
<devices>
<device name="" package="DCU-8">
<connects>
<connect gate="G$1" pin="COM1" pad="2"/>
<connect gate="G$1" pin="COM2" pad="6"/>
<connect gate="G$1" pin="GND" pad="4"/>
<connect gate="G$1" pin="IN1" pad="7"/>
<connect gate="G$1" pin="IN2" pad="3"/>
<connect gate="G$1" pin="NO1" pad="1"/>
<connect gate="G$1" pin="NO2" pad="5"/>
<connect gate="G$1" pin="V+" pad="8"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="VREF">
<gates>
<gate name="G$1" symbol="VREF"/>
</gates>
<devices>
<device name="" package="SOT23-3">
<connects>
<connect gate="G$1" pin="GND" pad="3"/>
<connect gate="G$1" pin="VIN" pad="1"/>
<connect gate="G$1" pin="VO" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MCP4728">
<description>12b I2C DAC: MCP4728</description>
<gates>
<gate name="G$1" symbol="MCP4728"/>
</gates>
<devices>
<device name="" package="MSOP10">
<connects>
<connect gate="G$1" pin="GND" pad="10"/>
<connect gate="G$1" pin="LDAC" pad="4"/>
<connect gate="G$1" pin="RDY" pad="5"/>
<connect gate="G$1" pin="SCL" pad="2"/>
<connect gate="G$1" pin="SDA" pad="3"/>
<connect gate="G$1" pin="V+" pad="1"/>
<connect gate="G$1" pin="VOA" pad="6"/>
<connect gate="G$1" pin="VOB" pad="7"/>
<connect gate="G$1" pin="VOC" pad="8"/>
<connect gate="G$1" pin="VOD" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ADS1015">
<description>12b I2C ADC: ADS1015</description>
<gates>
<gate name="G$1" symbol="ADS1015"/>
</gates>
<devices>
<device name="" package="MSOP10">
<connects>
<connect gate="G$1" pin="ADDR" pad="1"/>
<connect gate="G$1" pin="GND" pad="3"/>
<connect gate="G$1" pin="RDY" pad="2"/>
<connect gate="G$1" pin="SCL" pad="10"/>
<connect gate="G$1" pin="SDA" pad="9"/>
<connect gate="G$1" pin="V+" pad="8"/>
<connect gate="G$1" pin="VIN1" pad="4"/>
<connect gate="G$1" pin="VIN2" pad="5"/>
<connect gate="G$1" pin="VIN3" pad="6"/>
<connect gate="G$1" pin="VIN4" pad="7"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="TS5A23157">
<description>DUAL SPDT SWITCH: TS5A23157DGSR</description>
<gates>
<gate name="G$1" symbol="TS5A23157"/>
</gates>
<devices>
<device name="" package="MSOP10">
<connects>
<connect gate="G$1" pin="COM1" pad="10"/>
<connect gate="G$1" pin="COM2" pad="6"/>
<connect gate="G$1" pin="GND" pad="3"/>
<connect gate="G$1" pin="IN1" pad="1"/>
<connect gate="G$1" pin="IN2" pad="5"/>
<connect gate="G$1" pin="NC1" pad="9"/>
<connect gate="G$1" pin="NC2" pad="7"/>
<connect gate="G$1" pin="NO1" pad="2"/>
<connect gate="G$1" pin="NO2" pad="4"/>
<connect gate="G$1" pin="V+" pad="8"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="RESISTOR" prefix="R" uservalue="yes">
<description>&lt;p&gt;&lt;b&gt;Resistors&lt;/b&gt;&lt;/p&gt;
&lt;b&gt;0402&lt;/b&gt; - 0402 Surface Mount Package
&lt;ul&gt;
&lt;li&gt;10.0K 1% 1/16W [Digikey: 311-10.0KLRTR-ND]&lt;/li&gt;
&lt;/ul&gt;
&lt;b&gt;0603&lt;/b&gt; - 0603 Surface Mount Package&lt;br&gt;
&lt;ul&gt;
&lt;li&gt;0 Ohm 1/10 Watt 1% Resistor&lt;/li&gt;
&lt;li&gt;15 Ohm 1/10 Watt 1% Resistor&lt;/li&gt;
&lt;li&gt;33 Ohm 1/10 Watt 1% Resistor&lt;/li&gt;
&lt;li&gt;49.9 Ohm 1/10 Watt 1% Resistor&lt;/li&gt;
&lt;li&gt;100 Ohm 1/10 Watt 1% Resistor&lt;/li&gt;
&lt;li&gt;150 Ohm 1/10 Watt 1% Resistor&lt;/li&gt;
&lt;li&gt;240 Ohm 1/10 Watt 1% Resistor&lt;/li&gt;
&lt;li&gt;390 Ohm 1/10 Watt 1% Resistor&lt;/li&gt;
&lt;li&gt;560 Ohm 1/10 Watt 1% Resistor&lt;/li&gt;
&lt;li&gt;750 Ohm 1/10 Watt 1% Resistor&lt;/li&gt;
&lt;li&gt;1.0K Ohm 1/10 Watt 1% Resistor&lt;/li&gt;
&lt;li&gt;1.5K Ohm 1/10 Watt 1% Resistor&lt;/li&gt;
&lt;li&gt;2.0K Ohm 1/10 Watt 1% Resistor&lt;/li&gt;
&lt;li&gt;4.7K Ohm 1/10 Watt 1% Resistor&lt;/li&gt;
&lt;li&gt;10.0K Ohm 1/10 Watt 1% Resistor&lt;/li&gt;
&lt;li&gt;20.0K Ohm 1/10 Watt 1% Resistor&lt;/li&gt;
&lt;li&gt;33.0K Ohm 1/10 Watt 1% Resistor&lt;/li&gt;
&lt;li&gt;100.0K Ohm 1/10 Watt 1% Resistor&lt;/li&gt;
&lt;/ul&gt;
&lt;b&gt;0805&lt;/b&gt; - 0805 Surface Mount Package
&lt;ul&gt;
&lt;li&gt;0 Ohm 1/8 Watt 1% Resistor&lt;/li&gt;
&lt;li&gt;33 Ohm 1/8 Watt 1% Resistor&lt;/li&gt;
&lt;li&gt;100 Ohm 1/8 Watt 1% Resistor&lt;/li&gt;
&lt;li&gt;150 Ohm 1/8 Watt 1% Resistor&lt;/li&gt;
&lt;li&gt;200 Ohm 1/8 Watt 1% Resistor&lt;/li&gt;
&lt;li&gt;240 Ohm 1/8 Watt 1% Resistor&lt;/li&gt;
&lt;li&gt;330 Ohm 1/8 Watt 1% Resistor&lt;/li&gt;
&lt;li&gt;390 Ohm 1/8 Watt 1% Resistor&lt;/li&gt;
&lt;li&gt;470 Ohm 1/8 Watt 1% Resistor&lt;/li&gt;
&lt;li&gt;1.0K Ohm 1/8 Watt 1% Resistor&lt;/li&gt;
&lt;li&gt;1.5K Ohm 1/8 Watt 1% Resistor&lt;/li&gt;
&lt;li&gt;2.0K Ohm 1/8 Watt 1% Resistor&lt;/li&gt;
&lt;li&gt;4.7K Ohm 1/8 Watt 1% Resistor&lt;/li&gt;
&lt;li&gt;5.1K Ohm 1/8 Watt 1% Resistor&lt;/li&gt;
&lt;li&gt;5.6K Ohm 1/8 Watt 1% Resistor&lt;/li&gt;
&lt;li&gt;10.0K Ohm 1/8 Watt 1% Resistor&lt;/li&gt;
&lt;li&gt;22.0K Ohm 1/8 Watt 1% Resistor&lt;/li&gt;
&lt;li&gt;33.0K Ohm 1/8 Watt 1% Resistor&lt;/li&gt;
&lt;li&gt;100K Ohm 1/8 Watt 1% Resistor&lt;/li&gt;
&lt;/ul&gt;
&lt;b&gt;1206&lt;/b&gt; - 1206 Surface Mount Package&lt;br&gt;</description>
<gates>
<gate name="G$1" symbol="RESISTOR"/>
</gates>
<devices>
<device name="0805" package="0805">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="1206" package="1206">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="0603" package="0603">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="0402" package="0402">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="2512" package="2512">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="CAP_CERAMIC" prefix="C" uservalue="yes">
<description>&lt;p&gt;&lt;b&gt;Ceramic Capacitors&lt;/b&gt;&lt;/p&gt;
&lt;b&gt;0402&lt;/b&gt; - 0402 Surface Mount Capacitors
&lt;ul&gt;
&lt;li&gt;0.1uF 10V 10% [Digikey: 490-1318-2-ND]&lt;/li&gt;
&lt;/ul&gt;
&lt;b&gt;0603&lt;/b&gt; - 0603 Surface Mount Capacitors
&lt;ul&gt;
&lt;li&gt;16 pF 50V 5% [Digikey: 445-5051-2-ND]&lt;/li&gt;
&lt;li&gt;22 pF 50V [Digikey: PCC220ACVTR-ND]&lt;/li&gt;
&lt;li&gt;33 pF 50V 5% [Digikey: 490-1415-1-ND]&lt;/li&gt;
&lt;li&gt;56pF 50V 5% [Digikey: 490-1421-1-ND]&lt;/li&gt;
&lt;li&gt;220pF 50V 5% [Digikey: 445-1285-1-ND]&lt;/li&gt;
&lt;li&gt;680 pF 50V &lt;/li&gt;
&lt;li&gt;2200 pF 50V 5% C0G [Digikey: 445-1297-1-ND]&lt;/li&gt;
&lt;li&gt;5600 pF 100V 5% X7R [Digikey: 478-3711-1-ND]&lt;/li&gt;
&lt;li&gt;0.1 µF 25V 10% [Digikey: PCC2277TR-ND]&lt;/li&gt;
&lt;li&gt;0.22 µF 16V 10% X7R [Digikey: 445-1318-1-ND]&lt;/li&gt;
&lt;li&gt;1.0 µF 25V 10% [Digikey: 445-5146-2-ND]&lt;/li&gt;
&lt;/ul&gt;
&lt;b&gt;0603&lt;/b&gt; - RF Specific
&lt;ul&gt;
&lt;li&gt;3pF 250V +/-0.1pF RF [Digikey: 712-1347-1-ND]&lt;/li&gt;
&lt;li&gt;18 pF 250V 5%  [Digikey: 478-3505-1-ND or 712-1322-1-ND]&lt;/li&gt;
&lt;li&gt;56 pF 250V 5% C0G RF [Digikey: 490-4867-1-ND]&lt;/li&gt;
&lt;li&gt;68 pF 250V RF [Digikey: 490-4868-1-ND]&lt;/li&gt;
&lt;/ul&gt;
&lt;b&gt;0805&lt;/b&gt; - 0805 Surface Mount Capacitors
&lt;ul&gt;
&lt;li&gt;220 pF 250V 2% &lt;strong&gt;RF&lt;/strong&gt; Ceramic Capacitor [Digikey: 712-1398-1-ND]&lt;/li&gt;
&lt;li&gt;1000 pF 50V 2% NP0 Ceramic Capacitor [Digikey: 478-3760-1-ND]&lt;/li&gt;
&lt;li&gt;0.1 µF 25V 10% Ceramic Capacitor [Digikey: PCC1828TR-ND]&lt;/li&gt;
&lt;li&gt;1.0 µF 16V 10% Ceramic Capacitor[Digikey: 490-1691-2-ND]&lt;/li&gt;
&lt;li&gt;10.0 µF 10V 10% Ceramic Capacitor[Digikey: 709-1228-1-ND]&lt;/li&gt;
&lt;/ul&gt;
&lt;/ul&gt;&lt;b&gt;1206&lt;/b&gt; - 1206 Surface Mount Capacitors</description>
<gates>
<gate name="G$1" symbol="CAPACITOR"/>
</gates>
<devices>
<device name="0805" package="0805">
<connects>
<connect gate="G$1" pin="P$1" pad="1"/>
<connect gate="G$1" pin="P$2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="1206" package="1206">
<connects>
<connect gate="G$1" pin="P$1" pad="1"/>
<connect gate="G$1" pin="P$2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="0603" package="0603">
<connects>
<connect gate="G$1" pin="P$1" pad="1"/>
<connect gate="G$1" pin="P$2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="0402" package="0402">
<connects>
<connect gate="G$1" pin="P$1" pad="1"/>
<connect gate="G$1" pin="P$2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="CRYSTAL" prefix="Y" uservalue="yes">
<description>&lt;p&gt;&lt;b&gt;Crystals&lt;/b&gt;&lt;/p&gt;

&lt;p&gt;&lt;b&gt;HC49UP&lt;/b&gt; - Surface Mount Crystal
&lt;ul&gt;
&lt;li&gt;4.0MHz 18pF +/-30ppm Surface Mount Crystal [Digikey: 535-9857-1-ND]&lt;/li&gt;
&lt;li&gt;12.0 MHz Surface Mount Crystal [Digikey: 535-9869-6-ND]&lt;/li&gt;
&lt;li&gt;25.0 MHz Surface Mount Crystal [Digikey: 535-9078-1-ND]&lt;/li&gt;
&lt;/ul&gt;

&lt;p&gt;&lt;b&gt;3.2 x 2.5mm&lt;/b&gt; - MEMs SMT Crystal
&lt;ul&gt;
&lt;li&gt;12.0 MHz 8pF 15ppm 3.2 x 2.5mm Crystal [Digikey: 644-1047-1-ND]&lt;/li&gt;
&lt;li&gt;16.0 MHz 8pF 15ppm 3.2 x 2.5mm Crystal [Digikey: 644-1049-1-ND]&lt;/li&gt;
&lt;li&gt;16.0 MHz 10pF 10ppm 3.2 x 2.5mm Crystal [Digikey: 644-1100-1-ND]&lt;/li&gt;
&lt;li&gt;27.12 MHz 18pF 30ppm 3.2 x 2.5mm Crystal [Digikey: 887-1424-1-ND]&lt;/li&gt;
&lt;/ul&gt;

&lt;p&gt;&lt;b&gt;4.9 x 1.8mm&lt;/b&gt; - MEMs SMT Crystal
&lt;ul&gt;
&lt;li&gt;32.768 KHz 12.5pF 20ppm 4.9 x 1.8mm Crystal [Digikey: SE2415CT-ND]&lt;/li&gt;
&lt;/ul&gt;

&lt;p&gt;&lt;b&gt;Cylinder&lt;/b&gt;
&lt;ul&gt;
&lt;li&gt;32.768KHz Cylinder Crystal&lt;/li&gt;
&lt;/ul&gt;
&lt;/p&gt;

&lt;/p&gt;</description>
<gates>
<gate name="G$1" symbol="CRYSTAL"/>
</gates>
<devices>
<device name="SMD" package="HC49UP">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="32.768" package="CRYSTAL32SMT">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="THIN" package="CRYSTAL_3.2X2.5">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="THIN32K" package="CRYSTAL_4.9X1.8">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="" package="NX8045GB">
<connects>
<connect gate="G$1" pin="1" pad="P$1"/>
<connect gate="G$1" pin="2" pad="P$2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="SCHOTTKY" prefix="D">
<description>Protection Diode: MBRA140</description>
<gates>
<gate name="G$1" symbol="DIODE-SCHOTTKY"/>
</gates>
<devices>
<device name="" package="SMA-DIODE">
<connects>
<connect gate="G$1" pin="A" pad="A"/>
<connect gate="G$1" pin="C" pad="C"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="GND">
<description>&lt;b&gt;GND&lt;/b&gt;</description>
<gates>
<gate name="G$1" symbol="GND"/>
</gates>
<devices>
<device name="">
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="HEADER-1X1" prefix="JP" uservalue="yes">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
<gates>
<gate name="G$1" symbol="PINHD1"/>
</gates>
<devices>
<device name="" package="1X01_OVAL">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="ROUND" package="1X01_ROUND">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="2MM" package="1X01_2MM">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="2MM_OVAL" package="1X01_2MM_OVAL">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="HEADER-1X2" prefix="JP" uservalue="yes">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
<gates>
<gate name="G$1" symbol="PINHD2"/>
</gates>
<devices>
<device name="" package="1X02_OVAL">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="ROUND" package="1X02_ROUND">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="SMT" package="1X02_SMT">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="HEADER-1X3" prefix="JP" uservalue="yes">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
<gates>
<gate name="A" symbol="PINHD3"/>
</gates>
<devices>
<device name="" package="1X03_OVAL">
<connects>
<connect gate="A" pin="1" pad="1"/>
<connect gate="A" pin="2" pad="2"/>
<connect gate="A" pin="3" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="ROUND" package="1X03_ROUND">
<connects>
<connect gate="A" pin="1" pad="1"/>
<connect gate="A" pin="2" pad="2"/>
<connect gate="A" pin="3" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="SMT" package="1X03_SMT">
<connects>
<connect gate="A" pin="1" pad="1"/>
<connect gate="A" pin="2" pad="2"/>
<connect gate="A" pin="3" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="HEADER-1X4" prefix="JP" uservalue="yes">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
<gates>
<gate name="A" symbol="PINHD4"/>
</gates>
<devices>
<device name="" package="1X04_OVAL">
<connects>
<connect gate="A" pin="1" pad="1"/>
<connect gate="A" pin="2" pad="2"/>
<connect gate="A" pin="3" pad="3"/>
<connect gate="A" pin="4" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="ROUND" package="1X04_ROUND">
<connects>
<connect gate="A" pin="1" pad="1"/>
<connect gate="A" pin="2" pad="2"/>
<connect gate="A" pin="3" pad="3"/>
<connect gate="A" pin="4" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="SMT" package="1X04_SMT">
<connects>
<connect gate="A" pin="1" pad="1"/>
<connect gate="A" pin="2" pad="2"/>
<connect gate="A" pin="3" pad="3"/>
<connect gate="A" pin="4" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="HEADER-1X5" prefix="JP" uservalue="yes">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
<gates>
<gate name="A" symbol="PINHD5"/>
</gates>
<devices>
<device name="" package="1X05_OVAL">
<connects>
<connect gate="A" pin="1" pad="1"/>
<connect gate="A" pin="2" pad="2"/>
<connect gate="A" pin="3" pad="3"/>
<connect gate="A" pin="4" pad="4"/>
<connect gate="A" pin="5" pad="5"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="ROUND" package="1X05_ROUND">
<connects>
<connect gate="A" pin="1" pad="1"/>
<connect gate="A" pin="2" pad="2"/>
<connect gate="A" pin="3" pad="3"/>
<connect gate="A" pin="4" pad="4"/>
<connect gate="A" pin="5" pad="5"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="SMT" package="1X05_SMT">
<connects>
<connect gate="A" pin="1" pad="1"/>
<connect gate="A" pin="2" pad="2"/>
<connect gate="A" pin="3" pad="3"/>
<connect gate="A" pin="4" pad="4"/>
<connect gate="A" pin="5" pad="5"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="HEADER-1X6" prefix="JP" uservalue="yes">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
<gates>
<gate name="A" symbol="PINHD6"/>
</gates>
<devices>
<device name="OVAL" package="1X06_OVAL">
<connects>
<connect gate="A" pin="1" pad="1"/>
<connect gate="A" pin="2" pad="2"/>
<connect gate="A" pin="3" pad="3"/>
<connect gate="A" pin="4" pad="4"/>
<connect gate="A" pin="5" pad="5"/>
<connect gate="A" pin="6" pad="6"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="ROUND" package="1X06_ROUND">
<connects>
<connect gate="A" pin="1" pad="1"/>
<connect gate="A" pin="2" pad="2"/>
<connect gate="A" pin="3" pad="3"/>
<connect gate="A" pin="4" pad="4"/>
<connect gate="A" pin="5" pad="5"/>
<connect gate="A" pin="6" pad="6"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="SMT" package="1X06_SMT">
<connects>
<connect gate="A" pin="1" pad="1"/>
<connect gate="A" pin="2" pad="2"/>
<connect gate="A" pin="3" pad="3"/>
<connect gate="A" pin="4" pad="4"/>
<connect gate="A" pin="5" pad="5"/>
<connect gate="A" pin="6" pad="6"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="2MM" package="1X06_ROUND_2MM">
<connects>
<connect gate="A" pin="1" pad="1"/>
<connect gate="A" pin="2" pad="2"/>
<connect gate="A" pin="3" pad="3"/>
<connect gate="A" pin="4" pad="4"/>
<connect gate="A" pin="5" pad="5"/>
<connect gate="A" pin="6" pad="6"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="HEADER-1X7" prefix="JP" uservalue="yes">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
<gates>
<gate name="A" symbol="PINHD7"/>
</gates>
<devices>
<device name="" package="1X07_OVAL">
<connects>
<connect gate="A" pin="1" pad="1"/>
<connect gate="A" pin="2" pad="2"/>
<connect gate="A" pin="3" pad="3"/>
<connect gate="A" pin="4" pad="4"/>
<connect gate="A" pin="5" pad="5"/>
<connect gate="A" pin="6" pad="6"/>
<connect gate="A" pin="7" pad="7"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="ROUND" package="1X07_ROUND">
<connects>
<connect gate="A" pin="1" pad="1"/>
<connect gate="A" pin="2" pad="2"/>
<connect gate="A" pin="3" pad="3"/>
<connect gate="A" pin="4" pad="4"/>
<connect gate="A" pin="5" pad="5"/>
<connect gate="A" pin="6" pad="6"/>
<connect gate="A" pin="7" pad="7"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="HEADER-1X8" prefix="JP" uservalue="yes">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
<gates>
<gate name="A" symbol="PINHD8"/>
</gates>
<devices>
<device name="" package="1X08_OVAL">
<connects>
<connect gate="A" pin="1" pad="1"/>
<connect gate="A" pin="2" pad="2"/>
<connect gate="A" pin="3" pad="3"/>
<connect gate="A" pin="4" pad="4"/>
<connect gate="A" pin="5" pad="5"/>
<connect gate="A" pin="6" pad="6"/>
<connect gate="A" pin="7" pad="7"/>
<connect gate="A" pin="8" pad="8"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="ROUND" package="1X08_ROUND">
<connects>
<connect gate="A" pin="1" pad="1"/>
<connect gate="A" pin="2" pad="2"/>
<connect gate="A" pin="3" pad="3"/>
<connect gate="A" pin="4" pad="4"/>
<connect gate="A" pin="5" pad="5"/>
<connect gate="A" pin="6" pad="6"/>
<connect gate="A" pin="7" pad="7"/>
<connect gate="A" pin="8" pad="8"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="HEADER-1X9" prefix="JP" uservalue="yes">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
<gates>
<gate name="A" symbol="PINHD9"/>
</gates>
<devices>
<device name="" package="1X09_OVAL">
<connects>
<connect gate="A" pin="1" pad="1"/>
<connect gate="A" pin="2" pad="2"/>
<connect gate="A" pin="3" pad="3"/>
<connect gate="A" pin="4" pad="4"/>
<connect gate="A" pin="5" pad="5"/>
<connect gate="A" pin="6" pad="6"/>
<connect gate="A" pin="7" pad="7"/>
<connect gate="A" pin="8" pad="8"/>
<connect gate="A" pin="9" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="HEADER-1X10" prefix="JP" uservalue="yes">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
<gates>
<gate name="A" symbol="PINHD10"/>
</gates>
<devices>
<device name="" package="1X10_OVAL">
<connects>
<connect gate="A" pin="1" pad="1"/>
<connect gate="A" pin="10" pad="10"/>
<connect gate="A" pin="2" pad="2"/>
<connect gate="A" pin="3" pad="3"/>
<connect gate="A" pin="4" pad="4"/>
<connect gate="A" pin="5" pad="5"/>
<connect gate="A" pin="6" pad="6"/>
<connect gate="A" pin="7" pad="7"/>
<connect gate="A" pin="8" pad="8"/>
<connect gate="A" pin="9" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="SMT" package="1X10_SMT">
<connects>
<connect gate="A" pin="1" pad="1"/>
<connect gate="A" pin="10" pad="10"/>
<connect gate="A" pin="2" pad="2"/>
<connect gate="A" pin="3" pad="3"/>
<connect gate="A" pin="4" pad="4"/>
<connect gate="A" pin="5" pad="5"/>
<connect gate="A" pin="6" pad="6"/>
<connect gate="A" pin="7" pad="7"/>
<connect gate="A" pin="8" pad="8"/>
<connect gate="A" pin="9" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="ROUND" package="1X10_ROUND">
<connects>
<connect gate="A" pin="1" pad="1"/>
<connect gate="A" pin="10" pad="10"/>
<connect gate="A" pin="2" pad="2"/>
<connect gate="A" pin="3" pad="3"/>
<connect gate="A" pin="4" pad="4"/>
<connect gate="A" pin="5" pad="5"/>
<connect gate="A" pin="6" pad="6"/>
<connect gate="A" pin="7" pad="7"/>
<connect gate="A" pin="8" pad="8"/>
<connect gate="A" pin="9" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="1X10_2MM" package="1X10_ROUND_2MM">
<connects>
<connect gate="A" pin="1" pad="1"/>
<connect gate="A" pin="10" pad="10"/>
<connect gate="A" pin="2" pad="2"/>
<connect gate="A" pin="3" pad="3"/>
<connect gate="A" pin="4" pad="4"/>
<connect gate="A" pin="5" pad="5"/>
<connect gate="A" pin="6" pad="6"/>
<connect gate="A" pin="7" pad="7"/>
<connect gate="A" pin="8" pad="8"/>
<connect gate="A" pin="9" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="HEADER-2X5" prefix="JP" uservalue="yes">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
<gates>
<gate name="A" symbol="PINH2X5"/>
</gates>
<devices>
<device name="" package="2X05">
<connects>
<connect gate="A" pin="1" pad="1"/>
<connect gate="A" pin="10" pad="10"/>
<connect gate="A" pin="2" pad="2"/>
<connect gate="A" pin="3" pad="3"/>
<connect gate="A" pin="4" pad="4"/>
<connect gate="A" pin="5" pad="5"/>
<connect gate="A" pin="6" pad="6"/>
<connect gate="A" pin="7" pad="7"/>
<connect gate="A" pin="8" pad="8"/>
<connect gate="A" pin="9" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LPC1343" prefix="U" uservalue="yes">
<description>&lt;b&gt;LPC1343 &lt;/b&gt;&lt;p&gt;72 MHz 32-bit ARM Cortex-M3 microcontroller. 32 kB Flash, 8 kB SRAM, USB Device &lt;/p&gt;

&lt;p&gt;Mouser: 771-LPC1343FBD48151 &lt;br/&gt;
Digikey: 568-4945-ND&lt;/p&gt;</description>
<gates>
<gate name="G$1" symbol="LPC1343FBD48"/>
</gates>
<devices>
<device name="" package="LQFP48">
<connects>
<connect gate="G$1" pin="PIO0_1/CLKOUT/CT32B0_MAT2/USB_FTOGGLE" pad="4"/>
<connect gate="G$1" pin="PIO0_2/SSEL/CT16B0_CAP0" pad="10"/>
<connect gate="G$1" pin="PIO0_3/USB_VBUS" pad="14"/>
<connect gate="G$1" pin="PIO0_4/SCL" pad="15"/>
<connect gate="G$1" pin="PIO0_5/SDA" pad="16"/>
<connect gate="G$1" pin="PIO0_6/USB_CONNECT/SCK" pad="22"/>
<connect gate="G$1" pin="PIO0_7/CTS" pad="23"/>
<connect gate="G$1" pin="PIO0_8/MISO/CT16B0_MAT0" pad="27"/>
<connect gate="G$1" pin="PIO0_9/MOSI/CT16B0_MAT1/SWO" pad="28"/>
<connect gate="G$1" pin="PIO1_10/AD6/CT16B1_MAT1" pad="30"/>
<connect gate="G$1" pin="PIO1_11/AD7" pad="42"/>
<connect gate="G$1" pin="PIO1_4/AD5/CT32B1_MAT3/WAKEUP" pad="40"/>
<connect gate="G$1" pin="PIO1_5/RTS/CT32B0_CAP0" pad="45"/>
<connect gate="G$1" pin="PIO1_6/RXD/CT32B0_MAT0" pad="46"/>
<connect gate="G$1" pin="PIO1_7/TXD/CT32B0_MAT1" pad="47"/>
<connect gate="G$1" pin="PIO1_8/CT16B1_CAP0" pad="9"/>
<connect gate="G$1" pin="PIO1_9/CT16B1_MAT0" pad="17"/>
<connect gate="G$1" pin="PIO2_0/DTR" pad="2"/>
<connect gate="G$1" pin="PIO2_1/DSR" pad="13"/>
<connect gate="G$1" pin="PIO2_10" pad="25"/>
<connect gate="G$1" pin="PIO2_11/SCK" pad="31"/>
<connect gate="G$1" pin="PIO2_2/DCD" pad="26"/>
<connect gate="G$1" pin="PIO2_3/RI" pad="38"/>
<connect gate="G$1" pin="PIO2_4" pad="18"/>
<connect gate="G$1" pin="PIO2_5" pad="21"/>
<connect gate="G$1" pin="PIO2_6" pad="1"/>
<connect gate="G$1" pin="PIO2_7" pad="11"/>
<connect gate="G$1" pin="PIO2_8" pad="12"/>
<connect gate="G$1" pin="PIO2_9" pad="24"/>
<connect gate="G$1" pin="PIO3_0" pad="36"/>
<connect gate="G$1" pin="PIO3_1" pad="37"/>
<connect gate="G$1" pin="PIO3_2" pad="43"/>
<connect gate="G$1" pin="PIO3_3" pad="48"/>
<connect gate="G$1" pin="RESET/PIO0_0" pad="3"/>
<connect gate="G$1" pin="SWCLK/PIO0_10/SCK/CT16B0_MAT2" pad="29"/>
<connect gate="G$1" pin="SWDIO/PIO1_3/AD4/CT32B1_MAT2" pad="39"/>
<connect gate="G$1" pin="TDI/PIO0_11/AD0/CT32B0_MAT3" pad="32"/>
<connect gate="G$1" pin="TDO/PIO1_1/AD2/CT32B1_MAT0" pad="34"/>
<connect gate="G$1" pin="TMS/PIO1_0/AD1/CT32B1_CAP0" pad="33"/>
<connect gate="G$1" pin="TRST/PIO1_2/AD3/CT32B1_MAT1" pad="35"/>
<connect gate="G$1" pin="USB_DM" pad="19"/>
<connect gate="G$1" pin="USB_DP" pad="20"/>
<connect gate="G$1" pin="VDD(3V3)" pad="44"/>
<connect gate="G$1" pin="VDD(IO)" pad="8"/>
<connect gate="G$1" pin="VSS" pad="41"/>
<connect gate="G$1" pin="VSSIO" pad="5"/>
<connect gate="G$1" pin="XTALIN" pad="6"/>
<connect gate="G$1" pin="XTALOUT" pad="7"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ATXMEGAXXA4U" prefix="IC" uservalue="yes">
<description>ATXMEGA A4U Series (XMEGA+USB)</description>
<gates>
<gate name="G$1" symbol="XMEGA-A4U"/>
</gates>
<devices>
<device name="-AU" package="TQFP-44">
<connects>
<connect gate="G$1" pin="AVCC" pad="39"/>
<connect gate="G$1" pin="GND@1" pad="8"/>
<connect gate="G$1" pin="GND@2" pad="18"/>
<connect gate="G$1" pin="GND@3" pad="30"/>
<connect gate="G$1" pin="GND@4" pad="38"/>
<connect gate="G$1" pin="OC0A/PD0" pad="20"/>
<connect gate="G$1" pin="OC0A/SDA/PE0" pad="28"/>
<connect gate="G$1" pin="OC0B/XCK0/PD1" pad="21"/>
<connect gate="G$1" pin="OC0C/RXD0/PD2" pad="22"/>
<connect gate="G$1" pin="OC0D/TXD0/PD3" pad="23"/>
<connect gate="G$1" pin="PA0/ADC0/AREFA" pad="40"/>
<connect gate="G$1" pin="PA1/ADC1" pad="41"/>
<connect gate="G$1" pin="PA2/ADC2" pad="42"/>
<connect gate="G$1" pin="PA3/ADC3" pad="43"/>
<connect gate="G$1" pin="PA4/ADC4" pad="44"/>
<connect gate="G$1" pin="PA5/ADC5" pad="1"/>
<connect gate="G$1" pin="PA6/ADC6" pad="2"/>
<connect gate="G$1" pin="PA7/ADC7" pad="3"/>
<connect gate="G$1" pin="PB0/ADC8/AREFB" pad="4"/>
<connect gate="G$1" pin="PB1/ADC9" pad="5"/>
<connect gate="G$1" pin="PB2/ADC10/DAC0" pad="6"/>
<connect gate="G$1" pin="PB3/ADC11/DAC1" pad="7"/>
<connect gate="G$1" pin="PC0/OC0A/SDA" pad="10"/>
<connect gate="G$1" pin="PC1/OC0B/XCK0/SCL" pad="11"/>
<connect gate="G$1" pin="PC2/OC0C/RXD0" pad="12"/>
<connect gate="G$1" pin="PC3/OC0D/TXD0" pad="13"/>
<connect gate="G$1" pin="PC4/OC1A/#SS" pad="14"/>
<connect gate="G$1" pin="PC5/OC1B/MOSI/XCK1" pad="15"/>
<connect gate="G$1" pin="PC6/MISO/RXD1" pad="16"/>
<connect gate="G$1" pin="PC7/SCK/TXD1/CLKO/EVO" pad="17"/>
<connect gate="G$1" pin="PDI-DATA" pad="34"/>
<connect gate="G$1" pin="PR0/XTAL2" pad="36"/>
<connect gate="G$1" pin="PR1/XTAL1" pad="37"/>
<connect gate="G$1" pin="RESET/PDI-CLK" pad="35"/>
<connect gate="G$1" pin="RXD0/OC0C/PE2" pad="32"/>
<connect gate="G$1" pin="RXD1/MISO/USB-/PD6" pad="26"/>
<connect gate="G$1" pin="SS/PD4" pad="24"/>
<connect gate="G$1" pin="TXD0/OC0D/PE3" pad="33"/>
<connect gate="G$1" pin="TXD1/USB+/PD7" pad="27"/>
<connect gate="G$1" pin="VCC@1" pad="9"/>
<connect gate="G$1" pin="VCC@2" pad="19"/>
<connect gate="G$1" pin="VCC@3" pad="31"/>
<connect gate="G$1" pin="XCK0/OC0B/SCL/PE1" pad="29"/>
<connect gate="G$1" pin="XCK1/MOSI/PD5" pad="25"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-MH" package="QFN-44">
<connects>
<connect gate="G$1" pin="AVCC" pad="39"/>
<connect gate="G$1" pin="GND@1" pad="8"/>
<connect gate="G$1" pin="GND@2" pad="18"/>
<connect gate="G$1" pin="GND@3" pad="30"/>
<connect gate="G$1" pin="GND@4" pad="38"/>
<connect gate="G$1" pin="OC0A/PD0" pad="20"/>
<connect gate="G$1" pin="OC0A/SDA/PE0" pad="28"/>
<connect gate="G$1" pin="OC0B/XCK0/PD1" pad="21"/>
<connect gate="G$1" pin="OC0C/RXD0/PD2" pad="22"/>
<connect gate="G$1" pin="OC0D/TXD0/PD3" pad="23"/>
<connect gate="G$1" pin="PA0/ADC0/AREFA" pad="40"/>
<connect gate="G$1" pin="PA1/ADC1" pad="41"/>
<connect gate="G$1" pin="PA2/ADC2" pad="42"/>
<connect gate="G$1" pin="PA3/ADC3" pad="43"/>
<connect gate="G$1" pin="PA4/ADC4" pad="44"/>
<connect gate="G$1" pin="PA5/ADC5" pad="1"/>
<connect gate="G$1" pin="PA6/ADC6" pad="2"/>
<connect gate="G$1" pin="PA7/ADC7" pad="3"/>
<connect gate="G$1" pin="PB0/ADC8/AREFB" pad="4"/>
<connect gate="G$1" pin="PB1/ADC9" pad="5"/>
<connect gate="G$1" pin="PB2/ADC10/DAC0" pad="6"/>
<connect gate="G$1" pin="PB3/ADC11/DAC1" pad="7"/>
<connect gate="G$1" pin="PC0/OC0A/SDA" pad="10"/>
<connect gate="G$1" pin="PC1/OC0B/XCK0/SCL" pad="11"/>
<connect gate="G$1" pin="PC2/OC0C/RXD0" pad="12"/>
<connect gate="G$1" pin="PC3/OC0D/TXD0" pad="13"/>
<connect gate="G$1" pin="PC4/OC1A/#SS" pad="14"/>
<connect gate="G$1" pin="PC5/OC1B/MOSI/XCK1" pad="15"/>
<connect gate="G$1" pin="PC6/MISO/RXD1" pad="16"/>
<connect gate="G$1" pin="PC7/SCK/TXD1/CLKO/EVO" pad="17"/>
<connect gate="G$1" pin="PDI-DATA" pad="34"/>
<connect gate="G$1" pin="PR0/XTAL2" pad="36"/>
<connect gate="G$1" pin="PR1/XTAL1" pad="37"/>
<connect gate="G$1" pin="RESET/PDI-CLK" pad="35"/>
<connect gate="G$1" pin="RXD0/OC0C/PE2" pad="32"/>
<connect gate="G$1" pin="RXD1/MISO/USB-/PD6" pad="26"/>
<connect gate="G$1" pin="SS/PD4" pad="24"/>
<connect gate="G$1" pin="TXD0/OC0D/PE3" pad="33"/>
<connect gate="G$1" pin="TXD1/USB+/PD7" pad="27"/>
<connect gate="G$1" pin="VCC@1" pad="9"/>
<connect gate="G$1" pin="VCC@2" pad="19"/>
<connect gate="G$1" pin="VCC@3" pad="31"/>
<connect gate="G$1" pin="XCK0/OC0B/SCL/PE1" pad="29"/>
<connect gate="G$1" pin="XCK1/MOSI/PD5" pad="25"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="AD8608" prefix="IC">
<gates>
<gate name="A" symbol="OPAMP"/>
<gate name="B" symbol="OPAMP"/>
<gate name="C" symbol="OPAMP"/>
<gate name="D" symbol="OPAMP"/>
<gate name="G$1" symbol="PWR+-"/>
</gates>
<devices>
<device name="R" package="SO-20">
<connects>
<connect gate="A" pin="+IN" pad="3"/>
<connect gate="A" pin="-IN" pad="2"/>
<connect gate="A" pin="OUT" pad="1"/>
<connect gate="B" pin="+IN" pad="5"/>
<connect gate="B" pin="-IN" pad="6"/>
<connect gate="B" pin="OUT" pad="7"/>
<connect gate="C" pin="+IN" pad="10"/>
<connect gate="C" pin="-IN" pad="9"/>
<connect gate="C" pin="OUT" pad="8"/>
<connect gate="D" pin="+IN" pad="12"/>
<connect gate="D" pin="-IN" pad="13"/>
<connect gate="D" pin="OUT" pad="14"/>
<connect gate="G$1" pin="V+" pad="4"/>
<connect gate="G$1" pin="V-" pad="11"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="RU" package="TSSOP-14">
<connects>
<connect gate="A" pin="+IN" pad="3"/>
<connect gate="A" pin="-IN" pad="2"/>
<connect gate="A" pin="OUT" pad="1"/>
<connect gate="B" pin="+IN" pad="5"/>
<connect gate="B" pin="-IN" pad="6"/>
<connect gate="B" pin="OUT" pad="7"/>
<connect gate="C" pin="+IN" pad="10"/>
<connect gate="C" pin="-IN" pad="9"/>
<connect gate="C" pin="OUT" pad="8"/>
<connect gate="D" pin="+IN" pad="12"/>
<connect gate="D" pin="-IN" pad="13"/>
<connect gate="D" pin="OUT" pad="14"/>
<connect gate="G$1" pin="V+" pad="4"/>
<connect gate="G$1" pin="V-" pad="11"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MCP4922">
<description>MCP4922

12b SPI DAC</description>
<gates>
<gate name="G$1" symbol="MCP4922"/>
</gates>
<devices>
<device name="TSSOP" package="TSSOP-14">
<connects>
<connect gate="G$1" pin="AVSS" pad="12"/>
<connect gate="G$1" pin="CS" pad="3"/>
<connect gate="G$1" pin="LDAC" pad="8"/>
<connect gate="G$1" pin="MOSI" pad="5"/>
<connect gate="G$1" pin="NC@2" pad="2"/>
<connect gate="G$1" pin="NC@6" pad="6"/>
<connect gate="G$1" pin="NC@7" pad="7"/>
<connect gate="G$1" pin="SCK" pad="4"/>
<connect gate="G$1" pin="SHDN" pad="9"/>
<connect gate="G$1" pin="VCC" pad="1"/>
<connect gate="G$1" pin="VOUTA" pad="14"/>
<connect gate="G$1" pin="VOUTB" pad="10"/>
<connect gate="G$1" pin="VREFA" pad="13"/>
<connect gate="G$1" pin="VREFB" pad="11"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="SOIC" package="SO-20">
<connects>
<connect gate="G$1" pin="AVSS" pad="12"/>
<connect gate="G$1" pin="CS" pad="3"/>
<connect gate="G$1" pin="LDAC" pad="8"/>
<connect gate="G$1" pin="MOSI" pad="5"/>
<connect gate="G$1" pin="NC@2" pad="2"/>
<connect gate="G$1" pin="NC@6" pad="6"/>
<connect gate="G$1" pin="NC@7" pad="7"/>
<connect gate="G$1" pin="SCK" pad="4"/>
<connect gate="G$1" pin="SHDN" pad="9"/>
<connect gate="G$1" pin="VCC" pad="1"/>
<connect gate="G$1" pin="VOUTA" pad="14"/>
<connect gate="G$1" pin="VOUTB" pad="10"/>
<connect gate="G$1" pin="VREFA" pad="13"/>
<connect gate="G$1" pin="VREFB" pad="11"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MAX9919">
<description>&lt;b&gt;MAX9919&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;
single-channel current sense amp with high common mode voltage range and high bandwidth</description>
<gates>
<gate name="G$1" symbol="MAX9919"/>
</gates>
<devices>
<device name="" package="SO-08">
<connects>
<connect gate="G$1" pin="FB" pad="6"/>
<connect gate="G$1" pin="GND" pad="4"/>
<connect gate="G$1" pin="OUT" pad="5"/>
<connect gate="G$1" pin="REFIN" pad="7"/>
<connect gate="G$1" pin="RS+" pad="1"/>
<connect gate="G$1" pin="RS-" pad="2"/>
<connect gate="G$1" pin="SHDN" pad="3"/>
<connect gate="G$1" pin="VCC" pad="8"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="AD8606">
<gates>
<gate name="G$1" symbol="OPAMP"/>
<gate name="G$2" symbol="OPAMP"/>
<gate name="G$3" symbol="PWR+-"/>
</gates>
<devices>
<device name="" package="SO-08">
<connects>
<connect gate="G$1" pin="+IN" pad="3"/>
<connect gate="G$1" pin="-IN" pad="2"/>
<connect gate="G$1" pin="OUT" pad="1"/>
<connect gate="G$2" pin="+IN" pad="5"/>
<connect gate="G$2" pin="-IN" pad="6"/>
<connect gate="G$2" pin="OUT" pad="7"/>
<connect gate="G$3" pin="V+" pad="8"/>
<connect gate="G$3" pin="V-" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="RNETWORK" prefix="RN" uservalue="yes">
<description>4 Resistor Array 0603</description>
<gates>
<gate name="A" symbol="RESISTOR_B"/>
<gate name="B" symbol="RESISTOR_B"/>
<gate name="C" symbol="RESISTOR_B"/>
<gate name="D" symbol="RESISTOR_B"/>
</gates>
<devices>
<device name="" package="RN8P-4R-CRA06S">
<connects>
<connect gate="A" pin="1" pad="1"/>
<connect gate="A" pin="2" pad="8"/>
<connect gate="B" pin="1" pad="2"/>
<connect gate="B" pin="2" pad="7"/>
<connect gate="C" pin="1" pad="3"/>
<connect gate="C" pin="2" pad="6"/>
<connect gate="D" pin="1" pad="4"/>
<connect gate="D" pin="2" pad="5"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="TS5A3157">
<description>Single SPDT Switch in SOT23</description>
<gates>
<gate name="G$1" symbol="TS5A3157"/>
</gates>
<devices>
<device name="" package="SOT23-6">
<connects>
<connect gate="G$1" pin="COM" pad="4"/>
<connect gate="G$1" pin="GND" pad="2"/>
<connect gate="G$1" pin="IN" pad="6"/>
<connect gate="G$1" pin="NC" pad="3"/>
<connect gate="G$1" pin="NO" pad="1"/>
<connect gate="G$1" pin="V+" pad="5"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MCP1700">
<description>Voltage regulator</description>
<gates>
<gate name="G$1" symbol="VREF"/>
</gates>
<devices>
<device name="" package="SOT23-3">
<connects>
<connect gate="G$1" pin="GND" pad="3"/>
<connect gate="G$1" pin="VIN" pad="1"/>
<connect gate="G$1" pin="VO" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="VREG">
<gates>
<gate name="G$1" symbol="VREG"/>
</gates>
<devices>
<device name="MCP1700" package="SOT23-3">
<connects>
<connect gate="G$1" pin="GND" pad="1"/>
<connect gate="G$1" pin="VIN" pad="3"/>
<connect gate="G$1" pin="VO" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="AP1117" package="SOT-223">
<connects>
<connect gate="G$1" pin="GND" pad="1"/>
<connect gate="G$1" pin="VIN" pad="3"/>
<connect gate="G$1" pin="VO" pad="2 4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="IFX27001" package="TO252">
<connects>
<connect gate="G$1" pin="GND" pad="1"/>
<connect gate="G$1" pin="VIN" pad="3"/>
<connect gate="G$1" pin="VO" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ADXL3XX" prefix="U" uservalue="yes">
<description>&lt;p&gt;&lt;b&gt;ADXL3XX Low-Power 3 Axis Accelerometer&lt;/b&gt;&lt;/p&gt;
&lt;p&gt;
&lt;b&gt;LFCSP16-R&lt;/b&gt; - 16 Pin LFCSP Package (Reflow footprint)&lt;br&gt;
&lt;b&gt;LFSCP16-W&lt;/b&gt; - 16 Pin LFCSP Package (Wave footprint with extended pads for hand soldering)&lt;br&gt;
&lt;/p&gt;</description>
<gates>
<gate name="G$1" symbol="ADXL335"/>
</gates>
<devices>
<device name="" package="LFCSP-16">
<connects>
<connect gate="G$1" pin="GND1" pad="3"/>
<connect gate="G$1" pin="GND2" pad="5"/>
<connect gate="G$1" pin="GND3" pad="6"/>
<connect gate="G$1" pin="GND4" pad="7"/>
<connect gate="G$1" pin="TEST" pad="2"/>
<connect gate="G$1" pin="VS1" pad="14"/>
<connect gate="G$1" pin="VS2" pad="15"/>
<connect gate="G$1" pin="X" pad="12"/>
<connect gate="G$1" pin="Y" pad="10"/>
<connect gate="G$1" pin="Z" pad="8"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MAX31855">
<description>MAX31855 thermocouple interface</description>
<gates>
<gate name="G$1" symbol="MAX31855"/>
</gates>
<devices>
<device name="" package="SO-08">
<connects>
<connect gate="G$1" pin="CS" pad="6"/>
<connect gate="G$1" pin="DNC" pad="8"/>
<connect gate="G$1" pin="GND" pad="1"/>
<connect gate="G$1" pin="SCK" pad="5"/>
<connect gate="G$1" pin="SO" pad="7"/>
<connect gate="G$1" pin="T+" pad="3"/>
<connect gate="G$1" pin="T-" pad="2"/>
<connect gate="G$1" pin="VCC" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="OMEGA">
<gates>
<gate name="G$1" symbol="PINHD4"/>
</gates>
<devices>
<device name="PCC-SMP" package="PCC-SMP">
<connects>
<connect gate="G$1" pin="1" pad="GND@1"/>
<connect gate="G$1" pin="2" pad="+2"/>
<connect gate="G$1" pin="3" pad="-3"/>
<connect gate="G$1" pin="4" pad="GND@4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="FDS8984">
<description>N-Channel PowerTrench MOSFET 30V, 7A, 23mo</description>
<gates>
<gate name="1" symbol="MOSFET-P"/>
<gate name="2" symbol="MOSFET-P"/>
</gates>
<devices>
<device name="" package="SO-08">
<connects>
<connect gate="1" pin="D" pad="5"/>
<connect gate="1" pin="G" pad="2"/>
<connect gate="1" pin="S" pad="1"/>
<connect gate="2" pin="D" pad="8"/>
<connect gate="2" pin="G" pad="4"/>
<connect gate="2" pin="S" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ADP3120A">
<description>Dual Bootstrapped, 12 V MOSFET Driver with Output Disable</description>
<gates>
<gate name="G$1" symbol="ADP3120A"/>
</gates>
<devices>
<device name="" package="SO-08">
<connects>
<connect gate="G$1" pin="BST" pad="1"/>
<connect gate="G$1" pin="DRVH" pad="8"/>
<connect gate="G$1" pin="DRVL" pad="5"/>
<connect gate="G$1" pin="IN" pad="2"/>
<connect gate="G$1" pin="OD" pad="3"/>
<connect gate="G$1" pin="PGND" pad="6"/>
<connect gate="G$1" pin="SW" pad="7"/>
<connect gate="G$1" pin="VCC" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LT1999">
<description>LT1999</description>
<gates>
<gate name="G$1" symbol="LT1999"/>
</gates>
<devices>
<device name="" package="SO-08">
<connects>
<connect gate="G$1" pin="GND" pad="5"/>
<connect gate="G$1" pin="OUT" pad="7"/>
<connect gate="G$1" pin="RS+" pad="2"/>
<connect gate="G$1" pin="RS-" pad="3"/>
<connect gate="G$1" pin="SHDN" pad="8"/>
<connect gate="G$1" pin="VCC@1" pad="1"/>
<connect gate="G$1" pin="VCC@4" pad="4"/>
<connect gate="G$1" pin="VREF" pad="6"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MPL115A2" prefix="U">
<description>&lt;b&gt;&lt;h3&gt;MPL115A2 (I2C)&lt;/h3&gt;&lt;/b&gt;&lt;br&gt;
Miniature Digital Barometer&lt;br&gt;&lt;br&gt;
5.0x3.0x1.2mm LGA Package</description>
<gates>
<gate name="G$1" symbol="MPL115A"/>
</gates>
<devices>
<device name="" package="LGA-8">
<connects>
<connect gate="G$1" pin="CAP" pad="2"/>
<connect gate="G$1" pin="GND" pad="3"/>
<connect gate="G$1" pin="NC" pad="6"/>
<connect gate="G$1" pin="RST" pad="5"/>
<connect gate="G$1" pin="SCL" pad="8"/>
<connect gate="G$1" pin="SDA" pad="7"/>
<connect gate="G$1" pin="SHDN" pad="4"/>
<connect gate="G$1" pin="VDD" pad="1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="USB" prefix="CN" uservalue="yes">
<description>&lt;p&gt;&lt;b&gt;USB Connectors&lt;/b&gt;&lt;/p&gt;
&lt;b&gt;USBMINIB&lt;/b&gt; - Surface Mount Female Mini-B USB Connector 4UConnector: 06564&lt;/p&gt;
&lt;p&gt;By microbuilder.eu&lt;/p&gt;</description>
<gates>
<gate name="G$1" symbol="USB"/>
</gates>
<devices>
<device name="MINIB" package="USB-MINIB">
<connects>
<connect gate="G$1" pin="D+" pad="D+"/>
<connect gate="G$1" pin="D-" pad="D-"/>
<connect gate="G$1" pin="GND" pad="GND"/>
<connect gate="G$1" pin="ID" pad="ID"/>
<connect gate="G$1" pin="SHIELD" pad="GND1 GND2 GND3 GND4"/>
<connect gate="G$1" pin="VBUS" pad="VBUS"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="MICROB" package="USB-MICROB">
<connects>
<connect gate="G$1" pin="D+" pad="P3"/>
<connect gate="G$1" pin="D-" pad="P2"/>
<connect gate="G$1" pin="GND" pad="P5"/>
<connect gate="G$1" pin="ID" pad="P4"/>
<connect gate="G$1" pin="SHIELD" pad="PAD-LB PAD-LLB PAD-LT PAD-RB PAD-RRB PAD-RT"/>
<connect gate="G$1" pin="VBUS" pad="P1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ATTINYX4A">
<gates>
<gate name="G$1" symbol="ATTINY24"/>
</gates>
<devices>
<device name="MH-NOPAD" package="QFN-20-NOPAD">
<connects>
<connect gate="G$1" pin="GND" pad="8"/>
<connect gate="G$1" pin="PA0/ADC0" pad="5"/>
<connect gate="G$1" pin="PA1/ADC1" pad="4"/>
<connect gate="G$1" pin="PA2/ADC2" pad="3"/>
<connect gate="G$1" pin="PA3/ADC3" pad="2"/>
<connect gate="G$1" pin="PA4/SCL" pad="1"/>
<connect gate="G$1" pin="PA5/MISO" pad="20"/>
<connect gate="G$1" pin="PA6/MOSI" pad="16"/>
<connect gate="G$1" pin="PA7/ADC7" pad="15"/>
<connect gate="G$1" pin="PB0" pad="11"/>
<connect gate="G$1" pin="PB1" pad="12"/>
<connect gate="G$1" pin="PB2" pad="14"/>
<connect gate="G$1" pin="PB3/RESET" pad="13"/>
<connect gate="G$1" pin="VCC" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="MMH" package="VQFN-20">
<connects>
<connect gate="G$1" pin="GND" pad="8"/>
<connect gate="G$1" pin="PA0/ADC0" pad="5"/>
<connect gate="G$1" pin="PA1/ADC1" pad="4"/>
<connect gate="G$1" pin="PA2/ADC2" pad="3"/>
<connect gate="G$1" pin="PA3/ADC3" pad="2"/>
<connect gate="G$1" pin="PA4/SCL" pad="1"/>
<connect gate="G$1" pin="PA5/MISO" pad="20"/>
<connect gate="G$1" pin="PA6/MOSI" pad="16"/>
<connect gate="G$1" pin="PA7/ADC7" pad="15"/>
<connect gate="G$1" pin="PB0" pad="11"/>
<connect gate="G$1" pin="PB1" pad="12"/>
<connect gate="G$1" pin="PB2" pad="14"/>
<connect gate="G$1" pin="PB3/RESET" pad="13"/>
<connect gate="G$1" pin="VCC" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="MH" package="QFN20">
<connects>
<connect gate="G$1" pin="GND" pad="0 8"/>
<connect gate="G$1" pin="PA0/ADC0" pad="5"/>
<connect gate="G$1" pin="PA1/ADC1" pad="4"/>
<connect gate="G$1" pin="PA2/ADC2" pad="3"/>
<connect gate="G$1" pin="PA3/ADC3" pad="2"/>
<connect gate="G$1" pin="PA4/SCL" pad="1"/>
<connect gate="G$1" pin="PA5/MISO" pad="20"/>
<connect gate="G$1" pin="PA6/MOSI" pad="16"/>
<connect gate="G$1" pin="PA7/ADC7" pad="15"/>
<connect gate="G$1" pin="PB0" pad="11"/>
<connect gate="G$1" pin="PB1" pad="12"/>
<connect gate="G$1" pin="PB2" pad="14"/>
<connect gate="G$1" pin="PB3/RESET" pad="13"/>
<connect gate="G$1" pin="VCC" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="HEADER-2X3" prefix="JP" uservalue="yes">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
<gates>
<gate name="A" symbol="PINH2X3"/>
</gates>
<devices>
<device name="" package="2X03">
<connects>
<connect gate="A" pin="1" pad="1"/>
<connect gate="A" pin="2" pad="2"/>
<connect gate="A" pin="3" pad="3"/>
<connect gate="A" pin="4" pad="4"/>
<connect gate="A" pin="5" pad="5"/>
<connect gate="A" pin="6" pad="6"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LSM330DLCTR" prefix="U">
<description>I2C/SPI accelerometer/gyroscope</description>
<gates>
<gate name="G$1" symbol="LSM330DLCTR"/>
</gates>
<devices>
<device name="LGA" package="LGA28L">
<connects>
<connect gate="G$1" pin="CS_A" pad="17"/>
<connect gate="G$1" pin="CS_G" pad="10"/>
<connect gate="G$1" pin="GND" pad="2 11 14 16 18 19 20 23 24 25 27"/>
<connect gate="G$1" pin="INT1_A" pad="6"/>
<connect gate="G$1" pin="INT1_G" pad="21"/>
<connect gate="G$1" pin="INT2_A" pad="8"/>
<connect gate="G$1" pin="INT2_G" pad="5"/>
<connect gate="G$1" pin="SCL_A" pad="4"/>
<connect gate="G$1" pin="SCL_G" pad="13"/>
<connect gate="G$1" pin="SDA/SDI_A" pad="1"/>
<connect gate="G$1" pin="SDA/SDI_G" pad="9"/>
<connect gate="G$1" pin="SDO_A" pad="3"/>
<connect gate="G$1" pin="SDO_G" pad="7"/>
<connect gate="G$1" pin="VCONT" pad="26"/>
<connect gate="G$1" pin="VDD" pad="12 15 22 28"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MOT_RIC">
<gates>
<gate name="G$1" symbol="MOT"/>
</gates>
<devices>
<device name="CW" package="MOT_RIC_BM_CW">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="CCW" package="MOT_RIC_BM_CCW">
<connects>
<connect gate="G$1" pin="+" pad="-"/>
<connect gate="G$1" pin="-" pad="+"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="SAM3UXC" prefix="IC">
<description>&lt;b&gt;SAM3UXC&lt;/b&gt;&lt;p&gt;

Auto generated by &lt;i&gt;make-symbol-device-package-bsdl.ulp Rev. 43&lt;/i&gt;&lt;br&gt;
Source: sam3u_lqfp100.csv</description>
<gates>
<gate name="G$1" symbol="SAM3U_LQFP100"/>
</gates>
<devices>
<device name="" package="LQFP100">
<connects>
<connect gate="G$1" pin="AD12BVREF" pad="4"/>
<connect gate="G$1" pin="ADVREF" pad="2"/>
<connect gate="G$1" pin="DFSDM" pad="80"/>
<connect gate="G$1" pin="DFSDP" pad="81"/>
<connect gate="G$1" pin="DHSDM" pad="77"/>
<connect gate="G$1" pin="DHSDP" pad="76"/>
<connect gate="G$1" pin="ERASE" pad="43"/>
<connect gate="G$1" pin="FWUP" pad="42"/>
<connect gate="G$1" pin="GND" pad="35"/>
<connect gate="G$1" pin="GND@1" pad="61"/>
<connect gate="G$1" pin="GND@2" pad="89"/>
<connect gate="G$1" pin="GNDANA" pad="3"/>
<connect gate="G$1" pin="GNDBU" pad="46"/>
<connect gate="G$1" pin="GNDPLL" pad="72"/>
<connect gate="G$1" pin="GNDUTMI" pad="82"/>
<connect gate="G$1" pin="JTAGSEL" pad="48"/>
<connect gate="G$1" pin="NRST" pad="57"/>
<connect gate="G$1" pin="NRSTB" pad="47"/>
<connect gate="G$1" pin="PA0" pad="26"/>
<connect gate="G$1" pin="PA1" pad="27"/>
<connect gate="G$1" pin="PA10" pad="39"/>
<connect gate="G$1" pin="PA11" pad="40"/>
<connect gate="G$1" pin="PA12" pad="41"/>
<connect gate="G$1" pin="PA13" pad="10"/>
<connect gate="G$1" pin="PA14" pad="11"/>
<connect gate="G$1" pin="PA15" pad="12"/>
<connect gate="G$1" pin="PA16" pad="13"/>
<connect gate="G$1" pin="PA17" pad="14"/>
<connect gate="G$1" pin="PA18" pad="17"/>
<connect gate="G$1" pin="PA19" pad="18"/>
<connect gate="G$1" pin="PA2" pad="28"/>
<connect gate="G$1" pin="PA20" pad="19"/>
<connect gate="G$1" pin="PA21" pad="20"/>
<connect gate="G$1" pin="PA22" pad="5"/>
<connect gate="G$1" pin="PA23" pad="21"/>
<connect gate="G$1" pin="PA24" pad="23"/>
<connect gate="G$1" pin="PA25" pad="24"/>
<connect gate="G$1" pin="PA26" pad="25"/>
<connect gate="G$1" pin="PA27" pad="96"/>
<connect gate="G$1" pin="PA28" pad="84"/>
<connect gate="G$1" pin="PA29" pad="85"/>
<connect gate="G$1" pin="PA3" pad="29"/>
<connect gate="G$1" pin="PA30" pad="6"/>
<connect gate="G$1" pin="PA31" pad="86"/>
<connect gate="G$1" pin="PA4" pad="30"/>
<connect gate="G$1" pin="PA5" pad="31"/>
<connect gate="G$1" pin="PA6" pad="32"/>
<connect gate="G$1" pin="PA7" pad="33"/>
<connect gate="G$1" pin="PA8" pad="37"/>
<connect gate="G$1" pin="PA9" pad="38"/>
<connect gate="G$1" pin="PB0" pad="90"/>
<connect gate="G$1" pin="PB1" pad="91"/>
<connect gate="G$1" pin="PB10" pad="70"/>
<connect gate="G$1" pin="PB11" pad="93"/>
<connect gate="G$1" pin="PB12" pad="94"/>
<connect gate="G$1" pin="PB13" pad="95"/>
<connect gate="G$1" pin="PB14" pad="69"/>
<connect gate="G$1" pin="PB15" pad="16"/>
<connect gate="G$1" pin="PB16" pad="15"/>
<connect gate="G$1" pin="PB17" pad="68"/>
<connect gate="G$1" pin="PB18" pad="67"/>
<connect gate="G$1" pin="PB19" pad="66"/>
<connect gate="G$1" pin="PB2" pad="92"/>
<connect gate="G$1" pin="PB20" pad="65"/>
<connect gate="G$1" pin="PB21" pad="64"/>
<connect gate="G$1" pin="PB22" pad="63"/>
<connect gate="G$1" pin="PB23" pad="62"/>
<connect gate="G$1" pin="PB24" pad="58"/>
<connect gate="G$1" pin="PB3" pad="7"/>
<connect gate="G$1" pin="PB4" pad="8"/>
<connect gate="G$1" pin="PB5" pad="97"/>
<connect gate="G$1" pin="PB6" pad="98"/>
<connect gate="G$1" pin="PB7" pad="99"/>
<connect gate="G$1" pin="PB8" pad="100"/>
<connect gate="G$1" pin="PB9" pad="71"/>
<connect gate="G$1" pin="TCK" pad="56"/>
<connect gate="G$1" pin="TDI" pad="51"/>
<connect gate="G$1" pin="TDO" pad="54"/>
<connect gate="G$1" pin="TMS" pad="55"/>
<connect gate="G$1" pin="TST" pad="44"/>
<connect gate="G$1" pin="VBG" pad="78"/>
<connect gate="G$1" pin="VDDANA" pad="1"/>
<connect gate="G$1" pin="VDDBU" pad="45"/>
<connect gate="G$1" pin="VDDCORE" pad="9"/>
<connect gate="G$1" pin="VDDCORE@1" pad="34"/>
<connect gate="G$1" pin="VDDCORE@2" pad="59"/>
<connect gate="G$1" pin="VDDCORE@3" pad="83"/>
<connect gate="G$1" pin="VDDCORE@4" pad="87"/>
<connect gate="G$1" pin="VDDIN" pad="53"/>
<connect gate="G$1" pin="VDDIO" pad="22"/>
<connect gate="G$1" pin="VDDIO@1" pad="36"/>
<connect gate="G$1" pin="VDDIO@2" pad="60"/>
<connect gate="G$1" pin="VDDIO@3" pad="88"/>
<connect gate="G$1" pin="VDDOUT" pad="52"/>
<connect gate="G$1" pin="VDDPLL" pad="73"/>
<connect gate="G$1" pin="VDDUTMI" pad="79"/>
<connect gate="G$1" pin="XIN" pad="75"/>
<connect gate="G$1" pin="XIN32" pad="50"/>
<connect gate="G$1" pin="XOUT" pad="74"/>
<connect gate="G$1" pin="XOUT32" pad="49"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LED_RGB_PLCC6" prefix="LED" uservalue="yes">
<description>&lt;p&gt;&lt;b&gt;RGB LED&lt;/b&gt;&lt;/p&gt;
&lt;p&gt;Cree CLV6A-FKB - Digikey: CLV6A-FKB-CK1P1G1BB7R3R3TR-ND&lt;/p&gt;
&lt;ul&gt;
&lt;li&gt;DC Foreward Current: 20mA&lt;/li&gt;
&lt;li&gt;Foreward Voltage: R = 2.0, G = 3.2, B = 3.2&lt;/li&gt;
&lt;li&gt;Viewing Angle: 120°&lt;/li&gt;
&lt;/ul&gt;</description>
<gates>
<gate name="G$1" symbol="LEDRGB_PLCC6"/>
</gates>
<devices>
<device name="CREE-CLV6A" package="RGBLED_PLCC6">
<connects>
<connect gate="G$1" pin="BGND" pad="1"/>
<connect gate="G$1" pin="BLUE" pad="6"/>
<connect gate="G$1" pin="GGND" pad="2"/>
<connect gate="G$1" pin="GRN" pad="5"/>
<connect gate="G$1" pin="RED" pad="4"/>
<connect gate="G$1" pin="RGND" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM4674">
<gates>
<gate name="G$1" symbol="LM4764"/>
</gates>
<devices>
<device name="" package="QFN-16">
<connects>
<connect gate="G$1" pin="G0" pad="16"/>
<connect gate="G$1" pin="G1" pad="5"/>
<connect gate="G$1" pin="GND" pad="12"/>
<connect gate="G$1" pin="INL+" pad="4"/>
<connect gate="G$1" pin="INL-" pad="3"/>
<connect gate="G$1" pin="INR+" pad="1"/>
<connect gate="G$1" pin="INR-" pad="2"/>
<connect gate="G$1" pin="OUTLA" pad="7"/>
<connect gate="G$1" pin="OUTLB" pad="8"/>
<connect gate="G$1" pin="OUTRA" pad="14"/>
<connect gate="G$1" pin="OUTRB" pad="13"/>
<connect gate="G$1" pin="PGND" pad="11"/>
<connect gate="G$1" pin="PVDD" pad="6"/>
<connect gate="G$1" pin="SDL" pad="9"/>
<connect gate="G$1" pin="SDR" pad="10"/>
<connect gate="G$1" pin="VDD" pad="15"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="INA213">
<description>INA21x in SOT23</description>
<gates>
<gate name="G$1" symbol="INA213"/>
</gates>
<devices>
<device name="" package="SC-70">
<connects>
<connect gate="G$1" pin="GND" pad="P2"/>
<connect gate="G$1" pin="IN+" pad="P4"/>
<connect gate="G$1" pin="IN-" pad="P5"/>
<connect gate="G$1" pin="OUT" pad="P6"/>
<connect gate="G$1" pin="REF" pad="P1"/>
<connect gate="G$1" pin="V+" pad="P3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LME49726">
<gates>
<gate name="G$1" symbol="OPAMP"/>
<gate name="G$2" symbol="OPAMP"/>
<gate name="G$3" symbol="PWR+-"/>
</gates>
<devices>
<device name="" package="MSOP8">
<connects>
<connect gate="G$1" pin="+IN" pad="3"/>
<connect gate="G$1" pin="-IN" pad="2"/>
<connect gate="G$1" pin="OUT" pad="1"/>
<connect gate="G$2" pin="+IN" pad="5"/>
<connect gate="G$2" pin="-IN" pad="6"/>
<connect gate="G$2" pin="OUT" pad="7"/>
<connect gate="G$3" pin="V+" pad="8"/>
<connect gate="G$3" pin="V-" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="PCA9306">
<description>Bidirectional I2C level shifter.&lt;br&gt;
NOT compatible with all available part number pinout schemes- DOUBLE CHECK!!!</description>
<gates>
<gate name="G$1" symbol="PCA9306"/>
</gates>
<devices>
<device name="" package="SO-08">
<connects>
<connect gate="G$1" pin="EN" pad="8"/>
<connect gate="G$1" pin="GND" pad="1"/>
<connect gate="G$1" pin="SCL1" pad="3"/>
<connect gate="G$1" pin="SCL2" pad="6"/>
<connect gate="G$1" pin="SDA1" pad="4"/>
<connect gate="G$1" pin="SDA2" pad="5"/>
<connect gate="G$1" pin="VREF1" pad="2"/>
<connect gate="G$1" pin="VREF2" pad="7"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MAX232" prefix="U">
<description>&lt;b&gt;RS232 Transceiver&lt;/b&gt;
SN75C3232
&lt;br&gt;
MAX[3]232</description>
<gates>
<gate name="G$1" symbol="MAX232"/>
</gates>
<devices>
<device name="" package="SO-16">
<connects>
<connect gate="G$1" pin="C1+" pad="1"/>
<connect gate="G$1" pin="C1-" pad="3"/>
<connect gate="G$1" pin="C2+" pad="4"/>
<connect gate="G$1" pin="C2-" pad="5"/>
<connect gate="G$1" pin="GND" pad="15"/>
<connect gate="G$1" pin="R1IN" pad="13"/>
<connect gate="G$1" pin="R1OUT" pad="12"/>
<connect gate="G$1" pin="R2IN" pad="8"/>
<connect gate="G$1" pin="R2OUT" pad="9"/>
<connect gate="G$1" pin="T1IN" pad="11"/>
<connect gate="G$1" pin="T1OUT" pad="14"/>
<connect gate="G$1" pin="T2IN" pad="10"/>
<connect gate="G$1" pin="T2OUT" pad="7"/>
<connect gate="G$1" pin="V+" pad="2"/>
<connect gate="G$1" pin="V-" pad="6"/>
<connect gate="G$1" pin="VCC" pad="16"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="TB6612FNG" prefix="IC">
<description>&lt;b&gt;TB6612FNG&lt;/b&gt;
&lt;p&gt;
MOS dual H-bridge motor driver, 1.2A current 3.2A peak
3 or 5v logic and 3-15v motor</description>
<gates>
<gate name="G$1" symbol="TB6612FNG"/>
</gates>
<devices>
<device name="" package="SSOP-24">
<connects>
<connect gate="G$1" pin="AIN1" pad="21"/>
<connect gate="G$1" pin="AIN2" pad="22"/>
<connect gate="G$1" pin="AO1" pad="1"/>
<connect gate="G$1" pin="AO1'" pad="2"/>
<connect gate="G$1" pin="AO2" pad="5"/>
<connect gate="G$1" pin="AO2'" pad="6"/>
<connect gate="G$1" pin="BIN1" pad="17"/>
<connect gate="G$1" pin="BIN2" pad="16"/>
<connect gate="G$1" pin="BO1" pad="11"/>
<connect gate="G$1" pin="BO1'" pad="12"/>
<connect gate="G$1" pin="BO2" pad="7"/>
<connect gate="G$1" pin="BO2'" pad="8"/>
<connect gate="G$1" pin="GND" pad="18"/>
<connect gate="G$1" pin="PGND1" pad="3"/>
<connect gate="G$1" pin="PGND1'" pad="4"/>
<connect gate="G$1" pin="PGND2" pad="9"/>
<connect gate="G$1" pin="PGND2'" pad="10"/>
<connect gate="G$1" pin="PWMA" pad="23"/>
<connect gate="G$1" pin="PWMB" pad="15"/>
<connect gate="G$1" pin="STBY" pad="19"/>
<connect gate="G$1" pin="VCC" pad="20"/>
<connect gate="G$1" pin="VM1" pad="24"/>
<connect gate="G$1" pin="VM2" pad="13"/>
<connect gate="G$1" pin="VM3" pad="14"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="NXT-CONNECTOR">
<gates>
<gate name="G$1" symbol="NXT-CONN"/>
</gates>
<devices>
<device name="" package="NXT-FOOTPRINT">
<connects>
<connect gate="G$1" pin="4V3" pad="4"/>
<connect gate="G$1" pin="9V0" pad="1"/>
<connect gate="G$1" pin="GND" pad="2 3"/>
<connect gate="G$1" pin="SCL" pad="5"/>
<connect gate="G$1" pin="SDA" pad="6"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MIC2091">
<description>&lt;b&gt;MIC2091&lt;/b&gt; &lt;br/&gt;
high side switch with overcurrent and reverse current protection</description>
<gates>
<gate name="G$1" symbol="MIC2091"/>
</gates>
<devices>
<device name="" package="SOT23-5L">
<connects>
<connect gate="G$1" pin="EN" pad="3"/>
<connect gate="G$1" pin="FAULT" pad="4"/>
<connect gate="G$1" pin="GND" pad="2"/>
<connect gate="G$1" pin="VIN" pad="1"/>
<connect gate="G$1" pin="VOUT" pad="5"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MCP4013">
<gates>
<gate name="G$1" symbol="MCP4013"/>
</gates>
<devices>
<device name="" package="SOT23-6">
<connects>
<connect gate="G$1" pin="A" pad="6"/>
<connect gate="G$1" pin="GND" pad="2"/>
<connect gate="G$1" pin="U/~D" pad="3"/>
<connect gate="G$1" pin="VDD" pad="1"/>
<connect gate="G$1" pin="W" pad="5"/>
<connect gate="G$1" pin="~CS" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="74LVC1T45">
<description>&lt;b&gt;74LVC1T45&lt;/b&gt;&lt;br /&gt;
single-bit-wide bidirectional buffer</description>
<gates>
<gate name="G$1" symbol="74LVC1T45"/>
</gates>
<devices>
<device name="" package="SC-70">
<connects>
<connect gate="G$1" pin="A" pad="P3"/>
<connect gate="G$1" pin="B" pad="P4"/>
<connect gate="G$1" pin="DIR" pad="P5"/>
<connect gate="G$1" pin="GND" pad="P2"/>
<connect gate="G$1" pin="V+A" pad="P1"/>
<connect gate="G$1" pin="V+B" pad="P6"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="RT9053">
<description>&lt;b&gt;RT9053&lt;/b&gt;&lt;br/&gt;
400mA LDO with EN and ADJ</description>
<gates>
<gate name="G$1" symbol="VREG-ADJ-EN"/>
</gates>
<devices>
<device name="" package="SOT23-5L">
<connects>
<connect gate="G$1" pin="EN" pad="3"/>
<connect gate="G$1" pin="FB" pad="4"/>
<connect gate="G$1" pin="GND" pad="2"/>
<connect gate="G$1" pin="VIN" pad="1"/>
<connect gate="G$1" pin="VOUT" pad="5"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MCP6N11">
<description>&lt;b&gt;MCP6N11&lt;/b&gt;&lt;br/&gt;Microchip Instrumentation Amplifier</description>
<gates>
<gate name="G$1" symbol="MCP6N11"/>
</gates>
<devices>
<device name="" package="SO-08">
<connects>
<connect gate="G$1" pin="EN/CAL" pad="8"/>
<connect gate="G$1" pin="GND" pad="4"/>
<connect gate="G$1" pin="VDD" pad="7"/>
<connect gate="G$1" pin="VFG" pad="1"/>
<connect gate="G$1" pin="VI+" pad="3"/>
<connect gate="G$1" pin="VI-" pad="2"/>
<connect gate="G$1" pin="VOUT" pad="6"/>
<connect gate="G$1" pin="VREF" pad="5"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="CON_HEADER_PRG_AVR_ICSP" prefix="J">
<description>2x3 AVR ICSP programming header</description>
<gates>
<gate name="J" symbol="PRG_ICSP_AVR"/>
</gates>
<devices>
<device name="" package="HEADER_PRG_2X03">
<connects>
<connect gate="J" pin="+V" pad="2"/>
<connect gate="J" pin="GND" pad="6"/>
<connect gate="J" pin="MISO" pad="1"/>
<connect gate="J" pin="MOSI" pad="4"/>
<connect gate="J" pin="RST" pad="5"/>
<connect gate="J" pin="SCK" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="XS1-U8A-FB96">
<gates>
<gate name="G$1" symbol="XS1-U8A_I/O"/>
<gate name="G$2" symbol="XS1-U8A-FB96_POWER"/>
<gate name="G$3" symbol="XS1-U8A-FB96_CONFIG/JTAG"/>
</gates>
<devices>
<device name="DEFAULT" package="BGA96">
<connects>
<connect gate="G$1" pin="ADC_IN_0" pad="A2"/>
<connect gate="G$1" pin="ADC_IN_1" pad="B2"/>
<connect gate="G$1" pin="ADC_IN_2" pad="A3"/>
<connect gate="G$1" pin="ADC_IN_3" pad="B3"/>
<connect gate="G$1" pin="ADC_VREF" pad="A1"/>
<connect gate="G$1" pin="USB_DN" pad="A6"/>
<connect gate="G$1" pin="USB_DP" pad="A5"/>
<connect gate="G$1" pin="USB_ID" pad="B7"/>
<connect gate="G$1" pin="USB_VBUS" pad="A7"/>
<connect gate="G$1" pin="X0D00" pad="A9"/>
<connect gate="G$1" pin="X0D01" pad="B9"/>
<connect gate="G$1" pin="X0D10" pad="A10"/>
<connect gate="G$1" pin="X0D11" pad="B10"/>
<connect gate="G$1" pin="X0D12" pad="A11"/>
<connect gate="G$1" pin="X0D13" pad="M12"/>
<connect gate="G$1" pin="X0D14" pad="L11"/>
<connect gate="G$1" pin="X0D15" pad="M11"/>
<connect gate="G$1" pin="X0D16" pad="L10"/>
<connect gate="G$1" pin="X0D17" pad="M10"/>
<connect gate="G$1" pin="X0D18" pad="L9"/>
<connect gate="G$1" pin="X0D19" pad="M9"/>
<connect gate="G$1" pin="X0D20" pad="L8"/>
<connect gate="G$1" pin="X0D21" pad="M8"/>
<connect gate="G$1" pin="X0D22" pad="L7"/>
<connect gate="G$1" pin="X0D24" pad="B8"/>
<connect gate="G$1" pin="X0D35" pad="A8"/>
<connect gate="G$1" pin="X0D43/WAKE" pad="G1"/>
<connect gate="G$1" pin="X0D49" pad="A12"/>
<connect gate="G$1" pin="X0D50" pad="B11"/>
<connect gate="G$1" pin="X0D51" pad="B12"/>
<connect gate="G$1" pin="X0D52" pad="C11"/>
<connect gate="G$1" pin="X0D53" pad="C12"/>
<connect gate="G$1" pin="X0D54" pad="D11"/>
<connect gate="G$1" pin="X0D55" pad="D12"/>
<connect gate="G$1" pin="X0D56" pad="E11"/>
<connect gate="G$1" pin="X0D57" pad="E12"/>
<connect gate="G$1" pin="X0D58" pad="F11"/>
<connect gate="G$1" pin="X0D61" pad="F12"/>
<connect gate="G$1" pin="X0D62" pad="G11"/>
<connect gate="G$1" pin="X0D63" pad="G12"/>
<connect gate="G$1" pin="X0D64" pad="H11"/>
<connect gate="G$1" pin="X0D65" pad="H12"/>
<connect gate="G$1" pin="X0D66" pad="J11"/>
<connect gate="G$1" pin="X0D67" pad="J12"/>
<connect gate="G$1" pin="X0D68" pad="K11"/>
<connect gate="G$1" pin="X0D69" pad="K12"/>
<connect gate="G$1" pin="X0D70" pad="L12"/>
<connect gate="G$2" pin="PGND" pad="L1 L2 M3"/>
<connect gate="G$2" pin="SW1" pad="J1 J2"/>
<connect gate="G$2" pin="SW2" pad="M5"/>
<connect gate="G$2" pin="VDD1V8" pad="M4"/>
<connect gate="G$2" pin="VDDCORE" pad="K1 K2"/>
<connect gate="G$2" pin="VDDIO" pad="L6 M6 M7"/>
<connect gate="G$2" pin="VSS" pad="E5 E6 E7 E8 F5 F6 F7 F8 G5 G6 G7 G8 H5 H6 H7 H8"/>
<connect gate="G$2" pin="VSUP" pad="H1 M1 M2"/>
<connect gate="G$3" pin="DEBUG_N" pad="E2"/>
<connect gate="G$3" pin="MODE_0" pad="L5"/>
<connect gate="G$3" pin="MODE_1" pad="L4"/>
<connect gate="G$3" pin="MODE_2" pad="B5"/>
<connect gate="G$3" pin="MODE_3" pad="B6"/>
<connect gate="G$3" pin="NC" pad="A4 B4 G2 H2 L3"/>
<connect gate="G$3" pin="OSC_EXT_N" pad="F2"/>
<connect gate="G$3" pin="RST_N" pad="C2"/>
<connect gate="G$3" pin="TCK" pad="C1"/>
<connect gate="G$3" pin="TDI" pad="D2"/>
<connect gate="G$3" pin="TDO" pad="B1"/>
<connect gate="G$3" pin="TMS" pad="D1"/>
<connect gate="G$3" pin="XI/CLK" pad="E1"/>
<connect gate="G$3" pin="XO" pad="F1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="0.33MM" package="BGA96_0.33MM">
<connects>
<connect gate="G$1" pin="ADC_IN_0" pad="A2"/>
<connect gate="G$1" pin="ADC_IN_1" pad="B2"/>
<connect gate="G$1" pin="ADC_IN_2" pad="A3"/>
<connect gate="G$1" pin="ADC_IN_3" pad="B3"/>
<connect gate="G$1" pin="ADC_VREF" pad="A1"/>
<connect gate="G$1" pin="USB_DN" pad="A6"/>
<connect gate="G$1" pin="USB_DP" pad="A5"/>
<connect gate="G$1" pin="USB_ID" pad="B7"/>
<connect gate="G$1" pin="USB_VBUS" pad="A7"/>
<connect gate="G$1" pin="X0D00" pad="A9"/>
<connect gate="G$1" pin="X0D01" pad="B9"/>
<connect gate="G$1" pin="X0D10" pad="A10"/>
<connect gate="G$1" pin="X0D11" pad="B10"/>
<connect gate="G$1" pin="X0D12" pad="A11"/>
<connect gate="G$1" pin="X0D13" pad="M12"/>
<connect gate="G$1" pin="X0D14" pad="L11"/>
<connect gate="G$1" pin="X0D15" pad="M11"/>
<connect gate="G$1" pin="X0D16" pad="L10"/>
<connect gate="G$1" pin="X0D17" pad="M10"/>
<connect gate="G$1" pin="X0D18" pad="L9"/>
<connect gate="G$1" pin="X0D19" pad="M9"/>
<connect gate="G$1" pin="X0D20" pad="L8"/>
<connect gate="G$1" pin="X0D21" pad="M8"/>
<connect gate="G$1" pin="X0D22" pad="L7"/>
<connect gate="G$1" pin="X0D24" pad="B8"/>
<connect gate="G$1" pin="X0D35" pad="A8"/>
<connect gate="G$1" pin="X0D43/WAKE" pad="G1"/>
<connect gate="G$1" pin="X0D49" pad="A12"/>
<connect gate="G$1" pin="X0D50" pad="B11"/>
<connect gate="G$1" pin="X0D51" pad="B12"/>
<connect gate="G$1" pin="X0D52" pad="C11"/>
<connect gate="G$1" pin="X0D53" pad="C12"/>
<connect gate="G$1" pin="X0D54" pad="D11"/>
<connect gate="G$1" pin="X0D55" pad="D12"/>
<connect gate="G$1" pin="X0D56" pad="E11"/>
<connect gate="G$1" pin="X0D57" pad="E12"/>
<connect gate="G$1" pin="X0D58" pad="F11"/>
<connect gate="G$1" pin="X0D61" pad="F12"/>
<connect gate="G$1" pin="X0D62" pad="G11"/>
<connect gate="G$1" pin="X0D63" pad="G12"/>
<connect gate="G$1" pin="X0D64" pad="H11"/>
<connect gate="G$1" pin="X0D65" pad="H12"/>
<connect gate="G$1" pin="X0D66" pad="J11"/>
<connect gate="G$1" pin="X0D67" pad="J12"/>
<connect gate="G$1" pin="X0D68" pad="K11"/>
<connect gate="G$1" pin="X0D69" pad="K12"/>
<connect gate="G$1" pin="X0D70" pad="L12"/>
<connect gate="G$2" pin="PGND" pad="L1 L2 M3"/>
<connect gate="G$2" pin="SW1" pad="J1 J2"/>
<connect gate="G$2" pin="SW2" pad="M5"/>
<connect gate="G$2" pin="VDD1V8" pad="M4"/>
<connect gate="G$2" pin="VDDCORE" pad="K1 K2"/>
<connect gate="G$2" pin="VDDIO" pad="L6 M6 M7"/>
<connect gate="G$2" pin="VSS" pad="E5 E6 E7 E8 F5 F6 F7 F8 G5 G6 G7 G8 H5 H6 H7 H8"/>
<connect gate="G$2" pin="VSUP" pad="H1 M1 M2"/>
<connect gate="G$3" pin="DEBUG_N" pad="E2"/>
<connect gate="G$3" pin="MODE_0" pad="L5"/>
<connect gate="G$3" pin="MODE_1" pad="L4"/>
<connect gate="G$3" pin="MODE_2" pad="B5"/>
<connect gate="G$3" pin="MODE_3" pad="B6"/>
<connect gate="G$3" pin="NC" pad="A4 B4 G2 H2 L3"/>
<connect gate="G$3" pin="OSC_EXT_N" pad="F2"/>
<connect gate="G$3" pin="RST_N" pad="C2"/>
<connect gate="G$3" pin="TCK" pad="C1"/>
<connect gate="G$3" pin="TDI" pad="D2"/>
<connect gate="G$3" pin="TDO" pad="B1"/>
<connect gate="G$3" pin="TMS" pad="D1"/>
<connect gate="G$3" pin="XI/CLK" pad="E1"/>
<connect gate="G$3" pin="XO" pad="F1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ATTINYX61">
<gates>
<gate name="G$1" symbol="ATTINY261"/>
</gates>
<devices>
<device name="" package="SO-20">
<connects>
<connect gate="G$1" pin="AGND" pad="16"/>
<connect gate="G$1" pin="AVCC" pad="15"/>
<connect gate="G$1" pin="GND" pad="6"/>
<connect gate="G$1" pin="PA0" pad="20"/>
<connect gate="G$1" pin="PA1" pad="19"/>
<connect gate="G$1" pin="PA2" pad="18"/>
<connect gate="G$1" pin="PA3" pad="17"/>
<connect gate="G$1" pin="PA4" pad="14"/>
<connect gate="G$1" pin="PA5" pad="13"/>
<connect gate="G$1" pin="PA6" pad="12"/>
<connect gate="G$1" pin="PA7" pad="11"/>
<connect gate="G$1" pin="PB0" pad="1"/>
<connect gate="G$1" pin="PB1" pad="2"/>
<connect gate="G$1" pin="PB2" pad="3"/>
<connect gate="G$1" pin="PB3" pad="4"/>
<connect gate="G$1" pin="PB4" pad="7"/>
<connect gate="G$1" pin="PB5" pad="8"/>
<connect gate="G$1" pin="PB6" pad="9"/>
<connect gate="G$1" pin="PB7" pad="10"/>
<connect gate="G$1" pin="VCC" pad="5"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="TPD2E001">
<description>&lt;b&gt;TPD2E001&lt;br/&gt;&lt;a href="http://www.ti.com/lit/ds/symlink/tpd2e001.pdf"&gt;datasheet&lt;/a&gt;</description>
<gates>
<gate name="G$1" symbol="TPD2E001"/>
</gates>
<devices>
<device name="" package="R-PDSO-N5">
<connects>
<connect gate="G$1" pin="GND" pad="4"/>
<connect gate="G$1" pin="IO1" pad="3"/>
<connect gate="G$1" pin="IO2" pad="5"/>
<connect gate="G$1" pin="VCC" pad="1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="QRE1113">
<description>Reflective object sensor</description>
<gates>
<gate name="G$1" symbol="QRE1113"/>
</gates>
<devices>
<device name="" package="QRE1113">
<connects>
<connect gate="G$1" pin="A" pad="1"/>
<connect gate="G$1" pin="C" pad="3"/>
<connect gate="G$1" pin="E" pad="4"/>
<connect gate="G$1" pin="K" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MOSFET-P" prefix="Q" uservalue="yes">
<description>&lt;b&gt;P-FET&lt;/b&gt;</description>
<gates>
<gate name="G$1" symbol="MOSFET-P"/>
</gates>
<devices>
<device name="" package="SOT23-3">
<connects>
<connect gate="G$1" pin="D" pad="3"/>
<connect gate="G$1" pin="G" pad="1"/>
<connect gate="G$1" pin="S" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MOSFET-N" prefix="Q" uservalue="yes">
<description>&lt;b&gt;N-FET&lt;/b&gt;</description>
<gates>
<gate name="G$1" symbol="MOSFET-N"/>
</gates>
<devices>
<device name="" package="SOT23-3">
<connects>
<connect gate="G$1" pin="D" pad="3"/>
<connect gate="G$1" pin="G" pad="1"/>
<connect gate="G$1" pin="S" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="IRS218">
<description>&lt;b&gt;IRS2186/7&lt;/b&gt; FET Driver in SOIC&lt;br/&gt;
4a half-H bootstrapped FET driver</description>
<gates>
<gate name="G$1" symbol="IRS2186"/>
</gates>
<devices>
<device name="-6" package="SO-08">
<connects>
<connect gate="G$1" pin="COM" pad="3"/>
<connect gate="G$1" pin="HIN" pad="1"/>
<connect gate="G$1" pin="HO" pad="7"/>
<connect gate="G$1" pin="LIN" pad="2"/>
<connect gate="G$1" pin="LO" pad="4"/>
<connect gate="G$1" pin="VB" pad="8"/>
<connect gate="G$1" pin="VCC" pad="5"/>
<connect gate="G$1" pin="VS" pad="6"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-67" package="SO-08">
<connects>
<connect gate="G$1" pin="COM" pad="4"/>
<connect gate="G$1" pin="HIN" pad="2"/>
<connect gate="G$1" pin="HO" pad="7"/>
<connect gate="G$1" pin="LIN" pad="3"/>
<connect gate="G$1" pin="LO" pad="5"/>
<connect gate="G$1" pin="VB" pad="8"/>
<connect gate="G$1" pin="VCC" pad="1"/>
<connect gate="G$1" pin="VS" pad="6"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="PSMN">
<description>&lt;b&gt;NXP PSMN family FETs&lt;/b&gt;&lt;br/&gt;
PSMN1R0, PSMN102-200Y, etc.</description>
<gates>
<gate name="G$1" symbol="MOSFET-N-1"/>
</gates>
<devices>
<device name="" package="SO-08">
<connects>
<connect gate="G$1" pin="D" pad="5 6 7 8"/>
<connect gate="G$1" pin="G" pad="4"/>
<connect gate="G$1" pin="S" pad="1 2 3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
</devicesets>
</library>
</drawing>
</eagle>
