<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="9.1.2">
<drawing>
<board>
<plain>
<wire x1="9.525" y1="16.51" x2="9.525" y2="11.176" width="0" layer="20"/>
<wire x1="9.525" y1="5.334" x2="9.525" y2="0" width="0" layer="20"/>
<wire x1="9.525" y1="0" x2="26.035" y2="0" width="0" layer="20"/>
<wire x1="26.035" y1="0" x2="26.035" y2="5.334" width="0" layer="20"/>
<wire x1="26.035" y1="11.176" x2="26.035" y2="16.51" width="0" layer="20"/>
<wire x1="26.035" y1="16.51" x2="9.525" y2="16.51" width="0" layer="20"/>
<wire x1="9.525" y1="11.176" x2="2.794" y2="11.176" width="0" layer="20"/>
<wire x1="2.794" y1="11.176" x2="0" y2="8.255" width="0" layer="20" curve="90"/>
<wire x1="0" y1="8.255" x2="2.794" y2="5.334" width="0" layer="20" curve="90"/>
<wire x1="2.794" y1="5.334" x2="9.525" y2="5.334" width="0" layer="20"/>
<wire x1="26.035" y1="11.176" x2="32.766" y2="11.176" width="0" layer="20"/>
<wire x1="32.766" y1="11.176" x2="35.56" y2="8.255" width="0" layer="20" curve="-90"/>
<wire x1="35.56" y1="8.255" x2="32.766" y2="5.334" width="0" layer="20" curve="-90"/>
<wire x1="32.766" y1="5.334" x2="26.035" y2="5.334" width="0" layer="20"/>
<text>https://openmv.io</text>
<text>LEPTON-MOD R1</text>
<text>10/27/18</text>
</plain>
<libraries>
<library name="sfe">
<packages>
<package name="EIA3216">
</package>
<package name="0402-RES">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;&lt;p&gt;
chip</description>
</package>
<package name="1210">
</package>
</packages>
</library>
<library name="DF12">
<packages>
<package name="DF12-36-DP">
</package>
</packages>
</library>
<library name="leptonCustom">
<packages>
<package name="SOT23-5">
<description>&lt;b&gt;SOT23-5&lt;/b&gt; Zetex&lt;p&gt;
Source: http://www.zetex.com/3.0/pdf/ZXSC300.pdf</description>
</package>
<package name="CAM-SOCKET">
<description>SMIA Camera Socket
Molex 1050281001</description>
</package>
</packages>
</library>
<library name="SparkFun-Capacitors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find resistors, capacitors, inductors, test points, jumper pads, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="0402-CAP">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;&lt;p&gt;
chip</description>
</package>
<package name="0805">
</package>
</packages>
</library>
<library name="openmv">
<packages>
<package name="ROHS">
</package>
<package name="WEEE">
</package>
</packages>
</library>
<library name="testpad">
<description>&lt;b&gt;Test Pins/Pads&lt;/b&gt;&lt;p&gt;
Cream on SMD OFF.&lt;br&gt;
new: Attribute TP_SIGNAL_NAME&lt;br&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="TP16R">
<description>&lt;b&gt;TEST PAD&lt;/b&gt;</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="U$3" library="DF12" package="DF12-36-DP" value="DF12(3.0)-36DP-0.5V(86)"/>
<element name="U2" library="leptonCustom" package="SOT23-5" value="LM3670MF-1.2/NOPB">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="U4" library="leptonCustom" package="SOT23-5" value="ADP150AUJZ-2.8-R7">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C7" library="SparkFun-Capacitors" package="0805" value="10 uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C8" library="SparkFun-Capacitors" package="0402-CAP" value="1 uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C9" library="SparkFun-Capacitors" package="0402-CAP" value="1 uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C13" library="SparkFun-Capacitors" package="0805" value="10 uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C14" library="SparkFun-Capacitors" package="0402-CAP" value="0.1 uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C15" library="SparkFun-Capacitors" package="0402-CAP" value="0.1 uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C16" library="SparkFun-Capacitors" package="0402-CAP" value="0.1 uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="U5" library="leptonCustom" package="CAM-SOCKET" value="1050281001">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C18" library="SparkFun-Capacitors" package="0402-CAP" value="1 uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C19" library="sfe" package="EIA3216" value="47uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R2" library="sfe" package="0402-RES" value="10K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R1" library="sfe" package="0402-RES" value="10K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="U$5" library="openmv" package="ROHS" value=""/>
<element name="U$4" library="openmv" package="WEEE" value=""/>
<element name="L1" library="sfe" package="1210" value="10uH">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="CLK" library="testpad" package="TP16R" value="TPTP16R">
<attribute name="NAME"/>
<attribute name="TP_SIGNAL_NAME" value=""/>
<attribute name="VALUE"/>
</element>
<element name="SSEL" library="testpad" package="TP16R" value="TPTP16R">
<attribute name="NAME"/>
<attribute name="TP_SIGNAL_NAME" value=""/>
<attribute name="VALUE"/>
</element>
<element name="SCLK" library="testpad" package="TP16R" value="TPTP16R">
<attribute name="NAME"/>
<attribute name="TP_SIGNAL_NAME" value=""/>
<attribute name="VALUE"/>
</element>
<element name="MISO" library="testpad" package="TP16R" value="TPTP16R">
<attribute name="NAME"/>
<attribute name="TP_SIGNAL_NAME" value=""/>
<attribute name="VALUE"/>
</element>
<element name="MOSI" library="testpad" package="TP16R" value="TPTP16R">
<attribute name="NAME"/>
<attribute name="TP_SIGNAL_NAME" value=""/>
<attribute name="VALUE"/>
</element>
</elements>
<signals>
<signal name="GND">
<contactref element="U$3" pad="19"/>
<contactref element="U$3" pad="27"/>
<contactref element="U$3" pad="5"/>
<contactref element="U5" pad="P$32"/>
<contactref element="U5" pad="P$35"/>
<contactref element="U5" pad="P$36"/>
<contactref element="U5" pad="P$7"/>
<contactref element="U5" pad="P$24"/>
<contactref element="U5" pad="1"/>
<contactref element="U5" pad="P$8"/>
<contactref element="U5" pad="P$19"/>
<contactref element="U5" pad="P$11"/>
<contactref element="U5" pad="P$10"/>
<contactref element="U5" pad="P$30"/>
<contactref element="U5" pad="P$14"/>
<contactref element="U5" pad="P$1"/>
<contactref element="U5" pad="P$29"/>
<contactref element="U5" pad="P$31"/>
<contactref element="U5" pad="P$5"/>
<contactref element="U5" pad="P$17"/>
<contactref element="U5" pad="P$28"/>
<contactref element="U5" pad="P$26"/>
<contactref element="U5" pad="P$16"/>
<contactref element="U5" pad="P$9"/>
<contactref element="U5" pad="P$21"/>
<contactref element="U5" pad="P$15"/>
<contactref element="U5" pad="P$34"/>
<contactref element="U5" pad="P$12"/>
<contactref element="U5" pad="P$33"/>
<contactref element="U5" pad="P$22"/>
<contactref element="U5" pad="P$25"/>
<contactref element="U5" pad="P$13"/>
<contactref element="U5" pad="P$2"/>
<contactref element="U5" pad="P$27"/>
<contactref element="U5" pad="P$3"/>
<contactref element="U5" pad="P$23"/>
<contactref element="U5" pad="P$4"/>
<contactref element="U5" pad="P$20"/>
<contactref element="U5" pad="P$18"/>
<contactref element="U5" pad="P$6"/>
<contactref element="U5" pad="6"/>
<contactref element="U5" pad="8"/>
<contactref element="U5" pad="9"/>
<contactref element="U5" pad="10"/>
<contactref element="U5" pad="15"/>
<contactref element="U5" pad="18"/>
<contactref element="U5" pad="20"/>
<contactref element="U5" pad="25"/>
<contactref element="U5" pad="27"/>
<contactref element="U5" pad="30"/>
<contactref element="C7" pad="2"/>
<contactref element="C13" pad="2"/>
<contactref element="C8" pad="2"/>
<contactref element="C9" pad="2"/>
<contactref element="C16" pad="2"/>
<contactref element="C14" pad="2"/>
<contactref element="C18" pad="2"/>
<contactref element="U4" pad="2"/>
<contactref element="U2" pad="2"/>
<contactref element="C19" pad="C"/>
<contactref element="C15" pad="2"/>
</signal>
<signal name="VCC">
<contactref element="U$3" pad="2"/>
<contactref element="U$3" pad="10"/>
<contactref element="U$3" pad="20"/>
<contactref element="U$3" pad="30"/>
<contactref element="U$3" pad="36"/>
<contactref element="U2" pad="1"/>
<contactref element="C19" pad="A"/>
<contactref element="R2" pad="2"/>
<contactref element="R1" pad="2"/>
<contactref element="C8" pad="1"/>
<contactref element="U4" pad="1"/>
<contactref element="U4" pad="3"/>
<contactref element="C7" pad="1"/>
<contactref element="U2" pad="3"/>
</signal>
<signal name="DCMI_D0">
<contactref element="U$3" pad="31"/>
</signal>
<signal name="DCMI_D1">
<contactref element="U$3" pad="29"/>
</signal>
<signal name="DCMI_PCLK">
<contactref element="U$3" pad="14"/>
</signal>
<signal name="DCMI_HSYNC">
<contactref element="U$3" pad="18"/>
</signal>
<signal name="DCMI_VSYNC">
<contactref element="U$3" pad="16"/>
<contactref element="U5" pad="2"/>
</signal>
<signal name="DCMI_CLK">
<contactref element="U$3" pad="12"/>
<contactref element="U5" pad="26"/>
<contactref element="CLK" pad="TP"/>
</signal>
<signal name="DCMI_RST">
<contactref element="U$3" pad="21"/>
<contactref element="U5" pad="24"/>
<contactref element="C18" pad="1"/>
<contactref element="R1" pad="1"/>
</signal>
<signal name="DCMI_PWDN">
<contactref element="U$3" pad="25"/>
<contactref element="U5" pad="23"/>
<contactref element="R2" pad="1"/>
</signal>
<signal name="DCMI_D2">
<contactref element="U$3" pad="35"/>
</signal>
<signal name="DCMI_D3">
<contactref element="U$3" pad="28"/>
</signal>
<signal name="DCMI_D4">
<contactref element="U$3" pad="26"/>
</signal>
<signal name="DCMI_D5">
<contactref element="U$3" pad="33"/>
</signal>
<signal name="DCMI_D6">
<contactref element="U$3" pad="24"/>
</signal>
<signal name="DCMI_D7">
<contactref element="U$3" pad="22"/>
</signal>
<signal name="I2C1_SCL">
<contactref element="U$3" pad="32"/>
<contactref element="U5" pad="21"/>
</signal>
<signal name="I2C1_SDA">
<contactref element="U$3" pad="34"/>
<contactref element="U5" pad="22"/>
</signal>
<signal name="N$2">
</signal>
<signal name="N$4">
</signal>
<signal name="DCMI_FSIN">
<contactref element="U$3" pad="23"/>
</signal>
<signal name="SPI3_SCLK">
<contactref element="U$3" pad="13"/>
<contactref element="U5" pad="13"/>
<contactref element="SCLK" pad="TP"/>
</signal>
<signal name="SPI3_MISO">
<contactref element="U$3" pad="15"/>
<contactref element="U5" pad="12"/>
<contactref element="MISO" pad="TP"/>
</signal>
<signal name="SPI3_MOSI">
<contactref element="U$3" pad="17"/>
<contactref element="U5" pad="11"/>
<contactref element="MOSI" pad="TP"/>
</signal>
<signal name="SPI3_SSEL">
<contactref element="U$3" pad="11"/>
<contactref element="U5" pad="14"/>
<contactref element="SSEL" pad="TP"/>
</signal>
<signal name="VDDA">
<contactref element="U$3" pad="4"/>
</signal>
<signal name="RSVD1">
<contactref element="U$3" pad="1"/>
</signal>
<signal name="RSVD2">
<contactref element="U$3" pad="3"/>
</signal>
<signal name="RSVD5">
<contactref element="U$3" pad="6"/>
</signal>
<signal name="RSVD6">
<contactref element="U$3" pad="8"/>
</signal>
<signal name="RSVD3">
<contactref element="U$3" pad="7"/>
</signal>
<signal name="RSVD4">
<contactref element="U$3" pad="9"/>
</signal>
<signal name="GPIO2">
<contactref element="U5" pad="3"/>
</signal>
<signal name="GPIO1">
<contactref element="U5" pad="4"/>
</signal>
<signal name="GPIO0">
<contactref element="U5" pad="5"/>
</signal>
<signal name="MIPI_CLK_N">
<contactref element="U5" pad="28"/>
</signal>
<signal name="MIPI_CLK_P">
<contactref element="U5" pad="29"/>
</signal>
<signal name="MIPI_DATA_N">
<contactref element="U5" pad="31"/>
</signal>
<signal name="MIPI_DATA_P">
<contactref element="U5" pad="32"/>
</signal>
<signal name="2V8">
<contactref element="C14" pad="1"/>
<contactref element="U5" pad="19"/>
<contactref element="U4" pad="5"/>
<contactref element="C9" pad="1"/>
<contactref element="C15" pad="1"/>
<contactref element="U5" pad="16"/>
</signal>
<signal name="1V2">
<contactref element="U2" pad="4"/>
<contactref element="C13" pad="1"/>
<contactref element="U5" pad="7"/>
<contactref element="C16" pad="1"/>
<contactref element="L1" pad="2"/>
</signal>
<signal name="N$1">
<contactref element="U2" pad="5"/>
<contactref element="L1" pad="1"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
