<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="9.2.2">
<drawing>
<board>
<plain>
<wire x1="0" y1="16.51" x2="0" y2="11.176" width="0" layer="20"/>
<wire x1="0" y1="5.334" x2="0" y2="0" width="0" layer="20"/>
<wire x1="0" y1="0" x2="16.51" y2="0" width="0" layer="20"/>
<wire x1="16.51" y1="0" x2="16.51" y2="5.334" width="0" layer="20"/>
<wire x1="16.51" y1="11.176" x2="16.51" y2="16.51" width="0" layer="20"/>
<wire x1="16.51" y1="16.51" x2="0" y2="16.51" width="0" layer="20"/>
<text>https://openmv.io</text>
<text>OV2640-MOD R1</text>
<text>2019/5/1</text>
<wire x1="0" y1="11.176" x2="-6.731" y2="11.176" width="0" layer="20"/>
<wire x1="-6.731" y1="11.176" x2="-9.525" y2="8.255" width="0" layer="20" curve="90"/>
<wire x1="-9.525" y1="8.255" x2="-6.731" y2="5.334" width="0" layer="20" curve="90"/>
<wire x1="-6.731" y1="5.334" x2="0" y2="5.334" width="0" layer="20"/>
<wire x1="16.51" y1="11.176" x2="23.241" y2="11.176" width="0" layer="20"/>
<wire x1="23.241" y1="11.176" x2="26.035" y2="8.255" width="0" layer="20" curve="-90"/>
<wire x1="26.035" y1="8.255" x2="23.241" y2="5.334" width="0" layer="20" curve="-90"/>
<wire x1="23.241" y1="5.334" x2="16.51" y2="5.334" width="0" layer="20"/>
</plain>
<libraries>
<library name="sfe">
<packages>
<package name="EIA3216">
</package>
<package name="0402-CAP">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;&lt;p&gt;
chip</description>
</package>
</packages>
</library>
<library name="omnivision">
<description>&lt;b&gt;OmniVision Technologies, Inc.&lt;/b&gt;&lt;p&gt;
www.ovt.com&lt;br&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="LENSMOUNT-20MM">
</package>
<package name="CSP2">
</package>
</packages>
</library>
<library name="openmv">
<packages>
<package name="WEEE">
</package>
<package name="ROHS">
</package>
<package name="OMV-LOGO-SMALL">
</package>
</packages>
</library>
<library name="DF12">
<packages>
<package name="DF12-36-DP">
</package>
</packages>
</library>
<library name="heka">
<packages>
<package name="0402-CAP">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;&lt;p&gt;
chip</description>
</package>
</packages>
</library>
<library name="leptonCustom">
<packages>
<package name="SOT23-5">
<description>&lt;b&gt;SOT23-5&lt;/b&gt; Zetex&lt;p&gt;
Source: http://www.zetex.com/3.0/pdf/ZXSC300.pdf</description>
</package>
</packages>
</library>
<library name="SparkFun-Capacitors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find resistors, capacitors, inductors, test points, jumper pads, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="0402-CAP">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;&lt;p&gt;
chip</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="LM1" library="omnivision" package="LENSMOUNT-20MM" value="LENSMOUNT20MM"/>
<element name="U$1" library="openmv" package="WEEE" value=""/>
<element name="U$2" library="openmv" package="ROHS" value=""/>
<element name="U$4" library="openmv" package="OMV-LOGO-SMALL" value=""/>
<element name="U$3" library="DF12" package="DF12-36-DP" value="DF12-36-DP">
<attribute name="NAME"/>
</element>
<element name="U9" library="omnivision" package="CSP2" value="OV2640">
<attribute name="NAME"/>
</element>
<element name="C9" library="sfe" package="0402-CAP" value="0.1uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C8" library="sfe" package="0402-CAP" value="0.1uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C6" library="sfe" package="0402-CAP" value="0.1uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="U6" library="heka" package="0402-CAP" value="BEAD">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C4" library="sfe" package="0402-CAP" value="4.7uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C5" library="sfe" package="0402-CAP" value="0.1uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C7" library="sfe" package="0402-CAP" value="4.7uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="U4" library="leptonCustom" package="SOT23-5" value="ADP150AUJZ-2.8-R7">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C2" library="SparkFun-Capacitors" package="0402-CAP" value="1 uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C3" library="SparkFun-Capacitors" package="0402-CAP" value="1 uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C1" library="sfe" package="EIA3216" value="47uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
</elements>
<signals>
<signal name="GND">
<contactref element="U$3" pad="19"/>
<contactref element="U$3" pad="5"/>
<contactref element="U9" pad="A3"/>
<contactref element="U9" pad="A1"/>
<contactref element="U9" pad="G2"/>
<contactref element="U9" pad="E6"/>
<contactref element="U9" pad="A4"/>
<contactref element="U9" pad="E4"/>
<contactref element="C9" pad="2"/>
<contactref element="C8" pad="2"/>
<contactref element="C6" pad="2"/>
<contactref element="C4" pad="2"/>
<contactref element="C5" pad="2"/>
<contactref element="U9" pad="B2"/>
<contactref element="U9" pad="A2"/>
<contactref element="C7" pad="2"/>
<contactref element="U4" pad="2"/>
<contactref element="C2" pad="2"/>
<contactref element="C3" pad="2"/>
<contactref element="C1" pad="C"/>
</signal>
<signal name="VCC">
<contactref element="U$3" pad="2"/>
<contactref element="U$3" pad="10"/>
<contactref element="U$3" pad="20"/>
<contactref element="U$3" pad="30"/>
<contactref element="U$3" pad="36"/>
<contactref element="C1" pad="A"/>
<contactref element="C2" pad="1"/>
<contactref element="U4" pad="1"/>
<contactref element="U4" pad="3"/>
</signal>
<signal name="DCMI_D0">
<contactref element="U$3" pad="31"/>
<contactref element="U9" pad="F3"/>
</signal>
<signal name="DCMI_D1">
<contactref element="U$3" pad="29"/>
<contactref element="U9" pad="G3"/>
</signal>
<signal name="DCMI_PCLK">
<contactref element="U$3" pad="14"/>
<contactref element="U9" pad="E3"/>
</signal>
<signal name="DCMI_HSYNC">
<contactref element="U$3" pad="18"/>
<contactref element="U9" pad="C3"/>
</signal>
<signal name="DCMI_VSYNC">
<contactref element="U$3" pad="16"/>
<contactref element="U9" pad="D2"/>
</signal>
<signal name="DCMI_CLK">
<contactref element="U$3" pad="12"/>
<contactref element="U9" pad="C4"/>
</signal>
<signal name="DCMI_RST">
<contactref element="U$3" pad="21"/>
<contactref element="U9" pad="C6"/>
</signal>
<signal name="DCMI_PWDN">
<contactref element="U$3" pad="25"/>
<contactref element="U9" pad="B6"/>
</signal>
<signal name="DCMI_D2">
<contactref element="U$3" pad="35"/>
<contactref element="U9" pad="F4"/>
</signal>
<signal name="DCMI_D3">
<contactref element="U$3" pad="28"/>
<contactref element="U9" pad="G4"/>
</signal>
<signal name="DCMI_D4">
<contactref element="U$3" pad="26"/>
<contactref element="U9" pad="E5"/>
</signal>
<signal name="DCMI_D5">
<contactref element="U$3" pad="33"/>
<contactref element="U9" pad="G5"/>
</signal>
<signal name="DCMI_D6">
<contactref element="U$3" pad="24"/>
<contactref element="U9" pad="F5"/>
</signal>
<signal name="DCMI_D7">
<contactref element="U$3" pad="22"/>
<contactref element="U9" pad="G6"/>
</signal>
<signal name="I2C1_SCL">
<contactref element="U$3" pad="32"/>
<contactref element="U9" pad="C2"/>
</signal>
<signal name="I2C1_SDA">
<contactref element="U$3" pad="34"/>
<contactref element="U9" pad="C1"/>
</signal>
<signal name="N$2">
</signal>
<signal name="N$4">
</signal>
<signal name="DCMI_FSIN">
<contactref element="U$3" pad="23"/>
</signal>
<signal name="SPI3_SCLK">
<contactref element="U$3" pad="13"/>
</signal>
<signal name="SPI3_MISO">
<contactref element="U$3" pad="15"/>
</signal>
<signal name="SPI3_MOSI">
<contactref element="U$3" pad="17"/>
</signal>
<signal name="SPI3_SSEL">
<contactref element="U$3" pad="11"/>
</signal>
<signal name="VDDA">
<contactref element="U$3" pad="4"/>
</signal>
<signal name="RSVD1">
<contactref element="U$3" pad="1"/>
</signal>
<signal name="RSVD2">
<contactref element="U$3" pad="3"/>
</signal>
<signal name="RSVD5">
<contactref element="U$3" pad="6"/>
</signal>
<signal name="RSVD6">
<contactref element="U$3" pad="8"/>
</signal>
<signal name="RSVD3">
<contactref element="U$3" pad="7"/>
</signal>
<signal name="RSVD4">
<contactref element="U$3" pad="9"/>
</signal>
<signal name="N$5">
<contactref element="C8" pad="1"/>
<contactref element="U9" pad="C5"/>
</signal>
<signal name="N$6">
<contactref element="U9" pad="A5"/>
<contactref element="C9" pad="1"/>
</signal>
<signal name="2.8V">
<contactref element="U6" pad="2"/>
<contactref element="C4" pad="1"/>
<contactref element="U9" pad="B1"/>
<contactref element="U9" pad="F1"/>
<contactref element="C5" pad="1"/>
<contactref element="U9" pad="G1"/>
</signal>
<signal name="N$7">
<contactref element="U9" pad="F6"/>
<contactref element="U9" pad="F2"/>
<contactref element="C7" pad="1"/>
</signal>
<signal name="N$13">
<contactref element="U9" pad="B4"/>
<contactref element="U9" pad="B5"/>
<contactref element="U6" pad="1"/>
<contactref element="C6" pad="1"/>
<contactref element="U9" pad="B3"/>
</signal>
<signal name="2V8">
<contactref element="U4" pad="5"/>
<contactref element="C3" pad="1"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
