<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="7.2.0">
<drawing>
<board>
<plain>
<wire x1="11.1575" y1="16.3245" x2="60.69" y2="16.3245" width="0" layer="20"/>
<wire x1="60.69" y1="16.3245" x2="60.69" y2="53.745" width="0" layer="20"/>
<wire x1="60.69" y1="53.745" x2="11.1575" y2="53.745" width="0" layer="20"/>
<wire x1="11.1575" y1="53.745" x2="11.1575" y2="16.3245" width="0" layer="20"/>
<text>RESET</text>
<text>D3</text>
<text>D4</text>
<text>D0</text>
<text>D1</text>
<text>D2</text>
<text>GND</text>
<text>VCC</text>
<text>Dimitris Platis</text>
<text>dimitris@platis.solutions</text>
<text>VCC</text>
<text>GND</text>
<text>1</text>
<text>Dimitris Platis</text>
<text>dimitris@platis.solutions</text>
<text>Website: platis.solutions
Tel: 7777777785555
GitHub: platisd</text>
<hole x="14.224" y="19.304" drill="2.8"/>
<hole x="57.912" y="19.304" drill="2.8"/>
<text>ATtiny85</text>
<text>VCC</text>
<text>GND</text>
</plain>
<libraries>
<library name="SparkFun-DigitalIC">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find all manner of digital ICs- microcontrollers, memory chips, logic chips, FPGAs, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="SO08-EIAJ">
<description>Fits EIAJ packages (wide version of the SOIC-8).</description>
</package>
</packages>
</library>
<library name="pinhead">
<description>&lt;b&gt;Pin Header Connectors&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="1X02">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
</package>
<package name="1X04">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
</package>
<package name="1X07">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
</package>
<package name="2X03">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="U1" library="SparkFun-DigitalIC" package="SO08-EIAJ" value="Tiny85-20-SMT">
<attribute name="PROD_ID" value="IC-09092"/>
<attribute name="VALUE"/>
</element>
<element name="SV2" library="pinhead" package="1X04" value="">
<attribute name="VALUE"/>
</element>
<element name="SV3" library="pinhead" package="1X04" value="">
<attribute name="VALUE"/>
</element>
<element name="ICSP" library="pinhead" package="2X03" value=""/>
<element name="JP1" library="pinhead" package="1X02" value="">
<attribute name="VALUE"/>
</element>
<element name="JP3" library="pinhead" package="1X07" value="">
<attribute name="VALUE"/>
</element>
<element name="JP4" library="pinhead" package="1X07" value="">
<attribute name="VALUE"/>
</element>
<element name="JP5" library="pinhead" package="1X07" value="">
<attribute name="VALUE"/>
</element>
</elements>
<signals>
<signal name="N$1">
</signal>
<signal name="MISO">
<contactref element="U1" pad="6"/>
<contactref element="SV3" pad="2"/>
<contactref element="ICSP" pad="1"/>
</signal>
<signal name="VCC">
<contactref element="U1" pad="8"/>
<contactref element="SV3" pad="4"/>
<contactref element="JP1" pad="1"/>
<contactref element="ICSP" pad="2"/>
<contactref element="JP3" pad="7"/>
<contactref element="JP4" pad="7"/>
<contactref element="JP5" pad="7"/>
</signal>
<signal name="GND">
<contactref element="U1" pad="4"/>
<contactref element="SV2" pad="4"/>
<contactref element="JP1" pad="2"/>
<contactref element="ICSP" pad="6"/>
<contactref element="JP5" pad="1"/>
<contactref element="JP4" pad="1"/>
<contactref element="JP3" pad="1"/>
</signal>
<signal name="MOSI">
<contactref element="U1" pad="5"/>
<contactref element="SV3" pad="1"/>
<contactref element="ICSP" pad="4"/>
</signal>
<signal name="SCK">
<contactref element="U1" pad="7"/>
<contactref element="SV3" pad="3"/>
<contactref element="ICSP" pad="3"/>
</signal>
<signal name="RESET">
<contactref element="U1" pad="1"/>
<contactref element="SV2" pad="1"/>
<contactref element="ICSP" pad="5"/>
</signal>
<signal name="N$9">
<contactref element="U1" pad="2"/>
<contactref element="SV2" pad="2"/>
</signal>
<signal name="N$8">
<contactref element="U1" pad="3"/>
<contactref element="SV2" pad="3"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
