<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="7.2.0">
<drawing>
<board>
<plain>
<wire x1="0" y1="1" x2="1" y2="0" width="0" layer="20"/>
<wire x1="1" y1="0" x2="41.3" y2="0" width="0" layer="20"/>
<wire x1="41.3" y1="0" x2="42.3" y2="1" width="0" layer="20"/>
<wire x1="42.3" y1="1" x2="42.3" y2="26.4" width="0" layer="20"/>
<wire x1="42.3" y1="26.4" x2="41.3" y2="27.4" width="0" layer="20"/>
<wire x1="41.3" y1="27.4" x2="1" y2="27.4" width="0" layer="20"/>
<wire x1="1" y1="27.4" x2="0" y2="26.4" width="0" layer="20"/>
<wire x1="0" y1="26.4" x2="0" y2="1" width="0" layer="20"/>
<text>+</text>
<text>-</text>
</plain>
<libraries>
<library name="microbuilder">
<description>&lt;h2&gt;&lt;b&gt;microBuilder.eu&lt;/b&gt; Eagle Footprint Library&lt;/h2&gt;

&lt;p&gt;Footprints for common components used in our projects and products.  This is the same library that we use internally, and it is regularly updated.  The newest version can always be found at &lt;b&gt;www.microBuilder.eu&lt;/b&gt;.  If you find this library useful, please feel free to purchase something from our online store. Please also note that all holes are optimised for metric drill bits!&lt;/p&gt;

&lt;h3&gt;Obligatory Warning&lt;/h3&gt;
&lt;p&gt;While it probably goes without saying, there are no guarantees that the footprints or schematic symbols in this library are flawless, and we make no promises of fitness for production, prototyping or any other purpose. These libraries are provided for information puposes only, and are used at your own discretion.  While we make every effort to produce accurate footprints, and many of the items found in this library have be proven in production, we can't make any promises of suitability for a specific purpose. If you do find any errors, though, please feel free to contact us at www.microbuilder.eu to let us know about it so that we can update the library accordingly!&lt;/p&gt;

&lt;h3&gt;License&lt;/h3&gt;
&lt;p&gt;This work is placed in the public domain, and may be freely used for commercial and non-commercial work with the following conditions:&lt;/p&gt;
&lt;p&gt;THIS SOFTWARE IS PROVIDED ''AS IS'' AND ANY EXPRESS OR IMPLIED WARRANTIES, INCLUDING, BUT NOT LIMITED TO, THE IMPLIED WARRANTIES OF MERCHANTABILITY AND FITNESS FOR A PARTICULAR PURPOSE ARE DISCLAIMED.  IN NO EVENT SHALL THE INSTITUTE OR CONTRIBUTORS BE LIABLE FOR ANY DIRECT, INDIRECT, INCIDENTAL, SPECIAL, EXEMPLARY, OR CONSEQUENTIAL DAMAGES (INCLUDING,  BUT NOT LIMITED TO, PROCUREMENT OF SUBSTITUTE GOODS OR SERVICES; LOSS OF USE, DATA, OR PROFITS; OR BUSINESS INTERRUPTION) HOWEVER CAUSED AND ON ANY THEORY OF LIABILITY, WHETHER IN CONTRACT, STRICT LIABILITY, OR TORT (INCLUDING NEGLIGENCE OR OTHERWISE) ARISING IN ANY WAY OUT OF THE USE OF THIS SOFTWARE, EVEN IF ADVISED OF THE POSSIBILITY OF SUCH DAMAGE.
&lt;/p&gt;</description>
<packages>
<package name="LQFP48">
</package>
</packages>
</library>
<library name="rcl">
<packages>
<package name="C1206">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;</description>
</package>
<package name="R1206">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;</description>
</package>
<package name="SANYO-OSCON_SMD_C6">
<description>&lt;b&gt;SANYO OSCON Capacitor&lt;/b&gt; SMD type with conductive polymer electrolyte&lt;p&gt;
Source: e_os_all.pdf</description>
</package>
</packages>
</library>
<library name="Stefan_selfbus">
<packages>
<package name="SOT23-6">
<description>&lt;b&gt;Small Outline Transistor&lt;/b&gt; 6 lead</description>
</package>
<package name="PIS2812">
</package>
</packages>
</library>
<library name="diode">
<packages>
<package name="SMA">
<description>&lt;b&gt;SMA&lt;/b&gt; CASE 403D-02&lt;p&gt;
Source: http://www.onsemi.com/pub_link/Collateral/MBRA340T3-D.PDF</description>
</package>
<package name="MINIMELF">
<description>&lt;b&gt;Mini Melf Diode&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="led">
<packages>
<package name="LED3MM">
<description>&lt;B&gt;LED&lt;/B&gt;&lt;p&gt;
3 mm, round</description>
</package>
<package name="CHIPLED_1206">
<description>&lt;b&gt;CHIPLED&lt;/b&gt;&lt;p&gt;
Source: http://www.osram.convergy.de/ ... LG_LY N971.pdf</description>
</package>
</packages>
</library>
<library name="inductor-neosid">
<packages>
<package name="SD12_1000">
<description>NOMINAL &lt;b&gt;INDUCTANCE&lt;/b&gt;&lt;p&gt;
over 680 µH, grid 5 mm, diameter 12.5 mm, height 20 mm</description>
</package>
</packages>
</library>
<library name="transistor">
<packages>
<package name="SOT23">
<description>&lt;b&gt;SOT-23&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="transistor-pnp">
<packages>
<package name="SOT223">
<description>&lt;b&gt;SOT-223&lt;/b&gt;</description>
</package>
<package name="SOT23-BEC">
<description>&lt;b&gt;TO-236&lt;/b&gt; ITT Intermetall</description>
</package>
</packages>
</library>
<library name="pinhead-2">
<description>&lt;b&gt;Pin Header Connectors&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de, Modified by Cougar@CasaDelGato.Com&lt;/author&gt;</description>
<packages>
<package name="2X05M">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt; - 2</description>
</package>
</packages>
</library>
<library name="semicon-smd-ipc">
<packages>
<package name="SMB">
<description>&lt;b&gt;DIODE&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="selfbus">
<packages>
<package name="SMD1,27X2,54X8">
</package>
<package name="SMD1,27X2,54">
</package>
</packages>
</library>
<library name="con-wago">
<packages>
<package name="BUSKLEMME243-724">
</package>
</packages>
</library>
<library name="lpc">
<packages>
<package name="PAD">
</package>
</packages>
</library>
<library name="pinhead">
<description>&lt;b&gt;Pin Header Connectors&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="1X01">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="crystal">
<packages>
<package name="ASF">
<description>&lt;b&gt;CRYSTAL CLOCK OSCILLATORS&lt;/b&gt;&lt;p&gt;
5.0 Vdc or 3.3 Vdc - LOW PROFILE ULTRA MINIATURE CERAMIC SURFACE MOUNT&lt;br&gt;
Source: http://www.abracon.com/Oscillators/asf1-L-L1.pdf</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="IC1" library="microbuilder" package="LQFP48" value="LPC1115">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C104" library="rcl" package="C1206" value="100n">
<attribute name="REICHELT" value="X7R-G0805 100N"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="IC100" library="Stefan_selfbus" package="SOT23-6" value="BD9G101">
<attribute name="VALUE"/>
<attribute name="NAME"/>
</element>
<element name="L100" library="Stefan_selfbus" package="PIS2812" value="6.8µH">
<attribute name="REICHELT" value="L-1616FPS 6,8µ"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C100" library="rcl" package="C1206" value="4.7µF/50V">
<attribute name="REICHELT" value="X7R-G1206 4,7/50"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C103" library="rcl" package="C1206" value="22µ/6V">
<attribute name="REICHELT" value="X5R-G0805 22/6"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C102" library="rcl" package="C1206" value="15nF">
<attribute name="REICHELT" value="X7R-G0805 15N"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R101" library="rcl" package="R1206" value="2k4">
<attribute name="REICHELT" value="SMD 1/4W 2,4K"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R102" library="rcl" package="R1206" value="680R">
<attribute name="REICHELT" value="SMD-0805 680"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C101" library="rcl" package="C1206" value="220n">
<attribute name="REICHELT" value="Y5R-G0603 220N"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="D100" library="diode" package="SMA" value="MBRS1100">
<attribute name="REICHELT" value="MBRS 1100 SMD"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R9" library="rcl" package="R1206" value="47k">
<attribute name="REICHELT" value="SMD-0805 47,0K"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R8" library="rcl" package="R1206" value="82k">
<attribute name="REICHELT" value="SMD-0805 82,0K"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C2" library="rcl" package="C1206" value="100n">
<attribute name="REICHELT" value="X7R-G0805 100N"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C4" library="rcl" package="C1206" value="10n">
<attribute name="REICHELT" value="X7R-G0805 10N"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R6" library="rcl" package="R1206" value="5k6">
<attribute name="REICHELT" value="SMD-0805 5,60K"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C11" library="rcl" package="C1206" value="10n">
<attribute name="REICHELT" value="X7R-G0805 10N"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R5" library="rcl" package="R1206" value="100k">
<attribute name="REICHELT" value="SMD-0805 100K"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C1" library="rcl" package="SANYO-OSCON_SMD_C6" value="100µ/35V">
<attribute name="REICHELT" value="VF 100/35 K-D8"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R4" library="rcl" package="R1206" value="2k2">
<attribute name="REICHELT" value="SMD-0805 2,20K"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="L1" library="inductor-neosid" package="SD12_1000" value="150mH">
<attribute name="REICHELT" value="L-11P 150M"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R3" library="rcl" package="R1206" value="1k">
<attribute name="REICHELT" value="SMD-0805 1,00K"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R10" library="rcl" package="R1206" value="10k">
<attribute name="REICHELT" value="SMD-0805 10,0K"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C9" library="rcl" package="C1206" value="10n">
<attribute name="REICHELT" value="X7R-G0805 10N"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="T3" library="transistor" package="SOT23" value="BC847">
<attribute name="REICHELT" value="BC 847C SMD"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C3" library="rcl" package="C1206" value="10n">
<attribute name="REICHELT" value="X7R-G0805 10N"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R1" library="rcl" package="R1206" value="1k">
<attribute name="REICHELT" value="SMD-0805 1,00K"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R2" library="rcl" package="R1206" value="5R6">
<attribute name="REICHELT" value="SMD-0805 5,60"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R11" library="rcl" package="R1206" value="100k">
<attribute name="REICHELT" value="SMD-0805 100K"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R7" library="rcl" package="R1206" value="10k">
<attribute name="REICHELT" value="SMD-0805 10,0K"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="D3" library="diode" package="MINIMELF" value="1N4148">
<attribute name="REICHELT" value="1N 4148 SMD"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="D6" library="diode" package="MINIMELF" value="7V5">
<attribute name="REICHELT" value="SMD ZF 7,5"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R12" library="rcl" package="R1206" value="91k">
<attribute name="REICHELT" value="SMD 1/4W 91K"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C5" library="rcl" package="C1206" value="100p">
<attribute name="REICHELT" value="NPO-G0805 100P"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R14" library="rcl" package="R1206" value="100k">
<attribute name="REICHELT" value="SMD-0805 100K"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R15" library="rcl" package="R1206" value="100k">
<attribute name="REICHELT" value="SMD-0805 100K"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="D2" library="diode" package="MINIMELF" value="1N4148">
<attribute name="REICHELT" value="1N 4148 SMD"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R13" library="rcl" package="R1206" value="10k">
<attribute name="REICHELT" value="SMD-0805 10,0K"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="D5" library="diode" package="MINIMELF" value="1N4148">
<attribute name="REICHELT" value="1N 4148 SMD"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C12" library="rcl" package="C1206" value="100n">
<attribute name="REICHELT" value="X7R-G0805 100N"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="T2" library="transistor-pnp" package="SOT223" value="BCP52">
<attribute name="REICHELT" value="BCP 52-16 SMD"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="T1" library="transistor-pnp" package="SOT23-BEC" value="BC856">
<attribute name="REICHELT" value="BC 856B SMD"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C13" library="rcl" package="C1206" value="100n">
<attribute name="REICHELT" value="X7R-G0805 100N"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C6" library="rcl" package="C1206" value="10n">
<attribute name="REICHELT" value="X7R-G0805 10N"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="D7" library="diode" package="MINIMELF" value="3V6">
<attribute name="REICHELT" value="SMD ZF 3,6"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C10" library="rcl" package="C1206" value="100n">
<attribute name="REICHELT" value="X7R-G0805 100N"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="JP7" library="pinhead-2" package="2X05M" value="J">
<attribute name="REICHELT" value="MPE 150-3-010"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="D1" library="semicon-smd-ipc" package="SMB" value="SMAJ40C">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="LED1" library="led" package="CHIPLED_1206" value="red">
<attribute name="REICHELT" value="SMD-LED 0805 RT"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R16" library="rcl" package="R1206" value="1k">
<attribute name="REICHELT" value="SMD-0805 1,00K"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="JP1" library="selfbus" package="SMD1,27X2,54X8" value="WIREPADX8"/>
<element name="JP5" library="selfbus" package="SMD1,27X2,54" value="WIREPADX1"/>
<element name="JP6" library="selfbus" package="SMD1,27X2,54" value="WIREPADX1"/>
<element name="JP2" library="selfbus" package="SMD1,27X2,54X8" value="WIREPADX8"/>
<element name="R17" library="rcl" package="R1206" value="10k">
<attribute name="REICHELT" value="SMD-0805 1,00K"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R19" library="rcl" package="R1206" value="10k">
<attribute name="REICHELT" value="SMD-0805 1,00K"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="X1" library="con-wago" package="BUSKLEMME243-724" value="EIB"/>
<element name="JP4" library="selfbus" package="SMD1,27X2,54" value="WIREPADX1"/>
<element name="JP3" library="selfbus" package="SMD1,27X2,54" value="WIREPADX1"/>
<element name="R18" library="rcl" package="R1206" value="3,3k">
<attribute name="REICHELT" value="SMD-0805 3,30K"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R20" library="rcl" package="R1206" value="3,3k">
<attribute name="REICHELT" value="SMD-0805 3,30K"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="P1" library="lpc" package="PAD" value=" "/>
<element name="P2" library="lpc" package="PAD" value=" "/>
<element name="P3" library="lpc" package="PAD" value=" "/>
<element name="P4" library="lpc" package="PAD" value=" "/>
<element name="P5" library="lpc" package="PAD" value=" "/>
<element name="P6" library="lpc" package="PAD" value=" "/>
<element name="P7" library="lpc" package="PAD" value=" "/>
<element name="P8" library="lpc" package="PAD" value=" "/>
<element name="P9" library="lpc" package="PAD" value=" "/>
<element name="P10" library="lpc" package="PAD" value=" "/>
<element name="P11" library="lpc" package="PAD" value=" "/>
<element name="P12" library="lpc" package="PAD" value=" "/>
<element name="P13" library="lpc" package="PAD" value=" "/>
<element name="P14" library="lpc" package="PAD" value=" "/>
<element name="JP8" library="pinhead" package="1X01" value=""/>
<element name="JP9" library="pinhead" package="1X01" value=""/>
<element name="LED2" library="led" package="LED3MM" value="red">
<attribute name="REICHELT" value="SMD-LED 0805 RT"/>
</element>
<element name="Q2" library="crystal" package="ASF" value=""/>
<element name="C7" library="rcl" package="C1206" value="10n"/>
<element name="JP10" library="pinhead" package="1X01" value=""/>
</elements>
<signals>
<signal name="GND">
<contactref element="IC100" pad="2"/>
<contactref element="IC100" pad="2"/>
<contactref element="C100" pad="1"/>
<contactref element="R102" pad="1"/>
<contactref element="D100" pad="A"/>
<contactref element="C9" pad="1"/>
<contactref element="C1" pad="-"/>
<contactref element="R9" pad="1"/>
<contactref element="R2" pad="1"/>
<contactref element="R11" pad="1"/>
<contactref element="R5" pad="2"/>
<contactref element="C5" pad="1"/>
<contactref element="R13" pad="2"/>
<contactref element="D7" pad="A"/>
<contactref element="C10" pad="1"/>
<contactref element="T1" pad="C"/>
<contactref element="C6" pad="1"/>
<contactref element="JP7" pad="9"/>
<contactref element="D1" pad="2"/>
<contactref element="IC1" pad="5"/>
<contactref element="IC1" pad="41"/>
<contactref element="C11" pad="1"/>
<contactref element="C12" pad="1"/>
<contactref element="C13" pad="1"/>
<contactref element="JP5" pad="1"/>
<contactref element="C104" pad="2"/>
<contactref element="C103" pad="2"/>
<contactref element="R19" pad="1"/>
<contactref element="X1" pad="1"/>
<contactref element="JP9" pad="1"/>
<contactref element="Q2" pad="2"/>
<contactref element="C7" pad="1"/>
<contactref element="JP10" pad="1"/>
</signal>
<signal name="LX">
<contactref element="IC100" pad="6"/>
<contactref element="C102" pad="1"/>
<contactref element="L100" pad="P$1"/>
<contactref element="D100" pad="C"/>
</signal>
<signal name="N$19">
<contactref element="C102" pad="2"/>
<contactref element="IC100" pad="1"/>
</signal>
<signal name="N$2">
<contactref element="IC100" pad="3"/>
<contactref element="C101" pad="1"/>
<contactref element="R102" pad="2"/>
<contactref element="R101" pad="1"/>
</signal>
<signal name="EIB_IN">
<contactref element="R7" pad="1"/>
<contactref element="C5" pad="2"/>
<contactref element="T1" pad="E"/>
<contactref element="IC1" pad="9"/>
</signal>
<signal name="N$1">
<contactref element="R10" pad="1"/>
<contactref element="C2" pad="2"/>
</signal>
<signal name="EIB_OUT">
<contactref element="C4" pad="2"/>
<contactref element="IC1" pad="17"/>
</signal>
<signal name="EIB+">
<contactref element="D3" pad="A"/>
<contactref element="D2" pad="A"/>
<contactref element="D1" pad="1"/>
<contactref element="X1" pad="2"/>
</signal>
<signal name="N$8">
<contactref element="L1" pad="1"/>
<contactref element="D3" pad="C"/>
</signal>
<signal name="N$6">
<contactref element="R4" pad="1"/>
<contactref element="T3" pad="3"/>
</signal>
<signal name="DRAIN">
<contactref element="C3" pad="1"/>
<contactref element="R1" pad="1"/>
<contactref element="C2" pad="1"/>
<contactref element="R11" pad="2"/>
<contactref element="D2" pad="C"/>
<contactref element="T2" pad="3"/>
</signal>
<signal name="RESET">
<contactref element="R14" pad="1"/>
<contactref element="C9" pad="2"/>
<contactref element="IC1" pad="3"/>
<contactref element="JP7" pad="10"/>
</signal>
<signal name="N$3">
<contactref element="C4" pad="1"/>
<contactref element="R6" pad="2"/>
</signal>
<signal name="N$12">
<contactref element="T3" pad="1"/>
<contactref element="R6" pad="1"/>
<contactref element="R5" pad="1"/>
</signal>
<signal name="N$15">
<contactref element="R3" pad="2"/>
<contactref element="R1" pad="2"/>
<contactref element="C3" pad="2"/>
<contactref element="T2" pad="1"/>
</signal>
<signal name="N$7">
<contactref element="T3" pad="2"/>
<contactref element="R2" pad="2"/>
<contactref element="T2" pad="2"/>
</signal>
<signal name="N$14">
<contactref element="R8" pad="1"/>
<contactref element="R9" pad="2"/>
<contactref element="R10" pad="2"/>
<contactref element="T1" pad="B"/>
</signal>
<signal name="N$9">
<contactref element="D6" pad="C"/>
<contactref element="D5" pad="C"/>
</signal>
<signal name="REF">
<contactref element="R4" pad="2"/>
<contactref element="R3" pad="1"/>
<contactref element="D6" pad="A"/>
<contactref element="R12" pad="1"/>
</signal>
<signal name="BUS_V">
<contactref element="R12" pad="2"/>
<contactref element="R13" pad="1"/>
<contactref element="D7" pad="C"/>
<contactref element="C10" pad="2"/>
<contactref element="IC1" pad="42"/>
</signal>
<signal name="ISP_EN">
<contactref element="R15" pad="1"/>
<contactref element="IC1" pad="4"/>
<contactref element="JP7" pad="7"/>
</signal>
<signal name="SWCLK">
<contactref element="IC1" pad="29"/>
<contactref element="JP7" pad="4"/>
</signal>
<signal name="IO5">
<contactref element="JP1" pad="5"/>
<contactref element="IC1" pad="34"/>
</signal>
<signal name="IO7">
<contactref element="JP1" pad="7"/>
<contactref element="IC1" pad="37"/>
</signal>
<signal name="IO9">
<contactref element="JP2" pad="1"/>
<contactref element="IC1" pad="24"/>
</signal>
<signal name="IO10">
<contactref element="JP2" pad="2"/>
<contactref element="IC1" pad="27"/>
</signal>
<signal name="IO12">
<contactref element="JP2" pad="4"/>
<contactref element="IC1" pad="32"/>
</signal>
<signal name="SWDIO">
<contactref element="IC1" pad="39"/>
<contactref element="JP7" pad="2"/>
</signal>
<signal name="IO6">
<contactref element="JP1" pad="6"/>
<contactref element="IC1" pad="36"/>
</signal>
<signal name="IO2">
<contactref element="JP1" pad="2"/>
<contactref element="IC1" pad="26"/>
</signal>
<signal name="IO11">
<contactref element="JP2" pad="3"/>
<contactref element="IC1" pad="30"/>
</signal>
<signal name="IO13">
<contactref element="JP2" pad="5"/>
<contactref element="IC1" pad="33"/>
</signal>
<signal name="ISP_TXD">
<contactref element="IC1" pad="47"/>
<contactref element="JP7" pad="5"/>
</signal>
<signal name="ISP_RXD">
<contactref element="IC1" pad="46"/>
<contactref element="JP7" pad="3"/>
</signal>
<signal name="EIB_DC">
<contactref element="L1" pad="2"/>
<contactref element="C1" pad="+"/>
<contactref element="D5" pad="A"/>
<contactref element="IC100" pad="5"/>
<contactref element="C100" pad="2"/>
<contactref element="IC100" pad="4"/>
<contactref element="JP1" pad="1"/>
</signal>
<signal name="IO3">
<contactref element="JP1" pad="3"/>
<contactref element="IC1" pad="28"/>
</signal>
<signal name="IO4">
<contactref element="JP1" pad="4"/>
<contactref element="IC1" pad="31"/>
</signal>
<signal name="IO8">
<contactref element="JP1" pad="8"/>
<contactref element="IC1" pad="43"/>
</signal>
<signal name="PROG">
<contactref element="IC1" pad="2"/>
<contactref element="LED1" pad="C"/>
<contactref element="JP8" pad="1"/>
<contactref element="LED2" pad="K"/>
</signal>
<signal name="+3V3">
<contactref element="IC1" pad="8"/>
<contactref element="C13" pad="2"/>
<contactref element="C12" pad="2"/>
<contactref element="C11" pad="2"/>
<contactref element="IC1" pad="44"/>
<contactref element="R16" pad="2"/>
<contactref element="JP6" pad="1"/>
<contactref element="C101" pad="2"/>
<contactref element="R101" pad="2"/>
<contactref element="L100" pad="P$2"/>
<contactref element="R14" pad="2"/>
<contactref element="R15" pad="2"/>
<contactref element="R8" pad="2"/>
<contactref element="R7" pad="2"/>
<contactref element="C6" pad="2"/>
<contactref element="JP7" pad="1"/>
<contactref element="C104" pad="1"/>
<contactref element="C103" pad="1"/>
<contactref element="R17" pad="2"/>
<contactref element="R18" pad="2"/>
<contactref element="R20" pad="2"/>
<contactref element="Q2" pad="1"/>
<contactref element="C7" pad="2"/>
<contactref element="Q2" pad="4"/>
</signal>
<signal name="N$41">
<contactref element="R16" pad="1"/>
<contactref element="LED1" pad="A"/>
<contactref element="LED2" pad="A"/>
</signal>
<signal name="IO16">
<contactref element="JP2" pad="8"/>
<contactref element="IC1" pad="45"/>
</signal>
<signal name="IO17">
<contactref element="JP3" pad="1"/>
<contactref element="IC1" pad="16"/>
<contactref element="R18" pad="1"/>
</signal>
<signal name="IO18">
<contactref element="JP4" pad="1"/>
<contactref element="IC1" pad="15"/>
<contactref element="R20" pad="1"/>
</signal>
<signal name="ID">
<contactref element="R19" pad="2"/>
<contactref element="R17" pad="1"/>
<contactref element="IC1" pad="40"/>
</signal>
<signal name="IO15">
<contactref element="JP2" pad="7"/>
<contactref element="IC1" pad="38"/>
</signal>
<signal name="IO14">
<contactref element="JP2" pad="6"/>
<contactref element="IC1" pad="35"/>
</signal>
<signal name="EXT1">
<contactref element="P1" pad="1"/>
<contactref element="IC1" pad="10"/>
</signal>
<signal name="EXT2">
<contactref element="P2" pad="1"/>
<contactref element="IC1" pad="14"/>
</signal>
<signal name="EXT14">
<contactref element="IC1" pad="13"/>
<contactref element="P3" pad="1"/>
</signal>
<signal name="EXT10">
<contactref element="IC1" pad="11"/>
<contactref element="P5" pad="1"/>
</signal>
<signal name="EXT9">
<contactref element="IC1" pad="12"/>
<contactref element="P4" pad="1"/>
</signal>
<signal name="EXT13">
<contactref element="IC1" pad="19"/>
<contactref element="P7" pad="1"/>
</signal>
<signal name="EXT12">
<contactref element="IC1" pad="20"/>
<contactref element="P8" pad="1"/>
</signal>
<signal name="EXT11">
<contactref element="IC1" pad="1"/>
<contactref element="P9" pad="1"/>
</signal>
<signal name="EXT7">
<contactref element="IC1" pad="48"/>
<contactref element="P10" pad="1"/>
</signal>
<signal name="EXT6">
<contactref element="IC1" pad="18"/>
<contactref element="P11" pad="1"/>
</signal>
<signal name="EXT5">
<contactref element="IC1" pad="21"/>
<contactref element="P12" pad="1"/>
</signal>
<signal name="EXT3">
<contactref element="P13" pad="1"/>
<contactref element="IC1" pad="22"/>
</signal>
<signal name="EXT4">
<contactref element="P14" pad="1"/>
<contactref element="IC1" pad="23"/>
</signal>
<signal name="EXT8">
<contactref element="IC1" pad="25"/>
<contactref element="P6" pad="1"/>
</signal>
<signal name="N$4">
<contactref element="Q2" pad="3"/>
<contactref element="IC1" pad="6"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
