Reset on connect
Address:
Password:
`Ctrl+Insert` to copy and `Shift+Insert` to paste
Bridge data to EasyMQTT
ESP8266
To use ESP8266, simply connecto to MicroPython board using Wifi. Micropython must be previously installed on the board. Follow these instructions to install it.
File manager
...

## On device

...

## Blocks to code

workspace.bipes.xmlinternal

## Templates

main.py
ssd1306.py
Hello, User!

## Projects

## Settings

×

##

10 1 10 1 123 1 1 9 45 0 3.1 64 10 50 1 100 1 100 to int abc {textVariable} abc {textVariable} {textVariable} abc abc abc abc to str 5 {listVariable} {listVariable} {listVariable} {listVariable} , ticks_ms Execute Python custom with output 1 1 1 0 60
1200 -1 -1 Super Mario - Main Theme
Super Mario - Main Theme Super Mario - Title Music SMBtheme SMBwater SMBunderground Picaxe Simpsons Indiana TakeOnMe Entertainer Muppets Xfiles Looney 20thCenFox Bond MASH StarWars GoodBad TopGun A-Team Flintstones Jeopardy Gadget Smurfs MahnaMahna LeisureSuit MissionImp 160000000 1000 50 1000 50 0 50 152 220 204 70.8 52.9 31
0 1 0 40 40 Hello 0 0 40 40 0 0 60 40 0 0 60 40 5 10
8 50 152 220 204 70.8 52.9 0 0 0 0 0
4 20
14 13 1, 2, 4, 8, 16, 32, 64, 128 7 0 FALSE FALSE FALSE FALSE FALSE FALSE FALSE FALSE FALSE FALSE FALSE FALSE FALSE FALSE FALSE FALSE FALSE FALSE FALSE FALSE FALSE FALSE FALSE FALSE FALSE FALSE FALSE FALSE FALSE FALSE FALSE FALSE FALSE FALSE FALSE FALSE FALSE FALSE FALSE FALSE FALSE FALSE FALSE FALSE FALSE FALSE FALSE FALSE FALSE FALSE FALSE FALSE FALSE FALSE FALSE FALSE FALSE FALSE FALSE FALSE FALSE FALSE FALSE FALSE Start DHT11/22 sensor Measure DHT11/22 Sensor Read DHT11/22 Temperature Read DHT11/22 Humidity
10000
5 4
10000
1000 1000 1000 1000 90 file.txt file.txt File contents file.txt file.txt file.txt file.txt file.txt Connect to Wifi network Configure Access Point Mode Scan Wifi networks Wifi current IP Make HTTP GET Request URL Make HTTP POST Request URL Data
80 You reached BIPES WebServer!
smtp.gmail.com 587 email@gmail.com gmail_password email@email.com Email from BIPES! BIPES is nice!
3
towel.blinkenlights.nl 23 500 Hello 1883 Value Callback Function EasyMQTT Start EasyMQTT Publish Data EasyMQTT Stop 10 1 10 1 123 1 1 9 45 0 3.1 64 10 50 1 100 1 100 to int abc {textVariable} abc {textVariable} {textVariable} abc abc abc abc to str 5 {listVariable} {listVariable} {listVariable} {listVariable} , Project INFO Execute Python custom with output 1 1000 50 90 10 1 10 1 123 1 1 9 45 0 3.1 64 10 50 1 100 1 100 abc {textVariable} abc {textVariable} {textVariable} abc abc abc abc 5 {listVariable} {listVariable} {listVariable} {listVariable} , Project INFO Author IOT ID Description Execute Python custom with output 10 1 10 1 123 1 1 9 45 0 3.1 64 10 50 1 100 1 100 to int to float abc {textVariable} abc {textVariable} {textVariable} abc abc abc abc to str decode bytes to text 5 {listVariable} {listVariable} {listVariable} {listVariable} , Project INFO Execute Python custom with output 1 1 1 0 60 160000000 0 1000 50
4 20
5 4 40 40 Hello
14 13 1, 2, 4, 8, 16, 32, 64, 128 7 0 FALSE FALSE FALSE FALSE FALSE FALSE FALSE FALSE FALSE FALSE FALSE FALSE FALSE FALSE FALSE FALSE FALSE FALSE FALSE FALSE FALSE FALSE FALSE FALSE FALSE FALSE FALSE FALSE FALSE FALSE FALSE FALSE FALSE FALSE FALSE FALSE FALSE FALSE FALSE FALSE FALSE FALSE FALSE FALSE FALSE FALSE FALSE FALSE FALSE FALSE FALSE FALSE FALSE FALSE FALSE FALSE FALSE FALSE FALSE FALSE FALSE FALSE FALSE FALSE Start DHT11/22 sensor Measure DHT11/22 Sensor Read DHT11/22 Temperature Read DHT11/22 Humidity
10000
5 4
10000
90 1 70 1 _ file.txt file.txt File contents file.txt file.txt file.txt file.txt file.txt Connect to Wifi network Configure Access Point Mode Scan Wifi networks Wifi current IP Make HTTP GET Request URL Make HTTP POST Request URL Data
80 You reached BIPES WebServer!
smtp.gmail.com 587 email@gmail.com gmail_password email@email.com Email from BIPES! BIPES is nice!
3
towel.blinkenlights.nl 23 500 Hello
1883 Value
EasyMQTT Start EasyMQTT Publish Data EasyMQTT Stop 10 1 10 1 123 1 1 9 45 0 3.1 64 10 50 1 100 1 100 to int abc {textVariable} abc {textVariable} {textVariable} abc abc abc abc to str 5 {listVariable} {listVariable} {listVariable} {listVariable} , ticks_ms Execute Python custom with output 1 100 100 0 60 160000000 1000 50 1000 50
8 50 152 220 204 70.8 52.9 0 0 0 0 0
4 20
1 50 50 152 220 40 40 1 40 40 1 40 40 40 40 1
1 5 4 40 40 Hello 64 32 90 0
14 13 1, 2, 4, 8, 16, 32, 64, 128 7 0 FALSE FALSE FALSE FALSE FALSE FALSE FALSE FALSE FALSE FALSE FALSE FALSE FALSE FALSE FALSE FALSE FALSE FALSE FALSE FALSE FALSE FALSE FALSE FALSE FALSE FALSE FALSE FALSE FALSE FALSE FALSE FALSE FALSE FALSE FALSE FALSE FALSE FALSE FALSE FALSE FALSE FALSE FALSE FALSE FALSE FALSE FALSE FALSE FALSE FALSE FALSE FALSE FALSE FALSE FALSE FALSE FALSE FALSE FALSE FALSE FALSE FALSE FALSE FALSE Start DHT11/22 sensor
10000
5 4
10000
90 1 70 1 _
1200 -1 -1 Super Mario - Main Theme
Super Mario - Main Theme Super Mario - Title Music SMBtheme SMBwater SMBunderground Picaxe Simpsons Indiana TakeOnMe Entertainer Muppets Xfiles Looney 20thCenFox Bond MASH StarWars GoodBad TopGun A-Team Flintstones Jeopardy Gadget Smurfs MahnaMahna LeisureSuit MissionImp Configure Access Point Mode Wifi current IP http:// request http://bipes.net.br/test.txt
smtp.gmail.com 587 email@gmail.com gmail_password email@email.com Email from BIPES! BIPES is nice! EasyMQTT Stop 1200 -1 -1 Super Mario - Main Theme sound.wav Super Mario - Main Theme Super Mario - Title Music SMBtheme SMBwater SMBunderground Picaxe Simpsons Indiana TakeOnMe Entertainer Muppets Xfiles Looney 20thCenFox Bond MASH StarWars GoodBad TopGun A-Team Flintstones Jeopardy Gadget Smurfs MahnaMahna LeisureSuit MissionImp 5 5 1 50 152 220 10 1 10 1 123 1 1 9 45 0 3.1 64 10 50 1 100 1 100 to int abc {textVariable} abc {textVariable} {textVariable} abc abc abc abc to str 5 {listVariable} {listVariable} {listVariable} {listVariable} , ticks_ms Execute Python custom with output 1 100 100 0 60 160000000 1000 50 1000 50 8 50 152 220 204 70.8 52.9 0 0 0 0 0 0
4 20
1 50 50 152 220 40 40 1 40 40 1 40 40 40 40 1
<--> 40 40 Hello 0 10 10 10 10 20 20 10 10 20 20 10 10 20 20 1 0
14 13 1, 2, 4, 8, 16, 32, 64, 128 7 0 FALSE FALSE FALSE FALSE FALSE FALSE FALSE FALSE FALSE FALSE FALSE FALSE FALSE FALSE FALSE FALSE FALSE FALSE FALSE FALSE FALSE FALSE FALSE FALSE FALSE FALSE FALSE FALSE FALSE FALSE FALSE FALSE FALSE FALSE FALSE FALSE FALSE FALSE FALSE FALSE FALSE FALSE FALSE FALSE FALSE FALSE FALSE FALSE FALSE FALSE FALSE FALSE FALSE FALSE FALSE FALSE FALSE FALSE FALSE FALSE FALSE FALSE FALSE FALSE Callback Function 2 17 16 9600
22 21
10000
22 21 90 1
1200 -1 -1 Super Mario - Main Theme
Super Mario - Main Theme Super Mario - Title Music SMBtheme SMBwater SMBunderground Picaxe Simpsons Indiana TakeOnMe Entertainer Muppets Xfiles Looney 20thCenFox Bond MASH StarWars GoodBad TopGun A-Team Flintstones Jeopardy Gadget Smurfs MahnaMahna LeisureSuit MissionImp file.txt file.txt file.txt contents Line contents 80 file.txt file.txt file.txt file.txt Hello Configure Access Point Mode Wifi current IP http:// request http://bipes.net.br/test.txt request request http://bipes.net.br/test.txt EQ request 200 abc Success. Response content: request abc Request Error. Status code = request Make HTTP POST Request URL Data
80 You reached BIPES WebServer!
smtp.gmail.com 587 email@gmail.com gmail_password email@email.com Email from BIPES! BIPES is nice!
3
towel.blinkenlights.nl 23 500 Hello 1883 Value Callback Function EasyMQTT Stop
BIPES-BLE BIPES-BLE
1 Deploy code Content content 1 http://192.168.0.1/php_script.php column name content column name content
1 1 0 0 1
10 1 10 1 123 1 1 9 45 0 3.1 64 10 50 1 100 1 100 to int abc {textVariable} abc {textVariable} {textVariable} abc abc abc abc to str 5 {listVariable} {listVariable} {listVariable} {listVariable} , ticks_ms Execute Python custom with output 1 100 100 0 60 160000000 1000 50 1000 50 0 0 0
8 50 152 220 204 70.8 52.9 0 0 0 0 0
4 20
1 50 50 152 220 40 40 1 40 40 1 40 40 40 40 1
1 5 4 40 40 Hello 64 32 90 0
14 13 1, 2, 4, 8, 16, 32, 64, 128 7 0 FALSE FALSE FALSE FALSE FALSE FALSE FALSE FALSE FALSE FALSE FALSE FALSE FALSE FALSE FALSE FALSE FALSE FALSE FALSE FALSE FALSE FALSE FALSE FALSE FALSE FALSE FALSE FALSE FALSE FALSE FALSE FALSE FALSE FALSE FALSE FALSE FALSE FALSE FALSE FALSE FALSE FALSE FALSE FALSE FALSE FALSE FALSE FALSE FALSE FALSE FALSE FALSE FALSE FALSE FALSE FALSE FALSE FALSE FALSE FALSE FALSE FALSE FALSE FALSE Start DHT11/22 sensor
10000
5 4
10000
90 1 70 1 _
1200 -1 -1 Super Mario - Main Theme
Super Mario - Main Theme Super Mario - Title Music SMBtheme SMBwater SMBunderground Picaxe Simpsons Indiana TakeOnMe Entertainer Muppets Xfiles Looney 20thCenFox Bond MASH StarWars GoodBad TopGun A-Team Flintstones Jeopardy Gadget Smurfs MahnaMahna LeisureSuit MissionImp file.txt file.txt file.txt contents Line contents 80 file.txt file.txt file.txt file.txt Configure Access Point Mode Wifi current IP http:// request http://bipes.net.br/test.txt request request http://bipes.net.br/test.txt EQ request 200 abc Success. Response content: request abc Request Error. Status code = request Make HTTP POST Request URL Data
80 You reached BIPES WebServer!
smtp.gmail.com 587 email@gmail.com gmail_password email@email.com Email from BIPES! BIPES is nice!
3
towel.blinkenlights.nl 23 500 Hello 1883 Value Callback Function EasyMQTT Stop
BIPES-BLE BIPES-BLE
1 Deploy code Content content
1 1 0 0 1
10 1 10 1 123 1 1 9 45 0 3.1 64 10 50 1 100 1 100 to int abc {textVariable} abc {textVariable} {textVariable} abc abc abc abc to str 5 {listVariable} {listVariable} {listVariable} {listVariable} , ticks_ms Execute Python custom with output 1 100 100 0 60 160000000 0 1000 50 1000 50
8 50 152 220 204 70.8 52.9 0 0 0 0 0
4 20
1 5 4 40 40 1 40 40 1 40 40 40 40 1
1 5 4 40 40 Hello
14 13 1, 2, 4, 8, 16, 32, 64, 128 7 0 FALSE FALSE FALSE FALSE FALSE FALSE FALSE FALSE FALSE FALSE FALSE FALSE FALSE FALSE FALSE FALSE FALSE FALSE FALSE FALSE FALSE FALSE FALSE FALSE FALSE FALSE FALSE FALSE FALSE FALSE FALSE FALSE FALSE FALSE FALSE FALSE FALSE FALSE FALSE FALSE FALSE FALSE FALSE FALSE FALSE FALSE FALSE FALSE FALSE FALSE FALSE FALSE FALSE FALSE FALSE FALSE FALSE FALSE FALSE FALSE FALSE FALSE FALSE FALSE
10000
5 4
5 4
10000
90 1 70 1 _
1200 -1 -1 Super Mario - Main Theme
Super Mario - Main Theme Super Mario - Title Music SMBtheme SMBwater SMBunderground Picaxe Simpsons Indiana TakeOnMe Entertainer Muppets Xfiles Looney 20thCenFox Bond MASH StarWars GoodBad TopGun A-Team Flintstones Jeopardy Gadget Smurfs MahnaMahna LeisureSuit MissionImp file.txt file.txt file.txt contents Line contents 80 file.txt file.txt file.txt file.txt Configure Access Point Mode Wifi current IP http:// request http://bipes.net.br/test.txt request request http://bipes.net.br/test.txt EQ request 200 abc Success. Response content: request abc Request Error. Status code = request Make HTTP POST Request URL Data y 1 list
80 You reached BIPES WebServer!
smtp.gmail.com 587 email@gmail.com gmail_password email@email.com Email from BIPES! BIPES is nice!
3
towel.blinkenlights.nl 23 500 Hello 1883 Value Callback Function EasyMQTT Stop
1 Deploy code Content content
1 1 0 0 1
10 1 10 1 123 1 1 9 45 0 3.1 64 10 50 1 100 1 100 abc {textVariable} abc {textVariable} {textVariable} abc abc abc abc 5 {listVariable} {listVariable} {listVariable} {listVariable} , Project INFO Author IOT ID Description Execute Python custom with output 10 1 10 1 123 1 1 9 45 0 3.1 64 10 50 1 100 1 100 to int abc {textVariable} abc {textVariable} {textVariable} abc abc abc abc to str 5 {listVariable} {listVariable} {listVariable} {listVariable} , ticks_ms Execute Python custom with output 1 1 1 0 60
1200 -1 -1 Super Mario - Main Theme
Super Mario - Main Theme Super Mario - Title Music SMBtheme SMBwater SMBunderground Picaxe Simpsons Indiana TakeOnMe Entertainer Muppets Xfiles Looney 20thCenFox Bond MASH StarWars GoodBad TopGun A-Team Flintstones Jeopardy Gadget Smurfs MahnaMahna LeisureSuit MissionImp 160000000 1000 50 1000 50
0 1 0 40 40 Hello 0 0 40 40 0 0 60 40 0 0 60 40 5 10
2 50 152 220 204 70.8 52.9 0 0 0 0 0
4 20
14 13 1, 2, 4, 8, 16, 32, 64, 128 7 0 FALSE FALSE FALSE FALSE FALSE FALSE FALSE FALSE FALSE FALSE FALSE FALSE FALSE FALSE FALSE FALSE FALSE FALSE FALSE FALSE FALSE FALSE FALSE FALSE FALSE FALSE FALSE FALSE FALSE FALSE FALSE FALSE FALSE FALSE FALSE FALSE FALSE FALSE FALSE FALSE FALSE FALSE FALSE FALSE FALSE FALSE FALSE FALSE FALSE FALSE FALSE FALSE FALSE FALSE FALSE FALSE FALSE FALSE FALSE FALSE FALSE FALSE FALSE FALSE Start DHT11/22 sensor Measure DHT11/22 Sensor Read DHT11/22 Temperature Read DHT11/22 Humidity
Start HCSR04 Ultrasound sensor 10000
5 4
10000
90 file.txt file.txt File contents file.txt file.txt file.txt file.txt file.txt Connect to Wifi network Configure Access Point Mode Scan Wifi networks Wifi current IP Make HTTP GET Request URL Make HTTP POST Request URL Data
80 You reached BIPES WebServer!
smtp.gmail.com 587 email@gmail.com gmail_password email@email.com Email from BIPES! BIPES is nice!
3
towel.blinkenlights.nl 23 500 Hello Start MQTT Client 1883 Add data to MQTT Buffer Value Publish Buffer to MQTT Topic Publish Payload to MQTT Topic Set Callback to MQTT Messages Callback Function Subscribe to MQTT Topic Check for MQTT Server messages Wait for MQTT Server messages Disconnect MQTT Client EasyMQTT Start EasyMQTT Publish Data EasyMQTT Stop 10 1 10 1 123 1 1 9 45 0 3.1 64 10 50 1 100 1 100 to int abc {textVariable} abc {textVariable} {textVariable} abc abc abc abc to str 5 {listVariable} {listVariable} {listVariable} {listVariable} , ticks_ms Execute Python custom with output 1 1 1 0 60
1200 -1 -1 Super Mario - Main Theme
Super Mario - Main Theme Super Mario - Title Music SMBtheme SMBwater SMBunderground Picaxe Simpsons Indiana TakeOnMe Entertainer Muppets Xfiles Looney 20thCenFox Bond MASH StarWars GoodBad TopGun A-Team Flintstones Jeopardy Gadget Smurfs MahnaMahna LeisureSuit MissionImp 160000000 1000 50 1000 50
0 1 0 40 40 Hello 0 0 40 40 0 0 60 40 0 0 60 40 5 10
8 50 152 220 204 70.8 52.9 0 0 0 0 0
4 20
14 13 1, 2, 4, 8, 16, 32, 64, 128 7 0 FALSE FALSE FALSE FALSE FALSE FALSE FALSE FALSE FALSE FALSE FALSE FALSE FALSE FALSE FALSE FALSE FALSE FALSE FALSE FALSE FALSE FALSE FALSE FALSE FALSE FALSE FALSE FALSE FALSE FALSE FALSE FALSE FALSE FALSE FALSE FALSE FALSE FALSE FALSE FALSE FALSE FALSE FALSE FALSE FALSE FALSE FALSE FALSE FALSE FALSE FALSE FALSE FALSE FALSE FALSE FALSE FALSE FALSE FALSE FALSE FALSE FALSE FALSE FALSE Start DHT11/22 sensor Measure DHT11/22 Sensor Read DHT11/22 Temperature Read DHT11/22 Humidity
10000
5 4
10000
90 file.txt file.txt File contents file.txt file.txt file.txt file.txt file.txt Connect to Wifi network Configure Access Point Mode Scan Wifi networks Wifi current IP Make HTTP GET Request URL Make HTTP POST Request URL Data
80 You reached BIPES WebServer!
smtp.gmail.com 587 email@gmail.com gmail_password email@email.com Email from BIPES! BIPES is nice!
3
towel.blinkenlights.nl 23 500 Hello 1883 Value Callback Function EasyMQTT Start EasyMQTT Publish Data EasyMQTT Stop 10 1 10 1 123 1 1 9 45 0 3.1 64 10 50 1 100 1 100 to int abc {textVariable} abc {textVariable} {textVariable} abc abc abc abc to str 5 {listVariable} {listVariable} {listVariable} {listVariable} , ticks_ms Execute Python custom with output 1 1 1 0 60
1200 -1 -1 Super Mario - Main Theme
Super Mario - Main Theme Super Mario - Title Music SMBtheme SMBwater SMBunderground Picaxe Simpsons Indiana TakeOnMe Entertainer Muppets Xfiles Looney 20thCenFox Bond MASH StarWars GoodBad TopGun A-Team Flintstones Jeopardy Gadget Smurfs MahnaMahna LeisureSuit MissionImp 160000000 1000 50 1000 50
0 1 0 40 40 Hello 0 0 40 40 0 0 60 40 0 0 60 40 5 10
8 50 152 220 204 70.8 52.9 0 0 0 0 0
4 20
14 13 1, 2, 4, 8, 16, 32, 64, 128 7 0 FALSE FALSE FALSE FALSE FALSE FALSE FALSE FALSE FALSE FALSE FALSE FALSE FALSE FALSE FALSE FALSE FALSE FALSE FALSE FALSE FALSE FALSE FALSE FALSE FALSE FALSE FALSE FALSE FALSE FALSE FALSE FALSE FALSE FALSE FALSE FALSE FALSE FALSE FALSE FALSE FALSE FALSE FALSE FALSE FALSE FALSE FALSE FALSE FALSE FALSE FALSE FALSE FALSE FALSE FALSE FALSE FALSE FALSE FALSE FALSE FALSE FALSE FALSE FALSE Start DHT11/22 sensor Measure DHT11/22 Sensor Read DHT11/22 Temperature Read DHT11/22 Humidity
10000
5 4
10000
90 file.txt file.txt File contents file.txt file.txt file.txt file.txt file.txt Connect to Wifi network Configure Access Point Mode Scan Wifi networks Wifi current IP Make HTTP GET Request URL Make HTTP POST Request URL Data
80 You reached BIPES WebServer!
smtp.gmail.com 587 email@gmail.com gmail_password email@email.com Email from BIPES! BIPES is nice!
3
towel.blinkenlights.nl 23 500 Hello 1883 Value Callback Function EasyMQTT Start EasyMQTT Publish Data EasyMQTT Stop 10 1 10 1 123 1 1 9 45 0 3.1 64 10 50 1 100 1 100 to int abc {textVariable} abc {textVariable} {textVariable} abc abc abc abc to str 5 {listVariable} {listVariable} {listVariable} {listVariable} , Project INFO Execute Python custom with output 1 1 1 0 60 160000000 0 1000 50 1000 50
4 20
5 4 40 40 Hello
14 13 1, 2, 4, 8, 16, 32, 64, 128 7 0 FALSE FALSE FALSE FALSE FALSE FALSE FALSE FALSE FALSE FALSE FALSE FALSE FALSE FALSE FALSE FALSE FALSE FALSE FALSE FALSE FALSE FALSE FALSE FALSE FALSE FALSE FALSE FALSE FALSE FALSE FALSE FALSE FALSE FALSE FALSE FALSE FALSE FALSE FALSE FALSE FALSE FALSE FALSE FALSE FALSE FALSE FALSE FALSE FALSE FALSE FALSE FALSE FALSE FALSE FALSE FALSE FALSE FALSE FALSE FALSE FALSE FALSE FALSE FALSE Start DHT11/22 sensor Measure DHT11/22 Sensor Read DHT11/22 Temperature Read DHT11/22 Humidity
10000
5 4
10000
90 file.txt file.txt File contents file.txt file.txt file.txt file.txt file.txt Connect to Wifi network Configure Access Point Mode Scan Wifi networks Wifi current IP Make HTTP GET Request URL Make HTTP POST Request URL Data
80 You reached BIPES WebServer!
smtp.gmail.com 587 email@gmail.com gmail_password email@email.com Email from BIPES! BIPES is nice!
3
towel.blinkenlights.nl 23 500 Hello 1883 Value Callback Function EasyMQTT Start EasyMQTT Publish Data EasyMQTT Stop