Reset on connect
Address:
Password:
`Ctrl+Insert` to copy and `Shift+Insert` to paste
Bridge data to EasyMQTT
ESP8266
To use ESP8266, simply connecto to MicroPython board using Wifi. Micropython must be previously installed on the board. Follow these instructions to install it.
File manager
...

## On device

...

## Blocks to code

workspace.bipes.xmlinternal

## Templates

main.py
ssd1306.py
Hello, User!

## Projects

## Settings

×

##