PRINTER SETTINGS FOR ELASTIC SIDE BANDS

Printer: Ender 3 Pro
Material: NinjaFlex (White), 1.75mm
Software: Prusa Slicer

***SETTINGS***

Speed for all print moves - - -	8mm/s
Extruder temperature  - - - - -	240°C
Bed temperature - - - - - - - -	25°C
Retraction  - - - - - - - - - - Disabled
Infill  - - - - - - - - - - - - 100%
Support material  - - - - - - - Everywhere
Layer height  - - - - - - - - -	0.12mm


*IMPORTANT: You may need to make slight changes depending on 
	    your printer. These are common values used to 
            print flexible filaments.
