<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="9.6.2">
<drawing>
<library>
<packages>
<package name="SOIC16">
</package>
<package name="SPST-NO_UP">
</package>
<package name="DFN8-3X3">
<description>&lt;b&gt;DD Package 8-Lead Plastic DFN (3mm × 3mm)&lt;/b&gt;</description>
</package>
<package name="SOT23">
<description>&lt;b&gt;SOT-23&lt;/b&gt;</description>
</package>
<package name="SO14">
<description>&lt;b&gt;Small Outline Package&lt;/b&gt;</description>
</package>
<package name="SOT223">
<description>&lt;b&gt;Small Outline Transistor&lt;/b&gt;</description>
</package>
<package name="SOT23-5">
<description>&lt;b&gt;5-Lead Small Outline Transistor&lt;/b&gt; Package SOT-23&lt;p&gt;
Source: http://www.analog.com/UploadedFiles/Data_Sheets/346131962AD8067_a.pdf</description>
</package>
<package name="TO220H">
<description>&lt;b&gt;TO-220&lt;/b&gt;</description>
</package>
<package name="MB-25">
</package>
<package name="UFQFPN32">
</package>
<package name="DFN6-3X3">
</package>
<package name="SIM800L">
</package>
<package name="SIM808">
</package>
<package name="MICRO_MELF">
</package>
<package name="AITHINKER">
</package>
<package name="VFQFPN16">
</package>
<package name="SIM868">
</package>
<package name="ANT_3.1X1.6">
</package>
<package name="SIM28">
</package>
<package name="LQFP64">
</package>
<package name="LQFP48">
</package>
<package name="TO252">
</package>
<package name="SOIC8">
<description>&lt;b&gt;Small Outline IC&lt;/b&gt;</description>
</package>
<package name="HDSP-R">
<description>&lt;b&gt;LED DISPLAY&lt;/b&gt;&lt;p&gt;
 15-mm 2 character 7 segment, decimal point right</description>
</package>
<package name="CR2032H">
<description>&lt;b&gt;LI BATTERY&lt;/b&gt; Varta</description>
</package>
<package name="DEF_POT">
</package>
<package name="OPD-D391">
</package>
<package name="L0603">
<description>&lt;b&gt;INDUCTOR&lt;/b&gt;</description>
</package>
<package name="SMA">
</package>
<package name="VSON10">
</package>
<package name="SOT-23-6">
</package>
<package name="DFN10-3X3">
</package>
<package name="MPX4250DP">
</package>
<package name="MS4515DO-DS">
</package>
<package name="WSON10">
</package>
<package name="WSON6">
</package>
<package name="X2QFN">
</package>
<package name="CSP6">
</package>
<package name="VQFN24">
</package>
<package name="POWERPAK_1212-8">
</package>
<package name="LQFN24">
</package>
<package name="VQFN16">
</package>
<package name="BMP280">
</package>
<package name="QFN16">
<description>&lt;b&gt;RTE (S-PQFP-N16)&lt;/b&gt; 3x3 mm&lt;p&gt;
Source: www.ti.com .. tpa6132a2 direct path stereo $.65.pdf</description>
</package>
<package name="TDFN-10">
</package>
<package name="L2220">
</package>
<package name="SOT23-DBV">
<description>&lt;b&gt;Small Outline Transistor&lt;/b&gt; DBV (R-PDSO-G5)&lt;p&gt;
Source: http://focus.ti.com/lit/ds/symlink/tps77001.pdf</description>
</package>
<package name="POWERPAK_SO-8_SINGLE">
</package>
<package name="LQFP100_14X14">
<description>&lt;b&gt;LQFP100_PACKAGE&lt;/b&gt;&lt;p&gt;
Auto generated by &lt;i&gt;make-symbol-device-package-bsdl.ulp Rev. 44&lt;/i&gt;&lt;br&gt;</description>
</package>
<package name="EX-QFN-12">
</package>
<package name="LQFP176">
<description>&lt;b&gt;176-Lead Metric Thin Plastic Quad Flatpack&lt;/b&gt;&lt;p&gt;
Source: www.analog.com .. 144127970ADSP_BF531_2_3_a.pdf</description>
</package>
<package name="Q_5032_2P">
</package>
<package name="WSON10_4X4">
</package>
<package name="D2PACK">
<description>&lt;b&gt;D2PACK&lt;/b&gt;&lt;p&gt;
INTERNATIONAL RECTIFIER, irg4bc15ud-s.pdf</description>
</package>
<package name="L12.7X12.7">
<description>&lt;b&gt;INDUCTOR&lt;/b&gt;</description>
</package>
<package name="WSON12_4X4">
</package>
<package name="LPS3008">
<description>&lt;b&gt;INDUCTOR&lt;/b&gt;&lt;br&gt;
Coilcraft - LPS3008 series&lt;br&gt;
Shielded Power Inductor</description>
</package>
<package name="SDR1307">
</package>
<package name="LEAD-QFN24">
</package>
<package name="LQFP144">
<description>&lt;b&gt;LQFP144 - Low Profile Quad Flat Package &lt;/b&gt;&lt;p&gt; SOT459-1</description>
</package>
</packages>
<symbols>
<symbol name="MCP3208">
<description>MCP3208

8 channel ADC</description>
<pin name="CH0"/>
<pin name="CH1"/>
<pin name="CH2"/>
<pin name="CH3"/>
<pin name="CH4"/>
<pin name="CH5"/>
<pin name="CH6"/>
<pin name="CH7"/>
<pin name="DGND"/>
<pin name="AGND"/>
<pin name="VCC"/>
<pin name="V_REF"/>
<pin name="MOSI"/>
<pin name="MISO"/>
<pin name="SCK"/>
<pin name="CS" function="dot"/>
</symbol>
<symbol name="MOSFET-P">
<pin name="S"/>
<pin name="D"/>
<pin name="G" direction="in"/>
</symbol>
<symbol name="MOSFET-N">
<pin name="S"/>
<pin name="D"/>
<pin name="G" direction="in"/>
</symbol>
<symbol name="SWITCH">
<pin name="P1"/>
<pin name="P2"/>
</symbol>
<symbol name="CD54HC107">
<pin name="K1"/>
<pin name="~Q1" function="dot"/>
<pin name="CLK1" function="dot"/>
<pin name="J1"/>
<pin name="R1" function="dot"/>
<pin name="Q1"/>
<pin name="VCC"/>
<pin name="GND"/>
<pin name="K2"/>
<pin name="CLK2" function="dot"/>
<pin name="J2"/>
<pin name="R2" function="dot"/>
<pin name="~Q2" function="dot"/>
<pin name="Q2"/>
</symbol>
<symbol name="NOT">
<pin name="~X"/>
<pin name="X"/>
<pin name="VCC"/>
<pin name="GND"/>
</symbol>
<symbol name="LM1117">
<pin name="VI"/>
<pin name="VO"/>
<pin name="GND"/>
</symbol>
<symbol name="LM4040">
<pin name="CATHODE"/>
<pin name="ANODE"/>
</symbol>
<symbol name="OP_AMP">
<pin name="VS+"/>
<pin name="VS-"/>
<pin name="V+"/>
<pin name="V-"/>
<pin name="VOUT"/>
</symbol>
<symbol name="FULL_BRIDGET_RECTIFIER">
<pin name="AC1"/>
<pin name="AC2"/>
<pin name="GND"/>
<pin name="VCC"/>
</symbol>
<symbol name="STBC08">
<pin name="VCC"/>
<pin name="CHRG"/>
<pin name="PWR"/>
<pin name="GND"/>
<pin name="PROG"/>
<pin name="BAT"/>
</symbol>
<symbol name="STM32L062K8">
<pin name="PA3"/>
<pin name="PA4"/>
<pin name="PA5"/>
<pin name="PA6"/>
<pin name="PA7"/>
<pin name="PB0"/>
<pin name="PB1"/>
<pin name="VDD"/>
<pin name="PC14-OSC_IN"/>
<pin name="PC15-OSC_OUT"/>
<pin name="NRST"/>
<pin name="VDDA"/>
<pin name="PA0"/>
<pin name="PA1"/>
<pin name="PA2"/>
<pin name="VDD_USB"/>
<pin name="PA14"/>
<pin name="PA13"/>
<pin name="PA12"/>
<pin name="PA11"/>
<pin name="PA10"/>
<pin name="PA9"/>
<pin name="PA8"/>
<pin name="GND"/>
<pin name="BOOT0"/>
<pin name="PB7"/>
<pin name="PB6"/>
<pin name="PB5"/>
<pin name="PB4"/>
</symbol>
<symbol name="SIM808">
<pin name="VBUS"/>
<pin name="MIC1P"/>
<pin name="MIC1N"/>
<pin name="SPK1P"/>
<pin name="RF_SYNC"/>
<pin name="STATUS"/>
<pin name="VBAT"/>
<pin name="GND"/>
<pin name="SPK1N"/>
<pin name="SIM_PRE"/>
<pin name="SIM_CLK"/>
<pin name="SIM_DATA"/>
<pin name="SIM_RST"/>
<pin name="VSIM"/>
<pin name="VRTC"/>
<pin name="ANT_BT"/>
<pin name="GSM_RF_IN"/>
<pin name="VDD_EXT"/>
<pin name="USB_DP"/>
<pin name="USB_DM"/>
<pin name="COL0"/>
<pin name="COL1"/>
<pin name="COL2"/>
<pin name="COL3"/>
<pin name="ROW0"/>
<pin name="ROW1"/>
<pin name="ROW2"/>
<pin name="ROW3"/>
<pin name="NETLIGHT"/>
<pin name="PWM1"/>
<pin name="PCMSYNC"/>
<pin name="GPIO5"/>
<pin name="PCMIN"/>
<pin name="GPIO6"/>
<pin name="PCMCLK"/>
<pin name="PCMOUT"/>
<pin name="CTS"/>
<pin name="RTS"/>
<pin name="TXD"/>
<pin name="RXD"/>
<pin name="UART_DCD"/>
<pin name="UART_DTR"/>
<pin name="UART_RI"/>
<pin name="GPS_RF_IN"/>
<pin name="SDA"/>
<pin name="SCL"/>
<pin name="PWRKEY"/>
<pin name="RESET"/>
<pin name="ADC1"/>
<pin name="ADC2"/>
<pin name="PWM2"/>
<pin name="1PPM"/>
</symbol>
<symbol name="ZENNER_DIODE">
<pin name="P$1"/>
<pin name="P$2"/>
</symbol>
<symbol name="AITHINKER_A7">
<pin name="GPS_RF"/>
<pin name="EAR_R"/>
<pin name="EAR_L"/>
<pin name="MIC2_P"/>
<pin name="MIC+"/>
<pin name="MIC-"/>
<pin name="SIM_DATA"/>
<pin name="VSIM"/>
<pin name="SIM_CLK"/>
<pin name="SIM_RST"/>
<pin name="RST"/>
<pin name="UART_RTS"/>
<pin name="UART_CTS"/>
<pin name="INT"/>
<pin name="PWR_KEY"/>
<pin name="GPIO7"/>
<pin name="GPIO6"/>
<pin name="GPIO14"/>
<pin name="GPIO15"/>
<pin name="GPIO16"/>
<pin name="VBAT"/>
<pin name="GND"/>
<pin name="REC+"/>
<pin name="REC-"/>
<pin name="1V8_OUT"/>
<pin name="GSM_RF"/>
<pin name="UART_RX"/>
<pin name="UART_TX"/>
<pin name="HST_RX"/>
<pin name="HST_TX"/>
<pin name="GPS_TX"/>
<pin name="GPOIO13"/>
</symbol>
<symbol name="L6924U">
<pin name="TH"/>
<pin name="SD"/>
<pin name="GND"/>
<pin name="TPRG"/>
<pin name="ST2"/>
<pin name="ST1"/>
<pin name="VINSNS"/>
<pin name="VIN"/>
<pin name="ISEL"/>
<pin name="VOSNS"/>
<pin name="VOUT"/>
<pin name="VREF"/>
<pin name="IEDN"/>
<pin name="MODE"/>
<pin name="IUSB"/>
<pin name="IAC"/>
</symbol>
<symbol name="SIM868">
<pin name="GPS_VBAT"/>
<pin name="GSM_VBAT"/>
<pin name="VDD_EXT"/>
<pin name="GND"/>
<pin name="PWRKEY"/>
<pin name="MICP"/>
<pin name="MICN"/>
<pin name="SPK1P"/>
<pin name="SPK1N"/>
<pin name="SPK2P"/>
<pin name="SPK2N"/>
<pin name="GPS_RXD"/>
<pin name="GPS_TXD"/>
<pin name="1PPS"/>
<pin name="GPS_EN"/>
<pin name="VRTC"/>
<pin name="MCCA3"/>
<pin name="MCCA2"/>
<pin name="MCCA1"/>
<pin name="MCCA0"/>
<pin name="RF_SYNC"/>
<pin name="GPS_ANT"/>
<pin name="BT_ANT"/>
<pin name="GSM_ANT"/>
<pin name="SIM2_DET"/>
<pin name="SIM2_RST"/>
<pin name="SIM2_CLK"/>
<pin name="SIM2_DATA"/>
<pin name="SIM2_VDD"/>
<pin name="SIM1_DET"/>
<pin name="SIM1_RST"/>
<pin name="SIM1_CLK"/>
<pin name="SIM1_DATA"/>
<pin name="SIM1_VDD"/>
<pin name="SCL"/>
<pin name="SDA"/>
<pin name="ADC"/>
<pin name="USB_DP"/>
<pin name="USB_DM"/>
<pin name="USB_VBUS"/>
<pin name="MCCK"/>
<pin name="MCCM0"/>
<pin name="NETLIGHT"/>
<pin name="STATUS"/>
<pin name="GPIO1"/>
<pin name="GPIO2"/>
<pin name="UART1_DTR"/>
<pin name="UART1_RI"/>
<pin name="UART1_DCD"/>
<pin name="UART1_CTS"/>
<pin name="UART1_RTS"/>
<pin name="UART1_TXD"/>
<pin name="UART1_RXD"/>
<pin name="UART2_TXD"/>
<pin name="UART2_RXD"/>
</symbol>
<symbol name="SIM28">
<pin name="TM"/>
<pin name="SCS"/>
<pin name="EINT0"/>
<pin name="RF_IN"/>
<pin name="VCC"/>
<pin name="VBKP"/>
<pin name="RXD"/>
<pin name="VCC_RF"/>
<pin name="GND"/>
<pin name="SCL"/>
<pin name="SDA"/>
<pin name="GPIO0"/>
<pin name="SCK"/>
<pin name="MISO"/>
<pin name="MOSI"/>
<pin name="TXD"/>
</symbol>
<symbol name="FT232R">
<pin name="3V3OUT"/>
<pin name="OSCO"/>
<pin name="OSCI"/>
<pin name="USBDP"/>
<pin name="USBDM"/>
<pin name="VCC"/>
<pin name="VCCIO"/>
<pin name="AGND"/>
<pin name="GND"/>
<pin name="TEST"/>
<pin name="TXD"/>
<pin name="RXD"/>
<pin name="RTS"/>
<pin name="CTS"/>
<pin name="DTR"/>
<pin name="DSR"/>
<pin name="DCD"/>
<pin name="RI"/>
<pin name="CBUS0"/>
<pin name="CBUS1"/>
<pin name="CBUS2"/>
<pin name="CBUS3"/>
<pin name="CBUS4"/>
</symbol>
<symbol name="STM32F103C8">
<pin name="PB0"/>
<pin name="PA7"/>
<pin name="PA6"/>
<pin name="PA5"/>
<pin name="PA4"/>
<pin name="PA3"/>
<pin name="PA2"/>
<pin name="PA1"/>
<pin name="PA0"/>
<pin name="GND"/>
<pin name="GNDA"/>
<pin name="VCC"/>
<pin name="VBAT"/>
<pin name="PC13"/>
<pin name="PC14"/>
<pin name="PC15"/>
<pin name="OSC_IN"/>
<pin name="OSC_OUT"/>
<pin name="NRST"/>
<pin name="VCCA"/>
<pin name="PB1"/>
<pin name="PB2"/>
<pin name="PB10"/>
<pin name="PB11"/>
<pin name="PB12"/>
<pin name="PB13"/>
<pin name="PB14"/>
<pin name="PB15"/>
<pin name="PA8"/>
<pin name="PA9"/>
<pin name="PA10"/>
<pin name="PA11"/>
<pin name="PA12"/>
<pin name="PA13"/>
<pin name="PA14"/>
<pin name="PA15"/>
<pin name="PB3"/>
<pin name="PB4"/>
<pin name="PB5"/>
<pin name="PB6"/>
<pin name="PB7"/>
<pin name="BOOT"/>
<pin name="PB8"/>
<pin name="PB9"/>
</symbol>
<symbol name="M61T81">
<pin name="XO"/>
<pin name="SCL"/>
<pin name="SDA"/>
<pin name="GND"/>
<pin name="VCC"/>
<pin name="VBAT"/>
<pin name="XI"/>
<pin name="IRQ"/>
</symbol>
<symbol name="HD7-K2">
<pin name="G1" direction="pas"/>
<pin name="F1" direction="pas"/>
<pin name="D1" direction="pas"/>
<pin name="B1" direction="pas"/>
<pin name="A1" direction="pas"/>
<pin name="CC1" direction="pas"/>
<pin name="C1" direction="pas"/>
<pin name="E1" direction="pas"/>
<pin name="DP1" direction="pas"/>
<pin name="G2" direction="pas"/>
<pin name="F2" direction="pas"/>
<pin name="D2" direction="pas"/>
<pin name="B2" direction="pas"/>
<pin name="A2" direction="pas"/>
<pin name="CC2" direction="pas"/>
<pin name="C2" direction="pas"/>
<pin name="E2" direction="pas"/>
<pin name="DP2" direction="pas"/>
</symbol>
<symbol name="1V2+2">
<pin name="+" direction="pas"/>
<pin name="-" direction="pas"/>
<pin name="+@1" direction="pas"/>
</symbol>
<symbol name="POTENTIOMETER">
<pin name="A"/>
<pin name="E"/>
<pin name="S"/>
</symbol>
<symbol name="OPD-D391">
<pin name="P" direction="pas"/>
<pin name="G" direction="pas"/>
<pin name="E" direction="pas"/>
<pin name="C" direction="pas"/>
<pin name="B" direction="pas"/>
<pin name="CC1" direction="pas"/>
<pin name="D" direction="pas"/>
<pin name="F" direction="pas"/>
<pin name="A" direction="pas"/>
<pin name="CC2" direction="pas"/>
</symbol>
<symbol name="L-US">
<pin name="2" direction="pas"/>
<pin name="1" direction="pas"/>
</symbol>
<symbol name="TVS_DIODE_BID">
<pin name="P$1"/>
<pin name="P$2"/>
</symbol>
<symbol name="MOSFET-P_DIODE">
<pin name="S"/>
<pin name="D"/>
<pin name="G" direction="in"/>
</symbol>
<symbol name="STM32F405RG">
<pin name="PB0"/>
<pin name="PA7"/>
<pin name="PA6"/>
<pin name="PA5"/>
<pin name="PA4"/>
<pin name="PA3"/>
<pin name="PA2"/>
<pin name="PA1"/>
<pin name="PA0"/>
<pin name="GND"/>
<pin name="GNDA"/>
<pin name="VCC"/>
<pin name="VBAT"/>
<pin name="PC13"/>
<pin name="PC14"/>
<pin name="PC15"/>
<pin name="OSC_IN"/>
<pin name="OSC_OUT"/>
<pin name="NRST"/>
<pin name="VCCA"/>
<pin name="PB1"/>
<pin name="PB2"/>
<pin name="PB10"/>
<pin name="PB12"/>
<pin name="PB13"/>
<pin name="PB14"/>
<pin name="PB15"/>
<pin name="PA8"/>
<pin name="PA9"/>
<pin name="PA10"/>
<pin name="PA11"/>
<pin name="PA12"/>
<pin name="PA13"/>
<pin name="PA14"/>
<pin name="PA15"/>
<pin name="PB3"/>
<pin name="PB4"/>
<pin name="PB5"/>
<pin name="PB6"/>
<pin name="PB7"/>
<pin name="BOOT"/>
<pin name="PB8"/>
<pin name="PB9"/>
<pin name="VCAP1"/>
<pin name="PC3"/>
<pin name="PC2"/>
<pin name="PC1"/>
<pin name="PC0"/>
<pin name="PC4"/>
<pin name="PC5"/>
<pin name="PC6"/>
<pin name="PC7"/>
<pin name="PC8"/>
<pin name="PC9"/>
<pin name="PC10"/>
<pin name="PC11"/>
<pin name="PC12"/>
<pin name="PD2"/>
</symbol>
<symbol name="TPS6303X">
<pin name="L1"/>
<pin name="VIN"/>
<pin name="VINA"/>
<pin name="EN"/>
<pin name="PS/SYNC"/>
<pin name="GND"/>
<pin name="VOUT"/>
<pin name="L2"/>
<pin name="FB"/>
<pin name="PGND"/>
</symbol>
<symbol name="STM32F103RG">
<pin name="PB0"/>
<pin name="PA7"/>
<pin name="PA6"/>
<pin name="PA5"/>
<pin name="PA4"/>
<pin name="PA3"/>
<pin name="PA2"/>
<pin name="PA1"/>
<pin name="PA0"/>
<pin name="GND"/>
<pin name="GNDA"/>
<pin name="VCC"/>
<pin name="VBAT"/>
<pin name="PC13"/>
<pin name="PC14"/>
<pin name="PC15"/>
<pin name="OSC_IN"/>
<pin name="OSC_OUT"/>
<pin name="NRST"/>
<pin name="VCCA"/>
<pin name="PB1"/>
<pin name="PB2"/>
<pin name="PB10"/>
<pin name="PB11"/>
<pin name="PB12"/>
<pin name="PB13"/>
<pin name="PB14"/>
<pin name="PB15"/>
<pin name="PA8"/>
<pin name="PA9"/>
<pin name="PA10"/>
<pin name="PA11"/>
<pin name="PA12"/>
<pin name="SWDIO"/>
<pin name="SWCLK"/>
<pin name="PA15"/>
<pin name="PB3"/>
<pin name="PB4"/>
<pin name="PB5"/>
<pin name="PB6"/>
<pin name="PB7"/>
<pin name="BOOT"/>
<pin name="PB8"/>
<pin name="PB9"/>
<pin name="PC0"/>
<pin name="PC1"/>
<pin name="PC2"/>
<pin name="PC3"/>
<pin name="PC4"/>
<pin name="PC5"/>
<pin name="PC6"/>
<pin name="PC7"/>
<pin name="PC8"/>
<pin name="PC9"/>
<pin name="PC10"/>
<pin name="PC11"/>
<pin name="PC12"/>
<pin name="PD2"/>
</symbol>
<symbol name="MCP4725">
<pin name="GND"/>
<pin name="VCC"/>
<pin name="VOUT"/>
<pin name="A0"/>
<pin name="SCL"/>
<pin name="SDA"/>
</symbol>
<symbol name="A3901">
<pin name="IN1"/>
<pin name="IN2"/>
<pin name="IN3"/>
<pin name="IN4"/>
<pin name="GND"/>
<pin name="PAD"/>
<pin name="OUT1"/>
<pin name="OUT2"/>
<pin name="OUT3"/>
<pin name="OUT4"/>
<pin name="VCC"/>
</symbol>
<symbol name="STM32L151CB">
<pin name="VLCD"/>
<pin name="VDD"/>
<pin name="VDDA"/>
<pin name="GNDA"/>
<pin name="PA0"/>
<pin name="PA1"/>
<pin name="PA2"/>
<pin name="PA3"/>
<pin name="PA4"/>
<pin name="PA5"/>
<pin name="PA6"/>
<pin name="PA7"/>
<pin name="PA8"/>
<pin name="PA9"/>
<pin name="PA10"/>
<pin name="PA11"/>
<pin name="PA12"/>
<pin name="PA13/SWDIO"/>
<pin name="PA14/SWCLK"/>
<pin name="PA15"/>
<pin name="PB0"/>
<pin name="PB1"/>
<pin name="PB2"/>
<pin name="PB3"/>
<pin name="PB4"/>
<pin name="PB5"/>
<pin name="PB6"/>
<pin name="PB7"/>
<pin name="PB8"/>
<pin name="PB9"/>
<pin name="PB10"/>
<pin name="PB11"/>
<pin name="PB12"/>
<pin name="PB13"/>
<pin name="PB14"/>
<pin name="PB15"/>
<pin name="PC13"/>
<pin name="PC14"/>
<pin name="PC15"/>
<pin name="OSC_IN"/>
<pin name="OSC_OUT"/>
<pin name="NRST"/>
<pin name="BOOT0"/>
<pin name="GND"/>
</symbol>
<symbol name="MS4515DO">
<pin name="SCL/SCK"/>
<pin name="SDA/MISO"/>
<pin name="INT/SS"/>
<pin name="VCC"/>
<pin name="GND"/>
</symbol>
<symbol name="MPX4250">
<pin name="VOUT"/>
<pin name="VCC"/>
<pin name="GND"/>
</symbol>
<symbol name="BQ25071-Q1">
<description>LiFePO4, Single-Cell charger</description>
<pin name="IN"/>
<pin name="ISET"/>
<pin name="CHG"/>
<pin name="EN"/>
<pin name="BAT"/>
<pin name="OUT"/>
<pin name="TS"/>
<pin name="LDO"/>
<pin name="GND"/>
</symbol>
<symbol name="BQ2980">
<description>BQ2980xy Voltage, Current, Temperature Protectors with an Integrated High-Side NFET
Driver for Fast/Flash Charging Single-Cell Li-Ion and Li-Polymer Batteries</description>
<pin name="VSS"/>
<pin name="VDD"/>
<pin name="PACK"/>
<pin name="DSG"/>
<pin name="CHG"/>
<pin name="CTR"/>
<pin name="BAT"/>
<pin name="CS"/>
</symbol>
<symbol name="EFC8811R">
<description>&lt;b&gt;Power MOSFET&lt;/b&gt;&lt;br/&gt;
for 1-Cell Lithium-ion Battery Protection&lt;br/&gt;
12V, 3m2R, 27A, Dual N-Channel</description>
<pin name="S1"/>
<pin name="S2"/>
<pin name="G2"/>
<pin name="G1"/>
</symbol>
<symbol name="MCP1727">
<pin name="VIN"/>
<pin name="VOUT"/>
<pin name="SENSE"/>
<pin name="CDEL"/>
<pin name="PWRGD"/>
<pin name="SHDN"/>
<pin name="GND"/>
</symbol>
<symbol name="BQ24630">
<pin name="ACDRV"/>
<pin name="ISET1"/>
<pin name="ISET2"/>
<pin name="ACSET"/>
<pin name="VREF"/>
<pin name="CE"/>
<pin name="STAT1"/>
<pin name="STAT2"/>
<pin name="PG"/>
<pin name="TS"/>
<pin name="ACP"/>
<pin name="ACN"/>
<pin name="SRN"/>
<pin name="SRP"/>
<pin name="GND"/>
<pin name="LODRV"/>
<pin name="REGN"/>
<pin name="BTST"/>
<pin name="PH"/>
<pin name="HIDRV"/>
<pin name="BATDRV"/>
<pin name="VCC"/>
<pin name="VFB"/>
<pin name="TTC"/>
<pin name="PWRPAD"/>
</symbol>
<symbol name="MPU6050">
<pin name="CLKIN"/>
<pin name="AUX_DA"/>
<pin name="AUX_CL"/>
<pin name="VLOGIC"/>
<pin name="AD0"/>
<pin name="REGOUT"/>
<pin name="FSYNC"/>
<pin name="INT"/>
<pin name="VDD"/>
<pin name="GND"/>
<pin name="CLKOUT"/>
<pin name="SCL"/>
<pin name="SDA"/>
<pin name="CPOUT"/>
</symbol>
<symbol name="BMP280">
<pin name="GND"/>
<pin name="VDD"/>
<pin name="VDDIO"/>
<pin name="SCK"/>
<pin name="SDI"/>
<pin name="SDO"/>
<pin name="CSB"/>
</symbol>
<symbol name="BQ24072">
<pin name="TS"/>
<pin name="BAT"/>
<pin name="CE"/>
<pin name="EN2"/>
<pin name="EN1"/>
<pin name="PGOOD"/>
<pin name="GND"/>
<pin name="CHG"/>
<pin name="OUT"/>
<pin name="ILIM"/>
<pin name="IN"/>
<pin name="TMR"/>
<pin name="TD"/>
<pin name="ISET"/>
</symbol>
<symbol name="TSX339">
<pin name="VCC-"/>
<pin name="VCC+"/>
<pin name="IN4+"/>
<pin name="IN4-"/>
<pin name="IN3+"/>
<pin name="IN3-"/>
<pin name="IN2+"/>
<pin name="IN2-"/>
<pin name="IN1+"/>
<pin name="IN1-"/>
<pin name="OUT1"/>
<pin name="OUT2"/>
<pin name="OUT3"/>
<pin name="OUT4"/>
</symbol>
<symbol name="MAX17501">
<pin name="AGND"/>
<pin name="VIN"/>
<pin name="EN/UVLO"/>
<pin name="VCC"/>
<pin name="FB/VO"/>
<pin name="LX"/>
<pin name="GND"/>
<pin name="RESET"/>
<pin name="NC/COMP"/>
<pin name="SS"/>
</symbol>
<symbol name="TPS6217">
<pin name="GND"/>
<pin name="VIN"/>
<pin name="EN"/>
<pin name="FB"/>
<pin name="VOS"/>
<pin name="SW"/>
<pin name="SLEEP"/>
<pin name="PG"/>
<pin name="AGND"/>
</symbol>
<symbol name="TPS736XX">
<pin name="IN"/>
<pin name="OUT"/>
<pin name="GND"/>
<pin name="NR"/>
<pin name="EN"/>
</symbol>
<symbol name="STM321F103V_8_B">
<pin name="PE2"/>
<pin name="PE3"/>
<pin name="PE4"/>
<pin name="PE5"/>
<pin name="PE6"/>
<pin name="VBAT"/>
<pin name="PC13"/>
<pin name="PC14"/>
<pin name="PC15"/>
<pin name="PC0"/>
<pin name="PC1"/>
<pin name="PC2"/>
<pin name="PC3"/>
<pin name="PA0-WKUP"/>
<pin name="PA1"/>
<pin name="PA2"/>
<pin name="PA7"/>
<pin name="PC4"/>
<pin name="PC5"/>
<pin name="PB0"/>
<pin name="PB1"/>
<pin name="PB2/BOOT1"/>
<pin name="PE7"/>
<pin name="PE8"/>
<pin name="PE9"/>
<pin name="PE10"/>
<pin name="PE11"/>
<pin name="VCCA"/>
<pin name="GNDA"/>
<pin name="NRST"/>
<pin name="OSC_IN"/>
<pin name="OSC_OUT"/>
<pin name="PA3"/>
<pin name="PA4"/>
<pin name="PA5"/>
<pin name="PA6"/>
<pin name="VREF+"/>
<pin name="VREF-"/>
<pin name="GND"/>
<pin name="VCC"/>
<pin name="PE12"/>
<pin name="PE13"/>
<pin name="PE14"/>
<pin name="PE15"/>
<pin name="PB10"/>
<pin name="PB11"/>
<pin name="PB12"/>
<pin name="PB13"/>
<pin name="PB14"/>
<pin name="PB15"/>
<pin name="PD8"/>
<pin name="PD9"/>
<pin name="PD10"/>
<pin name="PD11"/>
<pin name="PD12"/>
<pin name="PD13"/>
<pin name="PD14"/>
<pin name="PD15"/>
<pin name="PC6"/>
<pin name="PC7"/>
<pin name="PC8"/>
<pin name="PC9"/>
<pin name="PA8"/>
<pin name="PA9"/>
<pin name="PA10"/>
<pin name="PA11"/>
<pin name="PA12"/>
<pin name="PA13/SWDIO"/>
<pin name="PA14/SWCLK"/>
<pin name="PA15"/>
<pin name="PC10"/>
<pin name="PC11"/>
<pin name="PC12"/>
<pin name="PD0"/>
<pin name="PD1"/>
<pin name="PD2"/>
<pin name="PD3"/>
<pin name="PD4"/>
<pin name="PD5"/>
<pin name="PD6"/>
<pin name="PD7"/>
<pin name="PB3"/>
<pin name="PB4"/>
<pin name="PB5"/>
<pin name="PB6"/>
<pin name="PB7"/>
<pin name="BOOT0"/>
<pin name="PB8"/>
<pin name="PB9"/>
<pin name="PE0"/>
<pin name="PE1"/>
</symbol>
<symbol name="ACS711">
<pin name="IP+"/>
<pin name="IP-"/>
<pin name="GND"/>
<pin name="VCC"/>
<pin name="FAULT"/>
<pin name="VIOUT"/>
</symbol>
<symbol name="STM32F429IGT6">
<pin name="PE2"/>
<pin name="PE3"/>
<pin name="PE4"/>
<pin name="PE5"/>
<pin name="PE6"/>
<pin name="VBAT"/>
<pin name="PI8"/>
<pin name="PC13"/>
<pin name="PC14"/>
<pin name="PC15"/>
<pin name="PI9"/>
<pin name="PI10"/>
<pin name="PI11"/>
<pin name="VCC"/>
<pin name="GND"/>
<pin name="PF0"/>
<pin name="PF1"/>
<pin name="PF2"/>
<pin name="PF3"/>
<pin name="PF4"/>
<pin name="PF5"/>
<pin name="PF6"/>
<pin name="PF7"/>
<pin name="PF8"/>
<pin name="PF9"/>
<pin name="PF10"/>
<pin name="PH0"/>
<pin name="PH1"/>
<pin name="NRST"/>
<pin name="PC0"/>
<pin name="PC1"/>
<pin name="PC2"/>
<pin name="PC3"/>
<pin name="VCCA"/>
<pin name="GNDA"/>
<pin name="VREF+"/>
<pin name="PA0"/>
<pin name="PA1"/>
<pin name="PA2"/>
<pin name="PH2"/>
<pin name="PH3"/>
<pin name="PH4"/>
<pin name="PH5"/>
<pin name="PA3"/>
<pin name="BYPASS_REG"/>
<pin name="PA4"/>
<pin name="PA5"/>
<pin name="PA6"/>
<pin name="PA7"/>
<pin name="PC4"/>
<pin name="PC5"/>
<pin name="PB0"/>
<pin name="PB1"/>
<pin name="PB2"/>
<pin name="PF11"/>
<pin name="PF12"/>
<pin name="PF13"/>
<pin name="PF14"/>
<pin name="PF15"/>
<pin name="PG0"/>
<pin name="PG1"/>
<pin name="PE7"/>
<pin name="PE8"/>
<pin name="PE9"/>
<pin name="PE10"/>
<pin name="PE11"/>
<pin name="PE12"/>
<pin name="PE13"/>
<pin name="PE14"/>
<pin name="PE15"/>
<pin name="PB10"/>
<pin name="PB11"/>
<pin name="VCAP1"/>
<pin name="PH6"/>
<pin name="PH7"/>
<pin name="PH8"/>
<pin name="PH9"/>
<pin name="PH10"/>
<pin name="PH11"/>
<pin name="PH12"/>
<pin name="PB12"/>
<pin name="PB13"/>
<pin name="PB14"/>
<pin name="PB15"/>
<pin name="PD8"/>
<pin name="PD9"/>
<pin name="PD10"/>
<pin name="PD11"/>
<pin name="PD12"/>
<pin name="PD13"/>
<pin name="PD14"/>
<pin name="PD15"/>
<pin name="PG2"/>
<pin name="PG3"/>
<pin name="PG4"/>
<pin name="PG5"/>
<pin name="PG6"/>
<pin name="PG7"/>
<pin name="PG8"/>
<pin name="PC6"/>
<pin name="PC7"/>
<pin name="PC8"/>
<pin name="PC9"/>
<pin name="PA8"/>
<pin name="PA9"/>
<pin name="PA10"/>
<pin name="PA11"/>
<pin name="PA12"/>
<pin name="PA13"/>
<pin name="VCAP2"/>
<pin name="PH13"/>
<pin name="PH14"/>
<pin name="PH15"/>
<pin name="PI0"/>
<pin name="PI1"/>
<pin name="PI2"/>
<pin name="PI3"/>
<pin name="PA14"/>
<pin name="PA15"/>
<pin name="PC10"/>
<pin name="PC11"/>
<pin name="PC12"/>
<pin name="PD0"/>
<pin name="PD1"/>
<pin name="PD2"/>
<pin name="PD3"/>
<pin name="PD4"/>
<pin name="PD5"/>
<pin name="PD6"/>
<pin name="PD7"/>
<pin name="PG9"/>
<pin name="PG10"/>
<pin name="PG11"/>
<pin name="PG12"/>
<pin name="PG13"/>
<pin name="PG14"/>
<pin name="PG15"/>
<pin name="PB3"/>
<pin name="PB4"/>
<pin name="PB5"/>
<pin name="PB6"/>
<pin name="PB7"/>
<pin name="BOOT0"/>
<pin name="PB8"/>
<pin name="PB9"/>
<pin name="PE0"/>
<pin name="PE1"/>
<pin name="PDR_ON"/>
<pin name="PI4"/>
<pin name="PI5"/>
<pin name="PI6"/>
<pin name="PI7"/>
</symbol>
<symbol name="CRYSTAL">
<pin name="2" direction="pas"/>
<pin name="1" direction="pas"/>
</symbol>
<symbol name="SN65HVD23X">
<pin name="D"/>
<pin name="R"/>
<pin name="RS"/>
<pin name="VREF"/>
<pin name="VCC"/>
<pin name="CANL"/>
<pin name="CANH"/>
<pin name="GND"/>
</symbol>
<symbol name="TPS54561">
<pin name="BOOT"/>
<pin name="VIN"/>
<pin name="EN"/>
<pin name="SS/TR"/>
<pin name="RT/CLK"/>
<pin name="FB"/>
<pin name="COMP"/>
<pin name="GND"/>
<pin name="SW"/>
<pin name="PWRGD"/>
</symbol>
<symbol name="POWER_SCHOTTKY_RECTIFIER">
<pin name="K"/>
<pin name="A"/>
</symbol>
<symbol name="FDC2X12">
<pin name="SCL"/>
<pin name="SDA"/>
<pin name="CLKIN"/>
<pin name="ADDR"/>
<pin name="INTB"/>
<pin name="SD"/>
<pin name="VCC"/>
<pin name="GND"/>
<pin name="IN0A"/>
<pin name="IN0B"/>
<pin name="IN1A"/>
<pin name="IN1B"/>
</symbol>
<symbol name="STM32H753VIT_PART1">
<pin name="PA0"/>
<pin name="PA1"/>
<pin name="PA2"/>
<pin name="PA3"/>
<pin name="PA4"/>
<pin name="PA5"/>
<pin name="PA6"/>
<pin name="PA7"/>
<pin name="PB0"/>
<pin name="PB1"/>
<pin name="PB2"/>
<pin name="PB10"/>
<pin name="PB11"/>
<pin name="PB12"/>
<pin name="PB13"/>
<pin name="PB14"/>
<pin name="PB15"/>
<pin name="PA8"/>
<pin name="PA9"/>
<pin name="PA10"/>
<pin name="PA11"/>
<pin name="PA12"/>
<pin name="PA13"/>
<pin name="PA14"/>
<pin name="PA15"/>
<pin name="PB3"/>
<pin name="PB4"/>
<pin name="PB5"/>
<pin name="PB6"/>
<pin name="PB7"/>
<pin name="PB8"/>
<pin name="PB9"/>
</symbol>
<symbol name="STM32H753VIT_PART2">
<pin name="PC13"/>
<pin name="PC14"/>
<pin name="PC15"/>
<pin name="PC0"/>
<pin name="PC1"/>
<pin name="PC2"/>
<pin name="PC3"/>
<pin name="PC4"/>
<pin name="PC5"/>
<pin name="PD8"/>
<pin name="PD9"/>
<pin name="PD10"/>
<pin name="PD11"/>
<pin name="PD12"/>
<pin name="PD13"/>
<pin name="PD14"/>
<pin name="PD15"/>
<pin name="PC6"/>
<pin name="PC7"/>
<pin name="PC8"/>
<pin name="PC9"/>
<pin name="PC10"/>
<pin name="PC11"/>
<pin name="PC12"/>
<pin name="PD0"/>
<pin name="PD1"/>
<pin name="PD2"/>
<pin name="PD3"/>
<pin name="PD4"/>
<pin name="PD5"/>
<pin name="PD6"/>
<pin name="PD7"/>
</symbol>
<symbol name="STM32H753VIT_PART3">
<pin name="PE0"/>
<pin name="PE1"/>
<pin name="PE2"/>
<pin name="PE3"/>
<pin name="PE4"/>
<pin name="PE5"/>
<pin name="PE6"/>
<pin name="PH0"/>
<pin name="PH1"/>
<pin name="PE7"/>
<pin name="PE8"/>
<pin name="PE9"/>
<pin name="PE10"/>
<pin name="PE11"/>
<pin name="PE12"/>
<pin name="PE13"/>
<pin name="PE14"/>
<pin name="PE15"/>
<pin name="BOOT0"/>
<pin name="VCC"/>
<pin name="GND"/>
<pin name="VBAT"/>
<pin name="NRST"/>
<pin name="VCCA"/>
<pin name="GNDA"/>
<pin name="VREF+"/>
<pin name="VCAP"/>
</symbol>
<symbol name="ICM-20948">
<pin name="REGOUT"/>
<pin name="FSYNC"/>
<pin name="INT1"/>
<pin name="VDD"/>
<pin name="GND"/>
<pin name="AUX_DA"/>
<pin name="CS"/>
<pin name="SCL/SCLK"/>
<pin name="SDO/AD0"/>
<pin name="VDDIO"/>
<pin name="AUX_CL"/>
<pin name="SDA/SDI"/>
</symbol>
<symbol name="STM32H753ZIT_PART1">
<pin name="PA0"/>
<pin name="PA1"/>
<pin name="PA2"/>
<pin name="PA3"/>
<pin name="PA4"/>
<pin name="PA5"/>
<pin name="PA6"/>
<pin name="PA7"/>
<pin name="PB0"/>
<pin name="PB1"/>
<pin name="PB2"/>
<pin name="PB10"/>
<pin name="PB11"/>
<pin name="PB12"/>
<pin name="PB13"/>
<pin name="PB14"/>
<pin name="PB15"/>
<pin name="PA8"/>
<pin name="PA9"/>
<pin name="PA10"/>
<pin name="PA11"/>
<pin name="PA12"/>
<pin name="PA13"/>
<pin name="PA14"/>
<pin name="PA15"/>
<pin name="PB3"/>
<pin name="PB4"/>
<pin name="PB5"/>
<pin name="PB6"/>
<pin name="PB7"/>
<pin name="PB8"/>
<pin name="PB9"/>
</symbol>
<symbol name="STM32H753ZIT_PART2">
<pin name="PC13"/>
<pin name="PC14"/>
<pin name="PC15"/>
<pin name="PC0"/>
<pin name="PC1"/>
<pin name="PC2"/>
<pin name="PC3"/>
<pin name="PC4"/>
<pin name="PC5"/>
<pin name="PD8"/>
<pin name="PD9"/>
<pin name="PD10"/>
<pin name="PD11"/>
<pin name="PD12"/>
<pin name="PD13"/>
<pin name="PD14"/>
<pin name="PD15"/>
<pin name="PC6"/>
<pin name="PC7"/>
<pin name="PC8"/>
<pin name="PC9"/>
<pin name="PC10"/>
<pin name="PC11"/>
<pin name="PC12"/>
<pin name="PD0"/>
<pin name="PD1"/>
<pin name="PD2"/>
<pin name="PD3"/>
<pin name="PD4"/>
<pin name="PD5"/>
<pin name="PD6"/>
<pin name="PD7"/>
</symbol>
<symbol name="STM32H753ZIT_PART3">
<pin name="PE0"/>
<pin name="PE1"/>
<pin name="PE2"/>
<pin name="PE3"/>
<pin name="PE4"/>
<pin name="PE5"/>
<pin name="PE6"/>
<pin name="PE7"/>
<pin name="PE8"/>
<pin name="PE9"/>
<pin name="PE10"/>
<pin name="PE11"/>
<pin name="PE12"/>
<pin name="PE13"/>
<pin name="PE14"/>
<pin name="PE15"/>
<pin name="PF0"/>
<pin name="PF1"/>
<pin name="PF2"/>
<pin name="PF3"/>
<pin name="PF4"/>
<pin name="PF5"/>
<pin name="PF6"/>
<pin name="PF7"/>
<pin name="PF8"/>
<pin name="PF9"/>
<pin name="PF10"/>
<pin name="PF11"/>
<pin name="PF12"/>
<pin name="PF13"/>
<pin name="PF14"/>
<pin name="PF15"/>
</symbol>
<symbol name="STM32H753ZIT_PART4">
<pin name="PG0"/>
<pin name="PG1"/>
<pin name="PG2"/>
<pin name="PG3"/>
<pin name="PG4"/>
<pin name="PG5"/>
<pin name="PG6"/>
<pin name="PH0"/>
<pin name="PH1"/>
<pin name="PG7"/>
<pin name="PG8"/>
<pin name="PG9"/>
<pin name="PG10"/>
<pin name="PG11"/>
<pin name="PG12"/>
<pin name="PG13"/>
<pin name="PG14"/>
<pin name="PG15"/>
<pin name="BOOT0"/>
<pin name="VCC"/>
<pin name="GND"/>
<pin name="VBAT"/>
<pin name="NRST"/>
<pin name="VCCA"/>
<pin name="GNDA"/>
<pin name="VREF+"/>
<pin name="VCAP"/>
<pin name="VDD33_USB"/>
<pin name="PDR_ON"/>
</symbol>
</symbols>
<devicesets>
<deviceset name="MCP3208-SOIC16" uservalue="yes">
<description>16 channel PWM driver</description>
<gates>
<gate name="G$1" symbol="MCP3208"/>
</gates>
<devices>
<device name="" package="SOIC16">
<connects>
<connect gate="G$1" pin="AGND" pad="14"/>
<connect gate="G$1" pin="CH0" pad="1"/>
<connect gate="G$1" pin="CH1" pad="2"/>
<connect gate="G$1" pin="CH2" pad="3"/>
<connect gate="G$1" pin="CH3" pad="4"/>
<connect gate="G$1" pin="CH4" pad="5"/>
<connect gate="G$1" pin="CH5" pad="6"/>
<connect gate="G$1" pin="CH6" pad="7"/>
<connect gate="G$1" pin="CH7" pad="8"/>
<connect gate="G$1" pin="CS" pad="10"/>
<connect gate="G$1" pin="DGND" pad="9"/>
<connect gate="G$1" pin="MISO" pad="12"/>
<connect gate="G$1" pin="MOSI" pad="11"/>
<connect gate="G$1" pin="SCK" pad="13"/>
<connect gate="G$1" pin="VCC" pad="16"/>
<connect gate="G$1" pin="V_REF" pad="15"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MOSFET-P" uservalue="yes">
<gates>
<gate name="G$1" symbol="MOSFET-P"/>
</gates>
<devices>
<device name="SOT23" package="SOT23">
<connects>
<connect gate="G$1" pin="D" pad="3"/>
<connect gate="G$1" pin="G" pad="1"/>
<connect gate="G$1" pin="S" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="DFN8" package="DFN8-3X3">
<connects>
<connect gate="G$1" pin="D" pad="5 6 7"/>
<connect gate="G$1" pin="G" pad="8"/>
<connect gate="G$1" pin="S" pad="1 2 3 4 EXP"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="SI7617DN" package="POWERPAK_1212-8">
<connects>
<connect gate="G$1" pin="D" pad="P5 P6 P7 P8 P9"/>
<connect gate="G$1" pin="G" pad="P4"/>
<connect gate="G$1" pin="S" pad="P1 P2 P3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MOSFET-N" uservalue="yes">
<gates>
<gate name="G$1" symbol="MOSFET-N"/>
</gates>
<devices>
<device name="SOT23" package="SOT23">
<connects>
<connect gate="G$1" pin="D" pad="3"/>
<connect gate="G$1" pin="G" pad="1"/>
<connect gate="G$1" pin="S" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="SIS412DN" package="POWERPAK_1212-8">
<connects>
<connect gate="G$1" pin="D" pad="P5 P6 P7 P8 P9"/>
<connect gate="G$1" pin="G" pad="P4"/>
<connect gate="G$1" pin="S" pad="P1 P2 P3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="TO252" package="TO252">
<connects>
<connect gate="G$1" pin="D" pad="P2"/>
<connect gate="G$1" pin="G" pad="P1"/>
<connect gate="G$1" pin="S" pad="P3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="" package="POWERPAK_SO-8_SINGLE">
<connects>
<connect gate="G$1" pin="D" pad="P4"/>
<connect gate="G$1" pin="G" pad="P2"/>
<connect gate="G$1" pin="S" pad="P1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="SWITCH" uservalue="yes">
<gates>
<gate name="G$1" symbol="SWITCH"/>
</gates>
<devices>
<device name="" package="SPST-NO_UP">
<connects>
<connect gate="G$1" pin="P1" pad="P$1"/>
<connect gate="G$1" pin="P2" pad="P$2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="CD54HC107" uservalue="yes">
<description>Double JK flip-flop</description>
<gates>
<gate name="G$1" symbol="CD54HC107"/>
</gates>
<devices>
<device name="" package="SO14">
<connects>
<connect gate="G$1" pin="CLK1" pad="12"/>
<connect gate="G$1" pin="CLK2" pad="9"/>
<connect gate="G$1" pin="GND" pad="7"/>
<connect gate="G$1" pin="J1" pad="1"/>
<connect gate="G$1" pin="J2" pad="8"/>
<connect gate="G$1" pin="K1" pad="4"/>
<connect gate="G$1" pin="K2" pad="11"/>
<connect gate="G$1" pin="Q1" pad="3"/>
<connect gate="G$1" pin="Q2" pad="5"/>
<connect gate="G$1" pin="R1" pad="13"/>
<connect gate="G$1" pin="R2" pad="10"/>
<connect gate="G$1" pin="VCC" pad="14"/>
<connect gate="G$1" pin="~Q1" pad="2"/>
<connect gate="G$1" pin="~Q2" pad="6"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM1117">
<description>LDO Regulator</description>
<gates>
<gate name="G$1" symbol="LM1117"/>
</gates>
<devices>
<device name="SOT223" package="SOT223">
<connects>
<connect gate="G$1" pin="GND" pad="1"/>
<connect gate="G$1" pin="VI" pad="3"/>
<connect gate="G$1" pin="VO" pad="2 4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="TO220H" package="TO220H">
<connects>
<connect gate="G$1" pin="GND" pad="2"/>
<connect gate="G$1" pin="VI" pad="1"/>
<connect gate="G$1" pin="VO" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="TO252" package="TO252">
<connects>
<connect gate="G$1" pin="GND" pad="P1"/>
<connect gate="G$1" pin="VI" pad="P3"/>
<connect gate="G$1" pin="VO" pad="P2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="" package="SOT23">
<connects>
<connect gate="G$1" pin="GND" pad="1"/>
<connect gate="G$1" pin="VI" pad="3"/>
<connect gate="G$1" pin="VO" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM4040">
<description>Shunt Voltage Reference
&lt;p&gt;
Fixed reverse breakdown voltages of:&lt;/br&gt;
2.048 V, 2.5 V, 3 V, 4.096 V, 5 V, 8.192 V, and 10 V
&lt;/p&gt;</description>
<gates>
<gate name="G$1" symbol="LM4040"/>
</gates>
<devices>
<device name="" package="SOT23">
<connects>
<connect gate="G$1" pin="ANODE" pad="2"/>
<connect gate="G$1" pin="CATHODE" pad="1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LMC7101">
<description>Low-Power Operational Amplifier
&lt;p&gt;1-MHz Gain Bandwidth&lt;br/&gt;Similar to Popular LMC6482 and LMC6484&lt;/p&gt;</description>
<gates>
<gate name="G$1" symbol="OP_AMP"/>
</gates>
<devices>
<device name="" package="SOT23-5">
<connects>
<connect gate="G$1" pin="V+" pad="3"/>
<connect gate="G$1" pin="V-" pad="4"/>
<connect gate="G$1" pin="VOUT" pad="1"/>
<connect gate="G$1" pin="VS+" pad="2"/>
<connect gate="G$1" pin="VS-" pad="5"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="NC7S14" uservalue="yes">
<description>NOT Gate
&lt;p&gt;ON Semiconductor&lt;br&gt;
Single high performance CMOS Inverter
with Schmitt Trigger input.&lt;/p&gt;</description>
<gates>
<gate name="G$1" symbol="NOT"/>
</gates>
<devices>
<device name="" package="SOT23-5">
<connects>
<connect gate="G$1" pin="GND" pad="3"/>
<connect gate="G$1" pin="VCC" pad="5"/>
<connect gate="G$1" pin="X" pad="2"/>
<connect gate="G$1" pin="~X" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="STBC08">
<gates>
<gate name="G$1" symbol="STBC08"/>
</gates>
<devices>
<device name="" package="DFN6-3X3">
<connects>
<connect gate="G$1" pin="BAT" pad="P1"/>
<connect gate="G$1" pin="CHRG" pad="P3"/>
<connect gate="G$1" pin="GND" pad="P4"/>
<connect gate="G$1" pin="PROG" pad="P5"/>
<connect gate="G$1" pin="PWR" pad="P2"/>
<connect gate="G$1" pin="VCC" pad="P6"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="STM32L062K8">
<gates>
<gate name="G$1" symbol="STM32L062K8"/>
</gates>
<devices>
<device name="" package="UFQFPN32">
<connects>
<connect gate="G$1" pin="BOOT0" pad="30"/>
<connect gate="G$1" pin="GND" pad="4 16 31 EXP"/>
<connect gate="G$1" pin="NRST" pad="3"/>
<connect gate="G$1" pin="PA0" pad="6"/>
<connect gate="G$1" pin="PA1" pad="7"/>
<connect gate="G$1" pin="PA10" pad="20"/>
<connect gate="G$1" pin="PA11" pad="21"/>
<connect gate="G$1" pin="PA12" pad="22"/>
<connect gate="G$1" pin="PA13" pad="23"/>
<connect gate="G$1" pin="PA14" pad="25"/>
<connect gate="G$1" pin="PA2" pad="8"/>
<connect gate="G$1" pin="PA3" pad="9"/>
<connect gate="G$1" pin="PA4" pad="10"/>
<connect gate="G$1" pin="PA5" pad="11"/>
<connect gate="G$1" pin="PA6" pad="12"/>
<connect gate="G$1" pin="PA7" pad="13"/>
<connect gate="G$1" pin="PA8" pad="18"/>
<connect gate="G$1" pin="PA9" pad="19"/>
<connect gate="G$1" pin="PB0" pad="14"/>
<connect gate="G$1" pin="PB1" pad="15"/>
<connect gate="G$1" pin="PB4" pad="26"/>
<connect gate="G$1" pin="PB5" pad="27"/>
<connect gate="G$1" pin="PB6" pad="28"/>
<connect gate="G$1" pin="PB7" pad="29"/>
<connect gate="G$1" pin="PC14-OSC_IN" pad="1"/>
<connect gate="G$1" pin="PC15-OSC_OUT" pad="2"/>
<connect gate="G$1" pin="VDD" pad="17 32"/>
<connect gate="G$1" pin="VDDA" pad="5"/>
<connect gate="G$1" pin="VDD_USB" pad="24"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="SIM808">
<description>Simcomm GPRS + GPS module</description>
<gates>
<gate name="G$1" symbol="SIM808"/>
</gates>
<devices>
<device name="" package="SIM808">
<connects>
<connect gate="G$1" pin="1PPM" pad="P37"/>
<connect gate="G$1" pin="ADC1" pad="P23"/>
<connect gate="G$1" pin="ADC2" pad="P24"/>
<connect gate="G$1" pin="ANT_BT" pad="P53"/>
<connect gate="G$1" pin="COL0" pad="P62"/>
<connect gate="G$1" pin="COL1" pad="P61"/>
<connect gate="G$1" pin="COL2" pad="P60"/>
<connect gate="G$1" pin="COL3" pad="P59"/>
<connect gate="G$1" pin="CTS" pad="P12"/>
<connect gate="G$1" pin="GND" pad="P1 P2 P3 P18 P28 P34 P36 P40 P51 P52 P54 P64 P65 P67 P68"/>
<connect gate="G$1" pin="GPIO5" pad="P43"/>
<connect gate="G$1" pin="GPIO6" pad="P44"/>
<connect gate="G$1" pin="GPS_RF_IN" pad="P35"/>
<connect gate="G$1" pin="GSM_RF_IN" pad="P66"/>
<connect gate="G$1" pin="MIC1N" pad="P20"/>
<connect gate="G$1" pin="MIC1P" pad="P19"/>
<connect gate="G$1" pin="NETLIGHT" pad="P50"/>
<connect gate="G$1" pin="PCMCLK" pad="P46"/>
<connect gate="G$1" pin="PCMIN" pad="P47"/>
<connect gate="G$1" pin="PCMOUT" pad="P48"/>
<connect gate="G$1" pin="PCMSYNC" pad="P45"/>
<connect gate="G$1" pin="PWM1" pad="P42"/>
<connect gate="G$1" pin="PWM2" pad="P41"/>
<connect gate="G$1" pin="PWRKEY" pad="P8"/>
<connect gate="G$1" pin="RESET" pad="P16"/>
<connect gate="G$1" pin="RF_SYNC" pad="P63"/>
<connect gate="G$1" pin="ROW0" pad="P58"/>
<connect gate="G$1" pin="ROW1" pad="P57"/>
<connect gate="G$1" pin="ROW2" pad="P56"/>
<connect gate="G$1" pin="ROW3" pad="P55"/>
<connect gate="G$1" pin="RTS" pad="P13"/>
<connect gate="G$1" pin="RXD" pad="P15"/>
<connect gate="G$1" pin="SCL" pad="P39"/>
<connect gate="G$1" pin="SDA" pad="P38"/>
<connect gate="G$1" pin="SIM_CLK" pad="P31"/>
<connect gate="G$1" pin="SIM_DATA" pad="P30"/>
<connect gate="G$1" pin="SIM_PRE" pad="P33"/>
<connect gate="G$1" pin="SIM_RST" pad="P32"/>
<connect gate="G$1" pin="SPK1N" pad="P22"/>
<connect gate="G$1" pin="SPK1P" pad="P21"/>
<connect gate="G$1" pin="STATUS" pad="P49"/>
<connect gate="G$1" pin="TXD" pad="P14"/>
<connect gate="G$1" pin="UART_DCD" pad="P11"/>
<connect gate="G$1" pin="UART_DTR" pad="P9"/>
<connect gate="G$1" pin="UART_RI" pad="P10"/>
<connect gate="G$1" pin="USB_DM" pad="P27"/>
<connect gate="G$1" pin="USB_DP" pad="P26"/>
<connect gate="G$1" pin="VBAT" pad="P4 P5 P6"/>
<connect gate="G$1" pin="VBUS" pad="P25"/>
<connect gate="G$1" pin="VDD_EXT" pad="P7"/>
<connect gate="G$1" pin="VRTC" pad="P17"/>
<connect gate="G$1" pin="VSIM" pad="P29"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ZENNER_DIODE" prefix="D">
<gates>
<gate name="G$1" symbol="ZENNER_DIODE"/>
</gates>
<devices>
<device name="" package="MICRO_MELF">
<connects>
<connect gate="G$1" pin="P$1" pad="P1"/>
<connect gate="G$1" pin="P$2" pad="P2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="AITHINKER_A7">
<description>GPS + GPRS module</description>
<gates>
<gate name="G$1" symbol="AITHINKER_A7"/>
</gates>
<devices>
<device name="" package="AITHINKER">
<connects>
<connect gate="G$1" pin="1V8_OUT" pad="P29"/>
<connect gate="G$1" pin="EAR_L" pad="P23"/>
<connect gate="G$1" pin="EAR_R" pad="P24"/>
<connect gate="G$1" pin="GND" pad="P2 P13 P18 P22 P25 P28 P34 P36 P39 P40"/>
<connect gate="G$1" pin="GPIO14" pad="P5"/>
<connect gate="G$1" pin="GPIO15" pad="P4"/>
<connect gate="G$1" pin="GPIO16" pad="P3"/>
<connect gate="G$1" pin="GPIO6" pad="P6"/>
<connect gate="G$1" pin="GPIO7" pad="P7"/>
<connect gate="G$1" pin="GPOIO13" pad="P38"/>
<connect gate="G$1" pin="GPS_RF" pad="P1"/>
<connect gate="G$1" pin="GPS_TX" pad="P37"/>
<connect gate="G$1" pin="GSM_RF" pad="P35"/>
<connect gate="G$1" pin="HST_RX" pad="P32"/>
<connect gate="G$1" pin="HST_TX" pad="P33"/>
<connect gate="G$1" pin="INT" pad="P9"/>
<connect gate="G$1" pin="MIC+" pad="P20"/>
<connect gate="G$1" pin="MIC-" pad="P19"/>
<connect gate="G$1" pin="MIC2_P" pad="P21"/>
<connect gate="G$1" pin="PWR_KEY" pad="P8"/>
<connect gate="G$1" pin="REC+" pad="P26"/>
<connect gate="G$1" pin="REC-" pad="P27"/>
<connect gate="G$1" pin="RST" pad="P12"/>
<connect gate="G$1" pin="SIM_CLK" pad="P15"/>
<connect gate="G$1" pin="SIM_DATA" pad="P17"/>
<connect gate="G$1" pin="SIM_RST" pad="P14"/>
<connect gate="G$1" pin="UART_CTS" pad="P10"/>
<connect gate="G$1" pin="UART_RTS" pad="P11"/>
<connect gate="G$1" pin="UART_RX" pad="P31"/>
<connect gate="G$1" pin="UART_TX" pad="P30"/>
<connect gate="G$1" pin="VBAT" pad="P41 P42"/>
<connect gate="G$1" pin="VSIM" pad="P16"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="L6924U">
<description>Li-Pol, Li-Ion USB/AC charger</description>
<gates>
<gate name="G$1" symbol="L6924U"/>
</gates>
<devices>
<device name="" package="VFQFPN16">
<connects>
<connect gate="G$1" pin="GND" pad="P$1 P6"/>
<connect gate="G$1" pin="IAC" pad="P16"/>
<connect gate="G$1" pin="IEDN" pad="P13"/>
<connect gate="G$1" pin="ISEL" pad="P9"/>
<connect gate="G$1" pin="IUSB" pad="P15"/>
<connect gate="G$1" pin="MODE" pad="P14"/>
<connect gate="G$1" pin="SD" pad="P7"/>
<connect gate="G$1" pin="ST1" pad="P4"/>
<connect gate="G$1" pin="ST2" pad="P3"/>
<connect gate="G$1" pin="TH" pad="P8"/>
<connect gate="G$1" pin="TPRG" pad="P5"/>
<connect gate="G$1" pin="VIN" pad="P1"/>
<connect gate="G$1" pin="VINSNS" pad="P2"/>
<connect gate="G$1" pin="VOSNS" pad="P10"/>
<connect gate="G$1" pin="VOUT" pad="P11"/>
<connect gate="G$1" pin="VREF" pad="P12"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="SIM868">
<description>Simcomm GPRS + GPS module</description>
<gates>
<gate name="G$1" symbol="SIM868"/>
</gates>
<devices>
<device name="" package="SIM868">
<connects>
<connect gate="G$1" pin="1PPS" pad="P60"/>
<connect gate="G$1" pin="ADC" pad="P38"/>
<connect gate="G$1" pin="BT_ANT" pad="P20"/>
<connect gate="G$1" pin="GND" pad="P8 P13 P19 P21 P27 P30 P31 P33 P36 P37 P45 P63 P66 P67 P69 P70 P71 P72 P73 P74 P75 P76 P77"/>
<connect gate="G$1" pin="GPIO1" pad="P57"/>
<connect gate="G$1" pin="GPIO2" pad="P58"/>
<connect gate="G$1" pin="GPS_ANT" pad="P68"/>
<connect gate="G$1" pin="GPS_EN" pad="P59"/>
<connect gate="G$1" pin="GPS_RXD" pad="P62"/>
<connect gate="G$1" pin="GPS_TXD" pad="P61"/>
<connect gate="G$1" pin="GPS_VBAT" pad="P34"/>
<connect gate="G$1" pin="GSM_ANT" pad="P32"/>
<connect gate="G$1" pin="GSM_VBAT" pad="P35"/>
<connect gate="G$1" pin="MCCA0" pad="P49"/>
<connect gate="G$1" pin="MCCA1" pad="P48"/>
<connect gate="G$1" pin="MCCA2" pad="P47"/>
<connect gate="G$1" pin="MCCA3" pad="P46"/>
<connect gate="G$1" pin="MCCK" pad="P50"/>
<connect gate="G$1" pin="MCCM0" pad="P51"/>
<connect gate="G$1" pin="MICN" pad="P10"/>
<connect gate="G$1" pin="MICP" pad="P9"/>
<connect gate="G$1" pin="NETLIGHT" pad="P41"/>
<connect gate="G$1" pin="PWRKEY" pad="P39"/>
<connect gate="G$1" pin="RF_SYNC" pad="P29"/>
<connect gate="G$1" pin="SCL" pad="P65"/>
<connect gate="G$1" pin="SDA" pad="P64"/>
<connect gate="G$1" pin="SIM1_CLK" pad="P16"/>
<connect gate="G$1" pin="SIM1_DATA" pad="P15"/>
<connect gate="G$1" pin="SIM1_DET" pad="P14"/>
<connect gate="G$1" pin="SIM1_RST" pad="P17"/>
<connect gate="G$1" pin="SIM1_VDD" pad="P18"/>
<connect gate="G$1" pin="SIM2_CLK" pad="P54"/>
<connect gate="G$1" pin="SIM2_DATA" pad="P53"/>
<connect gate="G$1" pin="SIM2_DET" pad="P52"/>
<connect gate="G$1" pin="SIM2_RST" pad="P55"/>
<connect gate="G$1" pin="SIM2_VDD" pad="P56"/>
<connect gate="G$1" pin="SPK1N" pad="P12"/>
<connect gate="G$1" pin="SPK1P" pad="P11"/>
<connect gate="G$1" pin="SPK2N" pad="P43"/>
<connect gate="G$1" pin="SPK2P" pad="P44"/>
<connect gate="G$1" pin="STATUS" pad="P42"/>
<connect gate="G$1" pin="UART1_CTS" pad="P4"/>
<connect gate="G$1" pin="UART1_DCD" pad="P5"/>
<connect gate="G$1" pin="UART1_DTR" pad="P6"/>
<connect gate="G$1" pin="UART1_RI" pad="P7"/>
<connect gate="G$1" pin="UART1_RTS" pad="P3"/>
<connect gate="G$1" pin="UART1_RXD" pad="P2"/>
<connect gate="G$1" pin="UART1_TXD" pad="P1"/>
<connect gate="G$1" pin="UART2_RXD" pad="P23"/>
<connect gate="G$1" pin="UART2_TXD" pad="P22"/>
<connect gate="G$1" pin="USB_DM" pad="P26"/>
<connect gate="G$1" pin="USB_DP" pad="P25"/>
<connect gate="G$1" pin="USB_VBUS" pad="P24"/>
<connect gate="G$1" pin="VDD_EXT" pad="P40"/>
<connect gate="G$1" pin="VRTC" pad="P28"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="SIM28">
<description>Simcomm GPS module</description>
<gates>
<gate name="G$1" symbol="SIM28"/>
</gates>
<devices>
<device name="" package="SIM28">
<connects>
<connect gate="G$1" pin="EINT0" pad="P4"/>
<connect gate="G$1" pin="GND" pad="P10 P12 P13 P24"/>
<connect gate="G$1" pin="GPIO0" pad="P17"/>
<connect gate="G$1" pin="MISO" pad="P15"/>
<connect gate="G$1" pin="MOSI" pad="P14"/>
<connect gate="G$1" pin="RF_IN" pad="P11"/>
<connect gate="G$1" pin="RXD" pad="P21"/>
<connect gate="G$1" pin="SCK" pad="P16"/>
<connect gate="G$1" pin="SCL" pad="P19"/>
<connect gate="G$1" pin="SCS" pad="P2"/>
<connect gate="G$1" pin="SDA" pad="P18"/>
<connect gate="G$1" pin="TM" pad="P3"/>
<connect gate="G$1" pin="TXD" pad="P20"/>
<connect gate="G$1" pin="VBKP" pad="P22"/>
<connect gate="G$1" pin="VCC" pad="P23"/>
<connect gate="G$1" pin="VCC_RF" pad="P9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="STM32F103C8">
<gates>
<gate name="G$1" symbol="STM32F103C8"/>
</gates>
<devices>
<device name="" package="LQFP48">
<connects>
<connect gate="G$1" pin="BOOT" pad="P44"/>
<connect gate="G$1" pin="GND" pad="P23 P35 P47"/>
<connect gate="G$1" pin="GNDA" pad="P8"/>
<connect gate="G$1" pin="NRST" pad="P7"/>
<connect gate="G$1" pin="OSC_IN" pad="P5"/>
<connect gate="G$1" pin="OSC_OUT" pad="P6"/>
<connect gate="G$1" pin="PA0" pad="P10"/>
<connect gate="G$1" pin="PA1" pad="P11"/>
<connect gate="G$1" pin="PA10" pad="P31"/>
<connect gate="G$1" pin="PA11" pad="P32"/>
<connect gate="G$1" pin="PA12" pad="P33"/>
<connect gate="G$1" pin="PA13" pad="P34"/>
<connect gate="G$1" pin="PA14" pad="P37"/>
<connect gate="G$1" pin="PA15" pad="P38"/>
<connect gate="G$1" pin="PA2" pad="P12"/>
<connect gate="G$1" pin="PA3" pad="P13"/>
<connect gate="G$1" pin="PA4" pad="P14"/>
<connect gate="G$1" pin="PA5" pad="P15"/>
<connect gate="G$1" pin="PA6" pad="P16"/>
<connect gate="G$1" pin="PA7" pad="P17"/>
<connect gate="G$1" pin="PA8" pad="P29"/>
<connect gate="G$1" pin="PA9" pad="P30"/>
<connect gate="G$1" pin="PB0" pad="P18"/>
<connect gate="G$1" pin="PB1" pad="P19"/>
<connect gate="G$1" pin="PB10" pad="P21"/>
<connect gate="G$1" pin="PB11" pad="P22"/>
<connect gate="G$1" pin="PB12" pad="P25"/>
<connect gate="G$1" pin="PB13" pad="P26"/>
<connect gate="G$1" pin="PB14" pad="P27"/>
<connect gate="G$1" pin="PB15" pad="P28"/>
<connect gate="G$1" pin="PB2" pad="P20"/>
<connect gate="G$1" pin="PB3" pad="P39"/>
<connect gate="G$1" pin="PB4" pad="P40"/>
<connect gate="G$1" pin="PB5" pad="P41"/>
<connect gate="G$1" pin="PB6" pad="P42"/>
<connect gate="G$1" pin="PB7" pad="P43"/>
<connect gate="G$1" pin="PB8" pad="P45"/>
<connect gate="G$1" pin="PB9" pad="P46"/>
<connect gate="G$1" pin="PC13" pad="P2"/>
<connect gate="G$1" pin="PC14" pad="P3"/>
<connect gate="G$1" pin="PC15" pad="P4"/>
<connect gate="G$1" pin="VBAT" pad="P1"/>
<connect gate="G$1" pin="VCC" pad="P24 P36 P48"/>
<connect gate="G$1" pin="VCCA" pad="P9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="M41T81">
<description>Real-time clock with alarm
&lt;p&gt;
I2C 400kHz&lt;br/&gt;
Counters for tenths/hundredths of seconds,
seconds, minutes, hours, day, date, month,
year, and century
&lt;/p&gt;</description>
<gates>
<gate name="G$1" symbol="M61T81"/>
</gates>
<devices>
<device name="" package="SOIC8">
<connects>
<connect gate="G$1" pin="GND" pad="4"/>
<connect gate="G$1" pin="IRQ" pad="6"/>
<connect gate="G$1" pin="SCL" pad="7"/>
<connect gate="G$1" pin="SDA" pad="8"/>
<connect gate="G$1" pin="VBAT" pad="3"/>
<connect gate="G$1" pin="VCC" pad="5"/>
<connect gate="G$1" pin="XI" pad="1"/>
<connect gate="G$1" pin="XO" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="HD-K123" prefix="DIS">
<description>Seven segment dispplay&lt;p&gt;
 2 x 1 character 7 segment, decimal points right
&lt;/p&gt;</description>
<gates>
<gate name="S" symbol="HD7-K2"/>
</gates>
<devices>
<device name="" package="HDSP-R">
<connects>
<connect gate="S" pin="A1" pad="16"/>
<connect gate="S" pin="A2" pad="11"/>
<connect gate="S" pin="B1" pad="15"/>
<connect gate="S" pin="B2" pad="10"/>
<connect gate="S" pin="C1" pad="3"/>
<connect gate="S" pin="C2" pad="8"/>
<connect gate="S" pin="CC1" pad="14"/>
<connect gate="S" pin="CC2" pad="13"/>
<connect gate="S" pin="D1" pad="2"/>
<connect gate="S" pin="D2" pad="6"/>
<connect gate="S" pin="DP1" pad="4"/>
<connect gate="S" pin="DP2" pad="9"/>
<connect gate="S" pin="E1" pad="1"/>
<connect gate="S" pin="E2" pad="5"/>
<connect gate="S" pin="F1" pad="18"/>
<connect gate="S" pin="F2" pad="12"/>
<connect gate="S" pin="G1" pad="17"/>
<connect gate="S" pin="G2" pad="7"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="CR2032H" prefix="G">
<description>Coin battery socket</description>
<gates>
<gate name="1" symbol="1V2+2"/>
</gates>
<devices>
<device name="" package="CR2032H">
<connects>
<connect gate="1" pin="+" pad="+"/>
<connect gate="1" pin="+@1" pad="+@1"/>
<connect gate="1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="POTENTIOMETER">
<gates>
<gate name="G$1" symbol="POTENTIOMETER"/>
</gates>
<devices>
<device name="" package="DEF_POT">
<connects>
<connect gate="G$1" pin="A" pad="P1"/>
<connect gate="G$1" pin="E" pad="P3"/>
<connect gate="G$1" pin="S" pad="P2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="OPD-D391">
<gates>
<gate name="G$1" symbol="OPD-D391"/>
</gates>
<devices>
<device name="" package="OPD-D391">
<connects>
<connect gate="G$1" pin="A" pad="P10"/>
<connect gate="G$1" pin="B" pad="P8"/>
<connect gate="G$1" pin="C" pad="P1"/>
<connect gate="G$1" pin="CC1" pad="P9"/>
<connect gate="G$1" pin="CC2" pad="P4"/>
<connect gate="G$1" pin="D" pad="P5"/>
<connect gate="G$1" pin="E" pad="P3"/>
<connect gate="G$1" pin="F" pad="P6"/>
<connect gate="G$1" pin="G" pad="P7"/>
<connect gate="G$1" pin="P" pad="P2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="INDUCTOR" prefix="L" uservalue="yes">
<gates>
<gate name="G$1" symbol="L-US"/>
</gates>
<devices>
<device name="" package="L0603">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="L2220" package="L2220">
<connects>
<connect gate="G$1" pin="1" pad="P$1"/>
<connect gate="G$1" pin="2" pad="P$2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="L_12.7X12.7" package="L12.7X12.7">
<connects>
<connect gate="G$1" pin="1" pad="P1"/>
<connect gate="G$1" pin="2" pad="P2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="LPS3008" package="LPS3008">
<connects>
<connect gate="G$1" pin="1" pad="P1"/>
<connect gate="G$1" pin="2" pad="P2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="SDR1307" package="SDR1307">
<connects>
<connect gate="G$1" pin="1" pad="P1"/>
<connect gate="G$1" pin="2" pad="P2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="TVS_DIODE_BID">
<gates>
<gate name="G$1" symbol="TVS_DIODE_BID"/>
</gates>
<devices>
<device name="" package="SMA">
<connects>
<connect gate="G$1" pin="P$1" pad="P$1"/>
<connect gate="G$1" pin="P$2" pad="P$2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MOSFET-P_DIODE">
<gates>
<gate name="G$1" symbol="MOSFET-P_DIODE"/>
</gates>
<devices>
<device name="" package="SOT23">
<connects>
<connect gate="G$1" pin="D" pad="3"/>
<connect gate="G$1" pin="G" pad="1"/>
<connect gate="G$1" pin="S" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="STM32F405RG">
<gates>
<gate name="G$1" symbol="STM32F405RG"/>
</gates>
<devices>
<device name="" package="LQFP64">
<connects>
<connect gate="G$1" pin="BOOT" pad="P$60"/>
<connect gate="G$1" pin="GND" pad="P$18 P$31 P$47 P$63"/>
<connect gate="G$1" pin="GNDA" pad="P$12"/>
<connect gate="G$1" pin="NRST" pad="P$7"/>
<connect gate="G$1" pin="OSC_IN" pad="P$5"/>
<connect gate="G$1" pin="OSC_OUT" pad="P$6"/>
<connect gate="G$1" pin="PA0" pad="P$14"/>
<connect gate="G$1" pin="PA1" pad="P$15"/>
<connect gate="G$1" pin="PA10" pad="P$43"/>
<connect gate="G$1" pin="PA11" pad="P$44"/>
<connect gate="G$1" pin="PA12" pad="P$45"/>
<connect gate="G$1" pin="PA13" pad="P$46"/>
<connect gate="G$1" pin="PA14" pad="P$49"/>
<connect gate="G$1" pin="PA15" pad="P$50"/>
<connect gate="G$1" pin="PA2" pad="P$16"/>
<connect gate="G$1" pin="PA3" pad="P$17"/>
<connect gate="G$1" pin="PA4" pad="P$20"/>
<connect gate="G$1" pin="PA5" pad="P$21"/>
<connect gate="G$1" pin="PA6" pad="P$22"/>
<connect gate="G$1" pin="PA7" pad="P$23"/>
<connect gate="G$1" pin="PA8" pad="P$41"/>
<connect gate="G$1" pin="PA9" pad="P$42"/>
<connect gate="G$1" pin="PB0" pad="P$26"/>
<connect gate="G$1" pin="PB1" pad="P$27"/>
<connect gate="G$1" pin="PB10" pad="P$29"/>
<connect gate="G$1" pin="PB12" pad="P$33"/>
<connect gate="G$1" pin="PB13" pad="P$34"/>
<connect gate="G$1" pin="PB14" pad="P$35"/>
<connect gate="G$1" pin="PB15" pad="P$36"/>
<connect gate="G$1" pin="PB2" pad="P$28"/>
<connect gate="G$1" pin="PB3" pad="P$55"/>
<connect gate="G$1" pin="PB4" pad="P$56"/>
<connect gate="G$1" pin="PB5" pad="P$57"/>
<connect gate="G$1" pin="PB6" pad="P$58"/>
<connect gate="G$1" pin="PB7" pad="P$59"/>
<connect gate="G$1" pin="PB8" pad="P$61"/>
<connect gate="G$1" pin="PB9" pad="P$62"/>
<connect gate="G$1" pin="PC0" pad="P$8"/>
<connect gate="G$1" pin="PC1" pad="P$9"/>
<connect gate="G$1" pin="PC10" pad="P$51"/>
<connect gate="G$1" pin="PC11" pad="P$52"/>
<connect gate="G$1" pin="PC12" pad="P$53"/>
<connect gate="G$1" pin="PC13" pad="P$2"/>
<connect gate="G$1" pin="PC14" pad="P$3"/>
<connect gate="G$1" pin="PC15" pad="P$4"/>
<connect gate="G$1" pin="PC2" pad="P$10"/>
<connect gate="G$1" pin="PC3" pad="P$11"/>
<connect gate="G$1" pin="PC4" pad="P$24"/>
<connect gate="G$1" pin="PC5" pad="P$25"/>
<connect gate="G$1" pin="PC6" pad="P$37"/>
<connect gate="G$1" pin="PC7" pad="P$38"/>
<connect gate="G$1" pin="PC8" pad="P$39"/>
<connect gate="G$1" pin="PC9" pad="P$40"/>
<connect gate="G$1" pin="PD2" pad="P$54"/>
<connect gate="G$1" pin="VBAT" pad="P$1"/>
<connect gate="G$1" pin="VCAP1" pad="P$30"/>
<connect gate="G$1" pin="VCC" pad="P$19 P$32 P$48 P$64"/>
<connect gate="G$1" pin="VCCA" pad="P$13"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="TPS6303X">
<gates>
<gate name="G$1" symbol="TPS6303X"/>
</gates>
<devices>
<device name="" package="VSON10">
<connects>
<connect gate="G$1" pin="EN" pad="P6"/>
<connect gate="G$1" pin="FB" pad="P10"/>
<connect gate="G$1" pin="GND" pad="P9"/>
<connect gate="G$1" pin="L1" pad="P4"/>
<connect gate="G$1" pin="L2" pad="P2"/>
<connect gate="G$1" pin="PGND" pad="P3 PG1 PG2 PG3 PG4"/>
<connect gate="G$1" pin="PS/SYNC" pad="P7"/>
<connect gate="G$1" pin="VIN" pad="P5"/>
<connect gate="G$1" pin="VINA" pad="P8"/>
<connect gate="G$1" pin="VOUT" pad="P1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="STM32F103RG">
<gates>
<gate name="G$1" symbol="STM32F103RG"/>
</gates>
<devices>
<device name="" package="LQFP64">
<connects>
<connect gate="G$1" pin="BOOT" pad="P$60"/>
<connect gate="G$1" pin="GND" pad="P$18 P$31 P$47 P$63"/>
<connect gate="G$1" pin="GNDA" pad="P$12"/>
<connect gate="G$1" pin="NRST" pad="P$7"/>
<connect gate="G$1" pin="OSC_IN" pad="P$5"/>
<connect gate="G$1" pin="OSC_OUT" pad="P$6"/>
<connect gate="G$1" pin="PA0" pad="P$14"/>
<connect gate="G$1" pin="PA1" pad="P$15"/>
<connect gate="G$1" pin="PA10" pad="P$43"/>
<connect gate="G$1" pin="PA11" pad="P$44"/>
<connect gate="G$1" pin="PA12" pad="P$45"/>
<connect gate="G$1" pin="PA15" pad="P$50"/>
<connect gate="G$1" pin="PA2" pad="P$16"/>
<connect gate="G$1" pin="PA3" pad="P$17"/>
<connect gate="G$1" pin="PA4" pad="P$20"/>
<connect gate="G$1" pin="PA5" pad="P$21"/>
<connect gate="G$1" pin="PA6" pad="P$22"/>
<connect gate="G$1" pin="PA7" pad="P$23"/>
<connect gate="G$1" pin="PA8" pad="P$41"/>
<connect gate="G$1" pin="PA9" pad="P$42"/>
<connect gate="G$1" pin="PB0" pad="P$26"/>
<connect gate="G$1" pin="PB1" pad="P$27"/>
<connect gate="G$1" pin="PB10" pad="P$29"/>
<connect gate="G$1" pin="PB11" pad="P$30"/>
<connect gate="G$1" pin="PB12" pad="P$33"/>
<connect gate="G$1" pin="PB13" pad="P$34"/>
<connect gate="G$1" pin="PB14" pad="P$35"/>
<connect gate="G$1" pin="PB15" pad="P$36"/>
<connect gate="G$1" pin="PB2" pad="P$28"/>
<connect gate="G$1" pin="PB3" pad="P$55"/>
<connect gate="G$1" pin="PB4" pad="P$56"/>
<connect gate="G$1" pin="PB5" pad="P$57"/>
<connect gate="G$1" pin="PB6" pad="P$58"/>
<connect gate="G$1" pin="PB7" pad="P$59"/>
<connect gate="G$1" pin="PB8" pad="P$61"/>
<connect gate="G$1" pin="PB9" pad="P$62"/>
<connect gate="G$1" pin="PC0" pad="P$8"/>
<connect gate="G$1" pin="PC1" pad="P$9"/>
<connect gate="G$1" pin="PC10" pad="P$51"/>
<connect gate="G$1" pin="PC11" pad="P$52"/>
<connect gate="G$1" pin="PC12" pad="P$53"/>
<connect gate="G$1" pin="PC13" pad="P$2"/>
<connect gate="G$1" pin="PC14" pad="P$3"/>
<connect gate="G$1" pin="PC15" pad="P$4"/>
<connect gate="G$1" pin="PC2" pad="P$10"/>
<connect gate="G$1" pin="PC3" pad="P$11"/>
<connect gate="G$1" pin="PC4" pad="P$24"/>
<connect gate="G$1" pin="PC5" pad="P$25"/>
<connect gate="G$1" pin="PC6" pad="P$37"/>
<connect gate="G$1" pin="PC7" pad="P$38"/>
<connect gate="G$1" pin="PC8" pad="P$39"/>
<connect gate="G$1" pin="PC9" pad="P$40"/>
<connect gate="G$1" pin="PD2" pad="P$54"/>
<connect gate="G$1" pin="SWCLK" pad="P$49"/>
<connect gate="G$1" pin="SWDIO" pad="P$46"/>
<connect gate="G$1" pin="VBAT" pad="P$1"/>
<connect gate="G$1" pin="VCC" pad="P$19 P$32 P$48 P$64" route="any"/>
<connect gate="G$1" pin="VCCA" pad="P$13"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MCP4725">
<description>12-Bit Digital-to-Analog converter
&lt;p&gt;
I2C up to 400kHz
&lt;/p&gt;</description>
<gates>
<gate name="G$1" symbol="MCP4725"/>
</gates>
<devices>
<device name="" package="SOT-23-6">
<connects>
<connect gate="G$1" pin="A0" pad="6"/>
<connect gate="G$1" pin="GND" pad="2"/>
<connect gate="G$1" pin="SCL" pad="5"/>
<connect gate="G$1" pin="SDA" pad="4"/>
<connect gate="G$1" pin="VCC" pad="3"/>
<connect gate="G$1" pin="VOUT" pad="1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="A3901">
<description>Motor Driver&lt;p&gt;
Dual, Full Bridge, Low Voltage
&lt;/p&gt;</description>
<gates>
<gate name="G$1" symbol="A3901"/>
</gates>
<devices>
<device name="" package="DFN10-3X3">
<connects>
<connect gate="G$1" pin="GND" pad="P3"/>
<connect gate="G$1" pin="IN1" pad="P1"/>
<connect gate="G$1" pin="IN2" pad="P2"/>
<connect gate="G$1" pin="IN3" pad="P4"/>
<connect gate="G$1" pin="IN4" pad="P5"/>
<connect gate="G$1" pin="OUT1" pad="P10"/>
<connect gate="G$1" pin="OUT2" pad="P9"/>
<connect gate="G$1" pin="OUT3" pad="P7"/>
<connect gate="G$1" pin="OUT4" pad="P6"/>
<connect gate="G$1" pin="PAD" pad="P11"/>
<connect gate="G$1" pin="VCC" pad="P8"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="STM32L151CB">
<gates>
<gate name="G$1" symbol="STM32L151CB"/>
</gates>
<devices>
<device name="" package="LQFP48">
<connects>
<connect gate="G$1" pin="BOOT0" pad="P44"/>
<connect gate="G$1" pin="GND" pad="P23 P35 P47"/>
<connect gate="G$1" pin="GNDA" pad="P8"/>
<connect gate="G$1" pin="NRST" pad="P7"/>
<connect gate="G$1" pin="OSC_IN" pad="P5"/>
<connect gate="G$1" pin="OSC_OUT" pad="P6"/>
<connect gate="G$1" pin="PA0" pad="P10"/>
<connect gate="G$1" pin="PA1" pad="P11"/>
<connect gate="G$1" pin="PA10" pad="P31"/>
<connect gate="G$1" pin="PA11" pad="P32"/>
<connect gate="G$1" pin="PA12" pad="P33"/>
<connect gate="G$1" pin="PA13/SWDIO" pad="P34"/>
<connect gate="G$1" pin="PA14/SWCLK" pad="P37"/>
<connect gate="G$1" pin="PA15" pad="P38"/>
<connect gate="G$1" pin="PA2" pad="P12"/>
<connect gate="G$1" pin="PA3" pad="P13"/>
<connect gate="G$1" pin="PA4" pad="P14"/>
<connect gate="G$1" pin="PA5" pad="P15"/>
<connect gate="G$1" pin="PA6" pad="P16"/>
<connect gate="G$1" pin="PA7" pad="P17"/>
<connect gate="G$1" pin="PA8" pad="P29"/>
<connect gate="G$1" pin="PA9" pad="P30"/>
<connect gate="G$1" pin="PB0" pad="P18"/>
<connect gate="G$1" pin="PB1" pad="P19"/>
<connect gate="G$1" pin="PB10" pad="P21"/>
<connect gate="G$1" pin="PB11" pad="P22"/>
<connect gate="G$1" pin="PB12" pad="P25"/>
<connect gate="G$1" pin="PB13" pad="P26"/>
<connect gate="G$1" pin="PB14" pad="P27"/>
<connect gate="G$1" pin="PB15" pad="P28"/>
<connect gate="G$1" pin="PB2" pad="P20"/>
<connect gate="G$1" pin="PB3" pad="P39"/>
<connect gate="G$1" pin="PB4" pad="P40"/>
<connect gate="G$1" pin="PB5" pad="P41"/>
<connect gate="G$1" pin="PB6" pad="P42"/>
<connect gate="G$1" pin="PB7" pad="P43"/>
<connect gate="G$1" pin="PB8" pad="P45"/>
<connect gate="G$1" pin="PB9" pad="P46"/>
<connect gate="G$1" pin="PC13" pad="P2"/>
<connect gate="G$1" pin="PC14" pad="P3"/>
<connect gate="G$1" pin="PC15" pad="P4"/>
<connect gate="G$1" pin="VDD" pad="P24 P36 P48"/>
<connect gate="G$1" pin="VDDA" pad="P9"/>
<connect gate="G$1" pin="VLCD" pad="P1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MPX4250DP">
<gates>
<gate name="G$1" symbol="MPX4250"/>
</gates>
<devices>
<device name="" package="MPX4250DP">
<connects>
<connect gate="G$1" pin="GND" pad="P2"/>
<connect gate="G$1" pin="VCC" pad="P3"/>
<connect gate="G$1" pin="VOUT" pad="P1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MS4515DO_DS">
<gates>
<gate name="G$1" symbol="MS4515DO"/>
</gates>
<devices>
<device name="" package="MS4515DO-DS">
<connects>
<connect gate="G$1" pin="GND" pad="P1"/>
<connect gate="G$1" pin="INT/SS" pad="P5"/>
<connect gate="G$1" pin="SCL/SCK" pad="P4"/>
<connect gate="G$1" pin="SDA/MISO" pad="P3"/>
<connect gate="G$1" pin="VCC" pad="P2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="BQ25071-Q1">
<description>LiFePO4, Single-Cell charger</description>
<gates>
<gate name="G$1" symbol="BQ25071-Q1"/>
</gates>
<devices>
<device name="" package="WSON10">
<connects>
<connect gate="G$1" pin="BAT" pad="P6"/>
<connect gate="G$1" pin="CHG" pad="P8"/>
<connect gate="G$1" pin="EN" pad="P7"/>
<connect gate="G$1" pin="GND" pad="P3 P9 PD"/>
<connect gate="G$1" pin="IN" pad="P1"/>
<connect gate="G$1" pin="ISET" pad="P2"/>
<connect gate="G$1" pin="LDO" pad="P4"/>
<connect gate="G$1" pin="OUT" pad="P10"/>
<connect gate="G$1" pin="TS" pad="P5"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="BQ2980">
<description>BQ2980xy Voltage, Current, Temperature Protectors with an Integrated High-Side NFET
Driver for Fast/Flash Charging Single-Cell Li-Ion and Li-Polymer Batteries</description>
<gates>
<gate name="G$1" symbol="BQ2980"/>
</gates>
<devices>
<device name="" package="X2QFN">
<connects>
<connect gate="G$1" pin="BAT" pad="P1"/>
<connect gate="G$1" pin="CHG" pad="P8"/>
<connect gate="G$1" pin="CS" pad="P4"/>
<connect gate="G$1" pin="CTR" pad="P5"/>
<connect gate="G$1" pin="DSG" pad="P7"/>
<connect gate="G$1" pin="PACK" pad="P6"/>
<connect gate="G$1" pin="VDD" pad="P2"/>
<connect gate="G$1" pin="VSS" pad="P3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="EFC8811R">
<description>&lt;b&gt;Power MOSFET&lt;/b&gt;&lt;br/&gt;
for 1-Cell Lithium-ion Battery Protection&lt;br/&gt;
12V, 3m2R, 27A, Dual N-Channel</description>
<gates>
<gate name="G$1" symbol="EFC8811R"/>
</gates>
<devices>
<device name="" package="CSP6">
<connects>
<connect gate="G$1" pin="G1" pad="P2"/>
<connect gate="G$1" pin="G2" pad="P5"/>
<connect gate="G$1" pin="S1" pad="P1 P3"/>
<connect gate="G$1" pin="S2" pad="P4 P6"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MCP1727">
<gates>
<gate name="G$1" symbol="MCP1727"/>
</gates>
<devices>
<device name="" package="SOIC8">
<connects>
<connect gate="G$1" pin="CDEL" pad="6"/>
<connect gate="G$1" pin="GND" pad="4"/>
<connect gate="G$1" pin="PWRGD" pad="5"/>
<connect gate="G$1" pin="SENSE" pad="7"/>
<connect gate="G$1" pin="SHDN" pad="3"/>
<connect gate="G$1" pin="VIN" pad="1 2"/>
<connect gate="G$1" pin="VOUT" pad="8"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="BQ24630">
<gates>
<gate name="G$1" symbol="BQ24630"/>
</gates>
<devices>
<device name="" package="VQFN24">
<connects>
<connect gate="G$1" pin="ACDRV" pad="P3"/>
<connect gate="G$1" pin="ACN" pad="P1"/>
<connect gate="G$1" pin="ACP" pad="P2"/>
<connect gate="G$1" pin="ACSET" pad="P16"/>
<connect gate="G$1" pin="BATDRV" pad="P23"/>
<connect gate="G$1" pin="BTST" pad="P22"/>
<connect gate="G$1" pin="CE" pad="P4"/>
<connect gate="G$1" pin="GND" pad="P17"/>
<connect gate="G$1" pin="HIDRV" pad="P21"/>
<connect gate="G$1" pin="ISET1" pad="P11"/>
<connect gate="G$1" pin="ISET2" pad="P15"/>
<connect gate="G$1" pin="LODRV" pad="P19"/>
<connect gate="G$1" pin="PG" pad="P8"/>
<connect gate="G$1" pin="PH" pad="P20"/>
<connect gate="G$1" pin="PWRPAD" pad="PAD"/>
<connect gate="G$1" pin="REGN" pad="P18"/>
<connect gate="G$1" pin="SRN" pad="P13"/>
<connect gate="G$1" pin="SRP" pad="P14"/>
<connect gate="G$1" pin="STAT1" pad="P5"/>
<connect gate="G$1" pin="STAT2" pad="P9"/>
<connect gate="G$1" pin="TS" pad="P6"/>
<connect gate="G$1" pin="TTC" pad="P7"/>
<connect gate="G$1" pin="VCC" pad="P24"/>
<connect gate="G$1" pin="VFB" pad="P12"/>
<connect gate="G$1" pin="VREF" pad="P10"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MPU6050">
<gates>
<gate name="G$1" symbol="MPU6050"/>
</gates>
<devices>
<device name="" package="LQFN24">
<connects>
<connect gate="G$1" pin="AD0" pad="P9"/>
<connect gate="G$1" pin="AUX_CL" pad="P7"/>
<connect gate="G$1" pin="AUX_DA" pad="P6"/>
<connect gate="G$1" pin="CLKIN" pad="P1"/>
<connect gate="G$1" pin="CLKOUT" pad="P22"/>
<connect gate="G$1" pin="CPOUT" pad="P20"/>
<connect gate="G$1" pin="FSYNC" pad="P11"/>
<connect gate="G$1" pin="GND" pad="P18"/>
<connect gate="G$1" pin="INT" pad="P12"/>
<connect gate="G$1" pin="REGOUT" pad="P10"/>
<connect gate="G$1" pin="SCL" pad="P23"/>
<connect gate="G$1" pin="SDA" pad="P24"/>
<connect gate="G$1" pin="VDD" pad="P13"/>
<connect gate="G$1" pin="VLOGIC" pad="P8"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="BMP280">
<gates>
<gate name="G$1" symbol="BMP280"/>
</gates>
<devices>
<device name="" package="BMP280">
<connects>
<connect gate="G$1" pin="CSB" pad="P2"/>
<connect gate="G$1" pin="GND" pad="P1 P7"/>
<connect gate="G$1" pin="SCK" pad="P4"/>
<connect gate="G$1" pin="SDI" pad="P3"/>
<connect gate="G$1" pin="SDO" pad="P5"/>
<connect gate="G$1" pin="VDD" pad="P8"/>
<connect gate="G$1" pin="VDDIO" pad="P6"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="BQ24072">
<gates>
<gate name="G$1" symbol="BQ24072"/>
</gates>
<devices>
<device name="" package="VQFN16">
<connects>
<connect gate="G$1" pin="BAT" pad="P2 P3"/>
<connect gate="G$1" pin="CE" pad="P4"/>
<connect gate="G$1" pin="CHG" pad="P9"/>
<connect gate="G$1" pin="EN1" pad="P6"/>
<connect gate="G$1" pin="EN2" pad="P5"/>
<connect gate="G$1" pin="GND" pad="P$17 P8"/>
<connect gate="G$1" pin="ILIM" pad="P12"/>
<connect gate="G$1" pin="IN" pad="P13"/>
<connect gate="G$1" pin="ISET" pad="P16"/>
<connect gate="G$1" pin="OUT" pad="P10 P11"/>
<connect gate="G$1" pin="PGOOD" pad="P7"/>
<connect gate="G$1" pin="TD" pad="P15"/>
<connect gate="G$1" pin="TMR" pad="P14"/>
<connect gate="G$1" pin="TS" pad="P1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="TSX339">
<gates>
<gate name="G$1" symbol="TSX339"/>
</gates>
<devices>
<device name="" package="QFN16">
<connects>
<connect gate="G$1" pin="IN1+" pad="P4"/>
<connect gate="G$1" pin="IN1-" pad="P2"/>
<connect gate="G$1" pin="IN2+" pad="P6"/>
<connect gate="G$1" pin="IN2-" pad="P5"/>
<connect gate="G$1" pin="IN3+" pad="P8"/>
<connect gate="G$1" pin="IN3-" pad="P7"/>
<connect gate="G$1" pin="IN4+" pad="P11"/>
<connect gate="G$1" pin="IN4-" pad="P9"/>
<connect gate="G$1" pin="OUT1" pad="P16"/>
<connect gate="G$1" pin="OUT2" pad="P15"/>
<connect gate="G$1" pin="OUT3" pad="P14"/>
<connect gate="G$1" pin="OUT4" pad="P13"/>
<connect gate="G$1" pin="VCC+" pad="P1"/>
<connect gate="G$1" pin="VCC-" pad="P12 TH"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MAX17501F">
<gates>
<gate name="G$1" symbol="MAX17501"/>
</gates>
<devices>
<device name="" package="TDFN-10">
<connects>
<connect gate="G$1" pin="AGND" pad="P1"/>
<connect gate="G$1" pin="EN/UVLO" pad="P3"/>
<connect gate="G$1" pin="FB/VO" pad="P5"/>
<connect gate="G$1" pin="GND" pad="EP P9"/>
<connect gate="G$1" pin="LX" pad="P10"/>
<connect gate="G$1" pin="NC/COMP" pad="P7"/>
<connect gate="G$1" pin="RESET" pad="P8"/>
<connect gate="G$1" pin="SS" pad="P6"/>
<connect gate="G$1" pin="VCC" pad="P4"/>
<connect gate="G$1" pin="VIN" pad="P2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="TPS62177">
<gates>
<gate name="G$1" symbol="TPS6217"/>
</gates>
<devices>
<device name="" package="WSON10">
<connects>
<connect gate="G$1" pin="AGND" pad="P4 P6 PD" route="any"/>
<connect gate="G$1" pin="EN" pad="P3"/>
<connect gate="G$1" pin="FB" pad="P5"/>
<connect gate="G$1" pin="GND" pad="P1"/>
<connect gate="G$1" pin="PG" pad="P7"/>
<connect gate="G$1" pin="SLEEP" pad="P8"/>
<connect gate="G$1" pin="SW" pad="P9"/>
<connect gate="G$1" pin="VIN" pad="P2"/>
<connect gate="G$1" pin="VOS" pad="P10"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="TPS736XX">
<gates>
<gate name="G$1" symbol="TPS736XX"/>
</gates>
<devices>
<device name="" package="SOT23-DBV">
<connects>
<connect gate="G$1" pin="EN" pad="3"/>
<connect gate="G$1" pin="GND" pad="2"/>
<connect gate="G$1" pin="IN" pad="1"/>
<connect gate="G$1" pin="NR" pad="4"/>
<connect gate="G$1" pin="OUT" pad="5"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="STM32F103V_8_B">
<gates>
<gate name="G$1" symbol="STM321F103V_8_B"/>
</gates>
<devices>
<device name="" package="LQFP100_14X14">
<connects>
<connect gate="G$1" pin="BOOT0" pad="94"/>
<connect gate="G$1" pin="GND" pad="10 27 49 74 99"/>
<connect gate="G$1" pin="GNDA" pad="19"/>
<connect gate="G$1" pin="NRST" pad="14"/>
<connect gate="G$1" pin="OSC_IN" pad="12"/>
<connect gate="G$1" pin="OSC_OUT" pad="13"/>
<connect gate="G$1" pin="PA0-WKUP" pad="23"/>
<connect gate="G$1" pin="PA1" pad="24"/>
<connect gate="G$1" pin="PA10" pad="69"/>
<connect gate="G$1" pin="PA11" pad="70"/>
<connect gate="G$1" pin="PA12" pad="71"/>
<connect gate="G$1" pin="PA13/SWDIO" pad="72"/>
<connect gate="G$1" pin="PA14/SWCLK" pad="76"/>
<connect gate="G$1" pin="PA15" pad="77"/>
<connect gate="G$1" pin="PA2" pad="25"/>
<connect gate="G$1" pin="PA3" pad="26"/>
<connect gate="G$1" pin="PA4" pad="29"/>
<connect gate="G$1" pin="PA5" pad="30"/>
<connect gate="G$1" pin="PA6" pad="31"/>
<connect gate="G$1" pin="PA7" pad="32"/>
<connect gate="G$1" pin="PA8" pad="67"/>
<connect gate="G$1" pin="PA9" pad="68"/>
<connect gate="G$1" pin="PB0" pad="35"/>
<connect gate="G$1" pin="PB1" pad="36"/>
<connect gate="G$1" pin="PB10" pad="47"/>
<connect gate="G$1" pin="PB11" pad="48"/>
<connect gate="G$1" pin="PB12" pad="51"/>
<connect gate="G$1" pin="PB13" pad="52"/>
<connect gate="G$1" pin="PB14" pad="53"/>
<connect gate="G$1" pin="PB15" pad="54"/>
<connect gate="G$1" pin="PB2/BOOT1" pad="37"/>
<connect gate="G$1" pin="PB3" pad="89"/>
<connect gate="G$1" pin="PB4" pad="90"/>
<connect gate="G$1" pin="PB5" pad="91"/>
<connect gate="G$1" pin="PB6" pad="92"/>
<connect gate="G$1" pin="PB7" pad="93"/>
<connect gate="G$1" pin="PB8" pad="95"/>
<connect gate="G$1" pin="PB9" pad="96"/>
<connect gate="G$1" pin="PC0" pad="15"/>
<connect gate="G$1" pin="PC1" pad="16"/>
<connect gate="G$1" pin="PC10" pad="78"/>
<connect gate="G$1" pin="PC11" pad="79"/>
<connect gate="G$1" pin="PC12" pad="80"/>
<connect gate="G$1" pin="PC13" pad="7"/>
<connect gate="G$1" pin="PC14" pad="8"/>
<connect gate="G$1" pin="PC15" pad="9"/>
<connect gate="G$1" pin="PC2" pad="17"/>
<connect gate="G$1" pin="PC3" pad="18"/>
<connect gate="G$1" pin="PC4" pad="33"/>
<connect gate="G$1" pin="PC5" pad="34"/>
<connect gate="G$1" pin="PC6" pad="63"/>
<connect gate="G$1" pin="PC7" pad="64"/>
<connect gate="G$1" pin="PC8" pad="65"/>
<connect gate="G$1" pin="PC9" pad="66"/>
<connect gate="G$1" pin="PD0" pad="81"/>
<connect gate="G$1" pin="PD1" pad="82"/>
<connect gate="G$1" pin="PD10" pad="57"/>
<connect gate="G$1" pin="PD11" pad="58"/>
<connect gate="G$1" pin="PD12" pad="59"/>
<connect gate="G$1" pin="PD13" pad="60"/>
<connect gate="G$1" pin="PD14" pad="61"/>
<connect gate="G$1" pin="PD15" pad="62"/>
<connect gate="G$1" pin="PD2" pad="83"/>
<connect gate="G$1" pin="PD3" pad="84"/>
<connect gate="G$1" pin="PD4" pad="85"/>
<connect gate="G$1" pin="PD5" pad="86"/>
<connect gate="G$1" pin="PD6" pad="87"/>
<connect gate="G$1" pin="PD7" pad="88"/>
<connect gate="G$1" pin="PD8" pad="55"/>
<connect gate="G$1" pin="PD9" pad="56"/>
<connect gate="G$1" pin="PE0" pad="97"/>
<connect gate="G$1" pin="PE1" pad="98"/>
<connect gate="G$1" pin="PE10" pad="41"/>
<connect gate="G$1" pin="PE11" pad="42"/>
<connect gate="G$1" pin="PE12" pad="43"/>
<connect gate="G$1" pin="PE13" pad="44"/>
<connect gate="G$1" pin="PE14" pad="45"/>
<connect gate="G$1" pin="PE15" pad="46"/>
<connect gate="G$1" pin="PE2" pad="1"/>
<connect gate="G$1" pin="PE3" pad="2"/>
<connect gate="G$1" pin="PE4" pad="3"/>
<connect gate="G$1" pin="PE5" pad="4"/>
<connect gate="G$1" pin="PE6" pad="5"/>
<connect gate="G$1" pin="PE7" pad="38"/>
<connect gate="G$1" pin="PE8" pad="39"/>
<connect gate="G$1" pin="PE9" pad="40"/>
<connect gate="G$1" pin="VBAT" pad="6"/>
<connect gate="G$1" pin="VCC" pad="11 28 50 75 100"/>
<connect gate="G$1" pin="VCCA" pad="22"/>
<connect gate="G$1" pin="VREF+" pad="21"/>
<connect gate="G$1" pin="VREF-" pad="20"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ACS711">
<gates>
<gate name="G$1" symbol="ACS711"/>
</gates>
<devices>
<device name="" package="EX-QFN-12">
<connects>
<connect gate="G$1" pin="FAULT" pad="P6"/>
<connect gate="G$1" pin="GND" pad="P5"/>
<connect gate="G$1" pin="IP+" pad="P1_2"/>
<connect gate="G$1" pin="IP-" pad="P3_4"/>
<connect gate="G$1" pin="VCC" pad="P12"/>
<connect gate="G$1" pin="VIOUT" pad="P11"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="STM32F429IGT6">
<gates>
<gate name="G$1" symbol="STM32F429IGT6"/>
</gates>
<devices>
<device name="" package="LQFP176">
<connects>
<connect gate="G$1" pin="BOOT0" pad="166"/>
<connect gate="G$1" pin="BYPASS_REG" pad="48"/>
<connect gate="G$1" pin="GND" pad="14 22 61 71 90 102 113 126 135 148 158"/>
<connect gate="G$1" pin="GNDA" pad="37"/>
<connect gate="G$1" pin="NRST" pad="31"/>
<connect gate="G$1" pin="PA0" pad="40"/>
<connect gate="G$1" pin="PA1" pad="41"/>
<connect gate="G$1" pin="PA10" pad="121"/>
<connect gate="G$1" pin="PA11" pad="122"/>
<connect gate="G$1" pin="PA12" pad="123"/>
<connect gate="G$1" pin="PA13" pad="124"/>
<connect gate="G$1" pin="PA14" pad="137"/>
<connect gate="G$1" pin="PA15" pad="138"/>
<connect gate="G$1" pin="PA2" pad="42"/>
<connect gate="G$1" pin="PA3" pad="47"/>
<connect gate="G$1" pin="PA4" pad="50"/>
<connect gate="G$1" pin="PA5" pad="51"/>
<connect gate="G$1" pin="PA6" pad="52"/>
<connect gate="G$1" pin="PA7" pad="53"/>
<connect gate="G$1" pin="PA8" pad="119"/>
<connect gate="G$1" pin="PA9" pad="120"/>
<connect gate="G$1" pin="PB0" pad="56"/>
<connect gate="G$1" pin="PB1" pad="57"/>
<connect gate="G$1" pin="PB10" pad="79"/>
<connect gate="G$1" pin="PB11" pad="80"/>
<connect gate="G$1" pin="PB12" pad="92"/>
<connect gate="G$1" pin="PB13" pad="93"/>
<connect gate="G$1" pin="PB14" pad="94"/>
<connect gate="G$1" pin="PB15" pad="95"/>
<connect gate="G$1" pin="PB2" pad="58"/>
<connect gate="G$1" pin="PB3" pad="161"/>
<connect gate="G$1" pin="PB4" pad="162"/>
<connect gate="G$1" pin="PB5" pad="163"/>
<connect gate="G$1" pin="PB6" pad="164"/>
<connect gate="G$1" pin="PB7" pad="165"/>
<connect gate="G$1" pin="PB8" pad="167"/>
<connect gate="G$1" pin="PB9" pad="168"/>
<connect gate="G$1" pin="PC0" pad="32"/>
<connect gate="G$1" pin="PC1" pad="33"/>
<connect gate="G$1" pin="PC10" pad="139"/>
<connect gate="G$1" pin="PC11" pad="140"/>
<connect gate="G$1" pin="PC12" pad="141"/>
<connect gate="G$1" pin="PC13" pad="8"/>
<connect gate="G$1" pin="PC14" pad="9"/>
<connect gate="G$1" pin="PC15" pad="10"/>
<connect gate="G$1" pin="PC2" pad="34"/>
<connect gate="G$1" pin="PC3" pad="35"/>
<connect gate="G$1" pin="PC4" pad="54"/>
<connect gate="G$1" pin="PC5" pad="55"/>
<connect gate="G$1" pin="PC6" pad="115"/>
<connect gate="G$1" pin="PC7" pad="116"/>
<connect gate="G$1" pin="PC8" pad="117"/>
<connect gate="G$1" pin="PC9" pad="118"/>
<connect gate="G$1" pin="PD0" pad="142"/>
<connect gate="G$1" pin="PD1" pad="143"/>
<connect gate="G$1" pin="PD10" pad="98"/>
<connect gate="G$1" pin="PD11" pad="99"/>
<connect gate="G$1" pin="PD12" pad="100"/>
<connect gate="G$1" pin="PD13" pad="101"/>
<connect gate="G$1" pin="PD14" pad="104"/>
<connect gate="G$1" pin="PD15" pad="105"/>
<connect gate="G$1" pin="PD2" pad="144"/>
<connect gate="G$1" pin="PD3" pad="145"/>
<connect gate="G$1" pin="PD4" pad="146"/>
<connect gate="G$1" pin="PD5" pad="147"/>
<connect gate="G$1" pin="PD6" pad="150"/>
<connect gate="G$1" pin="PD7" pad="151"/>
<connect gate="G$1" pin="PD8" pad="96"/>
<connect gate="G$1" pin="PD9" pad="97"/>
<connect gate="G$1" pin="PDR_ON" pad="171"/>
<connect gate="G$1" pin="PE0" pad="169"/>
<connect gate="G$1" pin="PE1" pad="170"/>
<connect gate="G$1" pin="PE10" pad="73"/>
<connect gate="G$1" pin="PE11" pad="74"/>
<connect gate="G$1" pin="PE12" pad="75"/>
<connect gate="G$1" pin="PE13" pad="76"/>
<connect gate="G$1" pin="PE14" pad="77"/>
<connect gate="G$1" pin="PE15" pad="78"/>
<connect gate="G$1" pin="PE2" pad="1"/>
<connect gate="G$1" pin="PE3" pad="2"/>
<connect gate="G$1" pin="PE4" pad="3"/>
<connect gate="G$1" pin="PE5" pad="4"/>
<connect gate="G$1" pin="PE6" pad="5"/>
<connect gate="G$1" pin="PE7" pad="68"/>
<connect gate="G$1" pin="PE8" pad="69"/>
<connect gate="G$1" pin="PE9" pad="70"/>
<connect gate="G$1" pin="PF0" pad="16"/>
<connect gate="G$1" pin="PF1" pad="17"/>
<connect gate="G$1" pin="PF10" pad="28"/>
<connect gate="G$1" pin="PF11" pad="59"/>
<connect gate="G$1" pin="PF12" pad="60"/>
<connect gate="G$1" pin="PF13" pad="63"/>
<connect gate="G$1" pin="PF14" pad="64"/>
<connect gate="G$1" pin="PF15" pad="65"/>
<connect gate="G$1" pin="PF2" pad="18"/>
<connect gate="G$1" pin="PF3" pad="19"/>
<connect gate="G$1" pin="PF4" pad="20"/>
<connect gate="G$1" pin="PF5" pad="21"/>
<connect gate="G$1" pin="PF6" pad="24"/>
<connect gate="G$1" pin="PF7" pad="25"/>
<connect gate="G$1" pin="PF8" pad="26"/>
<connect gate="G$1" pin="PF9" pad="27"/>
<connect gate="G$1" pin="PG0" pad="66"/>
<connect gate="G$1" pin="PG1" pad="67"/>
<connect gate="G$1" pin="PG10" pad="153"/>
<connect gate="G$1" pin="PG11" pad="154"/>
<connect gate="G$1" pin="PG12" pad="155"/>
<connect gate="G$1" pin="PG13" pad="156"/>
<connect gate="G$1" pin="PG14" pad="157"/>
<connect gate="G$1" pin="PG15" pad="160"/>
<connect gate="G$1" pin="PG2" pad="106"/>
<connect gate="G$1" pin="PG3" pad="107"/>
<connect gate="G$1" pin="PG4" pad="108"/>
<connect gate="G$1" pin="PG5" pad="109"/>
<connect gate="G$1" pin="PG6" pad="110"/>
<connect gate="G$1" pin="PG7" pad="111"/>
<connect gate="G$1" pin="PG8" pad="112"/>
<connect gate="G$1" pin="PG9" pad="152"/>
<connect gate="G$1" pin="PH0" pad="29"/>
<connect gate="G$1" pin="PH1" pad="30"/>
<connect gate="G$1" pin="PH10" pad="87"/>
<connect gate="G$1" pin="PH11" pad="88"/>
<connect gate="G$1" pin="PH12" pad="89"/>
<connect gate="G$1" pin="PH13" pad="128"/>
<connect gate="G$1" pin="PH14" pad="129"/>
<connect gate="G$1" pin="PH15" pad="130"/>
<connect gate="G$1" pin="PH2" pad="43"/>
<connect gate="G$1" pin="PH3" pad="44"/>
<connect gate="G$1" pin="PH4" pad="45"/>
<connect gate="G$1" pin="PH5" pad="46"/>
<connect gate="G$1" pin="PH6" pad="83"/>
<connect gate="G$1" pin="PH7" pad="84"/>
<connect gate="G$1" pin="PH8" pad="85"/>
<connect gate="G$1" pin="PH9" pad="86"/>
<connect gate="G$1" pin="PI0" pad="131"/>
<connect gate="G$1" pin="PI1" pad="132"/>
<connect gate="G$1" pin="PI10" pad="12"/>
<connect gate="G$1" pin="PI11" pad="13"/>
<connect gate="G$1" pin="PI2" pad="133"/>
<connect gate="G$1" pin="PI3" pad="134"/>
<connect gate="G$1" pin="PI4" pad="173"/>
<connect gate="G$1" pin="PI5" pad="174"/>
<connect gate="G$1" pin="PI6" pad="175"/>
<connect gate="G$1" pin="PI7" pad="176"/>
<connect gate="G$1" pin="PI8" pad="7"/>
<connect gate="G$1" pin="PI9" pad="11"/>
<connect gate="G$1" pin="VBAT" pad="6"/>
<connect gate="G$1" pin="VCAP1" pad="81"/>
<connect gate="G$1" pin="VCAP2" pad="125"/>
<connect gate="G$1" pin="VCC" pad="15 23 36 49 62 72 82 91 103 114 127 136 149 159 172"/>
<connect gate="G$1" pin="VCCA" pad="39"/>
<connect gate="G$1" pin="VREF+" pad="38"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="CRYSTAL">
<gates>
<gate name="G$1" symbol="CRYSTAL"/>
</gates>
<devices>
<device name="" package="Q_5032_2P">
<connects>
<connect gate="G$1" pin="1" pad="P1"/>
<connect gate="G$1" pin="2" pad="P2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="SN65HVD23X">
<gates>
<gate name="G$1" symbol="SN65HVD23X"/>
</gates>
<devices>
<device name="" package="SOIC8">
<connects>
<connect gate="G$1" pin="CANH" pad="7"/>
<connect gate="G$1" pin="CANL" pad="6"/>
<connect gate="G$1" pin="D" pad="1"/>
<connect gate="G$1" pin="GND" pad="2"/>
<connect gate="G$1" pin="R" pad="4"/>
<connect gate="G$1" pin="RS" pad="8"/>
<connect gate="G$1" pin="VCC" pad="3"/>
<connect gate="G$1" pin="VREF" pad="5"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="TPS54561">
<gates>
<gate name="G$1" symbol="TPS54561"/>
</gates>
<devices>
<device name="" package="WSON10_4X4">
<connects>
<connect gate="G$1" pin="BOOT" pad="P1"/>
<connect gate="G$1" pin="COMP" pad="P7"/>
<connect gate="G$1" pin="EN" pad="P3"/>
<connect gate="G$1" pin="FB" pad="P6"/>
<connect gate="G$1" pin="GND" pad="P8 PAD PAD1 PAD2 PAD3 PAD4"/>
<connect gate="G$1" pin="PWRGD" pad="P10"/>
<connect gate="G$1" pin="RT/CLK" pad="P5"/>
<connect gate="G$1" pin="SS/TR" pad="P4"/>
<connect gate="G$1" pin="SW" pad="P9"/>
<connect gate="G$1" pin="VIN" pad="P2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="POWER_SCHOTTKY_RECTIFIER">
<gates>
<gate name="G$1" symbol="POWER_SCHOTTKY_RECTIFIER"/>
</gates>
<devices>
<device name="D2PAK" package="D2PACK">
<connects>
<connect gate="G$1" pin="A" pad="1 3"/>
<connect gate="G$1" pin="K" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="FDC2X12">
<gates>
<gate name="G$1" symbol="FDC2X12"/>
</gates>
<devices>
<device name="" package="WSON12_4X4">
<connects>
<connect gate="G$1" pin="ADDR" pad="P4"/>
<connect gate="G$1" pin="CLKIN" pad="P3"/>
<connect gate="G$1" pin="GND" pad="P8 PAD PAD1 PAD2 PAD3 PAD4"/>
<connect gate="G$1" pin="IN0A" pad="P9"/>
<connect gate="G$1" pin="IN0B" pad="P10"/>
<connect gate="G$1" pin="IN1A" pad="P11"/>
<connect gate="G$1" pin="IN1B" pad="P12"/>
<connect gate="G$1" pin="INTB" pad="P5"/>
<connect gate="G$1" pin="SCL" pad="P1"/>
<connect gate="G$1" pin="SD" pad="P6"/>
<connect gate="G$1" pin="SDA" pad="P2"/>
<connect gate="G$1" pin="VCC" pad="P7"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="STM32H753VIT" prefix="U">
<gates>
<gate name="G$1" symbol="STM32H753VIT_PART1"/>
<gate name="G$2" symbol="STM32H753VIT_PART2"/>
<gate name="G$3" symbol="STM32H753VIT_PART3"/>
</gates>
<devices>
<device name="" package="LQFP100_14X14">
<connects>
<connect gate="G$1" pin="PA0" pad="22"/>
<connect gate="G$1" pin="PA1" pad="23"/>
<connect gate="G$1" pin="PA10" pad="69"/>
<connect gate="G$1" pin="PA11" pad="70"/>
<connect gate="G$1" pin="PA12" pad="71"/>
<connect gate="G$1" pin="PA13" pad="72"/>
<connect gate="G$1" pin="PA14" pad="76"/>
<connect gate="G$1" pin="PA15" pad="77"/>
<connect gate="G$1" pin="PA2" pad="24"/>
<connect gate="G$1" pin="PA3" pad="25"/>
<connect gate="G$1" pin="PA4" pad="28"/>
<connect gate="G$1" pin="PA5" pad="29"/>
<connect gate="G$1" pin="PA6" pad="30"/>
<connect gate="G$1" pin="PA7" pad="31"/>
<connect gate="G$1" pin="PA8" pad="67"/>
<connect gate="G$1" pin="PA9" pad="68"/>
<connect gate="G$1" pin="PB0" pad="34"/>
<connect gate="G$1" pin="PB1" pad="35"/>
<connect gate="G$1" pin="PB10" pad="46"/>
<connect gate="G$1" pin="PB11" pad="47"/>
<connect gate="G$1" pin="PB12" pad="51"/>
<connect gate="G$1" pin="PB13" pad="52"/>
<connect gate="G$1" pin="PB14" pad="53"/>
<connect gate="G$1" pin="PB15" pad="54"/>
<connect gate="G$1" pin="PB2" pad="36"/>
<connect gate="G$1" pin="PB3" pad="89"/>
<connect gate="G$1" pin="PB4" pad="90"/>
<connect gate="G$1" pin="PB5" pad="91"/>
<connect gate="G$1" pin="PB6" pad="92"/>
<connect gate="G$1" pin="PB7" pad="93"/>
<connect gate="G$1" pin="PB8" pad="95"/>
<connect gate="G$1" pin="PB9" pad="96"/>
<connect gate="G$2" pin="PC0" pad="15"/>
<connect gate="G$2" pin="PC1" pad="16"/>
<connect gate="G$2" pin="PC10" pad="78"/>
<connect gate="G$2" pin="PC11" pad="79"/>
<connect gate="G$2" pin="PC12" pad="80"/>
<connect gate="G$2" pin="PC13" pad="7"/>
<connect gate="G$2" pin="PC14" pad="8"/>
<connect gate="G$2" pin="PC15" pad="9"/>
<connect gate="G$2" pin="PC2" pad="17"/>
<connect gate="G$2" pin="PC3" pad="18"/>
<connect gate="G$2" pin="PC4" pad="32"/>
<connect gate="G$2" pin="PC5" pad="33"/>
<connect gate="G$2" pin="PC6" pad="63"/>
<connect gate="G$2" pin="PC7" pad="64"/>
<connect gate="G$2" pin="PC8" pad="65"/>
<connect gate="G$2" pin="PC9" pad="66"/>
<connect gate="G$2" pin="PD0" pad="81"/>
<connect gate="G$2" pin="PD1" pad="82"/>
<connect gate="G$2" pin="PD10" pad="57"/>
<connect gate="G$2" pin="PD11" pad="58"/>
<connect gate="G$2" pin="PD12" pad="59"/>
<connect gate="G$2" pin="PD13" pad="60"/>
<connect gate="G$2" pin="PD14" pad="61"/>
<connect gate="G$2" pin="PD15" pad="62"/>
<connect gate="G$2" pin="PD2" pad="83"/>
<connect gate="G$2" pin="PD3" pad="84"/>
<connect gate="G$2" pin="PD4" pad="85"/>
<connect gate="G$2" pin="PD5" pad="86"/>
<connect gate="G$2" pin="PD6" pad="87"/>
<connect gate="G$2" pin="PD7" pad="88"/>
<connect gate="G$2" pin="PD8" pad="55"/>
<connect gate="G$2" pin="PD9" pad="56"/>
<connect gate="G$3" pin="BOOT0" pad="94"/>
<connect gate="G$3" pin="GND" pad="11 27 50 75 100"/>
<connect gate="G$3" pin="GNDA" pad="21"/>
<connect gate="G$3" pin="NRST" pad="14"/>
<connect gate="G$3" pin="PE0" pad="97"/>
<connect gate="G$3" pin="PE1" pad="98"/>
<connect gate="G$3" pin="PE10" pad="40"/>
<connect gate="G$3" pin="PE11" pad="41"/>
<connect gate="G$3" pin="PE12" pad="42"/>
<connect gate="G$3" pin="PE13" pad="43"/>
<connect gate="G$3" pin="PE14" pad="44"/>
<connect gate="G$3" pin="PE15" pad="45"/>
<connect gate="G$3" pin="PE2" pad="1"/>
<connect gate="G$3" pin="PE3" pad="2"/>
<connect gate="G$3" pin="PE4" pad="3"/>
<connect gate="G$3" pin="PE5" pad="4"/>
<connect gate="G$3" pin="PE6" pad="5"/>
<connect gate="G$3" pin="PE7" pad="37"/>
<connect gate="G$3" pin="PE8" pad="38"/>
<connect gate="G$3" pin="PE9" pad="39"/>
<connect gate="G$3" pin="PH0" pad="12"/>
<connect gate="G$3" pin="PH1" pad="13"/>
<connect gate="G$3" pin="VBAT" pad="6"/>
<connect gate="G$3" pin="VCAP" pad="48 73"/>
<connect gate="G$3" pin="VCC" pad="10 26 49 74 99"/>
<connect gate="G$3" pin="VCCA" pad="19"/>
<connect gate="G$3" pin="VREF+" pad="20"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ICM-20948">
<gates>
<gate name="G$1" symbol="ICM-20948"/>
</gates>
<devices>
<device name="" package="LEAD-QFN24">
<connects>
<connect gate="G$1" pin="AUX_CL" pad="7"/>
<connect gate="G$1" pin="AUX_DA" pad="21"/>
<connect gate="G$1" pin="CS" pad="22"/>
<connect gate="G$1" pin="FSYNC" pad="11"/>
<connect gate="G$1" pin="GND" pad="18"/>
<connect gate="G$1" pin="INT1" pad="12"/>
<connect gate="G$1" pin="REGOUT" pad="10"/>
<connect gate="G$1" pin="SCL/SCLK" pad="23"/>
<connect gate="G$1" pin="SDA/SDI" pad="24"/>
<connect gate="G$1" pin="SDO/AD0" pad="9"/>
<connect gate="G$1" pin="VDD" pad="13"/>
<connect gate="G$1" pin="VDDIO" pad="8"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="STM32H753ZIT">
<gates>
<gate name="G$1" symbol="STM32H753ZIT_PART1"/>
<gate name="G$2" symbol="STM32H753ZIT_PART2"/>
<gate name="G$3" symbol="STM32H753ZIT_PART3"/>
<gate name="G$4" symbol="STM32H753ZIT_PART4"/>
</gates>
<devices>
<device name="LQFP144" package="LQFP144">
<connects>
<connect gate="G$1" pin="PA0" pad="34"/>
<connect gate="G$1" pin="PA1" pad="35"/>
<connect gate="G$1" pin="PA10" pad="102"/>
<connect gate="G$1" pin="PA11" pad="103"/>
<connect gate="G$1" pin="PA12" pad="104"/>
<connect gate="G$1" pin="PA13" pad="105"/>
<connect gate="G$1" pin="PA14" pad="109"/>
<connect gate="G$1" pin="PA15" pad="110"/>
<connect gate="G$1" pin="PA2" pad="36"/>
<connect gate="G$1" pin="PA3" pad="37"/>
<connect gate="G$1" pin="PA4" pad="40"/>
<connect gate="G$1" pin="PA5" pad="41"/>
<connect gate="G$1" pin="PA6" pad="42"/>
<connect gate="G$1" pin="PA7" pad="43"/>
<connect gate="G$1" pin="PA8" pad="100"/>
<connect gate="G$1" pin="PA9" pad="101"/>
<connect gate="G$1" pin="PB0" pad="46"/>
<connect gate="G$1" pin="PB1" pad="47"/>
<connect gate="G$1" pin="PB10" pad="69"/>
<connect gate="G$1" pin="PB11" pad="70"/>
<connect gate="G$1" pin="PB12" pad="73"/>
<connect gate="G$1" pin="PB13" pad="74"/>
<connect gate="G$1" pin="PB14" pad="75"/>
<connect gate="G$1" pin="PB15" pad="76"/>
<connect gate="G$1" pin="PB2" pad="48"/>
<connect gate="G$1" pin="PB3" pad="133"/>
<connect gate="G$1" pin="PB4" pad="134"/>
<connect gate="G$1" pin="PB5" pad="135"/>
<connect gate="G$1" pin="PB6" pad="136"/>
<connect gate="G$1" pin="PB7" pad="137"/>
<connect gate="G$1" pin="PB8" pad="139"/>
<connect gate="G$1" pin="PB9" pad="140"/>
<connect gate="G$2" pin="PC0" pad="26"/>
<connect gate="G$2" pin="PC1" pad="27"/>
<connect gate="G$2" pin="PC10" pad="111"/>
<connect gate="G$2" pin="PC11" pad="112"/>
<connect gate="G$2" pin="PC12" pad="113"/>
<connect gate="G$2" pin="PC13" pad="7"/>
<connect gate="G$2" pin="PC14" pad="8"/>
<connect gate="G$2" pin="PC15" pad="9"/>
<connect gate="G$2" pin="PC2" pad="28"/>
<connect gate="G$2" pin="PC3" pad="29"/>
<connect gate="G$2" pin="PC4" pad="44"/>
<connect gate="G$2" pin="PC5" pad="45"/>
<connect gate="G$2" pin="PC6" pad="96"/>
<connect gate="G$2" pin="PC7" pad="97"/>
<connect gate="G$2" pin="PC8" pad="98"/>
<connect gate="G$2" pin="PC9" pad="99"/>
<connect gate="G$2" pin="PD0" pad="114"/>
<connect gate="G$2" pin="PD1" pad="115"/>
<connect gate="G$2" pin="PD10" pad="79"/>
<connect gate="G$2" pin="PD11" pad="80"/>
<connect gate="G$2" pin="PD12" pad="81"/>
<connect gate="G$2" pin="PD13" pad="82"/>
<connect gate="G$2" pin="PD14" pad="85"/>
<connect gate="G$2" pin="PD15" pad="86"/>
<connect gate="G$2" pin="PD2" pad="116"/>
<connect gate="G$2" pin="PD3" pad="117"/>
<connect gate="G$2" pin="PD4" pad="118"/>
<connect gate="G$2" pin="PD5" pad="119"/>
<connect gate="G$2" pin="PD6" pad="122"/>
<connect gate="G$2" pin="PD7" pad="123"/>
<connect gate="G$2" pin="PD8" pad="77"/>
<connect gate="G$2" pin="PD9" pad="78"/>
<connect gate="G$3" pin="PE0" pad="141"/>
<connect gate="G$3" pin="PE1" pad="142"/>
<connect gate="G$3" pin="PE10" pad="63"/>
<connect gate="G$3" pin="PE11" pad="64"/>
<connect gate="G$3" pin="PE12" pad="65"/>
<connect gate="G$3" pin="PE13" pad="66"/>
<connect gate="G$3" pin="PE14" pad="67"/>
<connect gate="G$3" pin="PE15" pad="68"/>
<connect gate="G$3" pin="PE2" pad="1"/>
<connect gate="G$3" pin="PE3" pad="2"/>
<connect gate="G$3" pin="PE4" pad="3"/>
<connect gate="G$3" pin="PE5" pad="4"/>
<connect gate="G$3" pin="PE6" pad="5"/>
<connect gate="G$3" pin="PE7" pad="58"/>
<connect gate="G$3" pin="PE8" pad="59"/>
<connect gate="G$3" pin="PE9" pad="60"/>
<connect gate="G$3" pin="PF0" pad="10"/>
<connect gate="G$3" pin="PF1" pad="11"/>
<connect gate="G$3" pin="PF10" pad="22"/>
<connect gate="G$3" pin="PF11" pad="49"/>
<connect gate="G$3" pin="PF12" pad="50"/>
<connect gate="G$3" pin="PF13" pad="53"/>
<connect gate="G$3" pin="PF14" pad="54"/>
<connect gate="G$3" pin="PF15" pad="55"/>
<connect gate="G$3" pin="PF2" pad="12"/>
<connect gate="G$3" pin="PF3" pad="13"/>
<connect gate="G$3" pin="PF4" pad="14"/>
<connect gate="G$3" pin="PF5" pad="15"/>
<connect gate="G$3" pin="PF6" pad="18"/>
<connect gate="G$3" pin="PF7" pad="19"/>
<connect gate="G$3" pin="PF8" pad="20"/>
<connect gate="G$3" pin="PF9" pad="21"/>
<connect gate="G$4" pin="BOOT0" pad="138"/>
<connect gate="G$4" pin="GND" pad="16 38 51 61 83 94 107 120 130"/>
<connect gate="G$4" pin="GNDA" pad="31"/>
<connect gate="G$4" pin="NRST" pad="25"/>
<connect gate="G$4" pin="PDR_ON" pad="143"/>
<connect gate="G$4" pin="PG0" pad="56"/>
<connect gate="G$4" pin="PG1" pad="57"/>
<connect gate="G$4" pin="PG10" pad="125"/>
<connect gate="G$4" pin="PG11" pad="126"/>
<connect gate="G$4" pin="PG12" pad="127"/>
<connect gate="G$4" pin="PG13" pad="128"/>
<connect gate="G$4" pin="PG14" pad="129"/>
<connect gate="G$4" pin="PG15" pad="132"/>
<connect gate="G$4" pin="PG2" pad="87"/>
<connect gate="G$4" pin="PG3" pad="88"/>
<connect gate="G$4" pin="PG4" pad="89"/>
<connect gate="G$4" pin="PG5" pad="90"/>
<connect gate="G$4" pin="PG6" pad="91"/>
<connect gate="G$4" pin="PG7" pad="92"/>
<connect gate="G$4" pin="PG8" pad="93"/>
<connect gate="G$4" pin="PG9" pad="124"/>
<connect gate="G$4" pin="PH0" pad="23"/>
<connect gate="G$4" pin="PH1" pad="24"/>
<connect gate="G$4" pin="VBAT" pad="6"/>
<connect gate="G$4" pin="VCAP" pad="71 106"/>
<connect gate="G$4" pin="VCC" pad="17 30 39 52 62 72 84 108 121 131 144"/>
<connect gate="G$4" pin="VCCA" pad="33"/>
<connect gate="G$4" pin="VDD33_USB" pad="95"/>
<connect gate="G$4" pin="VREF+" pad="32"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
</devicesets>
</library>
</drawing>
</eagle>
