Index of Functions: A B C D E F G H I J K L M N O P Q R S T U V W X
Index Page ckopn_c
Table of contents
Procedure Abstract Required_Reading Keywords Brief_I/O Detailed_Input | Detailed_Output Parameters Exceptions Files Particulars Examples | Restrictions Literature_References Author_and_Institution Version Index_Entries
#### Procedure
       ckopn_c ( CK, open new file. )

       void ckopn_c (  ConstSpiceChar   * fname,
                       ConstSpiceChar   * ifname,
                       SpiceInt           ncomch,
                       SpiceInt         * handle  )
#### Abstract
       Open a new CK file, returning the handle of the opened file.
#### Required_Reading
       None.
#### Keywords
       CK
#### Brief_I/O
       VARIABLE  I/O  DESCRIPTION
       --------  ---  --------------------------------------------------
       fname      I   The name of the CK file to be opened.
       ifname     I   The internal filename for the CK.
       ncomch     I   The number of characters to reserve for comments.
       handle     O   The handle of the opened CK file.
#### Detailed_Input
       fname       The name of the CK file to be opened.

       ifname      The internal filename for the CK file that is being
                   created. The internal filename may be up to 60 characters
                   long. If you do not have any conventions for tagging your
                   files, an internal filename of "CK_file" is perfectly
                   acceptable. You may also leave it blank if you like.

       ncomch      This is the space, measured in characters, to be
                   initially set aside for the comment area when a new CK
                   file is opened. The amount of space actually set aside
                   may be greater than the amount requested, due to the
                   manner in which comment records are allocated in an CK
                   file. However, the amount of space set aside for comments
                   will always be at least the amount that was requested.

                   The value of ncomch should be greater than or equal to
                   zero, i.e., 0 <= ncomch. A negative value, should one
                   occur, will be assumed to be zero.
#### Detailed_Output
       handle      The handle of the opened CK file. If an error occurs the
                   value of this variable will not represent a valid handle.
#### Parameters
       None.
#### Exceptions
       1)  If the value of `ncomch' is negative, a value of zero (0) will
           be used for the number of comment characters to be set aside
           for comments.

       2)  If an error occurs while attempting to open a CK file the
           value of `handle' will not represent a valid file handle.

       3)  If any of the `fname' or `ifname' input string pointers is
           null, the error SPICE(NULLPOINTER) is signaled.

       4)  If any of the `fname' or `ifname' input strings has zero
           length, the error SPICE(EMPTYSTRING) is signaled.
#### Files
       See fname and handle.
#### Particulars
       Open a new CK file, reserving room for comments if requested.

       A ckcls_c call should balance every ckopn_c call.
#### Examples
       The numerical results shown for this example may differ across
       platforms. The results depend on the SPICE kernels used as
       input, the compiler and supporting libraries, and the machine
       specific arithmetic implementation.

       1) Create a CK type 3 segment; fill with data for a simple time
          dependent rotation and angular velocity, and reserve room in
          the CK comments area for 5000 characters.

          Example code begins here.

          /.
             Program ckopn_ex1
          ./
          #include "SpiceUsr.h"

          int main( )
          {

             /.
             Local parameters.
             ./
             #define CK3          "ckopn_ex1.bc"
             #define SPTICK       0.001
             #define INST         -77703
             #define MAXREC       201

             /.
             Local variables.
             ./
             SpiceChar          * ref;
             SpiceChar          * ifname;
             SpiceChar          * segid;

             SpiceDouble          avvs   [MAXREC][3];
             SpiceDouble          begtim;
             SpiceDouble          endtim;
             SpiceDouble          quats  [MAXREC][4];
             SpiceDouble          rate;
             SpiceDouble          rwmat  [3][3];
             SpiceDouble          spaces;
             SpiceDouble          sclkdp [MAXREC];
             SpiceDouble          starts [MAXREC/2];
             SpiceDouble          sticks;
             SpiceDouble          theta;
             SpiceDouble          wmat   [3][3];
             SpiceDouble          wquat  [4];

             SpiceInt             handle;
             SpiceInt             i;
             SpiceInt             ncomch;
             SpiceInt             nints;

             SpiceBoolean         avflag;

             /.
             `ncomch' is the number of characters to reserve for the
             kernel's comment area. This example doesn't write
             comments, so set to zero.
             ./
             ncomch = 0;

             /.
             The base reference from for the rotation data.
             ./
             ref = "J2000";

             /.
             Time spacing in encoded ticks and in seconds
             ./
             sticks = 10.0;
             spaces = sticks * SPTICK;

             /.
             Declare an angular rate in radians per sec.
             ./
             rate = 1.e-2;

             /.
             Internal file name and segment ID.
             ./
             segid  = "Test type 3 CK segment";
             ifname = "Test CK type 3 segment created by ckw03_c";

             /.
             Open a new kernel.
             ./
             ckopn_c ( CK3, ifname, ncomch, &handle );

             /.
             Create a 3x3 double precision identity matrix.
             ./
             ident_c ( wmat );

             /.
             Convert the matrix to quaternion.
             ./
             m2q_c ( wmat, wquat );

             /.
             Copy the work quaternion to the first row of
             `quats'.
             ./
             moved_c ( wquat, 4, quats[0] );

             /.
             Create an angular velocity vector. This vector is in the
             `ref' reference frame and indicates a constant rotation
             about the Z axis.
             ./
             vpack_c ( 0.0, 0.0, rate, avvs[0] );

             /.
             Set the initial value of the encoded ticks.
             ./
             sclkdp[0] = 1000.0;

             /.
             Fill the rest of the `avvs' and `quats' matrices
             with simple data.
             ./
             for ( i = 1; i < MAXREC; i++ )
             {

                /.
                Create the corresponding encoded tick value in
                increments of `sticks' with an initial value of
                1000.0 ticks.
                ./
                sclkdp[i] = 1000.0 + i * sticks;

                /.
                Create the transformation matrix for a rotation of
                `theta' about the Z axis. Calculate `theta' from the
                constant angular rate `rate' at increments of `spaces'.
                ./
                theta = i * rate * spaces;
                rotmat_c ( wmat, theta, 3, rwmat );

                /.
                Convert the `rwmat' matrix to SPICE type quaternion.
                ./
                m2q_c ( rwmat, wquat );

                /.
                Store the quaternion in the `quats' matrix.
                Store angular velocity in `avvs'.
                ./
                moved_c ( wquat, 4, quats[i] );
                vpack_c ( 0.0, 0.0, rate, avvs[i] );

             }

             /.
             Create an array start times for the interpolation
             intervals. The end time for a particular interval is
             determined as the time of the final data value prior in
              time to the next start time.
             ./
             nints = MAXREC/2;
             for ( i = 0; i < nints; i++ )
             {

                starts[i] = sclkdp[i*2];

             }

             /.
             Set the segment boundaries equal to the first and last
             time for the data arrays.
             ./
             begtim = sclkdp[0];
             endtim = sclkdp[MAXREC-1];

             /.
             This segment contains angular velocity.
             ./
             avflag = SPICETRUE;

             /.
             All information ready to write. Write to a CK type 3
             segment to the file indicated by `handle'.
             ./
             ckw03_c ( handle, begtim, endtim, INST, ref,   avflag, segid,
                       MAXREC, sclkdp, quats,  avvs, nints, starts       );

             /.
             SAFELY close the file.
             ./
             ckcls_c ( handle );

             return ( 0 );
          }

          When this program is executed, no output is presented on
          screen. After run completion, a new CK file exists in the
          output directory.
#### Restrictions
       None.
#### Literature_References
       None.
#### Author_and_Institution
       N.J. Bachman        (JPL)
       J. Diaz del Rio     (ODC Space)
       K.R. Gehringer      (JPL)
#### Version
       -CSPICE Version 1.1.2, 10-AUG-2021 (JDR)

           Updated -Examples section to comply with NAIF standard. Added
           complete code example based on existing fragment.

           Extended -Parameters section. Re-ordered header sections.

       -CSPICE Version 1.1.1, 09-NOV-2006 (NJB)

           Header comments indicating that `ncomch' is ignored have
           been deleted.

       -CSPICE Version 1.1.0, 08-FEB-1998 (NJB)

           References to C2F_CreateStr_Sig were removed; code was
           cleaned up accordingly. String checks are now done using
           the macro CHKFSTR.

       -CSPICE Version 1.0.0, 25-OCT-1997 (NJB) (KRG)

          Based on SPICELIB Version 1.0.0, 26-JAN-1995 (KRG)
#### Index_Entries
       open a new CK file
#### Link to routine ckopn_c source file ckopn_c.c

    Fri Dec 31 18:41:02 2021