Index of Functions: A B C D E F G H I J K L M N O P Q R S T U V W X
Index Page frinfo_c
Table of contents
Procedure Abstract Required_Reading Keywords Brief_I/O Detailed_Input | Detailed_Output Parameters Exceptions Files Particulars Examples | Restrictions Literature_References Author_and_Institution Version Index_Entries
#### Procedure
       frinfo_c ( Frame Information )

       void frinfo_c ( SpiceInt       frcode,
                       SpiceInt      *cent,
                       SpiceInt      *frclss,
                       SpiceInt      *clssid,
                       SpiceBoolean  *found   )
#### Abstract
       Retrieve the minimal attributes associated with a frame
       needed for converting transformations to and from it.
#### Required_Reading
       None.
#### Keywords
       FRAMES
#### Brief_I/O
       VARIABLE  I/O  DESCRIPTION
       --------  ---  --------------------------------------------------
       frcode     I   the idcode for some frame
       cent       O   the center of the frame
       frclss     O   the class (type) of the frame
       clssid     O   the idcode for the frame within its class.
       found      O   SPICETRUE if the requested information is available.
#### Detailed_Input
       frcode      is the ID code for some reference frame.
#### Detailed_Output
       cent        is the body ID code for the center of the reference
                   frame (if such an ID code is appropriate).

       frclss      is the class or type of the frame. This identifies
                   which subsystem will be used to perform frame
                   transformations.

       clssid      is the ID-code used for the frame within its class.
                   This may be different from the frame ID-code.

       found       is SPICETRUE if cent, frclss and frcode are available.
                   Otherwise, found is returned with the value SPICEFALSE.
#### Parameters
       None.
#### Exceptions
       1)  If a frame definition is encountered that does not define a
           central body for the frame, an error is signaled by a routine
           in the call tree of this routine.

       2)  If a frame definition is encountered that does not define
           a class for the frame, an error is signaled by a routine
           in the call tree of this routine.

       3)  If a frame definition is encountered that does not define a
           class ID for the frame, an error is signaled by a routine in
           the call tree of this routine.

       4)  If a kernel variable defining a frame name is found, but that
           variable has dimension greater than 1, the error
           SPICE(INVALIDDIMENSION) is signaled by a routine in the call
           tree of this routine.
#### Files
       None.
#### Particulars
       This is a low level routine needed by state transformation
       software to transform states and attitudes between different
       reference frames.

       The routine first examines local "hard-coded" information about
       reference frames to see if the requested frame belongs to this
       set. If it does that information is returned.

       If the requested information is not stored locally, the routine
       then examines the kernel pool to see if the requested information
       is stored there. If it is and has the expected format, the data
       is retrieved and returned.
#### Examples
       The numerical results shown for this example may differ across
       platforms. The results depend on the SPICE kernels used as
       input, the compiler and supporting libraries, and the machine
       specific arithmetic implementation.

       1) Given a frame ID, retrieve the SPICE body ID associated with the
          frame's center, the frame class (or type of the frame), and the
          ID used for the frame within its class.

          Example code begins here.

          /.
             Program frinfo_ex1
          ./
          #include <stdio.h>
          #include "SpiceUsr.h"

          int main( )
          {
             /.
             Local constants.
             ./
             SpiceInt                frcode = 13000;

             /.
             Local variables.
             ./
             SpiceBoolean            found;

             SpiceInt                cent;
             SpiceInt                clssid;
             SpiceInt                frclss;

             /.
             Retrieve the information for frame ID 13000.
             ./
             frinfo_c ( frcode, &cent, &frclss, &clssid, &found );

             if ( found )
             {
                printf ( "Frame center  : %d\n", (int)cent   );
                printf ( "Frame class   : %d\n", (int)frclss );
                printf ( "Frame class ID: %d\n", (int)clssid );
             }
             else
             {
                printf ( "There is insufficient data for frame %d\n",
                          (int)frcode                               );
             }

             return ( 0 );

          }

          When this program was executed on a Mac/Intel/cc/64-bit
          platform, the output was:

          Frame center  : 399
          Frame class   : 2
          Frame class ID: 3000
#### Restrictions
       None.
#### Literature_References
       None.
#### Author_and_Institution
       N.J. Bachman        (JPL)
       J. Diaz del Rio     (ODC Space)
       W.L. Taber          (JPL)
#### Version
       -CSPICE Version 1.2.1, 02-AUG-2021 (JDR)

           Edited the header to comply with NAIF standard. Added
           complete code example.

           Added -Exceptions section.

       -CSPICE Version 1.2.0, 22-JUL-1999 (NJB)

           Now uses logical local variable for found flag.

       -CSPICE Version 1.1.0, 16-MAY-1999 (NJB)

           Changed name of argument "class" to frclss for C++
           compatibility.

       -CSPICE Version 1.0.0, 21-JUN-1998 (NJB) (WLT)

           Based on SPICELIB Version 3.0.0, 03-JUN-1997 (WLT)
#### Index_Entries
       Fetch reference frame attributes
#### Link to routine frinfo_c source file frinfo_c.c

    Fri Dec 31 18:41:06 2021