Index of Functions: A B C D E F G H I J K L M N O P Q R S T U V W X
Index Page vsep_c
Table of contents
Procedure Abstract Required_Reading Keywords Brief_I/O Detailed_Input | Detailed_Output Parameters Exceptions Files Particulars Examples | Restrictions Literature_References Author_and_Institution Version Index_Entries
#### Procedure
       vsep_c ( Angular separation of vectors, 3 dimensions )

       SpiceDouble vsep_c ( ConstSpiceDouble     v1     [3],
                            ConstSpiceDouble     v2     [3] )
#### Abstract
       Find the separation angle in radians between two double
       precision, 3-dimensional vectors. This angle is defined as zero
       if either vector is zero.
#### Required_Reading
       None.
#### Keywords
       ANGLE
       VECTOR
#### Brief_I/O
       VARIABLE  I/O  DESCRIPTION
       --------  ---  --------------------------------------------------
       v1         I   First vector.
       v2         I   Second vector.

       The function returns the angle between `v1' and `v2' expressed in
       radians.
#### Detailed_Input
       v1,
       v2          are two double precision 3-dimensional vectors. Either
                   `v1' or `v2', or both, may be the zero vector.

                   An implicit assumption exists that `v1' and `v2' are
                   specified in the same reference frame. If this is not
                   the case, the numerical result of this routine has no
                   meaning.
#### Detailed_Output
       The function returns the angle between `v1' and `v2' expressed in
       radians.

       vsep_c is strictly non-negative. If either `v1' or `v2' is the zero
       vector, then vsep_c is defined to be 0 radians.
#### Parameters
       None.
#### Exceptions
       Error free.
#### Files
       None.
#### Particulars
       In the plane, it is a simple matter to calculate the angle
       between two vectors once the two vectors have been made to be
       unit length. Then, since the two vectors form the two equal
       sides of an isosceles triangle, the length of the third side
       is given by the expression

          length = 2.0 * sin ( vsep_c /2.0 )

       The length is given by the magnitude of the difference of the
       two unit vectors

          length = norm ( u1 - u2 )

       Once the length is found, the value of vsep_c may be calculated
       by inverting the first expression given above as

          vsep_c  = 2.0 * arcsin ( length/2.0 )

       This expression becomes increasingly unstable when vsep_c gets
       larger than pi/2 radians or 90 degrees. In this situation (which
       is easily detected by determining the sign of the dot product of
       `v1' and `v2') the supplementary angle is calculated first and
       then vsep_c is given by

             vsep_c  = pi - supplementary_angle
#### Examples
       The numerical results shown for this example may differ across
       platforms. The results depend on the SPICE kernels used as
       input, the compiler and supporting libraries, and the machine
       specific arithmetic implementation.

       1) Define two sets of 3-dimensional vectors and compute the
          angular separation between each vector in first set and the
          corresponding vector in the second set.

          Example code begins here.

          /.
             Program vsep_ex1
          ./
          #include <stdio.h>
          #include "SpiceUsr.h"

          int main( )
          {

             /.
             Local parameters.
             ./
             #define SETSIZ       3

             /.
             Local variables.
             ./
             SpiceInt             i;

             /.
             Define the two vector sets.
             ./
             SpiceDouble          v1     [SETSIZ][3] = {
                                       {1.0,  0.0,  0.0},
                                       {1.0,  0.0,  0.0},
                                       {3.0,  0.0,  0.0} };

             SpiceDouble          v2     [SETSIZ][3] = {
                                       { 1.0,  0.0,  0.0},
                                       { 0.0,  1.0,  0.0},
                                       {-5.0,  0.0,  0.0} };

             /.
             Calculate the angular separation between each pair
             of vectors.
             ./
             for ( i = 0; i < SETSIZ; i++ )
             {

                printf( "First vector            :  %5.1f %5.1f %5.1f\n",
                                           v1[i][0], v1[i][1], v1[i][2] );
                printf( "Second vector           :  %5.1f %5.1f %5.1f\n",
                                           v2[i][0], v2[i][1], v2[i][2] );
                printf( "Angular separation (rad):  %14.10f\n",
                                      vsep_c ( v1[i], v2[i] ) );
                printf( "\n" );

             }

             return ( 0 );
          }

          When this program was executed on a Mac/Intel/cc/64-bit
          platform, the output was:

          First vector            :    1.0   0.0   0.0
          Second vector           :    1.0   0.0   0.0
          Angular separation (rad):    0.0000000000

          First vector            :    1.0   0.0   0.0
          Second vector           :    0.0   1.0   0.0
          Angular separation (rad):    1.5707963268

          First vector            :    3.0   0.0   0.0
          Second vector           :   -5.0   0.0   0.0
          Angular separation (rad):    3.1415926536
#### Restrictions
       1)  The user is required to insure that the input vectors will not
           cause floating point overflow upon calculation of the vector
           dot product since no error detection or correction code is
           implemented. In practice, this is not a significant
           restriction.
#### Literature_References
       None.
#### Author_and_Institution
       N.J. Bachman        (JPL)
       J. Diaz del Rio     (ODC Space)
       K.R. Gehringer      (JPL)
       W.M. Owen           (JPL)
       W.L. Taber          (JPL)
       E.D. Wright         (JPL)
#### Version
       -CSPICE Version 1.1.2, 10-AUG-2021 (JDR)

           Edited the header to comply with NAIF standard. Added complete
           code example based on existing example.

       -CSPICE Version 1.1.1, 17-APR-2006 (EDW)

           Typo correction to the value of PI/2 in the -Examples
           section, 1.571 instead of 1.71.

       -CSPICE Version 1.1.0, 22-OCT-1998 (NJB)

           Made input vectors const.

       -CSPICE Version 1.0.0, 08-FEB-1998 (EDW) (KRG) (WMO) (WLT)
#### Index_Entries
       angular separation of 3-dimensional vectors
#### Link to routine vsep_c source file vsep_c.c

    Fri Dec 31 18:41:15 2021