Index of Functions: A B C D E F G H I J K L M N O P Q R S T U V W X
Index Page latrec_c
Table of contents
Procedure Abstract Required_Reading Keywords Brief_I/O Detailed_Input | Detailed_Output Parameters Exceptions Files Particulars Examples | Restrictions Literature_References Author_and_Institution Version Index_Entries
#### Procedure
       latrec_c ( Latitudinal to rectangular coordinates )

       void latrec_c ( SpiceDouble    radius,
                       SpiceDouble    lon,
                       SpiceDouble    lat,
                       SpiceDouble    rectan[3] )
#### Abstract
       Convert from latitudinal coordinates to rectangular coordinates.
#### Required_Reading
       None.
#### Keywords
       CONVERSION
       COORDINATES
#### Brief_I/O
       VARIABLE  I/O  DESCRIPTION
       --------  ---  --------------------------------------------------
       radius     I   Distance of a point from the origin.
       lon        I   Longitude of point in radians.
       lat        I   Latitude of point in radians.
       rectan     O   Rectangular coordinates of the point.
#### Detailed_Input
       radius      is the distance of a point from the origin.

       lon         is the longitude of the input point. This is the angle
                   between the prime meridian and the meridian containing
                   `rectan'. The direction of increasing longitude is from
                   the +X axis towards the +Y axis.

                   `lon' is measured in radians. On input, the range
                   of longitude is unrestricted.

       lat         is the latitude of the input point. This is the angle
                   from the XY plane of the ray from the origin through the
                   point.

                   `lat' is measured in radians. On input, the range of
                   latitude is unrestricted.
#### Detailed_Output
       rectan      are the rectangular coordinates of the input point.
                   `rectan' is a 3 vector.

                   The units associated with `rectan' are those
                   associated with the input `radius'.
#### Parameters
       None.
#### Exceptions
       Error free.
#### Files
       None.
#### Particulars
       This routine returns the rectangular coordinates of a point
       whose position is input in latitudinal coordinates.

       Latitudinal coordinates are defined by a distance from a central
       reference point, an angle from a reference meridian, and an angle
       above the equator of a sphere centered at the central reference
       point.
#### Examples
       The numerical results shown for these examples may differ across
       platforms. The results depend on the SPICE kernels used as
       input, the compiler and supporting libraries, and the machine
       specific arithmetic implementation.

       1) Compute the latitudinal coordinates of the position of the
          Moon as seen from the Earth, and convert them to rectangular
          coordinates.

          Use the meta-kernel shown below to load the required SPICE
          kernels.

             KPL/MK

             File name: latrec_ex1.tm

             This meta-kernel is intended to support operation of SPICE
             example programs. The kernels shown here should not be
             assumed to contain adequate or correct versions of data
             required by SPICE-based user applications.

             In order for an application to use this meta-kernel, the
             kernels referenced here must be present in the user's
             current working directory.

             The names and contents of the kernels referenced
             by this meta-kernel are as follows:

                File name                     Contents
                ---------                     --------
                de421.bsp                     Planetary ephemeris
                naif0012.tls                  Leapseconds

             \begindata

                KERNELS_TO_LOAD = ( 'de421.bsp',
                                    'naif0012.tls'  )

             \begintext

             End of meta-kernel

          Example code begins here.

          /.
             Program latrec_ex1
          ./
          #include <stdio.h>
          #include "SpiceUsr.h"

          int main( )
          {

             /.
             Local variables
             ./
             SpiceDouble          et;
             SpiceDouble          lat;
             SpiceDouble          lon;
             SpiceDouble          lt;
             SpiceDouble          pos    [3];
             SpiceDouble          radius;
             SpiceDouble          rectan [3];

             /.
             Load SPK and LSK kernels, use a meta kernel for
             convenience.
             ./
             furnsh_c ( "latrec_ex1.tm" );

             /.
             Look up the geometric state of the Moon as seen from
             the Earth at 2017 Mar 20, relative to the J2000
             reference frame.
             ./
             str2et_c ( "2017 Mar 20", &et );

             spkpos_c ( "Moon", et, "J2000", "NONE", "Earth", pos, &lt );

             /.
             Convert the position vector `pos' to latitudinal
             coordinates.
             ./
             reclat_c ( pos, &radius, &lon, &lat );

             /.
             Convert the latitudinal to rectangular coordinates.
             ./

             latrec_c ( radius, lon, lat, rectan );

             printf( " \n" );
             printf( "Original rectangular coordinates:\n" );
             printf( " \n" );
             printf( " X          (km):  %19.8f\n", pos[0] );
             printf( " Y          (km):  %19.8f\n", pos[1] );
             printf( " Z          (km):  %19.8f\n", pos[2] );
             printf( " \n" );
             printf( "Latitudinal coordinates:\n" );
             printf( " \n" );
             printf( " Radius     (km):  %19.8f\n", radius );
             printf( " Longitude (deg):  %19.8f\n", lon*dpr_c ( ) );
             printf( " Latitude  (deg):  %19.8f\n", lat*dpr_c ( ) );
             printf( " \n" );
             printf( "Rectangular coordinates from latrec_c:\n" );
             printf( " \n" );
             printf( " X          (km):  %19.8f\n", rectan[0] );
             printf( " Y          (km):  %19.8f\n", rectan[1] );
             printf( " Z          (km):  %19.8f\n", rectan[2] );
             printf( " \n" );

             return ( 0 );
          }

          When this program was executed on a Mac/Intel/cc/64-bit
          platform, the output was:

          Original rectangular coordinates:

           X          (km):      -55658.44323296
           Y          (km):     -379226.32931475
           Z          (km):     -126505.93063865

          Latitudinal coordinates:

           Radius     (km):      403626.33912495
           Longitude (deg):         -98.34959789
           Latitude  (deg):         -18.26566077

          Rectangular coordinates from latrec_c:

           X          (km):      -55658.44323296
           Y          (km):     -379226.32931475
           Z          (km):     -126505.93063865

       2) Create a table showing a variety of latitudinal coordinates
          and the corresponding rectangular coordinates.

          Corresponding latitudinal and rectangular coordinates are
          listed to three decimal places. Input angles are in degrees.

          Example code begins here.

          /.
             Program latrec_ex2
          ./
          #include <stdio.h>
          #include "SpiceUsr.h"

          int main( )
          {
             /.
             Local constants.
             ./
             #define NPTS            11

             /.
             Local variables.
             ./
             SpiceDouble             rectan[3];
             SpiceDouble             rlon;
             SpiceDouble             rlat;

             SpiceInt                i;

             /.
             Define eleven sets of latitude coordinates, `lon'
             and `lat' expressed in degrees.
             ./
             SpiceDouble             radius[NPTS] = { 0.0,    1.0,    1.0,
                                                      1.0,    1.0,    1.0,
                                                      1.0,    1.4142, 1.4142,
                                                      1.4142, 1.732          };

             SpiceDouble             lon   [NPTS] = {  0.0,  0.0,   90.0,
                                                       0.0, 180.0, -90.0,
                                                       0.0,  45.0,   0.0,
                                                      90.0,  45.0        };

             SpiceDouble             lat   [NPTS] = {   0.0,  0.0,     0.0,
                                                       90.0,  0.0,     0.0,
                                                      -90.0,  0.0,    45.0,
                                                       45.0,  35.2643      };

             /.
             Print a header for the data output.
             ./
             printf( "  radius    lon      lat    rect[0]  rect[1]  rect[2]\n" );
             printf( " -------  -------  -------  -------  -------  -------\n" );

             for ( i = 0; i < NPTS; i++ )
             {
                /.
                Convert `lon' and `lat' from degrees to radians.
                ./
                rlon = lon[i] * rpd_c();
                rlat = lat[i] * rpd_c();

                /.
                Convert the coordinates from latitudinal to rectangular.
                ./
                latrec_c ( radius[i], rlon, rlat, rectan );

                /.
                Output the row of the coordinate table.
                ./
                printf ( "%8.3f %8.3f %8.3f %8.3f %8.3f %8.3f\n",
                                        radius[i], lon[i],    lat[i],
                                        rectan[0], rectan[1], rectan[2] );
             }

             return( 0 );
          }

          When this program was executed on a Mac/Intel/cc/64-bit
          platform, the output was:

            radius    lon      lat    rect[0]  rect[1]  rect[2]
           -------  -------  -------  -------  -------  -------
             0.000    0.000    0.000    0.000    0.000    0.000
             1.000    0.000    0.000    1.000    0.000    0.000
             1.000   90.000    0.000    0.000    1.000    0.000
             1.000    0.000   90.000    0.000    0.000    1.000
             1.000  180.000    0.000   -1.000    0.000    0.000
             1.000  -90.000    0.000    0.000   -1.000    0.000
             1.000    0.000  -90.000    0.000    0.000   -1.000
             1.414   45.000    0.000    1.000    1.000    0.000
             1.414    0.000   45.000    1.000    0.000    1.000
             1.414   90.000   45.000    0.000    1.000    1.000
             1.732   45.000   35.264    1.000    1.000    1.000
#### Restrictions
       None.
#### Literature_References
       None.
#### Author_and_Institution
       C.H. Acton          (JPL)
       N.J. Bachman        (JPL)
       J. Diaz del Rio     (ODC Space)
       E.D. Wright         (JPL)
#### Version
       -CSPICE Version 1.1.0, 04-JUL-2021 (JDR)

           Changed input argument names "longitude" and "latitude to "lon"
           and "lat" for consistency with other routines.

           Edited the header to comply with NAIF standard. Added
           complete code examples based on existing example.

       -CSPICE Version 1.0.1, 29-JUL-2003 (NJB) (CHA)

           Various header corrections were made.

       -CSPICE Version 1.0.0, 16-APR-1999 (EDW)
#### Index_Entries
       latitudinal to rectangular coordinates
#### Link to routine latrec_c source file latrec_c.c

    Fri Dec 31 18:41:08 2021