Index of Functions: A B C D E F G H I J K L M N O P Q R S T U V W X
Index Page spksfs_c
Table of contents
Procedure Abstract Required_Reading Keywords Brief_I/O Detailed_Input | Detailed_Output Parameters Exceptions Files Particulars Examples | Restrictions Literature_References Author_and_Institution Version Index_Entries
#### Procedure
       spksfs_c ( S/P Kernel, Select file and segment )

       void spksfs_c ( SpiceInt        body,
                       SpiceDouble     et,
                       SpiceInt        idlen,
                       SpiceInt      * handle,
                       SpiceDouble     descr [5],
                       SpiceChar     * ident,
                       SpiceBoolean  * found     )
#### Abstract
       Search through loaded SPK files to find the highest-priority
       segment applicable to the body and time specified and buffer
       searched segments in the process, to attempt to avoid re-reading
       files.
#### Required_Reading
       SPK
#### Keywords
       EPHEMERIS
       FILES
#### Brief_I/O
       VARIABLE  I/O  DESCRIPTION
       --------  ---  --------------------------------------------------
       body       I   Body ID.
       et         I   Ephemeris time.
       idlen      I   Length of output segment ID string.
       handle     O   Handle of file containing the applicable segment.
       descr      O   Descriptor of the applicable segment.
       ident      O   Identifier of the applicable segment.
       found      O   Indicates whether or not a segment was found.
       SIDLEN     P   Maximum length of segment ID.
#### Detailed_Input
       body        is the NAIF integer code of an ephemeris object,
                   typically a solar system body.

       et          is a time, in seconds past the epoch J2000 TDB.

       idlen       is the allowed length of the output string. This length
                   must large enough to hold the output segment ID plus the
                   null terminator. SPK segment identifiers may contain up
                   to SIDLEN characters, excluding the null terminator.
#### Detailed_Output
       handle      is the handle of the SPK file containing a located
                   segment.

       descr       is the descriptor of a located SPK segment. `descr'
                   has length 5.

       ident       is the SPK segment identifier of a located SPK segment.

       found       is a logical flag indicating whether a requested segment was
                   found or not. The other output arguments are valid only if
                   `found' is set to SPICETRUE.
#### Parameters
       SIDLEN      is the maximum number of characters in an SPK segment
                   identifier, excluding the null terminator.

                   SIDLEN is set to 40.
#### Exceptions
       1)  If an attempt is made to call spksfs_c when there aren't any
           files loaded, the error SPICE(NOLOADEDFILES) is signaled by a
           routine in the call tree of this routine.

       2)  If an error occurs while this routine attempts to extract
           segment descriptors from loaded SPK files, the error is
           signaled by a routine in the call tree of this routine.

           Note however that I/O errors occurring during reads of DAF
           double precision records are NOT treated as SPICE errors
           and are not signaled.

       3)  If the `ident' output string pointer is null, the error
           SPICE(NULLPOINTER) is signaled.

       4)  If the `ident' output string has length less than two
           characters, the error SPICE(STRINGTOOSHORT) is signaled, since
           the output string is too short to contain one character of
           output data plus a null terminator.
#### Files
       All SPK files loaded by furnsh_c or spklef_c are potential search
       targets for spksfs_c.
#### Particulars
       This routine finds the highest-priority segment, in any loaded
       SPK file, such that the segment provides data for the specified
       body and epoch.
#### Examples
       The numerical results shown for this example may differ across
       platforms. The results depend on the SPICE kernels used as
       input, the compiler and supporting libraries, and the machine
       specific arithmetic implementation.

       1) Find a segment for the Pluto barycenter, with coverage for
          a specified epoch, in a JPL planetary SPK file, and display
          the segment's information.

          Use the meta-kernel shown below to load the required SPICE
          kernels.

             KPL/MK

             File name: spksfs_ex1.tm

             This meta-kernel is intended to support operation of SPICE
             example programs. The kernels shown here should not be
             assumed to contain adequate or correct versions of data
             required by SPICE-based user applications.

             In order for an application to use this meta-kernel, the
             kernels referenced here must be present in the user's
             current working directory.

             The names and contents of the kernels referenced
             by this meta-kernel are as follows:

                File name                     Contents
                ---------                     --------
                de421.bsp                     Planetary ephemeris
                naif0010.tls                  Leapseconds

             \begindata

                KERNELS_TO_LOAD = ( 'de421.bsp',
                                    'naif0010.tls'  )

             \begintext

             End of meta-kernel

          Example code begins here.

          /.
             Program spksfs_ex1
          ./
          #include <stdio.h>
          #include "SpiceUsr.h"

          int main()
          {
             /.
             Local parameters
             ./
             #define ND                       2
             #define NI                       6
             #define DSCSIZ                   5
             #define SIDLEN1                 41

             /.
             Local variables
             ./
             SpiceBoolean            found;

             SpiceChar               segid   [ SIDLEN1 ];
             SpiceChar             * reqtim;

             SpiceDouble             dc      [ ND ];
             SpiceDouble             descr   [ DSCSIZ ];
             SpiceDouble             et;

             SpiceInt                handle;
             SpiceInt                ic      [ NI ];
             SpiceInt                idcode;

             /.
             Load a meta-kernel that specifies a planetary SPK file
             and leapseconds kernel. The contents of this meta-kernel
             are displayed above.
             ./
             furnsh_c ( "spksfs_ex1.tm" );

             /.
             Get the NAIF ID code for the Pluto system barycenter.
             This is a built-in ID code, so something's seriously
             wrong if we can't find the code.
             ./
             bodn2c_c ( "PLUTO BARYCENTER", &idcode, &found );

             if ( !found )
             {
                sigerr_c( "SPICE(BUG)" );
             }

             /.
             Pick a request time; convert to seconds past J2000 TDB.
             ./
             reqtim = "2011 FEB 18 UTC";

             str2et_c ( reqtim, &et );

             /.
             Find a loaded segment for the specified body and time.
             ./
             spksfs_c ( idcode, et, SIDLEN1, &handle, descr, segid, &found );

             if ( !found )
             {
                printf ( "No descriptor was found for ID %d at "
                         "TDB %24.17e\n",
                         (int) idcode,
                         et                                       );
             }
             else
             {
                /.
                Display the DAF file handle.
                ./
                printf ( "\n"
                         "DAF handle: %d\n"
                         "\n",
                         (int)handle        );

                /.
                Display the segment ID.

                Unpack the descriptor. Display the contents.
                ./
                dafus_c ( descr, ND, NI, dc, ic );

                printf ( "Segment found.\n"
                         "   Segment ID:        %s\n"
                         "   Body ID code:      %d\n"
                         "   Center ID code:    %d\n"
                         "   Frame ID code:     %d\n"
                         "   SPK data type:     %d\n"
                         "   Start time (TDB):  %24.17e\n"
                         "   Stop time  (TDB):  %24.17e\n",
                         segid,
                         (int) ic[0],
                         (int) ic[1],
                         (int) ic[2],
                         (int) ic[3],
                         dc[0],
                         dc[1]                             );
             }

             return ( 0 );
          }

          When this program was executed on a Mac/Intel/cc/64-bit
          platform, the output was:

          DAF handle: 1

          Segment found.
             Segment ID:        DE-0421LE-0421
             Body ID code:      9
             Center ID code:    0
             Frame ID code:     1
             SPK data type:     2
             Start time (TDB):  -3.16919520000000000e+09
             Stop time  (TDB):   1.69685280000000000e+09
#### Restrictions
       1)  If a Fortran I/O error occurs while this routine searches a
           loaded SPK file, the internal state of SPK segment and file
           selection routines, which are all entry points in the f2c'd
           version for the Fortran routine SPKBSR, may be corrupted.
#### Literature_References
       None.
#### Author_and_Institution
       N.J. Bachman        (JPL)
       J. Diaz del Rio     (ODC Space)
       R.E. Thurman        (JPL)
       E.D. Wright         (JPL)
#### Version
       -CSPICE Version 1.0.2, 05-AUG-2021 (JDR)

           Edited the header to comply with NAIF standard.

           Moved SPK required reading from -Literature_References to
           -Required_Reading section. Added entries #3 and #4 to -Exceptions
           section.

       -CSPICE Version 1.0.1, 12-JUL-2016 (EDW)

           Edit to example program to use "%d" with explicit casts
           to int for printing SpiceInts with printf.

       -CSPICE Version 1.0.0, 05-OCT-2012 (NJB) (RET)
#### Index_Entries
       select SPK file and segment
#### Link to routine spksfs_c source file spksfs_c.c

    Fri Dec 31 18:41:13 2021