IFC building model
Schema: "IFC2X3"
Description: "ViewDefinition [CoordinationView_V2.0]"
File name: "110000XXXX"
Time stamp: "2021-01-26T16:26:43"
Preprocessor: "The EXPRESS Data Manager Version 5.02.0100.07 : 28 Aug 2013"
Originating system: "20200826_1250(x64) - Exporter 20.2.0.0 - Alternate UI 20.2.0.0"
Application: "Autodesk Revit 2020 (ENU)" version "2020" identifier "Revit" by Organization "Autodesk Revit 2020 (ENU)"

People and organizations
  Person "MSEI" of Organization (no name given)
  Owner history of Person "MSEI" of Organization (no name given) | application "Autodesk Revit 2020 (ENU)" version "2020" identifier "Revit" by Organization "Autodesk Revit 2020 (ENU)" | change NOCHANGE | created 1605876296 (2020-11-20T12:44:56Z)

Units
  LENGTHUNIT: MILLI METRE
  AREAUNIT: SQUARE_METRE
  VOLUMEUNIT: CUBIC_METRE
  PLANEANGLEUNIT: DEGREE (conversion based)
  MASSUNIT: KILO GRAM
  MASSDENSITYUNIT: derived
  MOMENTOFINERTIAUNIT: derived
  TIMEUNIT: SECOND
  FREQUENCYUNIT: HERTZ
  THERMODYNAMICTEMPERATUREUNIT: DEGREE_CELSIUS
  THERMALTRANSMITTANCEUNIT: derived
  VOLUMETRICFLOWRATEUNIT: derived
  ELECTRICCURRENTUNIT: AMPERE
  ELECTRICVOLTAGEUNIT: VOLT
  POWERUNIT: WATT
  FORCEUNIT: KILO NEWTON
  ILLUMINANCEUNIT: LUX
  LUMINOUSFLUXUNIT: LUMEN
  LUMINOUSINTENSITYUNIT: CANDELA
  USERDEFINED: derived "Luminous Efficacy"
  LINEARVELOCITYUNIT: derived
  PRESSUREUNIT: PASCAL
  USERDEFINED: derived "Friction Loss"
  LINEARFORCEUNIT: derived
  PLANARFORCEUNIT: derived

Spatial structure
IFCPROJECT "110000XXXX" | long name "Projekt Navn" | phase "FORPROJEKT"
  IFCSITE "Default" | latitude 55° 40′ 59.879999″ | longitude 12° 32′ 59.999999″ | elevation above sea level 0.
    IFCBUILDING | postal address: "Projekt Adresse", "Copenhagen", "Denmark"
      IFCBUILDINGSTOREY "Level 1" | long name "Level 1" | object type "Level:Circle 8mm Head - SP – RDK" | elevation 0.
        contains 85 elements
          2 x IFCFLOWMOVINGDEVICE | type IFCPUMPTYPE "02.00.05_Alpha:ALPHA2 25-40 A" | object type "02.00.05_Alpha:ALPHA2 25-40 A" | names: "02.00.05_Alpha:ALPHA2 25-40 A:1614379", "02.00.05_Alpha:ALPHA2 25-40 A:1703076" | material: materials ("<Unnamed>", "<Unnamed>", "<Unnamed>", "<Unnamed>", "<Unnamed>", "<Unnamed>") | property sets: Pset_DistributionFlowElementCommon, Pset_ManufacturerTypeInformation, Pset_ProductRequirements, Pset_QuantityTakeOff
          44 x IFCFLOWSEGMENT | type IFCPIPESEGMENTTYPE "Pipe Types:Galvaniseret rør" | object type "Pipe Types:Galvaniseret rør" | names: "Pipe Types:Galvaniseret rør:1614445", "Pipe Types:Galvaniseret rør:1619209", "Pipe Types:Galvaniseret rør:1625643" (+41 more) | property sets: Pset_DistributionFlowElementCommon, Pset_DuctConnection, Pset_ElementShading, Pset_FlowSegmentDuctSegment, Pset_FlowSegmentPipeSegment, Pset_PipeConnection
          4 x IFCFLOWFITTING | type IFCPIPEFITTINGTYPE "magi_pipe_fe_tee_centric_90_001:magi_pipe_fe_tee_centric_90_001" | object type "magi_pipe_fe_tee_centric_90_001:magi_pipe_fe_tee_centric_90_001" | names: "magi_pipe_fe_tee_centric_90_001:magi_pipe_fe_tee_centric_90_001:1619208", "magi_pipe_fe_tee_centric_90_001:magi_pipe_fe_tee_centric_90_001:1625755", "magi_pipe_fe_tee_centric_90_001:magi_pipe_fe_tee_centric_90_001:1647288" (+1 more) | material: "<Unnamed>" | property sets: Pset_DistributionFlowElementCommon, Pset_ProductRequirements, Pset_QuantityTakeOff
          2 x IFCFLOWCONTROLLER | type IFCVALVETYPE "02.00.05_ASV:ASV-PV Plus 25" | object type "02.00.05_ASV:ASV-PV Plus 25" | names: "02.00.05_ASV:ASV-PV Plus 25:1638649", "02.00.05_ASV:ASV-PV Plus 25:1646600" | material: materials ("<Unnamed>", "<Unnamed>", "<Unnamed>", "<Unnamed>", "<Unnamed>", "<Unnamed>", "<Unnamed>", "<Unnamed>", "<Unnamed>", "<Unnamed>") | property sets: Pset_DistributionFlowElementCommon, Pset_ManufacturerTypeInformation, Pset_ProductRequirements, Pset_QuantityTakeOff
          22 x IFCFLOWFITTING | type IFCPIPEFITTINGTYPE "magi_pipe_fe_elbow_short_001:magi_pipe_fe_elbow_short_001" | object type "magi_pipe_fe_elbow_short_001:magi_pipe_fe_elbow_short_001" | names: "magi_pipe_fe_elbow_short_001:magi_pipe_fe_elbow_short_001:1645494", "magi_pipe_fe_elbow_short_001:magi_pipe_fe_elbow_short_001:1645496", "magi_pipe_fe_elbow_short_001:magi_pipe_fe_elbow_short_001:1646642" (+19 more) | material: "<Unnamed>" | property sets: Pset_DistributionFlowElementCommon, Pset_ProductRequirements, Pset_QuantityTakeOff
          4 x IFCFLOWFITTING | type IFCPIPEFITTINGTYPE "magi_pipe_fe_elbow_short_001:magi_pipe_fe_elbow_short_001" | object type "magi_pipe_fe_elbow_short_001:magi_pipe_fe_elbow_short_001" | names: "magi_pipe_fe_elbow_short_001:magi_pipe_fe_elbow_short_001:1647204", "magi_pipe_fe_elbow_short_001:magi_pipe_fe_elbow_short_001:1647209", "magi_pipe_fe_elbow_short_001:magi_pipe_fe_elbow_short_001:1647216" (+1 more) | material: "<Unnamed>" | property sets: Pset_DistributionFlowElementCommon, Pset_ProductRequirements, Pset_QuantityTakeOff
          4 x IFCFLOWCONTROLLER | type IFCVALVETYPE "02.00.05_STADA:STADA-25" | object type "02.00.05_STADA:STADA-25" | names: "02.00.05_STADA:STADA-25:1648251", "02.00.05_STADA:STADA-25:1655452", "02.00.05_STADA:STADA-25:1655556" (+1 more) | material: materials ("<Unnamed>", "<Unnamed>", "<Unnamed>", "<Unnamed>", "<Unnamed>", "<Unnamed>", "<Unnamed>", "<Unnamed>", "<Unnamed>", "<Unnamed>", "<Unnamed>", "<Unnamed>", "<Unnamed>", "<Unnamed>", "<Unnamed>", "<Unnamed>", "<Unnamed>", "<Unnamed>") | property sets: Pset_DistributionFlowElementCommon, Pset_ManufacturerTypeInformation, Pset_ProductRequirements, Pset_QuantityTakeOff
          1 x IFCFLOWCONTROLLER | type IFCVALVETYPE "02.00.05_kont:41210" | object type "02.00.05_kont:41210" | names: "02.00.05_kont:41210:1662687" | material: materials ("<Unnamed>", "<Unnamed>", "<Unnamed>", "<Unnamed>", "<Unnamed>", "<Unnamed>", "<Unnamed>", "<Unnamed>", "<Unnamed>") | property sets: Pset_DistributionFlowElementCommon, Pset_ManufacturerTypeInformation, Pset_ProductRequirements, Pset_QuantityTakeOff
          2 x IFCFLOWTERMINAL | type IFCDISTRIBUTIONELEMENTTYPE "02.00.05_radiator:5P-655" | object type "02.00.05_radiator:5P-655" | names: "02.00.05_radiator:5P-655:1670656", "02.00.05_radiator:5P-655:1670836" | material: "MEE_RadiatorUnFilled2DSymbol_RDK" | property sets: Pset_DistributionFlowElementCommon, Pset_ProductRequirements, Pset_QuantityTakeOff

Types
  IFCPUMPTYPE "02.00.05_Alpha:ALPHA2 25-40 A" | 2 occurrences | material: materials ("<Unnamed>", "<Unnamed>", "<Unnamed>", "<Unnamed>", "<Unnamed>", "<Unnamed>") | property sets: Pset_DistributionFlowElementCommon, Pset_ManufacturerTypeInformation, Pset_ProductRequirements, Pset_QuantityTakeOff
  IFCPIPESEGMENTTYPE "Pipe Types:Galvaniseret rør" | 44 occurrences | property sets: Pset_DistributionFlowElementCommon, Pset_ProductRequirements, Pset_QuantityTakeOff
  IFCPIPEFITTINGTYPE "magi_pipe_fe_tee_centric_90_001:magi_pipe_fe_tee_centric_90_001" | 4 occurrences | material: "<Unnamed>" | property sets: Pset_DistributionFlowElementCommon, Pset_ProductRequirements, Pset_QuantityTakeOff
  IFCVALVETYPE "02.00.05_ASV:ASV-PV Plus 25" | 2 occurrences | material: materials ("<Unnamed>", "<Unnamed>", "<Unnamed>", "<Unnamed>", "<Unnamed>", "<Unnamed>", "<Unnamed>", "<Unnamed>", "<Unnamed>", "<Unnamed>") | property sets: Pset_DistributionFlowElementCommon, Pset_ManufacturerTypeInformation, Pset_ProductRequirements, Pset_QuantityTakeOff
  IFCPIPEFITTINGTYPE "magi_pipe_fe_elbow_short_001:magi_pipe_fe_elbow_short_001" | 22 occurrences | material: "<Unnamed>" | property sets: Pset_DistributionFlowElementCommon, Pset_ProductRequirements, Pset_QuantityTakeOff
  IFCPIPEFITTINGTYPE "magi_pipe_fe_elbow_short_001:magi_pipe_fe_elbow_short_001" | 4 occurrences | material: "<Unnamed>" | property sets: Pset_DistributionFlowElementCommon, Pset_ProductRequirements, Pset_QuantityTakeOff
  IFCVALVETYPE "02.00.05_STADA:STADA-25" | 4 occurrences | material: materials ("<Unnamed>", "<Unnamed>", "<Unnamed>", "<Unnamed>", "<Unnamed>", "<Unnamed>", "<Unnamed>", "<Unnamed>", "<Unnamed>", "<Unnamed>", "<Unnamed>", "<Unnamed>", "<Unnamed>", "<Unnamed>", "<Unnamed>", "<Unnamed>", "<Unnamed>", "<Unnamed>") | property sets: Pset_DistributionFlowElementCommon, Pset_ManufacturerTypeInformation, Pset_ProductRequirements, Pset_QuantityTakeOff
  IFCVALVETYPE "02.00.05_kont:41210" | 1 occurrence | material: materials ("<Unnamed>", "<Unnamed>", "<Unnamed>", "<Unnamed>", "<Unnamed>", "<Unnamed>", "<Unnamed>", "<Unnamed>", "<Unnamed>") | property sets: Pset_DistributionFlowElementCommon, Pset_ManufacturerTypeInformation, Pset_ProductRequirements, Pset_QuantityTakeOff
  IFCDISTRIBUTIONELEMENTTYPE "02.00.05_radiator:5P-655" | 2 occurrences | material: "MEE_RadiatorUnFilled2DSymbol_RDK" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff

Property sets
  Pset_ProductRequirements | properties | on 44 objects (44 IFCFLOWSEGMENT) | on 2 type objects
    Category = "Pipes" (IFCLABEL)
  Pset_ProductRequirements | properties | on 30 objects (30 IFCFLOWFITTING) | on 3 type objects
    Category = "Pipe Fittings" (IFCLABEL)
  Pset_ProductRequirements | properties | on 7 objects (7 IFCFLOWCONTROLLER) | on 3 type objects
    Category = "Pipe Accessories" (IFCLABEL)
  Pset_ProductRequirements | properties | on 4 objects (2 IFCFLOWMOVINGDEVICE, 2 IFCFLOWTERMINAL) | on 2 type objects
    Category = "Mechanical Equipment" (IFCLABEL)
  Pset_ProductRequirements | properties | on 2 objects (1 IFCBUILDING, 1 IFCSITE)
    Category = "Project Information" (IFCLABEL)
  Pset_ProductRequirements | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Category = "Levels" (IFCLABEL)
    Name = "Level 1" (IFCLABEL)
  Pset_DistributionFlowElementCommon | properties | on 44 objects (44 IFCFLOWSEGMENT) | on 2 type objects
    Reference = "Galvaniseret rør" (IFCIDENTIFIER)
  Pset_DistributionFlowElementCommon | properties | on 26 objects (26 IFCFLOWFITTING) | on 2 type objects
    Reference = "magi_pipe_fe_elbow_short_001" (IFCIDENTIFIER)
  Pset_DistributionFlowElementCommon | properties | on 4 objects (4 IFCFLOWFITTING) | on 1 type object
    Reference = "magi_pipe_fe_tee_centric_90_001" (IFCIDENTIFIER)
  Pset_DistributionFlowElementCommon | properties | on 4 objects (4 IFCFLOWCONTROLLER) | on 1 type object
    Reference = "STADA-25" (IFCIDENTIFIER)
  Pset_DistributionFlowElementCommon | properties | on 2 objects (2 IFCFLOWMOVINGDEVICE) | on 1 type object
    Reference = "ALPHA2 25-40 A" (IFCIDENTIFIER)
  Pset_DistributionFlowElementCommon | properties | on 2 objects (2 IFCFLOWCONTROLLER) | on 1 type object
    Reference = "ASV-PV Plus 25" (IFCIDENTIFIER)
  Pset_DistributionFlowElementCommon | properties | on 2 objects (2 IFCFLOWTERMINAL)
    Reference = "5P-655" (IFCIDENTIFIER)
  Pset_DistributionFlowElementCommon | properties | on 1 object (1 IFCFLOWCONTROLLER) | on 1 type object
    Reference = "41210" (IFCIDENTIFIER)
  Pset_ManufacturerTypeInformation | properties | on 4 objects (4 IFCFLOWCONTROLLER) | on 1 type object
    Manufacturer = "IMI Hydronic Engineering" (IFCLABEL)
  Pset_ManufacturerTypeInformation | properties | on 2 objects (2 IFCFLOWMOVINGDEVICE) | on 1 type object
    Manufacturer = "Grundfos" (IFCLABEL)
  Pset_ManufacturerTypeInformation | properties | on 2 objects (2 IFCFLOWCONTROLLER) | on 1 type object
    Manufacturer = "Danfoss" (IFCLABEL)
  Pset_ManufacturerTypeInformation | properties | on 1 object (1 IFCFLOWCONTROLLER) | on 1 type object
    Manufacturer = "Aquatherm" (IFCLABEL)
  Pset_QuantityTakeOff | properties | on 44 objects (44 IFCFLOWSEGMENT) | on 2 type objects
    Reference = "Galvaniseret rør" (IFCIDENTIFIER)
  Pset_QuantityTakeOff | properties | on 26 objects (26 IFCFLOWFITTING) | on 2 type objects
    Reference = "magi_pipe_fe_elbow_short_001" (IFCIDENTIFIER)
  Pset_QuantityTakeOff | properties | on 4 objects (4 IFCFLOWFITTING) | on 1 type object
    Reference = "magi_pipe_fe_tee_centric_90_001" (IFCIDENTIFIER)
  Pset_QuantityTakeOff | properties | on 4 objects (4 IFCFLOWCONTROLLER) | on 1 type object
    Reference = "STADA-25" (IFCIDENTIFIER)
  Pset_QuantityTakeOff | properties | on 2 objects (2 IFCFLOWMOVINGDEVICE) | on 1 type object
    Reference = "ALPHA2 25-40 A" (IFCIDENTIFIER)
  Pset_QuantityTakeOff | properties | on 2 objects (2 IFCFLOWCONTROLLER) | on 1 type object
    Reference = "ASV-PV Plus 25" (IFCIDENTIFIER)
  Pset_QuantityTakeOff | properties | on 2 objects (2 IFCFLOWTERMINAL) | on 1 type object
    Reference = "5P-655" (IFCIDENTIFIER)
  Pset_QuantityTakeOff | properties | on 1 object (1 IFCFLOWCONTROLLER) | on 1 type object
    Reference = "41210" (IFCIDENTIFIER)
  Pset_DuctConnection | properties | on 44 objects (44 IFCFLOWSEGMENT)
    ConnectionType = ["Generic"] (IFCTEXT)
  Pset_ElementShading | properties | on 44 objects (44 IFCFLOWSEGMENT)
    Roughness = 0.0450000017881393 (IFCPOSITIVELENGTHMEASURE) [MILLI METRE]
  Pset_FlowSegmentDuctSegment | properties | on 2 objects (2 IFCFLOWSEGMENT)
    Length = 480.075000000031 (IFCPOSITIVELENGTHMEASURE) [MILLI METRE]
  Pset_FlowSegmentDuctSegment | properties | on 2 objects (2 IFCFLOWSEGMENT)
    Length = 260.446116911296 (IFCPOSITIVELENGTHMEASURE) [MILLI METRE]
  Pset_FlowSegmentDuctSegment | properties | on 2 objects (2 IFCFLOWSEGMENT)
    Length = 312.400000000002 (IFCPOSITIVELENGTHMEASURE) [MILLI METRE]
  Pset_FlowSegmentDuctSegment | properties | on 2 objects (2 IFCFLOWSEGMENT)
    Length = 262.969670197159 (IFCPOSITIVELENGTHMEASURE) [MILLI METRE]
  Pset_FlowSegmentDuctSegment | properties | on 2 objects (2 IFCFLOWSEGMENT)
    Length = 2632.4 (IFCPOSITIVELENGTHMEASURE) [MILLI METRE]
  Pset_FlowSegmentDuctSegment | properties | on 2 objects (2 IFCFLOWSEGMENT)
    Length = 56.7696701971546 (IFCPOSITIVELENGTHMEASURE) [MILLI METRE]
  Pset_FlowSegmentDuctSegment | properties | on 1 object (1 IFCFLOWSEGMENT)
    Length = 390.478292343424 (IFCPOSITIVELENGTHMEASURE) [MILLI METRE]
  Pset_FlowSegmentDuctSegment | properties | on 1 object (1 IFCFLOWSEGMENT)
    Length = 576.420408303681 (IFCPOSITIVELENGTHMEASURE) [MILLI METRE]
  Pset_FlowSegmentDuctSegment: 30 more contents on 30 objects not shown
  Pset_FlowSegmentPipeSegment | properties | on 2 objects (2 IFCFLOWSEGMENT)
    InvertElevation = -13.5999999999897 (IFCLENGTHMEASURE) [MILLI METRE]
    Length = 480.075000000031 (IFCPOSITIVELENGTHMEASURE) [MILLI METRE]
  Pset_FlowSegmentPipeSegment | properties | on 2 objects (2 IFCFLOWSEGMENT)
    InvertElevation = 586.4 (IFCLENGTHMEASURE) [MILLI METRE]
    Length = 260.446116911296 (IFCPOSITIVELENGTHMEASURE) [MILLI METRE]
  Pset_FlowSegmentPipeSegment | properties | on 2 objects (2 IFCFLOWSEGMENT)
    InvertElevation = -13.6000000000011 (IFCLENGTHMEASURE) [MILLI METRE]
    Length = 262.969670197159 (IFCPOSITIVELENGTHMEASURE) [MILLI METRE]
  Pset_FlowSegmentPipeSegment | properties | on 1 object (1 IFCFLOWSEGMENT)
    InvertElevation = -13.6000000000009 (IFCLENGTHMEASURE) [MILLI METRE]
    Length = 390.478292343424 (IFCPOSITIVELENGTHMEASURE) [MILLI METRE]
  Pset_FlowSegmentPipeSegment | properties | on 1 object (1 IFCFLOWSEGMENT)
    InvertElevation = -13.6 (IFCLENGTHMEASURE) [MILLI METRE]
    Length = 576.420408303681 (IFCPOSITIVELENGTHMEASURE) [MILLI METRE]
  Pset_FlowSegmentPipeSegment | properties | on 1 object (1 IFCFLOWSEGMENT)
    InvertElevation = -13.5999999999942 (IFCLENGTHMEASURE) [MILLI METRE]
    Length = 261.164227230474 (IFCPOSITIVELENGTHMEASURE) [MILLI METRE]
  Pset_FlowSegmentPipeSegment | properties | on 1 object (1 IFCFLOWSEGMENT)
    InvertElevation = -13.5999999999941 (IFCLENGTHMEASURE) [MILLI METRE]
    Length = 252.93337965286 (IFCPOSITIVELENGTHMEASURE) [MILLI METRE]
  Pset_FlowSegmentPipeSegment | properties | on 1 object (1 IFCFLOWSEGMENT)
    InvertElevation = -13.5999999999896 (IFCLENGTHMEASURE) [MILLI METRE]
    Length = 555.200000000007 (IFCPOSITIVELENGTHMEASURE) [MILLI METRE]
  Pset_FlowSegmentPipeSegment: 33 more contents on 33 objects not shown
  Pset_PipeConnection | properties | on 44 objects (44 IFCFLOWSEGMENT)
    ConnectionType = ["Generic"] (IFCLABEL)
  Pset_AirSideSystemInformation | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Name = "Level 1" (IFCLABEL)
  Pset_BuildingStoreyCommon | properties | on 1 object (1 IFCBUILDINGSTOREY)
    AboveGround = UNKNOWN (IFCLOGICAL)
  Pset_BuildingCommon | properties | on 1 object (1 IFCBUILDING)
    IsLandmarked = UNKNOWN (IFCLOGICAL)
    NumberOfStoreys = 1 (IFCINTEGER)