<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="9.7.0">
<drawing>
<board>
<plain>
<wire x1="27.178" y1="7.62" x2="27.178" y2="5.08" width="0" layer="20"/>
<wire x1="27.178" y1="5.08" x2="22.098" y2="0" width="0" layer="20" curve="-90"/>
<wire x1="22.098" y1="0" x2="5.08" y2="0" width="0" layer="20"/>
<wire x1="5.08" y1="0" x2="0" y2="5.08" width="0" layer="20" curve="-90"/>
<wire x1="0" y1="5.08" x2="0" y2="40.64" width="0" layer="20"/>
<wire x1="0" y1="40.64" x2="5.08" y2="45.72" width="0" layer="20" curve="-90"/>
<wire x1="5.08" y1="45.72" x2="22.098" y2="45.72" width="0" layer="20"/>
<wire x1="22.098" y1="45.72" x2="27.178" y2="40.64" width="0" layer="20" curve="-90"/>
<wire x1="27.178" y1="40.64" x2="27.178" y2="38.1" width="0" layer="20"/>
<wire x1="27.178" y1="38.1" x2="29.21" y2="38.1" width="0" layer="20"/>
<wire x1="29.21" y1="38.1" x2="29.21" y2="7.62" width="0" layer="20"/>
<wire x1="29.21" y1="7.62" x2="27.178" y2="7.62" width="0" layer="20"/>
<hole x="25.146" y="40.64" drill="1"/>
<hole x="25.146" y="5.08" drill="1"/>
<text>IV</text>
<text>330</text>
</plain>
<libraries>
<library name="eagle-ltspice">
<description>Default symbols for import LTspice schematics&lt;p&gt;
2012-10-29 alf@cadsoft.de&lt;br&gt;</description>
<packages>
<package name="R0805">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;</description>
</package>
</packages>
</library>
<library name="Capacitor">
<description>&lt;B&gt;Capacitors - Fixed, Variable, Trimmers</description>
<packages>
<package name="CAPC4532X135">
<description>Chip, 4.50 X 3.20 X 1.35 mm body
&lt;p&gt;Chip package with body size 4.50 X 3.20 X 1.35 mm&lt;/p&gt;</description>
</package>
</packages>
</library>
<library name="IC_Power-Management">
<description>&lt;B&gt;Voltage Regulators, Drivers, Switching controllers</description>
<packages>
<package name="SOT230P700X170-4">
<description>4-SOT223, 2.30 mm pitch, 7.00 mm span, 6.50 X 3.50 X 1.70 mm body
&lt;p&gt;4-pin SOT223 package with 2.30 mm pitch, 7.00 mm span with body size 6.50 X 3.50 X 1.70 mm&lt;/p&gt;</description>
</package>
</packages>
</library>
<library name="SparkFun-Switches">
<description>&lt;h3&gt;SparkFun Switches, Buttons, Encoders&lt;/h3&gt;
In this library you'll find switches, buttons, joysticks, and anything that moves to create or disrupt an electrical connection.
&lt;br&gt;
&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is &lt;b&gt; the end user's responsibility&lt;/b&gt; to ensure correctness and suitablity for a given componet or application. 
&lt;br&gt;
&lt;br&gt;If you enjoy using this library, please buy one of our products at &lt;a href=" www.sparkfun.com"&gt;SparkFun.com&lt;/a&gt;.
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;
&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="TACTILE_SWITCH_SMD_4.6X2.8MM">
<description>&lt;h3&gt;Momentary Switch (Pushbutton) - SPST - SMD, 4.6 x 2.8mm&lt;/h3&gt;
&lt;p&gt;Normally-open (NO) SPST momentary switches (buttons, pushbuttons).&lt;/p&gt;
&lt;p&gt;&lt;a href="http://www.ck-components.com/media/1479/kmr2.pdf"&gt;Datasheet&lt;/a&gt;&lt;/p&gt;</description>
</package>
</packages>
</library>
<library name="Connector">
<description>&lt;b&gt;Pin Headers,Terminal blocks, D-Sub, Backplane, FFC/FPC, Socket</description>
<packages>
<package name="1X11/90">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
</package>
<package name="1X04/90">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="esp-12e-f">
<packages>
<package name="ESP-12E">
</package>
</packages>
</library>
<library name="LED">
<description>&lt;B&gt;LED parts CHIP-Flat Top, Round Top</description>
<packages>
<package name="LEDC2012X110N_FLAT-B">
<description>Chip LED, 2.00 X 1.25 X 1.10 mm body
 &lt;p&gt;Chip LED package with body size 2.00 X 1.25 X 1.10 mm&lt;/p&gt;</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="R1" library="eagle-ltspice" package="R0805" value="330">
<attribute name="SPICEMODEL" value="NONE"/>
<attribute name="SPICEPREFIX" value="R"/>
</element>
<element name="VR1" library="IC_Power-Management" package="SOT230P700X170-4" value="NCP1117ST33T3G">
<attribute name="CATEGORY" value="IC_Power-Management"/>
<attribute name="DESCRIPTION" value=""/>
<attribute name="MANUFACTURER" value="ON Semiconductor"/>
<attribute name="MPN" value="NCP1117ST33T3G"/>
<attribute name="NAME"/>
<attribute name="OPERATING_TEMP" value="0 to +125 °C"/>
<attribute name="PART_STATUS" value="Active"/>
<attribute name="ROHS_COMPLIANT" value="RoHS3 Compliant"/>
<attribute name="SERIES" value="NCP1117, NCV1117"/>
<attribute name="SUB-CATEGORY" value="Voltage Regulator"/>
<attribute name="THERMALLOSS" value=""/>
<attribute name="TYPE" value="Linear"/>
</element>
<element name="PRG" library="SparkFun-Switches" package="TACTILE_SWITCH_SMD_4.6X2.8MM" value="MOMENTARY-SWITCH-SPST-SMD-4.6X2.8MM">
<attribute name="NAME"/>
<attribute name="PROD_ID" value="SWCH-13065"/>
</element>
<element name="RES" library="SparkFun-Switches" package="TACTILE_SWITCH_SMD_4.6X2.8MM" value="MOMENTARY-SWITCH-SPST-SMD-4.6X2.8MM">
<attribute name="NAME"/>
<attribute name="PROD_ID" value="SWCH-13065"/>
</element>
<element name="G850V" library="Connector" package="1X11/90" value="PINHD-1X11/90">
<attribute name="CATEGORY" value="CONNECTOR"/>
<attribute name="DESCRIPTION" value=""/>
<attribute name="MANUFACTURER" value=""/>
<attribute name="MPN" value=""/>
<attribute name="NAME"/>
<attribute name="OPERATING_TEMP" value=""/>
<attribute name="PART_STATUS" value=""/>
<attribute name="ROHS_COMPLIANT" value=""/>
<attribute name="SERIES" value=""/>
<attribute name="SUB-CATEGORY" value="PIN-HEADER"/>
<attribute name="THERMALLOSS" value=""/>
<attribute name="TYPE" value=""/>
</element>
<element name="R2" library="eagle-ltspice" package="R0805" value="1K">
<attribute name="NAME"/>
<attribute name="SPICEMODEL" value="NONE"/>
<attribute name="SPICEPREFIX" value="R"/>
<attribute name="VALUE"/>
</element>
<element name="R3" library="eagle-ltspice" package="R0805" value="1K">
<attribute name="NAME"/>
<attribute name="SPICEMODEL" value="NONE"/>
<attribute name="SPICEPREFIX" value="R"/>
<attribute name="VALUE"/>
</element>
<element name="R4" library="eagle-ltspice" package="R0805" value="1K">
<attribute name="NAME"/>
<attribute name="SPICEMODEL" value="NONE"/>
<attribute name="SPICEPREFIX" value="R"/>
<attribute name="VALUE"/>
</element>
<element name="R5" library="eagle-ltspice" package="R0805" value="1K">
<attribute name="NAME"/>
<attribute name="SPICEMODEL" value="NONE"/>
<attribute name="SPICEPREFIX" value="R"/>
<attribute name="VALUE"/>
</element>
<element name="R6" library="eagle-ltspice" package="R0805" value="1K">
<attribute name="NAME"/>
<attribute name="SPICEMODEL" value="NONE"/>
<attribute name="SPICEPREFIX" value="R"/>
<attribute name="VALUE"/>
</element>
<element name="R7" library="eagle-ltspice" package="R0805" value="1K">
<attribute name="NAME"/>
<attribute name="SPICEMODEL" value="NONE"/>
<attribute name="SPICEPREFIX" value="R"/>
<attribute name="VALUE"/>
</element>
<element name="JP1" library="Connector" package="1X04/90" value="PINHD-1X4/90">
<attribute name="CATEGORY" value="CONNECTOR"/>
<attribute name="DESCRIPTION" value=""/>
<attribute name="MANUFACTURER" value=""/>
<attribute name="MPN" value=""/>
<attribute name="NAME"/>
<attribute name="OPERATING_TEMP" value=""/>
<attribute name="PART_STATUS" value=""/>
<attribute name="ROHS_COMPLIANT" value=""/>
<attribute name="SERIES" value=""/>
<attribute name="SUB-CATEGORY" value="PIN-HEADER"/>
<attribute name="THERMALLOSS" value=""/>
<attribute name="TYPE" value=""/>
</element>
<element name="R8" library="eagle-ltspice" package="R0805" value="1K8">
<attribute name="NAME"/>
<attribute name="SPICEMODEL" value="NONE"/>
<attribute name="SPICEPREFIX" value="R"/>
<attribute name="VALUE"/>
</element>
<element name="R9" library="eagle-ltspice" package="R0805" value="3K3">
<attribute name="NAME"/>
<attribute name="SPICEMODEL" value="NONE"/>
<attribute name="SPICEPREFIX" value="R"/>
<attribute name="VALUE"/>
</element>
<element name="IC1" library="esp-12e-f" package="ESP-12E" value="ESP-12E/F"/>
<element name="D1" library="LED" package="LEDC2012X110N_FLAT-B" value="LED">
<attribute name="CATEGORY" value="LED"/>
<attribute name="COLOR" value="BLUE"/>
<attribute name="DESCRIPTION" value="CHIP LED FLAT"/>
<attribute name="MANUFACTURER" value=""/>
<attribute name="MPN" value=""/>
<attribute name="NAME"/>
<attribute name="OPERATING_TEMP" value=""/>
<attribute name="PART_STATUS" value=""/>
<attribute name="ROHS_COMPLIANT" value=""/>
<attribute name="SERIES" value=""/>
<attribute name="SUB-CATEGORY" value="CHIP"/>
<attribute name="THERMALLOSS" value=""/>
<attribute name="TYPE" value="FLAT_TOP"/>
<attribute name="VALUE"/>
</element>
<element name="R10" library="eagle-ltspice" package="R0805" value="330">
<attribute name="NAME"/>
<attribute name="SPICEMODEL" value="NONE"/>
<attribute name="SPICEPREFIX" value="R"/>
<attribute name="VALUE"/>
</element>
<element name="C1" library="Capacitor" package="CAPC4532X135" value="100uF">
<attribute name="CATEGORY" value="Capacitor"/>
<attribute name="MANUFACTURER" value=""/>
<attribute name="MPN" value=""/>
<attribute name="NAME"/>
<attribute name="OPERATING_TEMP" value=""/>
<attribute name="PART_STATUS" value=""/>
<attribute name="ROHS_COMPLIANT" value=""/>
<attribute name="SERIES" value=""/>
<attribute name="SUB-CATEGORY" value=""/>
<attribute name="THERMALLOSS" value=""/>
<attribute name="TYPE" value=""/>
<attribute name="VALUE"/>
<attribute name="VOLTAGE_RATING" value=""/>
</element>
</elements>
<signals>
<signal name="GND">
<contactref element="VR1" pad="1"/>
<contactref element="RES" pad="1"/>
<contactref element="RES" pad="2"/>
<contactref element="PRG" pad="1"/>
<contactref element="PRG" pad="2"/>
<contactref element="G850V" pad="3"/>
<contactref element="R6" pad="1"/>
<contactref element="JP1" pad="4"/>
<contactref element="R9" pad="1"/>
<contactref element="IC1" pad="GND"/>
<contactref element="R10" pad="1"/>
<contactref element="C1" pad="2"/>
</signal>
<signal name="VCC">
<contactref element="VR1" pad="2"/>
<contactref element="R2" pad="2"/>
<contactref element="R3" pad="2"/>
<contactref element="R4" pad="2"/>
<contactref element="R5" pad="2"/>
<contactref element="R7" pad="2"/>
<contactref element="JP1" pad="1"/>
<contactref element="IC1" pad="VCC"/>
<contactref element="C1" pad="1"/>
</signal>
<signal name="N$8">
<contactref element="R1" pad="1"/>
<contactref element="RES" pad="3"/>
<contactref element="RES" pad="4"/>
<contactref element="R2" pad="1"/>
<contactref element="IC1" pad="RST"/>
</signal>
<signal name="N$4">
<contactref element="JP1" pad="3"/>
<contactref element="IC1" pad="TXD/IO1"/>
</signal>
<signal name="N$2">
<contactref element="R6" pad="2"/>
<contactref element="IC1" pad="IO15"/>
</signal>
<signal name="N$3">
<contactref element="PRG" pad="3"/>
<contactref element="PRG" pad="4"/>
<contactref element="R4" pad="1"/>
<contactref element="IC1" pad="IO0"/>
</signal>
<signal name="N$6">
<contactref element="R5" pad="1"/>
<contactref element="IC1" pad="IO2"/>
</signal>
<signal name="N$10">
<contactref element="R3" pad="1"/>
<contactref element="IC1" pad="EN"/>
</signal>
<signal name="N$7">
<contactref element="R1" pad="2"/>
<contactref element="IC1" pad="IO16"/>
</signal>
<signal name="N$1">
<contactref element="JP1" pad="2"/>
<contactref element="IC1" pad="RXD/IO3"/>
</signal>
<signal name="VSS">
<contactref element="G850V" pad="2"/>
<contactref element="VR1" pad="3"/>
</signal>
<signal name="DTR">
<contactref element="G850V" pad="5"/>
</signal>
<signal name="CD">
<contactref element="G850V" pad="8"/>
</signal>
<signal name="DSR">
<contactref element="G850V" pad="10"/>
</signal>
<signal name="CI">
<contactref element="G850V" pad="11"/>
</signal>
<signal name="RTS(4)CTS(9)">
<contactref element="G850V" pad="4"/>
<contactref element="G850V" pad="9"/>
<contactref element="R7" pad="1"/>
</signal>
<signal name="RX_G850">
<contactref element="G850V" pad="6"/>
<contactref element="IC1" pad="IO4"/>
</signal>
<signal name="TX_G850">
<contactref element="G850V" pad="7"/>
<contactref element="R8" pad="2"/>
</signal>
<signal name="N$5">
<contactref element="G850V" pad="1"/>
</signal>
<signal name="N$9">
<contactref element="R9" pad="2"/>
<contactref element="R8" pad="1"/>
<contactref element="IC1" pad="IO5"/>
</signal>
<signal name="N$11">
<contactref element="IC1" pad="IO10"/>
<contactref element="D1" pad="A"/>
</signal>
<signal name="N$12">
<contactref element="D1" pad="C"/>
<contactref element="R10" pad="2"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
