<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="6.5.0">
<drawing>
<board>
<plain>
<wire x1="0.8128" y1="0" x2="27.94" y2="0" width="0" layer="20"/>
<wire x1="28.7528" y1="0.8128" x2="28.7528" y2="19.939" width="0" layer="20"/>
<wire x1="0" y1="19.939" x2="0" y2="0.8128" width="0" layer="20"/>
<text>BricksTer
8884bt</text>
<text>rev. 2</text>
<text>github.com/codefox421/brickster</text>
<wire x1="0" y1="0.8128" x2="0.8128" y2="0" width="0" layer="20" curve="90"/>
<wire x1="27.94" y1="0" x2="28.7528" y2="0.8128" width="0" layer="20" curve="90"/>
<wire x1="0" y1="19.939" x2="0.8128" y2="20.7518" width="0" layer="20" curve="-90"/>
<wire x1="28.7528" y1="19.939" x2="27.94" y2="20.7518" width="0" layer="20" curve="90"/>
<wire x1="2.3749" y1="27.94" x2="2.3749" y2="20.7518" width="0" layer="20"/>
<wire x1="2.3749" y1="27.94" x2="3.1877" y2="28.7528" width="0" layer="20" curve="-90"/>
<wire x1="26.3779" y1="20.7518" x2="26.3779" y2="27.94" width="0" layer="20"/>
<wire x1="25.5651" y1="28.7528" x2="26.3779" y2="27.94" width="0" layer="20" curve="-90"/>
<wire x1="3.1877" y1="28.7528" x2="25.5651" y2="28.7528" width="0" layer="20"/>
<wire x1="0.8128" y1="20.7518" x2="2.3749" y2="20.7518" width="0" layer="20"/>
<wire x1="27.94" y1="20.7518" x2="26.3779" y2="20.7518" width="0" layer="20"/>
<hole x="6.3754" y="24.7523" drill="4.75"/>
<hole x="22.3774" y="24.7523" drill="4.75"/>
<text>BricksTer
8884bt</text>
</plain>
<libraries>
<library name="brickster">
<description>&lt;b&gt;BricksTer 8884bt Components&lt;/b&gt;&lt;br/&gt;
&lt;br /&gt;
More information: &lt;a href="https://github.com/codefox421/brickster"&gt;https://github.com/codefox421/brickster&lt;/a&gt;&lt;br /&gt;
&lt;br /&gt;
&lt;i&gt;Created by: Nick Iaconis&lt;/i&gt;</description>
<packages>
<package name="MBS-2">
</package>
<package name="SOT223">
</package>
<package name="14S1">
</package>
<package name="0805">
</package>
<package name="1206">
</package>
<package name="SMD_PF">
</package>
<package name="PWP_R-PDSO-G16">
</package>
<package name="BLUETOOTH_SMD">
</package>
<package name="0805_POL">
</package>
</packages>
</library>
<library name="SparkFun-Connectors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find connectors and sockets- basically anything that can be plugged into or onto.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; CC v3.0 Share-Alike You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="2X3-NS">
</package>
</packages>
</library>
<library name="SparkFun-Aesthetics">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find non-functional items- supply symbols, logos, notations, frame blocks, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; CC v3.0 Share-Alike You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="OSHW-LOGO-M">
</package>
<package name="OSHW-LOGO-M-MASK">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="U3" library="brickster" package="SOT223" value="IC_RT9164A">
<attribute name="NAME"/>
</element>
<element name="U1" library="brickster" package="14S1" value="IC_ATTINY_X4A">
<attribute name="NAME"/>
</element>
<element name="C3" library="brickster" package="0805" value="0.01uF">
<attribute name="NAME"/>
</element>
<element name="J1" library="SparkFun-Connectors" package="2X3-NS" value="AVR_SPI_PRG_6NS"/>
<element name="B3" library="brickster" package="MBS-2" value="B_CDBHM240L-HF">
<attribute name="NAME"/>
</element>
<element name="B4" library="brickster" package="MBS-2" value="B_CDBHM240L-HF">
<attribute name="NAME"/>
</element>
<element name="LOGO1" library="SparkFun-Aesthetics" package="OSHW-LOGO-M-MASK" value="OSHW-LOGOM"/>
<element name="C1" library="brickster" package="0805" value="0.1uF">
<attribute name="NAME"/>
</element>
<element name="C2" library="brickster" package="1206" value="10uF">
<attribute name="NAME"/>
</element>
<element name="C5" library="brickster" package="1206" value="10uF">
<attribute name="NAME"/>
</element>
<element name="J2" library="brickster" package="SMD_PF" value="CON_PF_SMD"/>
<element name="J3" library="brickster" package="SMD_PF" value="CON_PF_SMD"/>
<element name="J4" library="brickster" package="SMD_PF" value="CON_PF_SMD"/>
<element name="U2" library="brickster" package="PWP_R-PDSO-G16" value="IC_DRV8833">
<attribute name="NAME"/>
</element>
<element name="C4" library="brickster" package="0805" value="2.2uF">
<attribute name="NAME"/>
</element>
<element name="B2" library="brickster" package="MBS-2" value="B_CDBHM240L-HF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R2" library="brickster" package="0805" value="3.3k">
<attribute name="NAME"/>
</element>
<element name="U4" library="brickster" package="BLUETOOTH_SMD" value="HC-06"/>
<element name="D1" library="brickster" package="0805_POL" value="LED0805">
<attribute name="NAME"/>
</element>
<element name="LOGO2" library="SparkFun-Aesthetics" package="OSHW-LOGO-M-MASK" value="OSHW-LOGOM"/>
</elements>
<signals>
<signal name="GND">
<contactref element="C5" pad="2"/>
<contactref element="J1" pad="6"/>
<contactref element="U1" pad="14"/>
<contactref element="B3" pad="-"/>
<contactref element="B4" pad="-"/>
<contactref element="U3" pad="1"/>
<contactref element="C1" pad="P$2"/>
<contactref element="C2" pad="2"/>
<contactref element="J3" pad="GND"/>
<contactref element="J4" pad="GND"/>
<contactref element="U2" pad="17"/>
<contactref element="U2" pad="13"/>
<contactref element="U2" pad="6"/>
<contactref element="U2" pad="3"/>
<contactref element="C4" pad="P$1"/>
<contactref element="J2" pad="GND"/>
<contactref element="B2" pad="-"/>
<contactref element="U4" pad="13"/>
<contactref element="U4" pad="21"/>
<contactref element="U4" pad="22"/>
<contactref element="D1" pad="P$1"/>
</signal>
<signal name="ATTX/BTRX">
<contactref element="U4" pad="2"/>
<contactref element="U1" pad="12"/>
</signal>
<signal name="A01">
<contactref element="J3" pad="C2"/>
<contactref element="U2" pad="2"/>
<contactref element="B3" pad="AC1"/>
</signal>
<signal name="A02">
<contactref element="J3" pad="C1"/>
<contactref element="U2" pad="4"/>
<contactref element="B3" pad="AC2"/>
</signal>
<signal name="B02">
<contactref element="J4" pad="C1"/>
<contactref element="B4" pad="AC1"/>
<contactref element="U2" pad="5"/>
</signal>
<signal name="B01">
<contactref element="J4" pad="C2"/>
<contactref element="B4" pad="AC2"/>
<contactref element="U2" pad="7"/>
</signal>
<signal name="AIN2">
<contactref element="U2" pad="15"/>
<contactref element="U1" pad="3"/>
</signal>
<signal name="AIN1">
<contactref element="U2" pad="16"/>
<contactref element="U1" pad="2"/>
</signal>
<signal name="BIN1">
<contactref element="U2" pad="9"/>
<contactref element="U1" pad="6"/>
</signal>
<signal name="BIN2">
<contactref element="U1" pad="5"/>
<contactref element="U2" pad="10"/>
</signal>
<signal name="RESET">
<contactref element="J1" pad="5"/>
<contactref element="U1" pad="4"/>
</signal>
<signal name="MOSI">
<contactref element="U1" pad="7"/>
<contactref element="J1" pad="4"/>
</signal>
<signal name="MISO">
<contactref element="U1" pad="8"/>
<contactref element="J1" pad="1"/>
</signal>
<signal name="SCK">
<contactref element="U1" pad="9"/>
<contactref element="J1" pad="3"/>
</signal>
<signal name="ATRX/BTTX">
<contactref element="U4" pad="1"/>
<contactref element="U1" pad="13"/>
</signal>
<signal name="3.3V">
<contactref element="U3" pad="2"/>
<contactref element="C2" pad="1"/>
<contactref element="U1" pad="1"/>
<contactref element="J1" pad="2"/>
<contactref element="U3" pad="4"/>
<contactref element="U2" pad="1"/>
<contactref element="U4" pad="12"/>
</signal>
<signal name="VIN">
<contactref element="U3" pad="3"/>
<contactref element="C1" pad="P$1"/>
<contactref element="B3" pad="+"/>
<contactref element="B4" pad="+"/>
<contactref element="J3" pad="9V"/>
<contactref element="J4" pad="9V"/>
<contactref element="C5" pad="1"/>
<contactref element="U2" pad="12"/>
<contactref element="C3" pad="P$1"/>
<contactref element="J2" pad="9V"/>
<contactref element="B2" pad="+"/>
</signal>
<signal name="PF_C1">
<contactref element="J2" pad="C1"/>
<contactref element="B2" pad="AC1"/>
</signal>
<signal name="PF_C2">
<contactref element="J2" pad="C2"/>
<contactref element="B2" pad="AC2"/>
</signal>
<signal name="N$1">
<contactref element="C3" pad="P$2"/>
<contactref element="U2" pad="11"/>
</signal>
<signal name="N$2">
<contactref element="U2" pad="14"/>
<contactref element="C4" pad="P$2"/>
</signal>
<signal name="LED">
<contactref element="U4" pad="24"/>
<contactref element="R2" pad="P$1"/>
</signal>
<signal name="N$3">
<contactref element="U4" pad="3"/>
<contactref element="U4" pad="4"/>
</signal>
<signal name="KEY">
<contactref element="U4" pad="26"/>
<contactref element="U1" pad="11"/>
</signal>
<signal name="N$4">
<contactref element="R2" pad="P$2"/>
<contactref element="D1" pad="P$2"/>
</signal>
<signal name="BTRST">
<contactref element="U4" pad="11"/>
<contactref element="U1" pad="10"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
