<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="7.7.0">
<drawing>
<library>
<description>&lt;b&gt;DIY Modules for Arduino, Raspberry Pi, CubieBoard etc.&lt;/b&gt;
&lt;br&gt;&lt;br&gt;
The library contains a list of symbols and footprints for popular, cheap and easy-to-use electronic modules.&lt;br&gt;
The modules are intend to work with microprocessor-based platforms such as &lt;a href="http://arduino.cc"&gt;Arduino&lt;/a&gt;, &lt;a href="http://raspberrypi.org/"&gt;Raspberry Pi&lt;/a&gt;, &lt;a href="http://cubieboard.org/"&gt;CubieBoard&lt;/a&gt;, &lt;a href="http://beagleboard.org/"&gt;BeagleBone&lt;/a&gt; and many others. There are many manufacturers of the modules in the world. Almost all of them can be bought on &lt;a href="ebay.com"&gt;ebay.com&lt;/a&gt;.&lt;br&gt;
&lt;br&gt;
By using this library, you can design a PCB for devices created with usage of modules. Even if you do not need to create PCB design, you can also use the library to quickly document your work by drawing schematics of devices built by you.&lt;br&gt;
&lt;br&gt;
The latest version, examples, photos and much more can be found at: &lt;b&gt;&lt;a href="http://diymodules.org/eagle"&gt;diymodules.org/eagle&lt;/a&gt;&lt;/b&gt;&lt;br&gt;&lt;br&gt;
Comments, suggestions and bug reports please send to: &lt;b&gt;&lt;a href="mailto:eagle@diymodules.org"&gt;eagle@diymodules.org&lt;/b&gt;&lt;/a&gt;&lt;br&gt;&lt;br&gt;
&lt;i&gt;Version: 1.1.0 (2016-Oct-24)&lt;/i&gt;&lt;br&gt;
&lt;i&gt;Created by: Miroslaw Brudnowski&lt;/i&gt;&lt;br&gt;&lt;br&gt;
&lt;i&gt;Released under the Creative Commons Attribution 4.0 International License: &lt;a href="http://creativecommons.org/licenses/by/4.0"&gt;http://creativecommons.org/licenses/by/4.0&lt;/a&gt;&lt;/i&gt;
&lt;br&gt;&lt;br&gt;
&lt;center&gt;&lt;a href="http://diymodules.org/eagle"&gt;&lt;img src="http://diymodules.org/img/diymodules-lbr-image.php?v=1.1.0" alt="DIYmodules.org"&gt;&lt;/a&gt;&lt;/center&gt;</description>
<packages>
<package name="ARDUINO-PRO-MINI">
<description>&lt;b&gt;Arduino Pro Mini&lt;/b&gt;</description>
</package>
<package name="ARDUINO-PRO-MINI#APC">
<description>&lt;b&gt;Arduino Pro Mini&lt;/b&gt;&lt;br&gt;
Footprint with angle programming connector</description>
</package>
<package name="WIRELESS-NRF24L01">
<description>&lt;b&gt;2.4 GHz Wireless Module&lt;/b&gt; based on &lt;b&gt;NRF24L01&lt;/b&gt; chip</description>
</package>
<package name="ARDUINO-PRO-MINI#NP">
<description>&lt;b&gt;Arduino Pro Mini&lt;/b&gt;&lt;br&gt;
Footprint without programming pads</description>
</package>
<package name="ARDUINO-PRO-MINI#SMP">
<description>&lt;b&gt;Arduino Pro Mini&lt;/b&gt;&lt;br&gt;
Footprint with 2 connectors only</description>
</package>
<package name="WIRELESS-XY-MK-5V">
<description>&lt;b&gt;RF Wireless XY-MK-5V Receiver&lt;/b&gt;</description>
</package>
<package name="WIRELESS-XY-FST">
<description>&lt;b&gt;RF Wireless XY-FST Transmitter&lt;/b&gt;</description>
</package>
<package name="WIRELESS-XY-MK-5V#V">
<description>&lt;b&gt;RF Wireless XY-MK-5V Receiver&lt;/b&gt; vertically mounted</description>
</package>
<package name="WIRELESS-XY-FST#V">
<description>&lt;b&gt;RF Wireless XY-FST Transmitter&lt;/b&gt; vertically mounted</description>
</package>
<package name="ARDUINO-NANO-3.0#ISP">
<description>&lt;b&gt;Arduino Nano 3.0&lt;/b&gt;&lt;br&gt;
Footprint with ISP pads</description>
</package>
<package name="ARDUINO-NANO-3.0">
<description>&lt;b&gt;Arduino Nano 3.0&lt;/b&gt;</description>
</package>
<package name="ETHERNET-ENC28J60">
<description>&lt;b&gt;Ethernet Module&lt;/b&gt; based on &lt;b&gt;ENC28J60&lt;/b&gt; chip</description>
</package>
<package name="BATTERY-HOLDER-2AA">
<description>&lt;b&gt;2 x AA Battery Holder&lt;/b&gt;</description>
</package>
<package name="BATTERY-HOLDER-2AAA">
<description>&lt;b&gt;2 x AAA Battery Holder&lt;/b&gt;</description>
</package>
<package name="DISPLAY-NOKIA-3310">
<description>&lt;b&gt;84x48 Dot Matrix LCD Module&lt;/b&gt; based on &lt;b&gt;Nokia 3310&lt;/b&gt; display</description>
</package>
<package name="DC-DC-STEP-UP-5V-USB">
<description>&lt;b&gt;DC/DC Step-Up Converter&lt;/b&gt; with &lt;b&gt;USB-A&lt;/b&gt; connector</description>
</package>
<package name="ULTRASONIC-HC-SR04">
<description>&lt;b&gt;Ultrasonic Ranging Module HC-SR04&lt;/b&gt;</description>
</package>
<package name="ULTRASONIC-HC-SR04#V">
<description>&lt;b&gt;Ultrasonic Ranging Module HC-SR04&lt;/b&gt; vertically mounted</description>
</package>
<package name="MOTION-PIR-DYP-ME003">
<description>&lt;b&gt;PIR Motion Sensor Module DYP-ME003&lt;/b&gt; based on &lt;b&gt;BISS0001&lt;/b&gt; pyroelectic detector</description>
</package>
<package name="REG-AMS1117">
<description>&lt;b&gt;Linear Regulator&lt;/b&gt; based on &lt;b&gt;AMS1117&lt;/b&gt; chip</description>
</package>
<package name="ADC-DAC-PCF8591">
<description>&lt;b&gt;4-Channel ADC and 1-Channel DAC Module&lt;/b&gt; based on &lt;b&gt;PCF8591&lt;/b&gt; chip</description>
</package>
<package name="DRIVER-ULN2003">
<description>&lt;b&gt;7-Channel Darlington NPN Transistor Module&lt;/b&gt; based on &lt;b&gt;ULN2003&lt;/b&gt; chip&lt;br&gt;</description>
</package>
<package name="DRIVER-ULN2003#MC">
<description>&lt;b&gt;7-Channel Darlington NPN Transistor Module&lt;/b&gt; based on &lt;b&gt;ULN2003&lt;/b&gt; chip&lt;br&gt;
Footprint with motor connector</description>
</package>
<package name="SOUND-DETECTOR">
<description>&lt;b&gt;Sound Detection Module&lt;/b&gt;</description>
</package>
<package name="SOUND-BUZZER">
<description>&lt;b&gt;Sound Buzzer Module&lt;/b&gt;</description>
</package>
<package name="CURRENT-SENSOR-ACS712#IC">
<description>&lt;b&gt;Isolated Bipolar Current Sensors&lt;/b&gt; based on &lt;b&gt;ACS712&lt;/b&gt; chip&lt;br&gt;
Footprint with input connector</description>
</package>
<package name="CURRENT-SENSOR-ACS712">
<description>&lt;b&gt;Isolated Bipolar Current Sensors&lt;/b&gt; based on &lt;b&gt;ACS712&lt;/b&gt; chip</description>
</package>
<package name="SOIL-MOISTURE-SENSOR">
<description>&lt;b&gt;Soil Moisture Sensor&lt;/b&gt;</description>
</package>
<package name="RELAY-2-SRD#RC">
<description>&lt;b&gt;2-Channel Relay Module&lt;/b&gt; based on &lt;b&gt;SRD-05VDC-SL-C&lt;/b&gt; relays&lt;br&gt;
Footprint with relays connector</description>
</package>
<package name="COMPASS-HMC5883L">
<description>&lt;b&gt;3-Axis Digital Compass Module&lt;/b&gt; based on &lt;b&gt;HMC5883L&lt;/b&gt; chip</description>
</package>
<package name="WIRELESS-WIFI-ESP-01">
<description>&lt;b&gt;Wireless Wi-Fi ESP-01 Module&lt;/b&gt; based on &lt;b&gt;ESP8266&lt;/b&gt; chip</description>
</package>
<package name="DC-DC-STEP-DOWN-LM2596">
<description>&lt;b&gt;DC/DC Step-Down Regulator&lt;/b&gt; based on &lt;b&gt;LM2596-ADJ&lt;/b&gt; chip</description>
</package>
<package name="CARD-SD-ADAPTER">
<description>&lt;b&gt;Full Size SD Card Adapter Module&lt;/b&gt; with onboard 3.3V regulator</description>
</package>
<package name="LCD-I2C-CONVERTER">
<description>&lt;b&gt;I2C Bus to 4-Bit Parallel LCD Interface&lt;/b&gt; with LED backlight driver</description>
</package>
<package name="RTC_EEPROM_BATTERY">
<description>&lt;b&gt;RTC Module with Battery and EEPROM&lt;/b&gt; based on &lt;b&gt;DS1307&lt;/b&gt; and &lt;b&gt;AT24C32&lt;/b&gt; chips</description>
</package>
<package name="AMPLIFIER-PAM8403">
<description>&lt;b&gt;Stereo Class-D 3W Audio Amplifier&lt;/b&gt; based on &lt;b&gt;PAM8403&lt;/b&gt; chip</description>
</package>
<package name="BREADBOARD-POWER-V1">
<description>&lt;b&gt;Breadboard Power Adapter&lt;/b&gt; with onboard 3.3V and 5V regulators</description>
</package>
<package name="RELAY-2-SRD">
<description>&lt;b&gt;2-Channel Relay Module&lt;/b&gt; based on &lt;b&gt;SRD-05VDC-SL-C&lt;/b&gt; relays</description>
</package>
<package name="DC-DC-STEP-UP-5V">
<description>&lt;b&gt;DC/DC Step-Up Converter&lt;/b&gt;</description>
</package>
<package name="WIRELESS-NRD24L01-PA-EXT">
<description>&lt;b&gt;2.4 GHz Wireless Module&lt;/b&gt; based on &lt;b&gt;NRF24L01&lt;/b&gt; chip with preamplifier and external antenna</description>
</package>
<package name="AC-DC-3.5W">
<description>&lt;b&gt;AC/DC 3.5W Converter&lt;/b&gt;</description>
</package>
<package name="BATTERY-CHARGER-LI-5V">
<description>&lt;b&gt;Lithium Battery 5V Charger&lt;/b&gt;</description>
</package>
<package name="FLAME-DETECTOR">
<description>&lt;b&gt;Flame Detector&lt;/b&gt;</description>
</package>
<package name="IR-RECEIVER">
<description>&lt;b&gt;IR Receiver Module&lt;/b&gt;</description>
</package>
<package name="IR-RECEIVER#NC">
<description>&lt;b&gt;IR Receiver Module&lt;/b&gt;&lt;br&gt;
Symbol wihtout IR sensor connector</description>
</package>
<package name="STEPPER-MOTOR-EASY-DRIVER">
<description>&lt;b&gt;Stepper Motor Easy Driver&lt;/b&gt;</description>
</package>
<package name="RS485-TTL-CONVERTER">
<description>&lt;b&gt;RS485 to TTL converter&lt;/b&gt; based on &lt;b&gt;MAX485&lt;/b&gt; chip</description>
</package>
<package name="TOUCH-KEYPAD-4X4">
<description>&lt;b&gt;16 Channel Capacitive Touch Keypad&lt;/b&gt;</description>
</package>
<package name="LIGHT-DETECTOR">
<description>&lt;b&gt;Light Detection Module&lt;/b&gt;</description>
</package>
<package name="GSM-MODEM-SIM900A">
<description>&lt;b&gt;GSM Mini Module&lt;/b&gt; based on &lt;b&gt;SIM900A&lt;/b&gt;</description>
</package>
<package name="LED-24XRGB-RING">
<description>&lt;b&gt;24 LEDs RGB Ring&lt;/b&gt; based on &lt;b&gt;WS2812B&lt;/b&gt;</description>
</package>
<package name="N-MOSFET-SWITCH">
<description>&lt;b&gt;Low Side N-MOSFET Switch&lt;/b&gt; with &lt;b&gt;Optocoupler&lt;/b&gt;</description>
</package>
<package name="N-MOSFET-SWITCH#IC">
<description>&lt;b&gt;Low Side N-MOSFET Switch&lt;/b&gt; with &lt;b&gt;Optocoupler&lt;/b&gt;&lt;br /&gt;
Package with connector pins</description>
</package>
<package name="BREADBOARD-POWER-V2">
<description>&lt;b&gt;Breadboard Power Adapter&lt;/b&gt; with onboard 3.3V and 5V regulators</description>
</package>
<package name="SPARKFUN-AD-MUX-16X1">
<description>&lt;b&gt;SparkFun Analog/Digital MUX Breakout&lt;/b&gt; based on &lt;b&gt;CD74HC4067&lt;/b&gt; chip</description>
</package>
</packages>
<symbols>
<symbol name="ARDUINO-NANO-3.0#ISP">
<description>&lt;b&gt;Arduino Nano 3.0&lt;/b&gt; with ISP pads</description>
<pin name="D1/TX"/>
<pin name="D0/RX"/>
<pin name="RST.1"/>
<pin name="GND.1" direction="pwr"/>
<pin name="D2"/>
<pin name="D3"/>
<pin name="D4"/>
<pin name="D5"/>
<pin name="D6"/>
<pin name="D7"/>
<pin name="D8"/>
<pin name="D9"/>
<pin name="D10"/>
<pin name="D11/MOSI"/>
<pin name="D12/MISO"/>
<pin name="VIN" direction="pwr"/>
<pin name="GND.2" direction="pwr"/>
<pin name="RST.2"/>
<pin name="5V" direction="pwr"/>
<pin name="A7"/>
<pin name="A6"/>
<pin name="A5"/>
<pin name="A4"/>
<pin name="A3"/>
<pin name="A2"/>
<pin name="A1"/>
<pin name="A0"/>
<pin name="AREF"/>
<pin name="3V3" direction="pwr"/>
<pin name="D13/SCK"/>
<pin name="ISP_MISO"/>
<pin name="ISP_5V"/>
<pin name="ISP_SCK"/>
<pin name="ISP_MOSI"/>
<pin name="ISP_RST"/>
<pin name="ISP_GND"/>
</symbol>
<symbol name="ARDUINO-NANO-3.0">
<description>&lt;b&gt;Arduino Nano 3.0&lt;/b&gt;</description>
<pin name="D1/TX"/>
<pin name="D0/RX"/>
<pin name="RST.1"/>
<pin name="GND.1" direction="pwr"/>
<pin name="D2"/>
<pin name="D3"/>
<pin name="D4"/>
<pin name="D5"/>
<pin name="D6"/>
<pin name="D7"/>
<pin name="D8"/>
<pin name="D9"/>
<pin name="D10"/>
<pin name="D11/MOSI"/>
<pin name="D12/MISO"/>
<pin name="VIN" direction="pwr"/>
<pin name="GND.2" direction="pwr"/>
<pin name="RST.2"/>
<pin name="5V" direction="pwr"/>
<pin name="A7"/>
<pin name="A6"/>
<pin name="A5"/>
<pin name="A4"/>
<pin name="A3"/>
<pin name="A2"/>
<pin name="A1"/>
<pin name="A0"/>
<pin name="AREF"/>
<pin name="3V3" direction="pwr"/>
<pin name="D13/SCK"/>
</symbol>
<symbol name="ARDUINO-PRO-MINI">
<description>&lt;b&gt;Arduino Pro Mini&lt;/b&gt;</description>
<pin name="D1/TX"/>
<pin name="D0/RX"/>
<pin name="RST.1"/>
<pin name="GND.1" direction="pwr"/>
<pin name="D2"/>
<pin name="D3"/>
<pin name="D4"/>
<pin name="D5"/>
<pin name="D6"/>
<pin name="D7"/>
<pin name="D8"/>
<pin name="D9"/>
<pin name="RAW" direction="pwr"/>
<pin name="GND.2" direction="pwr"/>
<pin name="RST.2"/>
<pin name="VCC" direction="pwr"/>
<pin name="A3"/>
<pin name="A2"/>
<pin name="A1"/>
<pin name="A0"/>
<pin name="D13"/>
<pin name="D12"/>
<pin name="D11"/>
<pin name="D10"/>
<pin name="P_GND"/>
<pin name="P_CTS"/>
<pin name="P_VCC"/>
<pin name="P_RXD"/>
<pin name="P_TXD"/>
<pin name="P_DTR"/>
<pin name="A7"/>
<pin name="A6"/>
<pin name="GND.3"/>
<pin name="A4"/>
<pin name="A5"/>
</symbol>
<symbol name="ARDUINO-PRO-MINI#NP">
<description>&lt;b&gt;Arduino Pro Mini&lt;/b&gt; without programming pins</description>
<pin name="D1/TX"/>
<pin name="D0/RX"/>
<pin name="RST.1"/>
<pin name="GND.1" direction="pwr"/>
<pin name="D2"/>
<pin name="D3"/>
<pin name="D4"/>
<pin name="D5"/>
<pin name="D6"/>
<pin name="D7"/>
<pin name="D8"/>
<pin name="D9"/>
<pin name="RAW" direction="pwr"/>
<pin name="GND.2" direction="pwr"/>
<pin name="RST.2"/>
<pin name="VCC" direction="pwr"/>
<pin name="A3"/>
<pin name="A2"/>
<pin name="A1"/>
<pin name="A0"/>
<pin name="D13"/>
<pin name="D12"/>
<pin name="D11"/>
<pin name="D10"/>
<pin name="A7"/>
<pin name="A6"/>
<pin name="GND.3"/>
<pin name="A4"/>
<pin name="A5"/>
</symbol>
<symbol name="ARDUINO-PRO-MINI#SMP">
<description>&lt;b&gt;Arduino Pro Mini&lt;/b&gt; with 2 connectors only</description>
<pin name="D1/TX"/>
<pin name="D0/RX"/>
<pin name="RST.1"/>
<pin name="GND.1" direction="pwr"/>
<pin name="D2"/>
<pin name="D3"/>
<pin name="D4"/>
<pin name="D5"/>
<pin name="D6"/>
<pin name="D7"/>
<pin name="D8"/>
<pin name="D9"/>
<pin name="RAW" direction="pwr"/>
<pin name="GND.2" direction="pwr"/>
<pin name="RST.2"/>
<pin name="VCC" direction="pwr"/>
<pin name="A3"/>
<pin name="A2"/>
<pin name="A1"/>
<pin name="A0"/>
<pin name="D13"/>
<pin name="D12"/>
<pin name="D11"/>
<pin name="D10"/>
</symbol>
<symbol name="BATTERY-HOLDER">
<description>&lt;b&gt;Battery Holder&lt;/b&gt;</description>
<pin name="BAT+" direction="pwr"/>
<pin name="BAT-" direction="pwr"/>
</symbol>
<symbol name="DC-DC-STEP-UP-5V-USB">
<description>&lt;b&gt;DC/DC Step-Up Converter&lt;/b&gt; with &lt;b&gt;USB-A&lt;/b&gt; connector</description>
<pin name="IN+" direction="pwr"/>
<pin name="IN-" direction="pwr"/>
</symbol>
<symbol name="DISPLAY-NOKIA-3310">
<description>&lt;b&gt;84x48 Dot Matrix LCD Module&lt;/b&gt; based on &lt;b&gt;Nokia 3310&lt;/b&gt; display</description>
<pin name="VCC.2" direction="pwr"/>
<pin name="GND.2" direction="pwr"/>
<pin name="SCE.2"/>
<pin name="RST.2"/>
<pin name="D/C.2"/>
<pin name="DIN.2"/>
<pin name="SCK.2"/>
<pin name="LED.2" direction="in"/>
<pin name="VCC.1" direction="pwr"/>
<pin name="GND.1" direction="pwr"/>
<pin name="SCE.1"/>
<pin name="RST.1"/>
<pin name="D/C.1"/>
<pin name="DIN.1"/>
<pin name="SCK.1"/>
<pin name="LED.1" direction="in"/>
</symbol>
<symbol name="ETHERNET-ENC28J60">
<description>&lt;b&gt;Ethernet Module&lt;/b&gt; based on &lt;b&gt;ENC28J60&lt;/b&gt; chip</description>
<pin name="GND.1" direction="pwr"/>
<pin name="3V3" direction="pwr"/>
<pin name="CS"/>
<pin name="RST"/>
<pin name="SI"/>
<pin name="SCK"/>
<pin name="WOL"/>
<pin name="SO"/>
<pin name="CLK"/>
<pin name="INT"/>
<pin name="GND.2" direction="pwr"/>
<pin name="5V" direction="pwr"/>
</symbol>
<symbol name="WIRELESS-NRF24L01">
<description>&lt;b&gt;2.4 GHz Wireless Module&lt;/b&gt; based on &lt;b&gt;NRF24L01&lt;/b&gt; chip</description>
<pin name="GND" direction="pwr"/>
<pin name="VCC" direction="pwr"/>
<pin name="CE"/>
<pin name="CSN"/>
<pin name="SCK"/>
<pin name="MOSI"/>
<pin name="MISO"/>
<pin name="IRQ"/>
</symbol>
<symbol name="WIRELESS-XY-FST">
<description>&lt;b&gt;RF Wireless XY-FST Transmitter&lt;/b&gt;</description>
<pin name="ANT" direction="out"/>
<pin name="GND" direction="pwr"/>
<pin name="VCC" direction="pwr"/>
<pin name="ATAD" direction="in"/>
</symbol>
<symbol name="WIRELESS-XY-FST#V">
<description>&lt;b&gt;RF Wireless XY-FST Transmitter&lt;/b&gt; vertically mounted</description>
<pin name="GND" direction="pwr"/>
<pin name="VCC" direction="pwr"/>
<pin name="ATAD" direction="in"/>
</symbol>
<symbol name="WIRELESS-XY-MK-5V">
<description>&lt;b&gt;RF Wireless XY-MK-5V Receiver&lt;/b&gt;</description>
<pin name="GND"/>
<pin name="DATA.1"/>
<pin name="DATA.2"/>
<pin name="VCC"/>
<pin name="ANT" direction="out"/>
</symbol>
<symbol name="ADC-DAC-PCF8591">
<description>&lt;b&gt;4-Channel ADC and 1-Channel DAC Module&lt;/b&gt; based on &lt;b&gt;PCF8591&lt;/b&gt; chip</description>
<pin name="AOUT"/>
<pin name="AIN0"/>
<pin name="AIN1"/>
<pin name="AIN2"/>
<pin name="AIN3"/>
<pin name="SCL"/>
<pin name="SDA"/>
<pin name="GND" direction="pwr"/>
<pin name="VCC" direction="pwr"/>
</symbol>
<symbol name="AMPLIFIER-PAM8403">
<description>&lt;b&gt;Stereo Class-D 3W Audio Amplifier&lt;/b&gt; based on &lt;b&gt;PAM8403&lt;/b&gt; chip</description>
<pin name="IN.L" direction="in"/>
<pin name="IN.COM" direction="in"/>
<pin name="IN.R"/>
<pin name="+5V" direction="pwr"/>
<pin name="GND" direction="pwr"/>
<pin name="OUT.L-" direction="out"/>
<pin name="OUT.L+" direction="out"/>
<pin name="OUT.R+" direction="out"/>
<pin name="OUT.R-" direction="out"/>
</symbol>
<symbol name="BREADBOARD-POWER-V1">
<description>&lt;b&gt;Breadboard Power Adapter&lt;/b&gt; with onboard 3.3V and 5V regulators</description>
<pin name="P.1"/>
<pin name="P.2"/>
<pin name="P.3"/>
<pin name="P.4"/>
<pin name="P.5"/>
<pin name="M.1"/>
<pin name="M.2"/>
<pin name="M.3"/>
<pin name="M.4"/>
<pin name="M.5"/>
</symbol>
<symbol name="CARD-SD-ADAPTER">
<description>&lt;b&gt;Full Size SD Card Adapter Module&lt;/b&gt; with onboard 3.3V regulator</description>
<pin name="GND.1" direction="pwr"/>
<pin name="3V3" direction="pwr"/>
<pin name="5V" direction="pwr"/>
<pin name="CS"/>
<pin name="MOSI"/>
<pin name="SCK"/>
<pin name="MISO"/>
<pin name="GND.2" direction="pwr"/>
</symbol>
<symbol name="COMPASS-HMC5883L">
<description>&lt;b&gt;3-Axis Digital Compass Module&lt;/b&gt; based on &lt;b&gt;HMC5883L&lt;/b&gt; chip</description>
<pin name="VCC" direction="pwr"/>
<pin name="GND" direction="pwr"/>
<pin name="SCL"/>
<pin name="SDA"/>
<pin name="DRDY"/>
</symbol>
<symbol name="CURRENT-SENSOR-ACS712">
<description>&lt;b&gt;Isolated Bipolar Current Sensors&lt;/b&gt; based on &lt;b&gt;ACS712&lt;/b&gt; chip</description>
<pin name="VCC" direction="pwr"/>
<pin name="OUT" direction="out"/>
<pin name="GND" direction="pwr"/>
</symbol>
<symbol name="CURRENT-SENSOR-ACS712#IC">
<description>&lt;b&gt;Isolated Bipolar Current Sensors&lt;/b&gt; based on &lt;b&gt;ACS712&lt;/b&gt; chip&lt;br&gt;
Symbol with input pads</description>
<pin name="VCC" direction="pwr"/>
<pin name="OUT" direction="out"/>
<pin name="GND" direction="pwr"/>
<pin name="IN+"/>
<pin name="IN-"/>
</symbol>
<symbol name="DC-DC-STEP-DOWN-LM2596">
<description>&lt;b&gt;DC/DC Step-Down Regulator&lt;/b&gt; based on &lt;b&gt;LM2596-ADJ&lt;/b&gt; chip</description>
<pin name="IN+"/>
<pin name="IN-"/>
<pin name="OUT+"/>
<pin name="OUT-"/>
</symbol>
<symbol name="DRIVER-ULN2003">
<description>&lt;b&gt;7-Channel Darlington NPN Transistor Module&lt;/b&gt; based on &lt;b&gt;ULN2003&lt;/b&gt; chip&lt;br&gt;</description>
<pin name="IN.1"/>
<pin name="GND" direction="pwr"/>
<pin name="VCC.1" direction="pwr"/>
<pin name="VCC.2"/>
<pin name="MOT+"/>
<pin name="OUT.A"/>
<pin name="IN.2"/>
<pin name="IN.3"/>
<pin name="IN.4"/>
<pin name="IN.5"/>
<pin name="IN.6"/>
<pin name="IN.7"/>
<pin name="OUT.B"/>
<pin name="OUT.C"/>
<pin name="OUT.D"/>
<pin name="OUT.E"/>
<pin name="OUT.F"/>
<pin name="OUT.G"/>
</symbol>
<symbol name="DRIVER-ULN2003#MC">
<description>&lt;b&gt;7-Channel Darlington NPN Transistor Module&lt;/b&gt; based on &lt;b&gt;ULN2003&lt;/b&gt; chip&lt;br&gt;
Symbol with motor connector pins</description>
<pin name="IN.1"/>
<pin name="GND" direction="pwr"/>
<pin name="VCC.1" direction="pwr"/>
<pin name="VCC.2"/>
<pin name="MOT+"/>
<pin name="OUT.A"/>
<pin name="IN.2"/>
<pin name="IN.3"/>
<pin name="IN.4"/>
<pin name="IN.5"/>
<pin name="IN.6"/>
<pin name="IN.7"/>
<pin name="OUT.B"/>
<pin name="OUT.C"/>
<pin name="OUT.D"/>
<pin name="OUT.E"/>
<pin name="OUT.F"/>
<pin name="OUT.G"/>
<pin name="MOT.+"/>
<pin name="MOT.A"/>
<pin name="MOT.B"/>
<pin name="MOT.C"/>
<pin name="MOT.D"/>
</symbol>
<symbol name="LCD-I2C-CONVERTER">
<description>&lt;b&gt;I2C Bus to 4-Bit Parallel LCD Interface&lt;/b&gt; with LED backlight driver</description>
<pin name="GND" direction="pwr"/>
<pin name="SCL"/>
<pin name="SDA"/>
<pin name="VCC" direction="pwr"/>
<pin name="VSS"/>
<pin name="VDD"/>
<pin name="VEE"/>
<pin name="RS"/>
<pin name="R/W"/>
<pin name="DB0"/>
<pin name="DB1"/>
<pin name="DB2"/>
<pin name="DB3"/>
<pin name="DB4"/>
<pin name="DB5"/>
<pin name="DB6"/>
<pin name="DB7"/>
<pin name="LED.A"/>
<pin name="LED.K"/>
<pin name="EN"/>
</symbol>
<symbol name="LIGHT-DETECTOR">
<description>&lt;b&gt;Light Detection Module&lt;/b&gt;</description>
<pin name="5V" direction="pwr"/>
<pin name="OUT"/>
<pin name="GND" direction="pwr"/>
</symbol>
<symbol name="MOTION-PIR-DYP-ME003">
<description>&lt;b&gt;PIR Motion Sensor Module DYP-ME003&lt;/b&gt; based on &lt;b&gt;BISS0001&lt;/b&gt; pyroelectic detector</description>
<pin name="GND" direction="pwr"/>
<pin name="OUT" direction="out"/>
<pin name="VCC" direction="pwr"/>
</symbol>
<symbol name="REG-AMS1117">
<description>&lt;b&gt;Linear Regulator&lt;/b&gt; based on &lt;b&gt;AMS1117&lt;/b&gt; chip</description>
<pin name="VIN"/>
<pin name="GND.I"/>
<pin name="VOUT"/>
<pin name="GND.O"/>
</symbol>
<symbol name="RELAY-2-SRD#RC">
<description>&lt;b&gt;2-Channel Relay Module&lt;/b&gt; based on &lt;b&gt;SRD-05VDC-SL-C&lt;/b&gt; relays&lt;br&gt;
Symbol with relays pins</description>
<pin name="REL.1.NO"/>
<pin name="REL.1.COM"/>
<pin name="REL.1.NC"/>
<pin name="REL.2.NO"/>
<pin name="REL.2.COM"/>
<pin name="REL.2.NC"/>
<pin name="VCC.1" direction="pwr"/>
<pin name="IN2"/>
<pin name="IN1"/>
<pin name="GND.1" direction="pwr"/>
<pin name="GND.2" direction="pwr"/>
<pin name="VCC.2" direction="pwr"/>
<pin name="JD-VCC"/>
</symbol>
<symbol name="RELAY-2-SRD">
<description>&lt;b&gt;2-Channel Relay Module&lt;/b&gt; based on &lt;b&gt;SRD-05VDC-SL-C&lt;/b&gt; relays</description>
<pin name="VCC.1" direction="pwr"/>
<pin name="IN2"/>
<pin name="IN1"/>
<pin name="GND.1" direction="pwr"/>
<pin name="GND.2" direction="pwr"/>
<pin name="VCC.2" direction="pwr"/>
<pin name="JD-VCC"/>
</symbol>
<symbol name="RTC-EEPROM-BATTERY">
<description>&lt;b&gt;RTC Module with Battery and EEPROM&lt;/b&gt; based on &lt;b&gt;DS1307&lt;/b&gt; and &lt;b&gt;AT24C32&lt;/b&gt; chips</description>
<pin name="GND.1" direction="pwr"/>
<pin name="VCC.1" direction="pwr"/>
<pin name="SDA.1"/>
<pin name="SCL.1"/>
<pin name="DS.1"/>
<pin name="BAT"/>
<pin name="GND.2" direction="pwr"/>
<pin name="VCC.2" direction="pwr"/>
<pin name="SDA.2"/>
<pin name="SCL.2"/>
<pin name="DS.2"/>
<pin name="SQ"/>
</symbol>
<symbol name="SOIL-MOISTURE-SENSOR">
<description>&lt;b&gt;Soil Moisture Sensor&lt;/b&gt;</description>
<pin name="VCC" direction="pwr"/>
<pin name="GND" direction="pwr"/>
<pin name="DO" direction="out"/>
<pin name="A0"/>
<pin name="SENS.2"/>
<pin name="SENS.1"/>
</symbol>
<symbol name="SOUND-DETECTOR">
<description>&lt;b&gt;Sound Detection Module&lt;/b&gt;</description>
<pin name="GND" direction="pwr"/>
<pin name="OUT" direction="out"/>
<pin name="+5V" direction="pwr"/>
</symbol>
<symbol name="ULTRASONIC-HC-SR04">
<description>&lt;b&gt;Ultrasonic Ranging Module HC-SR04&lt;/b&gt;</description>
<pin name="VCC" direction="pwr"/>
<pin name="TRIG" direction="in"/>
<pin name="ECHO" direction="out"/>
<pin name="GND" direction="pwr"/>
</symbol>
<symbol name="WIRELESS-WIFI-ESP-01">
<description>&lt;b&gt;Wireless Wi-Fi ESP-01 Module&lt;/b&gt; based on &lt;b&gt;ESP8266&lt;/b&gt; chip</description>
<pin name="GND" direction="pwr"/>
<pin name="UTXD"/>
<pin name="GPIO2"/>
<pin name="CH_PD"/>
<pin name="GPIO0"/>
<pin name="RST"/>
<pin name="URXD"/>
<pin name="VCC" direction="pwr"/>
</symbol>
<symbol name="DC-DC-STEP-UP-5V">
<description>&lt;b&gt;DC/DC Step-Up Converter&lt;/b&gt;</description>
<pin name="IN+" direction="pwr"/>
<pin name="IN-" direction="pwr"/>
<pin name="GND"/>
<pin name="D+"/>
<pin name="D-"/>
<pin name="5V"/>
</symbol>
<symbol name="WIRELESS-NRF24L01-PA-EXT">
<description>&lt;b&gt;2.4 GHz Wireless Module&lt;/b&gt; based on &lt;b&gt;NRF24L01&lt;/b&gt; chip with preamplifier and external antenna</description>
<pin name="GND" direction="pwr"/>
<pin name="VCC" direction="pwr"/>
<pin name="CE"/>
<pin name="CSN"/>
<pin name="SCK"/>
<pin name="MOSI"/>
<pin name="MISO"/>
<pin name="IRQ"/>
</symbol>
<symbol name="AC-DC-3.5W">
<description>&lt;b&gt;AC/DC 3.5W Converter&lt;/b&gt;</description>
<pin name="AC1"/>
<pin name="AC2"/>
<pin name="OUT-"/>
<pin name="OUT+"/>
<pin name="5V"/>
</symbol>
<symbol name="BATTERY-CHARGER-LI-5V">
<description>&lt;b&gt;Lithium Battery 5V Charger&lt;/b&gt;</description>
<pin name="IN+"/>
<pin name="IN-"/>
<pin name="BAT+"/>
<pin name="BAT-"/>
</symbol>
<symbol name="FLAME-DETECTOR">
<description>&lt;b&gt;Flame Detector&lt;/b&gt;</description>
<pin name="VCC" direction="pwr"/>
<pin name="GND" direction="pwr"/>
<pin name="DO"/>
<pin name="AO"/>
</symbol>
<symbol name="IR-RECEIVER">
<description>&lt;b&gt;IR Receiver Module&lt;/b&gt;</description>
<pin name="VCC.1"/>
<pin name="VCC.2"/>
<pin name="GND.1"/>
<pin name="GND.2"/>
<pin name="IN.1"/>
<pin name="IN.2"/>
<pin name="VCC"/>
<pin name="GND"/>
<pin name="IN"/>
</symbol>
<symbol name="IR-RECEIVER#NC">
<description>&lt;b&gt;IR Receiver Module&lt;/b&gt; without IR sensor connector</description>
<pin name="VCC.1"/>
<pin name="VCC.2"/>
<pin name="GND.1"/>
<pin name="GND.2"/>
<pin name="IN.1"/>
<pin name="IN.2"/>
</symbol>
<symbol name="STEPPER-MOTOR-EASY-DRIVER">
<description>&lt;b&gt;Stepper Motor Easy Driver&lt;/b&gt;</description>
<pin name="GND.1"/>
<pin name="+5V"/>
<pin name="SLP"/>
<pin name="MS1"/>
<pin name="GND.2"/>
<pin name="STER"/>
<pin name="DIR"/>
<pin name="A.1"/>
<pin name="A.2"/>
<pin name="B.1"/>
<pin name="B.2"/>
<pin name="PFD"/>
<pin name="RST"/>
<pin name="ENA"/>
<pin name="MS2"/>
<pin name="GND"/>
<pin name="M+"/>
</symbol>
<symbol name="RS485-TTL-CONVERTER">
<description>&lt;b&gt;RS485 to TTL converter&lt;/b&gt; based on &lt;b&gt;MAX485&lt;/b&gt; chip</description>
<pin name="B" direction="pas"/>
<pin name="A" direction="pas"/>
<pin name="GND" direction="pwr"/>
<pin name="VCC" direction="pwr"/>
<pin name="RO" direction="pas"/>
<pin name="RE" direction="pas"/>
<pin name="DE" direction="pas"/>
<pin name="DI" direction="pas"/>
</symbol>
<symbol name="TOUCH-KEYPAD-4X4">
<description>&lt;b&gt;16 Channel Capacitive Touch Keypad&lt;/b&gt;</description>
<pin name="OUT8"/>
<pin name="OUT6"/>
<pin name="OUT5"/>
<pin name="OUT4"/>
<pin name="OUT3"/>
<pin name="OUT2"/>
<pin name="OUT1"/>
<pin name="SDO"/>
<pin name="SCL"/>
<pin name="GND" direction="pwr"/>
<pin name="VCC" direction="pwr"/>
<pin name="OUT7"/>
</symbol>
<symbol name="N-MOSFET-SWITCH">
<description>&lt;b&gt;Low Side N-MOSFET Switch&lt;/b&gt; with &lt;b&gt;Optocoupler&lt;/b&gt;</description>
<pin name="GND" direction="pwr"/>
<pin name="VCC" direction="pwr"/>
<pin name="CTRL"/>
</symbol>
<symbol name="N-MOSFET-SWITCH#IC">
<description>&lt;b&gt;Low Side N-MOSFET Switch&lt;/b&gt; with &lt;b&gt;Optocoupler&lt;/b&gt;&lt;br /&gt;
Symbol with connector pins</description>
<pin name="GND" direction="pwr"/>
<pin name="VCC" direction="pwr"/>
<pin name="CTRL"/>
<pin name="IN.V+" direction="pwr"/>
<pin name="IN.COM" direction="pwr"/>
<pin name="OUT.V+" direction="pwr"/>
<pin name="OUT.SW" direction="pwr"/>
</symbol>
<symbol name="SOUND-BUZZER">
<description>&lt;b&gt;Sound Buzzer Module&lt;/b&gt;</description>
<pin name="VCC" direction="pwr"/>
<pin name="EN" direction="in"/>
<pin name="GND" direction="pwr"/>
</symbol>
<symbol name="BREADBOARD-POWER-V2">
<description>&lt;b&gt;Breadboard Power Adapter&lt;/b&gt; with onboard 3.3V and 5V regulators</description>
<pin name="P.1"/>
<pin name="P.2"/>
<pin name="M.1"/>
<pin name="M.2"/>
</symbol>
<symbol name="LED-24XRGB-RING">
<description>&lt;b&gt;24 LEDs RGB Ring&lt;/b&gt; based on &lt;b&gt;WS2812B&lt;/b&gt;</description>
<pin name="GND.1" direction="pwr"/>
<pin name="VCC.1" direction="pwr"/>
<pin name="IN" direction="in"/>
<pin name="GND.2" direction="pwr"/>
<pin name="VCC.2" direction="pwr"/>
<pin name="OUT" direction="in"/>
</symbol>
<symbol name="GSM-MODEM-SIM900A">
<description>&lt;b&gt;GSM Mini Moodule&lt;/b&gt; based on &lt;b&gt;SIM900A&lt;/b&gt;</description>
<pin name="VCC5" direction="pwr"/>
<pin name="GND.1" direction="pwr"/>
<pin name="VCC4" direction="pwr"/>
<pin name="VCCMCU" direction="pwr"/>
<pin name="SIMR"/>
<pin name="SIMT"/>
<pin name="GND.2" direction="pwr"/>
<pin name="RST"/>
</symbol>
<symbol name="SPARKFUN-AD-MUX-16X1">
<description>&lt;b&gt;SparkFun Analog/Digital MUX Breakout&lt;/b&gt; based on &lt;b&gt;CD74HC4067&lt;/b&gt; chip</description>
<pin name="C15"/>
<pin name="GND" direction="pwr"/>
<pin name="VCC" direction="pwr"/>
<pin name="EN" direction="in"/>
<pin name="S0"/>
<pin name="S1"/>
<pin name="S2"/>
<pin name="S3"/>
<pin name="C14"/>
<pin name="C13"/>
<pin name="C12"/>
<pin name="C11"/>
<pin name="C10"/>
<pin name="C9"/>
<pin name="C8"/>
<pin name="C7"/>
<pin name="C6"/>
<pin name="C5"/>
<pin name="C4"/>
<pin name="C3"/>
<pin name="C2"/>
<pin name="C1"/>
<pin name="C0"/>
<pin name="SIG"/>
</symbol>
</symbols>
<devicesets>
<deviceset name="ARDUINO-NANO-3.0#ISP" prefix="M">
<description>&lt;b&gt;Arduino Nano 3.0&lt;/b&gt; with ISP pads
&lt;p&gt;&lt;img alt="photo" src="http://www.diymodules.org/img/device-photo.php?name=ARDUINO-NANO-3.0"&gt;&lt;/p&gt;</description>
<gates>
<gate name="G$1" symbol="ARDUINO-NANO-3.0#ISP"/>
</gates>
<devices>
<device name="" package="ARDUINO-NANO-3.0#ISP">
<connects>
<connect gate="G$1" pin="3V3" pad="J2.14"/>
<connect gate="G$1" pin="5V" pad="J2.4"/>
<connect gate="G$1" pin="A0" pad="J2.12"/>
<connect gate="G$1" pin="A1" pad="J2.11"/>
<connect gate="G$1" pin="A2" pad="J2.10"/>
<connect gate="G$1" pin="A3" pad="J2.9"/>
<connect gate="G$1" pin="A4" pad="J2.8"/>
<connect gate="G$1" pin="A5" pad="J2.7"/>
<connect gate="G$1" pin="A6" pad="J2.6"/>
<connect gate="G$1" pin="A7" pad="J2.5"/>
<connect gate="G$1" pin="AREF" pad="J2.13"/>
<connect gate="G$1" pin="D0/RX" pad="J1.2"/>
<connect gate="G$1" pin="D1/TX" pad="J1.1"/>
<connect gate="G$1" pin="D10" pad="J1.13"/>
<connect gate="G$1" pin="D11/MOSI" pad="J1.14"/>
<connect gate="G$1" pin="D12/MISO" pad="J1.15"/>
<connect gate="G$1" pin="D13/SCK" pad="J2.15"/>
<connect gate="G$1" pin="D2" pad="J1.5"/>
<connect gate="G$1" pin="D3" pad="J1.6"/>
<connect gate="G$1" pin="D4" pad="J1.7"/>
<connect gate="G$1" pin="D5" pad="J1.8"/>
<connect gate="G$1" pin="D6" pad="J1.9"/>
<connect gate="G$1" pin="D7" pad="J1.10"/>
<connect gate="G$1" pin="D8" pad="J1.11"/>
<connect gate="G$1" pin="D9" pad="J1.12"/>
<connect gate="G$1" pin="GND.1" pad="J1.4"/>
<connect gate="G$1" pin="GND.2" pad="J2.2"/>
<connect gate="G$1" pin="ISP_5V" pad="J4.2"/>
<connect gate="G$1" pin="ISP_GND" pad="J4.6"/>
<connect gate="G$1" pin="ISP_MISO" pad="J4.1"/>
<connect gate="G$1" pin="ISP_MOSI" pad="J4.4"/>
<connect gate="G$1" pin="ISP_RST" pad="J4.5"/>
<connect gate="G$1" pin="ISP_SCK" pad="J4.3"/>
<connect gate="G$1" pin="RST.1" pad="J1.3"/>
<connect gate="G$1" pin="RST.2" pad="J2.3"/>
<connect gate="G$1" pin="VIN" pad="J2.1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ARDUINO-NANO-3.0" prefix="M">
<description>&lt;b&gt;Arduino Nano 3.0&lt;/b&gt;
&lt;p&gt;&lt;img alt="photo" src="http://www.diymodules.org/img/device-photo.php?name=ARDUINO-NANO-3.0"&gt;&lt;/p&gt;</description>
<gates>
<gate name="G$1" symbol="ARDUINO-NANO-3.0"/>
</gates>
<devices>
<device name="" package="ARDUINO-NANO-3.0">
<connects>
<connect gate="G$1" pin="3V3" pad="J2.14"/>
<connect gate="G$1" pin="5V" pad="J2.4"/>
<connect gate="G$1" pin="A0" pad="J2.12"/>
<connect gate="G$1" pin="A1" pad="J2.11"/>
<connect gate="G$1" pin="A2" pad="J2.10"/>
<connect gate="G$1" pin="A3" pad="J2.9"/>
<connect gate="G$1" pin="A4" pad="J2.8"/>
<connect gate="G$1" pin="A5" pad="J2.7"/>
<connect gate="G$1" pin="A6" pad="J2.6"/>
<connect gate="G$1" pin="A7" pad="J2.5"/>
<connect gate="G$1" pin="AREF" pad="J2.13"/>
<connect gate="G$1" pin="D0/RX" pad="J1.2"/>
<connect gate="G$1" pin="D1/TX" pad="J1.1"/>
<connect gate="G$1" pin="D10" pad="J1.13"/>
<connect gate="G$1" pin="D11/MOSI" pad="J1.14"/>
<connect gate="G$1" pin="D12/MISO" pad="J1.15"/>
<connect gate="G$1" pin="D13/SCK" pad="J2.15"/>
<connect gate="G$1" pin="D2" pad="J1.5"/>
<connect gate="G$1" pin="D3" pad="J1.6"/>
<connect gate="G$1" pin="D4" pad="J1.7"/>
<connect gate="G$1" pin="D5" pad="J1.8"/>
<connect gate="G$1" pin="D6" pad="J1.9"/>
<connect gate="G$1" pin="D7" pad="J1.10"/>
<connect gate="G$1" pin="D8" pad="J1.11"/>
<connect gate="G$1" pin="D9" pad="J1.12"/>
<connect gate="G$1" pin="GND.1" pad="J1.4"/>
<connect gate="G$1" pin="GND.2" pad="J2.2"/>
<connect gate="G$1" pin="RST.1" pad="J1.3"/>
<connect gate="G$1" pin="RST.2" pad="J2.3"/>
<connect gate="G$1" pin="VIN" pad="J2.1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ARDUINO-PRO-MINI-*" prefix="M">
<description>&lt;b&gt;Arduino Pro Mini&lt;/b&gt;
&lt;p&gt;&lt;img alt="photo" src="http://www.diymodules.org/img/device-photo.php?name=ARDUINO-PRO-MINI-"&gt;&lt;/p&gt;</description>
<gates>
<gate name="G$1" symbol="ARDUINO-PRO-MINI"/>
</gates>
<devices>
<device name="" package="ARDUINO-PRO-MINI">
<connects>
<connect gate="G$1" pin="A0" pad="J6.8"/>
<connect gate="G$1" pin="A1" pad="J6.7"/>
<connect gate="G$1" pin="A2" pad="J6.6"/>
<connect gate="G$1" pin="A3" pad="J6.5"/>
<connect gate="G$1" pin="A4" pad="J2.1"/>
<connect gate="G$1" pin="A5" pad="J2.2"/>
<connect gate="G$1" pin="A6" pad="J3.2"/>
<connect gate="G$1" pin="A7" pad="J3.3"/>
<connect gate="G$1" pin="D0/RX" pad="J7.11"/>
<connect gate="G$1" pin="D1/TX" pad="J7.12"/>
<connect gate="G$1" pin="D10" pad="J6.12"/>
<connect gate="G$1" pin="D11" pad="J6.11"/>
<connect gate="G$1" pin="D12" pad="J6.10"/>
<connect gate="G$1" pin="D13" pad="J6.9"/>
<connect gate="G$1" pin="D2" pad="J7.8"/>
<connect gate="G$1" pin="D3" pad="J7.7"/>
<connect gate="G$1" pin="D4" pad="J7.6"/>
<connect gate="G$1" pin="D5" pad="J7.5"/>
<connect gate="G$1" pin="D6" pad="J7.4"/>
<connect gate="G$1" pin="D7" pad="J7.3"/>
<connect gate="G$1" pin="D8" pad="J7.2"/>
<connect gate="G$1" pin="D9" pad="J7.1"/>
<connect gate="G$1" pin="GND.1" pad="J7.9"/>
<connect gate="G$1" pin="GND.2" pad="J6.2"/>
<connect gate="G$1" pin="GND.3" pad="J3.1"/>
<connect gate="G$1" pin="P_CTS" pad="J1.2"/>
<connect gate="G$1" pin="P_DTR" pad="J1.6"/>
<connect gate="G$1" pin="P_GND" pad="J1.1"/>
<connect gate="G$1" pin="P_RXD" pad="J1.4"/>
<connect gate="G$1" pin="P_TXD" pad="J1.5"/>
<connect gate="G$1" pin="P_VCC" pad="J1.3"/>
<connect gate="G$1" pin="RAW" pad="J6.1"/>
<connect gate="G$1" pin="RST.1" pad="J7.10"/>
<connect gate="G$1" pin="RST.2" pad="J6.3"/>
<connect gate="G$1" pin="VCC" pad="J6.4"/>
</connects>
<technologies>
<technology name="3.3V"/>
<technology name="5.0V"/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ARDUINO-PRO-MINI-*#NP" prefix="M">
<description>&lt;b&gt;Arduino Pro Mini&lt;/b&gt; without programming pads
&lt;p&gt;&lt;img alt="photo" src="http://www.diymodules.org/img/device-photo.php?name=ARDUINO-PRO-MINI-"&gt;&lt;/p&gt;</description>
<gates>
<gate name="G$1" symbol="ARDUINO-PRO-MINI#NP"/>
</gates>
<devices>
<device name="" package="ARDUINO-PRO-MINI#NP">
<connects>
<connect gate="G$1" pin="A0" pad="J6.8"/>
<connect gate="G$1" pin="A1" pad="J6.7"/>
<connect gate="G$1" pin="A2" pad="J6.6"/>
<connect gate="G$1" pin="A3" pad="J6.5"/>
<connect gate="G$1" pin="A4" pad="J2.1"/>
<connect gate="G$1" pin="A5" pad="J2.2"/>
<connect gate="G$1" pin="A6" pad="J3.2"/>
<connect gate="G$1" pin="A7" pad="J3.3"/>
<connect gate="G$1" pin="D0/RX" pad="J7.11"/>
<connect gate="G$1" pin="D1/TX" pad="J7.12"/>
<connect gate="G$1" pin="D10" pad="J6.12"/>
<connect gate="G$1" pin="D11" pad="J6.11"/>
<connect gate="G$1" pin="D12" pad="J6.10"/>
<connect gate="G$1" pin="D13" pad="J6.9"/>
<connect gate="G$1" pin="D2" pad="J7.8"/>
<connect gate="G$1" pin="D3" pad="J7.7"/>
<connect gate="G$1" pin="D4" pad="J7.6"/>
<connect gate="G$1" pin="D5" pad="J7.5"/>
<connect gate="G$1" pin="D6" pad="J7.4"/>
<connect gate="G$1" pin="D7" pad="J7.3"/>
<connect gate="G$1" pin="D8" pad="J7.2"/>
<connect gate="G$1" pin="D9" pad="J7.1"/>
<connect gate="G$1" pin="GND.1" pad="J7.9"/>
<connect gate="G$1" pin="GND.2" pad="J6.2"/>
<connect gate="G$1" pin="GND.3" pad="J3.1"/>
<connect gate="G$1" pin="RAW" pad="J6.1"/>
<connect gate="G$1" pin="RST.1" pad="J6.3"/>
<connect gate="G$1" pin="RST.2" pad="J7.10"/>
<connect gate="G$1" pin="VCC" pad="J6.4"/>
</connects>
<technologies>
<technology name="3.3V"/>
<technology name="5.0V"/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ARDUINO-PRO-MINI-*#APC" prefix="M">
<description>&lt;b&gt;Arduino Pro Mini&lt;/b&gt; with angle programming connector
&lt;p&gt;&lt;img alt="photo" src="http://www.diymodules.org/img/device-photo.php?name=ARDUINO-PRO-MINI-"&gt;&lt;/p&gt;</description>
<gates>
<gate name="G$1" symbol="ARDUINO-PRO-MINI#NP"/>
</gates>
<devices>
<device name="" package="ARDUINO-PRO-MINI#APC">
<connects>
<connect gate="G$1" pin="A0" pad="J6.8"/>
<connect gate="G$1" pin="A1" pad="J6.7"/>
<connect gate="G$1" pin="A2" pad="J6.6"/>
<connect gate="G$1" pin="A3" pad="J6.5"/>
<connect gate="G$1" pin="A4" pad="J2.1"/>
<connect gate="G$1" pin="A5" pad="J2.2"/>
<connect gate="G$1" pin="A6" pad="J3.2"/>
<connect gate="G$1" pin="A7" pad="J3.3"/>
<connect gate="G$1" pin="D0/RX" pad="J7.11"/>
<connect gate="G$1" pin="D1/TX" pad="J7.12"/>
<connect gate="G$1" pin="D10" pad="J6.12"/>
<connect gate="G$1" pin="D11" pad="J6.11"/>
<connect gate="G$1" pin="D12" pad="J6.10"/>
<connect gate="G$1" pin="D13" pad="J6.9"/>
<connect gate="G$1" pin="D2" pad="J7.8"/>
<connect gate="G$1" pin="D3" pad="J7.7"/>
<connect gate="G$1" pin="D4" pad="J7.6"/>
<connect gate="G$1" pin="D5" pad="J7.5"/>
<connect gate="G$1" pin="D6" pad="J7.4"/>
<connect gate="G$1" pin="D7" pad="J7.3"/>
<connect gate="G$1" pin="D8" pad="J7.2"/>
<connect gate="G$1" pin="D9" pad="J7.1"/>
<connect gate="G$1" pin="GND.1" pad="J7.9"/>
<connect gate="G$1" pin="GND.2" pad="J6.2"/>
<connect gate="G$1" pin="GND.3" pad="J3.1"/>
<connect gate="G$1" pin="RAW" pad="J6.1"/>
<connect gate="G$1" pin="RST.1" pad="J7.10"/>
<connect gate="G$1" pin="RST.2" pad="J6.3"/>
<connect gate="G$1" pin="VCC" pad="J6.4"/>
</connects>
<technologies>
<technology name="3.3V"/>
<technology name="5.0V"/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ARDUINO-PRO-MINI-*#SMP" prefix="M">
<description>&lt;b&gt;Arduino Pro Mini&lt;/b&gt; with 2 connectors only
&lt;p&gt;&lt;img alt="photo" src="http://www.diymodules.org/img/device-photo.php?name=ARDUINO-PRO-MINI-"&gt;&lt;/p&gt;</description>
<gates>
<gate name="G$1" symbol="ARDUINO-PRO-MINI#SMP"/>
</gates>
<devices>
<device name="" package="ARDUINO-PRO-MINI#SMP">
<connects>
<connect gate="G$1" pin="A0" pad="J6.8"/>
<connect gate="G$1" pin="A1" pad="J6.7"/>
<connect gate="G$1" pin="A2" pad="J6.6"/>
<connect gate="G$1" pin="A3" pad="J6.5"/>
<connect gate="G$1" pin="D0/RX" pad="J7.11"/>
<connect gate="G$1" pin="D1/TX" pad="J7.12"/>
<connect gate="G$1" pin="D10" pad="J6.12"/>
<connect gate="G$1" pin="D11" pad="J6.11"/>
<connect gate="G$1" pin="D12" pad="J6.10"/>
<connect gate="G$1" pin="D13" pad="J6.9"/>
<connect gate="G$1" pin="D2" pad="J7.8"/>
<connect gate="G$1" pin="D3" pad="J7.7"/>
<connect gate="G$1" pin="D4" pad="J7.6"/>
<connect gate="G$1" pin="D5" pad="J7.5"/>
<connect gate="G$1" pin="D6" pad="J7.4"/>
<connect gate="G$1" pin="D7" pad="J7.3"/>
<connect gate="G$1" pin="D8" pad="J7.2"/>
<connect gate="G$1" pin="D9" pad="J7.1"/>
<connect gate="G$1" pin="GND.1" pad="J7.9"/>
<connect gate="G$1" pin="GND.2" pad="J6.2"/>
<connect gate="G$1" pin="RAW" pad="J6.1"/>
<connect gate="G$1" pin="RST.1" pad="J7.10"/>
<connect gate="G$1" pin="RST.2" pad="J6.3"/>
<connect gate="G$1" pin="VCC" pad="J6.4"/>
</connects>
<technologies>
<technology name="3.3V"/>
<technology name="5.0V"/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="BATTERY-HOLDER">
<description>&lt;b&gt;Battery Holder&lt;/b&gt;
&lt;p&gt;&lt;img alt="photo" src="http://www.diymodules.org/img/device-photo.php?name=BATTERY-HOLDER"&gt;&lt;/p&gt;</description>
<gates>
<gate name="G$1" symbol="BATTERY-HOLDER"/>
</gates>
<devices>
<device name="-2AA" package="BATTERY-HOLDER-2AA">
<connects>
<connect gate="G$1" pin="BAT+" pad="BAT+"/>
<connect gate="G$1" pin="BAT-" pad="BAT-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-2AAA" package="BATTERY-HOLDER-2AAA">
<connects>
<connect gate="G$1" pin="BAT+" pad="BAT+"/>
<connect gate="G$1" pin="BAT-" pad="BAT-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="DC-DC-STEP-UP-5V-USB" prefix="M">
<description>&lt;b&gt;DC/DC Step-Up Converter&lt;/b&gt; with &lt;b&gt;USB-A&lt;/b&gt; connector
&lt;p&gt;&lt;img alt="photo" src="http://www.diymodules.org/img/device-photo.php?name=DC-DC-STEP-UP-5V-USB"&gt;&lt;/p&gt;</description>
<gates>
<gate name="G$1" symbol="DC-DC-STEP-UP-5V-USB"/>
</gates>
<devices>
<device name="" package="DC-DC-STEP-UP-5V-USB">
<connects>
<connect gate="G$1" pin="IN+" pad="IN+"/>
<connect gate="G$1" pin="IN-" pad="IN-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="DISPLAY-NOKIA-3310">
<description>&lt;b&gt;84x48 Dot Matrix LCD Module&lt;/b&gt; based on &lt;b&gt;Nokia 3310&lt;/b&gt; display
&lt;p&gt;&lt;img alt="photo" src="http://www.diymodules.org/img/device-photo.php?name=DISPLAY-NOKIA-3310"&gt;&lt;/p&gt;</description>
<gates>
<gate name="G$1" symbol="DISPLAY-NOKIA-3310"/>
</gates>
<devices>
<device name="" package="DISPLAY-NOKIA-3310">
<connects>
<connect gate="G$1" pin="D/C.1" pad="J1.5"/>
<connect gate="G$1" pin="D/C.2" pad="J2.5"/>
<connect gate="G$1" pin="DIN.1" pad="J1.6"/>
<connect gate="G$1" pin="DIN.2" pad="J2.6"/>
<connect gate="G$1" pin="GND.1" pad="J1.2"/>
<connect gate="G$1" pin="GND.2" pad="J2.2"/>
<connect gate="G$1" pin="LED.1" pad="J1.8"/>
<connect gate="G$1" pin="LED.2" pad="J2.8"/>
<connect gate="G$1" pin="RST.1" pad="J1.4"/>
<connect gate="G$1" pin="RST.2" pad="J2.4"/>
<connect gate="G$1" pin="SCE.1" pad="J1.3"/>
<connect gate="G$1" pin="SCE.2" pad="J2.3"/>
<connect gate="G$1" pin="SCK.1" pad="J1.7"/>
<connect gate="G$1" pin="SCK.2" pad="J2.7"/>
<connect gate="G$1" pin="VCC.1" pad="J1.1"/>
<connect gate="G$1" pin="VCC.2" pad="J2.1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ETHERNET-ENC28J60" prefix="M">
<description>&lt;b&gt;Ethernet Module&lt;/b&gt; based on &lt;b&gt;ENC28J60&lt;/b&gt; chip
&lt;p&gt;&lt;img alt="photo" src="http://www.diymodules.org/img/device-photo.php?name=ETHERNET-ENC28J60"&gt;&lt;/p&gt;</description>
<gates>
<gate name="G$1" symbol="ETHERNET-ENC28J60"/>
</gates>
<devices>
<device name="" package="ETHERNET-ENC28J60">
<connects>
<connect gate="G$1" pin="3V3" pad="2"/>
<connect gate="G$1" pin="5V" pad="12"/>
<connect gate="G$1" pin="CLK" pad="9"/>
<connect gate="G$1" pin="CS" pad="3"/>
<connect gate="G$1" pin="GND.1" pad="1"/>
<connect gate="G$1" pin="GND.2" pad="11"/>
<connect gate="G$1" pin="INT" pad="10"/>
<connect gate="G$1" pin="RST" pad="4"/>
<connect gate="G$1" pin="SCK" pad="6"/>
<connect gate="G$1" pin="SI" pad="5"/>
<connect gate="G$1" pin="SO" pad="8"/>
<connect gate="G$1" pin="WOL" pad="7"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WIRELESS-NRF24L01" prefix="M">
<description>&lt;b&gt;2.4 GHz Wireless Module&lt;/b&gt; based on &lt;b&gt;NRF24L01&lt;/b&gt; chip
&lt;p&gt;&lt;img alt="photo" src="http://www.diymodules.org/img/device-photo.php?name=WIRELESS-NRF24L01"&gt;&lt;/p&gt;</description>
<gates>
<gate name="G$1" symbol="WIRELESS-NRF24L01"/>
</gates>
<devices>
<device name="" package="WIRELESS-NRF24L01">
<connects>
<connect gate="G$1" pin="CE" pad="3"/>
<connect gate="G$1" pin="CSN" pad="4"/>
<connect gate="G$1" pin="GND" pad="1"/>
<connect gate="G$1" pin="IRQ" pad="8"/>
<connect gate="G$1" pin="MISO" pad="7"/>
<connect gate="G$1" pin="MOSI" pad="6"/>
<connect gate="G$1" pin="SCK" pad="5"/>
<connect gate="G$1" pin="VCC" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WIRELESS-XY-FST" prefix="M">
<description>&lt;b&gt;RF Wireless XY-FST Transmitter&lt;/b&gt;
&lt;p&gt;&lt;img alt="photo" src="http://www.diymodules.org/img/device-photo.php?name=WIRELESS-XY-FST"&gt;&lt;/p&gt;</description>
<gates>
<gate name="G$1" symbol="WIRELESS-XY-FST"/>
</gates>
<devices>
<device name="" package="WIRELESS-XY-FST">
<connects>
<connect gate="G$1" pin="ANT" pad="ANT"/>
<connect gate="G$1" pin="ATAD" pad="3"/>
<connect gate="G$1" pin="GND" pad="1"/>
<connect gate="G$1" pin="VCC" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WIRELESS-XY-FST#V" prefix="M">
<description>&lt;b&gt;RF Wireless XY-FST Transmitter&lt;/b&gt; vertically mounted
&lt;p&gt;&lt;img alt="photo" src="http://www.diymodules.org/img/device-photo.php?name=WIRELESS-XY-FST"&gt;&lt;/p&gt;</description>
<gates>
<gate name="G$1" symbol="WIRELESS-XY-FST#V"/>
</gates>
<devices>
<device name="" package="WIRELESS-XY-FST#V">
<connects>
<connect gate="G$1" pin="ATAD" pad="3"/>
<connect gate="G$1" pin="GND" pad="1"/>
<connect gate="G$1" pin="VCC" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WIRELESS-XY-MK-5V" prefix="M">
<description>&lt;b&gt;RF Wireless XY-MK-5V Receiver&lt;/b&gt;
&lt;p&gt;&lt;img alt="photo" src="http://www.diymodules.org/img/device-photo.php?name=WIRELESS-XY-MK-5V"&gt;&lt;/p&gt;</description>
<gates>
<gate name="G$1" symbol="WIRELESS-XY-MK-5V"/>
</gates>
<devices>
<device name="" package="WIRELESS-XY-MK-5V">
<connects>
<connect gate="G$1" pin="ANT" pad="ANT"/>
<connect gate="G$1" pin="DATA.1" pad="2"/>
<connect gate="G$1" pin="DATA.2" pad="3"/>
<connect gate="G$1" pin="GND" pad="1"/>
<connect gate="G$1" pin="VCC" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-V" package="WIRELESS-XY-MK-5V#V">
<connects>
<connect gate="G$1" pin="ANT" pad="ANT"/>
<connect gate="G$1" pin="DATA.1" pad="2"/>
<connect gate="G$1" pin="DATA.2" pad="3"/>
<connect gate="G$1" pin="GND" pad="1"/>
<connect gate="G$1" pin="VCC" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ADC-DAC-PCF8591">
<description>&lt;b&gt;4-Channel ADC and 1-Channel DAC Module&lt;/b&gt; based on &lt;b&gt;PCF8591&lt;/b&gt; chip
&lt;p&gt;&lt;img alt="photo" src="http://www.diymodules.org/img/device-photo.php?name=ADC-DAC-PCF8591"&gt;&lt;/p&gt;</description>
<gates>
<gate name="G$1" symbol="ADC-DAC-PCF8591"/>
</gates>
<devices>
<device name="" package="ADC-DAC-PCF8591">
<connects>
<connect gate="G$1" pin="AIN0" pad="J1.2"/>
<connect gate="G$1" pin="AIN1" pad="J1.3"/>
<connect gate="G$1" pin="AIN2" pad="J1.4"/>
<connect gate="G$1" pin="AIN3" pad="J1.5"/>
<connect gate="G$1" pin="AOUT" pad="J1.1"/>
<connect gate="G$1" pin="GND" pad="J2.3"/>
<connect gate="G$1" pin="SCL" pad="J2.1"/>
<connect gate="G$1" pin="SDA" pad="J2.2"/>
<connect gate="G$1" pin="VCC" pad="J2.4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="AMPLIFIER-PAM8403">
<description>&lt;b&gt;Stereo Class-D 3W Audio Amplifier&lt;/b&gt; based on &lt;b&gt;PAM8403&lt;/b&gt; chip
&lt;p&gt;&lt;img alt="photo" src="http://www.diymodules.org/img/device-photo.php?name=AMPLIFIER-PAM8403"&gt;&lt;/p&gt;</description>
<gates>
<gate name="G$1" symbol="AMPLIFIER-PAM8403"/>
</gates>
<devices>
<device name="" package="AMPLIFIER-PAM8403">
<connects>
<connect gate="G$1" pin="+5V" pad="+5V"/>
<connect gate="G$1" pin="GND" pad="GND"/>
<connect gate="G$1" pin="IN.COM" pad="IN.COM"/>
<connect gate="G$1" pin="IN.L" pad="IN.L"/>
<connect gate="G$1" pin="IN.R" pad="IN.R"/>
<connect gate="G$1" pin="OUT.L+" pad="OUT.L+"/>
<connect gate="G$1" pin="OUT.L-" pad="OUT.L-"/>
<connect gate="G$1" pin="OUT.R+" pad="OUT.R+"/>
<connect gate="G$1" pin="OUT.R-" pad="OUT.R-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="BREADBOARD-POWER-V1" uservalue="yes">
<description>&lt;b&gt;Breadboard Power Adapter&lt;/b&gt; with onboard 3.3V and 5V regulators
&lt;p&gt;&lt;img alt="photo" src="http://www.diymodules.org/img/device-photo.php?name=BREADBOARD-POWER-V1"&gt;&lt;/p&gt;</description>
<gates>
<gate name="G$1" symbol="BREADBOARD-POWER-V1"/>
<gate name="G$2" symbol="BREADBOARD-POWER-V1"/>
</gates>
<devices>
<device name="" package="BREADBOARD-POWER-V1">
<connects>
<connect gate="G$1" pin="M.1" pad="A.M.1"/>
<connect gate="G$1" pin="M.2" pad="A.M.2"/>
<connect gate="G$1" pin="M.3" pad="A.M.3"/>
<connect gate="G$1" pin="M.4" pad="A.M.4"/>
<connect gate="G$1" pin="M.5" pad="A.M.5"/>
<connect gate="G$1" pin="P.1" pad="A.P.1"/>
<connect gate="G$1" pin="P.2" pad="A.P.2"/>
<connect gate="G$1" pin="P.3" pad="A.P.3"/>
<connect gate="G$1" pin="P.4" pad="A.P.4"/>
<connect gate="G$1" pin="P.5" pad="A.P.5"/>
<connect gate="G$2" pin="M.1" pad="B.M.1"/>
<connect gate="G$2" pin="M.2" pad="B.M.2"/>
<connect gate="G$2" pin="M.3" pad="B.M.3"/>
<connect gate="G$2" pin="M.4" pad="B.M.4"/>
<connect gate="G$2" pin="M.5" pad="B.M.5"/>
<connect gate="G$2" pin="P.1" pad="B.P.1"/>
<connect gate="G$2" pin="P.2" pad="B.P.2"/>
<connect gate="G$2" pin="P.3" pad="B.P.3"/>
<connect gate="G$2" pin="P.4" pad="B.P.4"/>
<connect gate="G$2" pin="P.5" pad="B.P.5"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="CARD-SD-ADAPTER">
<description>&lt;b&gt;Full Size SD Card Adapter Module&lt;/b&gt; with onboard 3.3V regulator
&lt;p&gt;&lt;img alt="photo" src="http://www.diymodules.org/img/device-photo.php?name=CARD-SD-ADAPTER"&gt;&lt;/p&gt;</description>
<gates>
<gate name="G$1" symbol="CARD-SD-ADAPTER"/>
</gates>
<devices>
<device name="" package="CARD-SD-ADAPTER">
<connects>
<connect gate="G$1" pin="3V3" pad="3"/>
<connect gate="G$1" pin="5V" pad="5"/>
<connect gate="G$1" pin="CS" pad="7"/>
<connect gate="G$1" pin="GND.1" pad="1"/>
<connect gate="G$1" pin="GND.2" pad="15"/>
<connect gate="G$1" pin="MISO" pad="13"/>
<connect gate="G$1" pin="MOSI" pad="9"/>
<connect gate="G$1" pin="SCK" pad="11"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="COMPASS-HMC5883L" uservalue="yes">
<description>&lt;b&gt;3-Axis Digital Compass Module&lt;/b&gt; based on &lt;b&gt;HMC5883L&lt;/b&gt; chip
&lt;p&gt;&lt;img alt="photo" src="http://www.diymodules.org/img/device-photo.php?name=COMPASS-HMC5883L"&gt;&lt;/p&gt;</description>
<gates>
<gate name="G$1" symbol="COMPASS-HMC5883L"/>
</gates>
<devices>
<device name="" package="COMPASS-HMC5883L">
<connects>
<connect gate="G$1" pin="DRDY" pad="5"/>
<connect gate="G$1" pin="GND" pad="2"/>
<connect gate="G$1" pin="SCL" pad="3"/>
<connect gate="G$1" pin="SDA" pad="4"/>
<connect gate="G$1" pin="VCC" pad="1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="CURRENT-SENSOR-ACS712">
<description>&lt;b&gt;Isolated Bipolar Current Sensors&lt;/b&gt; based on &lt;b&gt;ACS712&lt;/b&gt; chip
&lt;p&gt;&lt;img alt="photo" src="http://www.diymodules.org/img/device-photo.php?name=CURRENT-SENSOR-ACS712"&gt;&lt;/p&gt;</description>
<gates>
<gate name="G$1" symbol="CURRENT-SENSOR-ACS712"/>
</gates>
<devices>
<device name="" package="CURRENT-SENSOR-ACS712">
<connects>
<connect gate="G$1" pin="GND" pad="3"/>
<connect gate="G$1" pin="OUT" pad="2"/>
<connect gate="G$1" pin="VCC" pad="1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="CURRENT-SENSOR-ACS712#IC">
<description>&lt;b&gt;Isolated Bipolar Current Sensors&lt;/b&gt; based on &lt;b&gt;ACS712&lt;/b&gt; chip&lt;br&gt;
Symbol with input pins
&lt;p&gt;&lt;img alt="photo" src="http://www.diymodules.org/img/device-photo.php?name=CURRENT-SENSOR-ACS712"&gt;&lt;/p&gt;</description>
<gates>
<gate name="G$1" symbol="CURRENT-SENSOR-ACS712#IC"/>
</gates>
<devices>
<device name="" package="CURRENT-SENSOR-ACS712#IC">
<connects>
<connect gate="G$1" pin="GND" pad="3"/>
<connect gate="G$1" pin="IN+" pad="P1.1"/>
<connect gate="G$1" pin="IN-" pad="P1.2"/>
<connect gate="G$1" pin="OUT" pad="2"/>
<connect gate="G$1" pin="VCC" pad="1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="DC-DC-STEP-DOWN-LM2596">
<description>&lt;b&gt;DC/DC Step-Down Regulator&lt;/b&gt; based on &lt;b&gt;LM2596-ADJ&lt;/b&gt; chip
&lt;p&gt;&lt;img alt="photo" src="http://www.diymodules.org/img/device-photo.php?name=DC-DC-STEP-DOWN-LM2596"&gt;&lt;/p&gt;</description>
<gates>
<gate name="G$1" symbol="DC-DC-STEP-DOWN-LM2596"/>
</gates>
<devices>
<device name="" package="DC-DC-STEP-DOWN-LM2596">
<connects>
<connect gate="G$1" pin="IN+" pad="IN+"/>
<connect gate="G$1" pin="IN-" pad="IN-"/>
<connect gate="G$1" pin="OUT+" pad="OUT+"/>
<connect gate="G$1" pin="OUT-" pad="OUT-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="DRIVER-ULN2003">
<description>&lt;b&gt;7-Channel Darlington NPN Transistor Module&lt;/b&gt; based on &lt;b&gt;ULN2003&lt;/b&gt; chip&lt;br&gt;
&lt;p&gt;&lt;img alt="photo" src="http://www.diymodules.org/img/device-photo.php?name=DRIVER-ULN2003"&gt;&lt;/p&gt;</description>
<gates>
<gate name="G$1" symbol="DRIVER-ULN2003"/>
</gates>
<devices>
<device name="" package="DRIVER-ULN2003">
<connects>
<connect gate="G$1" pin="GND" pad="J3.1"/>
<connect gate="G$1" pin="IN.1" pad="J1.1"/>
<connect gate="G$1" pin="IN.2" pad="J1.2"/>
<connect gate="G$1" pin="IN.3" pad="J1.3"/>
<connect gate="G$1" pin="IN.4" pad="J1.4"/>
<connect gate="G$1" pin="IN.5" pad="J1.5"/>
<connect gate="G$1" pin="IN.6" pad="J1.6"/>
<connect gate="G$1" pin="IN.7" pad="J1.7"/>
<connect gate="G$1" pin="MOT+" pad="J3.4"/>
<connect gate="G$1" pin="OUT.A" pad="J2.1"/>
<connect gate="G$1" pin="OUT.B" pad="J2.2"/>
<connect gate="G$1" pin="OUT.C" pad="J2.3"/>
<connect gate="G$1" pin="OUT.D" pad="J2.4"/>
<connect gate="G$1" pin="OUT.E" pad="J2.5"/>
<connect gate="G$1" pin="OUT.F" pad="J2.6"/>
<connect gate="G$1" pin="OUT.G" pad="J2.7"/>
<connect gate="G$1" pin="VCC.1" pad="J3.2"/>
<connect gate="G$1" pin="VCC.2" pad="J3.3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="DRIVER-ULN2003#MC">
<description>&lt;b&gt;7-Channel Darlington NPN Transistor Module&lt;/b&gt; based on &lt;b&gt;ULN2003&lt;/b&gt; chip&lt;br&gt;
Symbol with motor connector pins
&lt;p&gt;&lt;img alt="photo" src="http://www.diymodules.org/img/device-photo.php?name=DRIVER-ULN2003"&gt;&lt;/p&gt;</description>
<gates>
<gate name="G$1" symbol="DRIVER-ULN2003#MC"/>
</gates>
<devices>
<device name="" package="DRIVER-ULN2003#MC">
<connects>
<connect gate="G$1" pin="GND" pad="J3.1"/>
<connect gate="G$1" pin="IN.1" pad="J1.1"/>
<connect gate="G$1" pin="IN.2" pad="J1.2"/>
<connect gate="G$1" pin="IN.3" pad="J1.3"/>
<connect gate="G$1" pin="IN.4" pad="J1.4"/>
<connect gate="G$1" pin="IN.5" pad="J1.5"/>
<connect gate="G$1" pin="IN.6" pad="J1.6"/>
<connect gate="G$1" pin="IN.7" pad="J1.7"/>
<connect gate="G$1" pin="MOT+" pad="J3.4"/>
<connect gate="G$1" pin="MOT.+" pad="P3.5"/>
<connect gate="G$1" pin="MOT.A" pad="P3.4"/>
<connect gate="G$1" pin="MOT.B" pad="P3.3"/>
<connect gate="G$1" pin="MOT.C" pad="P3.2"/>
<connect gate="G$1" pin="MOT.D" pad="P3.1"/>
<connect gate="G$1" pin="OUT.A" pad="J2.1"/>
<connect gate="G$1" pin="OUT.B" pad="J2.2"/>
<connect gate="G$1" pin="OUT.C" pad="J2.3"/>
<connect gate="G$1" pin="OUT.D" pad="J2.4"/>
<connect gate="G$1" pin="OUT.E" pad="J2.5"/>
<connect gate="G$1" pin="OUT.F" pad="J2.6"/>
<connect gate="G$1" pin="OUT.G" pad="J2.7"/>
<connect gate="G$1" pin="VCC.1" pad="J3.2"/>
<connect gate="G$1" pin="VCC.2" pad="J3.3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LCD-I2C-CONVERTER">
<description>&lt;b&gt;I2C Bus to 4-Bit Parallel LCD Interface&lt;/b&gt; with LED backlight driver
&lt;p&gt;&lt;img alt="photo" src="http://www.diymodules.org/img/device-photo.php?name=LCD-I2C-CONVERTER"&gt;&lt;/p&gt;</description>
<gates>
<gate name="G$1" symbol="LCD-I2C-CONVERTER"/>
</gates>
<devices>
<device name="" package="LCD-I2C-CONVERTER">
<connects>
<connect gate="G$1" pin="DB0" pad="J2.7"/>
<connect gate="G$1" pin="DB1" pad="J2.8"/>
<connect gate="G$1" pin="DB2" pad="J2.9"/>
<connect gate="G$1" pin="DB3" pad="J2.10"/>
<connect gate="G$1" pin="DB4" pad="J2.11"/>
<connect gate="G$1" pin="DB5" pad="J2.12"/>
<connect gate="G$1" pin="DB6" pad="J2.13"/>
<connect gate="G$1" pin="DB7" pad="J2.14"/>
<connect gate="G$1" pin="EN" pad="J2.6"/>
<connect gate="G$1" pin="GND" pad="J1.4"/>
<connect gate="G$1" pin="LED.A" pad="J2.15"/>
<connect gate="G$1" pin="LED.K" pad="J2.16"/>
<connect gate="G$1" pin="R/W" pad="J2.5"/>
<connect gate="G$1" pin="RS" pad="J2.4"/>
<connect gate="G$1" pin="SCL" pad="J1.3"/>
<connect gate="G$1" pin="SDA" pad="J1.2"/>
<connect gate="G$1" pin="VCC" pad="J1.1"/>
<connect gate="G$1" pin="VDD" pad="J2.2"/>
<connect gate="G$1" pin="VEE" pad="J2.3"/>
<connect gate="G$1" pin="VSS" pad="J2.1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LIGHT-DETECTOR">
<description>&lt;b&gt;Light Detection Module&lt;/b&gt;
&lt;p&gt;&lt;img alt="photo" src="http://www.diymodules.org/img/device-photo.php?name=LIGHT-DETECTOR"&gt;&lt;/p&gt;</description>
<gates>
<gate name="G$1" symbol="LIGHT-DETECTOR"/>
</gates>
<devices>
<device name="" package="LIGHT-DETECTOR">
<connects>
<connect gate="G$1" pin="5V" pad="1"/>
<connect gate="G$1" pin="GND" pad="3"/>
<connect gate="G$1" pin="OUT" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MOTION-PIR-DYP-ME003">
<description>&lt;b&gt;PIR Motion Sensor Module DYP-ME003&lt;/b&gt; based on &lt;b&gt;BISS0001&lt;/b&gt; pyroelectic detector
&lt;p&gt;&lt;img alt="photo" src="http://www.diymodules.org/img/device-photo.php?name=MOTION-PIR-DYP-ME003"&gt;&lt;/p&gt;</description>
<gates>
<gate name="G$1" symbol="MOTION-PIR-DYP-ME003"/>
</gates>
<devices>
<device name="" package="MOTION-PIR-DYP-ME003">
<connects>
<connect gate="G$1" pin="GND" pad="1"/>
<connect gate="G$1" pin="OUT" pad="2"/>
<connect gate="G$1" pin="VCC" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="REG-AMS1117-*">
<description>&lt;b&gt;Linear Regulator&lt;/b&gt; based on &lt;b&gt;AMS1117&lt;/b&gt; chip
&lt;p&gt;&lt;img alt="photo" src="http://www.diymodules.org/img/device-photo.php?name=REG-AMS1117-"&gt;&lt;/p&gt;</description>
<gates>
<gate name="G$1" symbol="REG-AMS1117"/>
</gates>
<devices>
<device name="" package="REG-AMS1117">
<connects>
<connect gate="G$1" pin="GND.I" pad="J1.2"/>
<connect gate="G$1" pin="GND.O" pad="J2.2"/>
<connect gate="G$1" pin="VIN" pad="J1.1"/>
<connect gate="G$1" pin="VOUT" pad="J2.1"/>
</connects>
<technologies>
<technology name="3.3V"/>
<technology name="5.0V"/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="RELAY-2-SRD#RC">
<description>&lt;b&gt;2-Channel Relay Module&lt;/b&gt; based on &lt;b&gt;SRD-05VDC-SL-C&lt;/b&gt; relays&lt;br&gt;
Symbol with relays pins
&lt;p&gt;&lt;img alt="photo" src="http://www.diymodules.org/img/device-photo.php?name=RELAY-2-SRD"&gt;&lt;/p&gt;</description>
<gates>
<gate name="G$1" symbol="RELAY-2-SRD#RC"/>
</gates>
<devices>
<device name="" package="RELAY-2-SRD#RC">
<connects>
<connect gate="G$1" pin="GND.1" pad="J1.4"/>
<connect gate="G$1" pin="GND.2" pad="J2.3"/>
<connect gate="G$1" pin="IN1" pad="J1.3"/>
<connect gate="G$1" pin="IN2" pad="J1.2"/>
<connect gate="G$1" pin="JD-VCC" pad="J2.1"/>
<connect gate="G$1" pin="REL.1.COM" pad="P1.5"/>
<connect gate="G$1" pin="REL.1.NC" pad="P1.6"/>
<connect gate="G$1" pin="REL.1.NO" pad="P1.4"/>
<connect gate="G$1" pin="REL.2.COM" pad="P1.2"/>
<connect gate="G$1" pin="REL.2.NC" pad="P1.3"/>
<connect gate="G$1" pin="REL.2.NO" pad="P1.1"/>
<connect gate="G$1" pin="VCC.1" pad="J1.1"/>
<connect gate="G$1" pin="VCC.2" pad="J2.2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="RELAY-2-SRD">
<description>&lt;b&gt;2-Channel Relay Module&lt;/b&gt; based on &lt;b&gt;SRD-05VDC-SL-C&lt;/b&gt; relays
&lt;p&gt;&lt;img alt="photo" src="http://www.diymodules.org/img/device-photo.php?name=REALY-2-SRD"&gt;&lt;/p&gt;</description>
<gates>
<gate name="G$1" symbol="RELAY-2-SRD"/>
</gates>
<devices>
<device name="" package="RELAY-2-SRD">
<connects>
<connect gate="G$1" pin="GND.1" pad="J1.4"/>
<connect gate="G$1" pin="GND.2" pad="J2.3"/>
<connect gate="G$1" pin="IN1" pad="J1.3"/>
<connect gate="G$1" pin="IN2" pad="J1.2"/>
<connect gate="G$1" pin="JD-VCC" pad="J2.1"/>
<connect gate="G$1" pin="VCC.1" pad="J1.1"/>
<connect gate="G$1" pin="VCC.2" pad="J2.2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="RTC-EEPROM-BATTERY">
<description>&lt;b&gt;RTC Module with Battery and EEPROM&lt;/b&gt; based on &lt;b&gt;DS1307&lt;/b&gt; and &lt;b&gt;AT24C32&lt;/b&gt; chips
&lt;p&gt;&lt;img alt="photo" src="http://www.diymodules.org/img/device-photo.php?name=RTC-EEPROM-BATTERY"&gt;&lt;/p&gt;</description>
<gates>
<gate name="G$1" symbol="RTC-EEPROM-BATTERY"/>
</gates>
<devices>
<device name="" package="RTC_EEPROM_BATTERY">
<connects>
<connect gate="G$1" pin="BAT" pad="J2.1"/>
<connect gate="G$1" pin="DS.1" pad="J1.5"/>
<connect gate="G$1" pin="DS.2" pad="J2.6"/>
<connect gate="G$1" pin="GND.1" pad="J1.1"/>
<connect gate="G$1" pin="GND.2" pad="J2.2"/>
<connect gate="G$1" pin="SCL.1" pad="J1.4"/>
<connect gate="G$1" pin="SCL.2" pad="J2.5"/>
<connect gate="G$1" pin="SDA.1" pad="J1.3"/>
<connect gate="G$1" pin="SDA.2" pad="J2.4"/>
<connect gate="G$1" pin="SQ" pad="J2.7"/>
<connect gate="G$1" pin="VCC.1" pad="J1.2"/>
<connect gate="G$1" pin="VCC.2" pad="J2.3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="SOIL-MOISTURE-SENSOR">
<description>&lt;b&gt;Soil Moisture Sensor&lt;/b&gt;
&lt;p&gt;&lt;img alt="photo" src="http://www.diymodules.org/img/device-photo.php?name=SOIL-MOISTURE-SENSOR"&gt;&lt;/p&gt;</description>
<gates>
<gate name="G$1" symbol="SOIL-MOISTURE-SENSOR"/>
</gates>
<devices>
<device name="" package="SOIL-MOISTURE-SENSOR">
<connects>
<connect gate="G$1" pin="A0" pad="J1.1"/>
<connect gate="G$1" pin="DO" pad="J1.2"/>
<connect gate="G$1" pin="GND" pad="J1.3"/>
<connect gate="G$1" pin="SENS.1" pad="J2.1"/>
<connect gate="G$1" pin="SENS.2" pad="J2.2"/>
<connect gate="G$1" pin="VCC" pad="J1.4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="SOUND-DETECTOR">
<description>&lt;b&gt;Sound Detection Module&lt;/b&gt;
&lt;p&gt;&lt;img alt="photo" src="http://www.diymodules.org/img/device-photo.php?name=SOUND-DETECTOR"&gt;&lt;/p&gt;</description>
<gates>
<gate name="G$1" symbol="SOUND-DETECTOR"/>
</gates>
<devices>
<device name="" package="SOUND-DETECTOR">
<connects>
<connect gate="G$1" pin="+5V" pad="3"/>
<connect gate="G$1" pin="GND" pad="1"/>
<connect gate="G$1" pin="OUT" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ULTRASONIC-HC-SR04">
<description>&lt;b&gt;Ultrasonic Ranging Module HC-SR04&lt;/b&gt;
&lt;p&gt;&lt;img alt="photo" src="http://www.diymodules.org/img/device-photo.php?name=ULTRASONIC-HC-SR04"&gt;&lt;/p&gt;</description>
<gates>
<gate name="G$1" symbol="ULTRASONIC-HC-SR04"/>
</gates>
<devices>
<device name="" package="ULTRASONIC-HC-SR04">
<connects>
<connect gate="G$1" pin="ECHO" pad="3"/>
<connect gate="G$1" pin="GND" pad="4"/>
<connect gate="G$1" pin="TRIG" pad="2"/>
<connect gate="G$1" pin="VCC" pad="1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="#V" package="ULTRASONIC-HC-SR04#V">
<connects>
<connect gate="G$1" pin="ECHO" pad="3"/>
<connect gate="G$1" pin="GND" pad="4"/>
<connect gate="G$1" pin="TRIG" pad="2"/>
<connect gate="G$1" pin="VCC" pad="1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WIRELESS-WIFI-ESP-01">
<description>&lt;b&gt;Wireless Wi-Fi ESP-01 Module&lt;/b&gt; based on &lt;b&gt;ESP8266&lt;/b&gt; chip
&lt;p&gt;&lt;img alt="photo" src="http://www.diymodules.org/img/device-photo.php?name=WIRELESS-WIFI-ESP-01"&gt;&lt;/p&gt;</description>
<gates>
<gate name="G$1" symbol="WIRELESS-WIFI-ESP-01"/>
</gates>
<devices>
<device name="" package="WIRELESS-WIFI-ESP-01">
<connects>
<connect gate="G$1" pin="CH_PD" pad="B2"/>
<connect gate="G$1" pin="GND" pad="A1"/>
<connect gate="G$1" pin="GPIO0" pad="C1"/>
<connect gate="G$1" pin="GPIO2" pad="B1"/>
<connect gate="G$1" pin="RST" pad="C2"/>
<connect gate="G$1" pin="URXD" pad="D1"/>
<connect gate="G$1" pin="UTXD" pad="A2"/>
<connect gate="G$1" pin="VCC" pad="D2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="DC-DC-STEP-UP-5V">
<description>&lt;b&gt;DC/DC Step-Up Converter&lt;/b&gt;
&lt;p&gt;&lt;img alt="photo" src="http://www.diymodules.org/img/device-photo.php?name=DC-DC-STEP-UP-5V"&gt;&lt;/p&gt;</description>
<gates>
<gate name="G$1" symbol="DC-DC-STEP-UP-5V"/>
</gates>
<devices>
<device name="" package="DC-DC-STEP-UP-5V">
<connects>
<connect gate="G$1" pin="5V" pad="5V"/>
<connect gate="G$1" pin="D+" pad="D+"/>
<connect gate="G$1" pin="D-" pad="D-"/>
<connect gate="G$1" pin="GND" pad="GND"/>
<connect gate="G$1" pin="IN+" pad="IN+"/>
<connect gate="G$1" pin="IN-" pad="IN-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WIRELESS-NRF24L01-PA-EXT" prefix="M">
<description>&lt;b&gt;2.4 GHz Wireless Module&lt;/b&gt; based on &lt;b&gt;NRF24L01&lt;/b&gt; chip with preamplifier and external antenna
&lt;p&gt;&lt;img alt="photo" src="http://www.diymodules.org/img/device-photo.php?name=WIRELESS-NRF24L01-PA-EXT"&gt;&lt;/p&gt;</description>
<gates>
<gate name="G$1" symbol="WIRELESS-NRF24L01-PA-EXT"/>
</gates>
<devices>
<device name="" package="WIRELESS-NRD24L01-PA-EXT">
<connects>
<connect gate="G$1" pin="CE" pad="3"/>
<connect gate="G$1" pin="CSN" pad="4"/>
<connect gate="G$1" pin="GND" pad="1"/>
<connect gate="G$1" pin="IRQ" pad="8"/>
<connect gate="G$1" pin="MISO" pad="7"/>
<connect gate="G$1" pin="MOSI" pad="6"/>
<connect gate="G$1" pin="SCK" pad="5"/>
<connect gate="G$1" pin="VCC" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="AC-DC-3.5W">
<description>&lt;b&gt;AC/DC 3.5W Converter&lt;/b&gt;
&lt;p&gt;&lt;img alt="photo" src="http://www.diymodules.org/img/device-photo.php?name=AC-DC-3.5W"&gt;&lt;/p&gt;</description>
<gates>
<gate name="G$1" symbol="AC-DC-3.5W"/>
</gates>
<devices>
<device name="" package="AC-DC-3.5W">
<connects>
<connect gate="G$1" pin="5V" pad="J2.2"/>
<connect gate="G$1" pin="AC1" pad="J1.1"/>
<connect gate="G$1" pin="AC2" pad="J1.2"/>
<connect gate="G$1" pin="OUT+" pad="J2.3"/>
<connect gate="G$1" pin="OUT-" pad="J2.1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="BATTERY-CHARGER-LI-5V">
<description>&lt;b&gt;Lithium Battery 5V Charger&lt;/b&gt;
&lt;p&gt;&lt;img alt="photo" src="http://www.diymodules.org/img/device-photo.php?name=BATTERY-CHARGER-LI-5V"&gt;&lt;/p&gt;</description>
<gates>
<gate name="G$1" symbol="BATTERY-CHARGER-LI-5V"/>
</gates>
<devices>
<device name="" package="BATTERY-CHARGER-LI-5V">
<connects>
<connect gate="G$1" pin="BAT+" pad="BAT+"/>
<connect gate="G$1" pin="BAT-" pad="BAT-"/>
<connect gate="G$1" pin="IN+" pad="IN+"/>
<connect gate="G$1" pin="IN-" pad="IN-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="FLAME-DETECTOR">
<description>&lt;b&gt;Flame Detector&lt;/b&gt;
&lt;p&gt;&lt;img alt="photo" src="http://www.diymodules.org/img/device-photo.php?name=FLAME-DETECTOR"&gt;&lt;/p&gt;</description>
<gates>
<gate name="G$1" symbol="FLAME-DETECTOR"/>
</gates>
<devices>
<device name="" package="FLAME-DETECTOR">
<connects>
<connect gate="G$1" pin="AO" pad="4"/>
<connect gate="G$1" pin="DO" pad="3"/>
<connect gate="G$1" pin="GND" pad="2"/>
<connect gate="G$1" pin="VCC" pad="1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="IR-RECEIVER">
<description>&lt;b&gt;IR Receiver Module&lt;/b&gt;
&lt;p&gt;&lt;img alt="photo" src="http://www.diymodules.org/img/device-photo.php?name=IR-RECEIVER"&gt;&lt;/p&gt;</description>
<gates>
<gate name="G$1" symbol="IR-RECEIVER"/>
</gates>
<devices>
<device name="" package="IR-RECEIVER">
<connects>
<connect gate="G$1" pin="GND" pad="C.2"/>
<connect gate="G$1" pin="GND.1" pad="A.2"/>
<connect gate="G$1" pin="GND.2" pad="B.2"/>
<connect gate="G$1" pin="IN" pad="C.1"/>
<connect gate="G$1" pin="IN.1" pad="A.3"/>
<connect gate="G$1" pin="IN.2" pad="B.3"/>
<connect gate="G$1" pin="VCC" pad="C.3"/>
<connect gate="G$1" pin="VCC.1" pad="A.1"/>
<connect gate="G$1" pin="VCC.2" pad="B.1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="IR-RECEIVER#NC">
<description>&lt;b&gt;IR Receiver Module&lt;/b&gt; without IR sensor connector
&lt;p&gt;&lt;img alt="photo" src="http://www.diymodules.org/img/device-photo.php?name=IR-RECEIVER"&gt;&lt;/p&gt;</description>
<gates>
<gate name="G$1" symbol="IR-RECEIVER#NC"/>
</gates>
<devices>
<device name="" package="IR-RECEIVER#NC">
<connects>
<connect gate="G$1" pin="GND.1" pad="A.2"/>
<connect gate="G$1" pin="GND.2" pad="B.2"/>
<connect gate="G$1" pin="IN.1" pad="A.3"/>
<connect gate="G$1" pin="IN.2" pad="B.3"/>
<connect gate="G$1" pin="VCC.1" pad="A.1"/>
<connect gate="G$1" pin="VCC.2" pad="B.1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="STEPPER-MOTOR-EASY-DRIVER">
<description>&lt;b&gt;Stepper Motor Easy Driver&lt;/b&gt;
&lt;p&gt;&lt;img alt="photo" src="http://www.diymodules.org/img/device-photo.php?name=STEPPER-MOTOR-EASY-DRIVER"&gt;&lt;/p&gt;</description>
<gates>
<gate name="G$1" symbol="STEPPER-MOTOR-EASY-DRIVER"/>
</gates>
<devices>
<device name="" package="STEPPER-MOTOR-EASY-DRIVER">
<connects>
<connect gate="G$1" pin="+5V" pad="JP4.1"/>
<connect gate="G$1" pin="A.1" pad="JP3.1"/>
<connect gate="G$1" pin="A.2" pad="JP3.2"/>
<connect gate="G$1" pin="B.1" pad="JP3.3"/>
<connect gate="G$1" pin="B.2" pad="JP3.4"/>
<connect gate="G$1" pin="DIR" pad="JP2.3"/>
<connect gate="G$1" pin="ENA" pad="JP6.1"/>
<connect gate="G$1" pin="GND" pad="JP1.1"/>
<connect gate="G$1" pin="GND.1" pad="JP4.2"/>
<connect gate="G$1" pin="GND.2" pad="JP2.1"/>
<connect gate="G$1" pin="M+" pad="JP1.2"/>
<connect gate="G$1" pin="MS1" pad="JP5.1"/>
<connect gate="G$1" pin="MS2" pad="JP6.2"/>
<connect gate="G$1" pin="PFD" pad="JP7.1"/>
<connect gate="G$1" pin="RST" pad="JP7.2"/>
<connect gate="G$1" pin="SLP" pad="JP5.2"/>
<connect gate="G$1" pin="STER" pad="JP2.2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="RS485-TTL-CONVERTER">
<description>&lt;b&gt;RS485 to TTL converter&lt;/b&gt; based on &lt;b&gt;MAX485&lt;/b&gt; chip
&lt;p&gt;&lt;img alt="photo" src="http://www.diymodules.org/img/device-photo.php?name=RS485-TTL-CONVERTER"&gt;&lt;/p&gt;</description>
<gates>
<gate name="G$1" symbol="RS485-TTL-CONVERTER"/>
</gates>
<devices>
<device name="" package="RS485-TTL-CONVERTER">
<connects>
<connect gate="G$1" pin="A" pad="J2.3"/>
<connect gate="G$1" pin="B" pad="J2.2"/>
<connect gate="G$1" pin="DE" pad="J1.2"/>
<connect gate="G$1" pin="DI" pad="J1.1"/>
<connect gate="G$1" pin="GND" pad="J2.4"/>
<connect gate="G$1" pin="RE" pad="J1.3"/>
<connect gate="G$1" pin="RO" pad="J1.4"/>
<connect gate="G$1" pin="VCC" pad="J2.1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="TOUCH-KEYPAD-4X4">
<description>&lt;b&gt;16 Channel Capacitive Touch Keypad&lt;/b&gt;
&lt;p&gt;&lt;img alt="photo" src="http://www.diymodules.org/img/device-photo.php?name=TOUCH-KEYPAD-4X4"&gt;&lt;/p&gt;</description>
<gates>
<gate name="G$1" symbol="TOUCH-KEYPAD-4X4"/>
</gates>
<devices>
<device name="" package="TOUCH-KEYPAD-4X4">
<connects>
<connect gate="G$1" pin="GND" pad="2"/>
<connect gate="G$1" pin="OUT1" pad="5"/>
<connect gate="G$1" pin="OUT2" pad="6"/>
<connect gate="G$1" pin="OUT3" pad="7"/>
<connect gate="G$1" pin="OUT4" pad="8"/>
<connect gate="G$1" pin="OUT5" pad="9"/>
<connect gate="G$1" pin="OUT6" pad="10"/>
<connect gate="G$1" pin="OUT7" pad="11"/>
<connect gate="G$1" pin="OUT8" pad="12"/>
<connect gate="G$1" pin="SCL" pad="3"/>
<connect gate="G$1" pin="SDO" pad="4"/>
<connect gate="G$1" pin="VCC" pad="1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="SOUND-BUZZER">
<description>&lt;b&gt;Sound Buzzer Module&lt;/b&gt;
&lt;p&gt;&lt;img alt="photo" src="http://www.diymodules.org/img/device-photo.php?name=SOUND-BUZZER"&gt;&lt;/p&gt;</description>
<gates>
<gate name="G$1" symbol="SOUND-BUZZER"/>
</gates>
<devices>
<device name="" package="SOUND-BUZZER">
<connects>
<connect gate="G$1" pin="EN" pad="2"/>
<connect gate="G$1" pin="GND" pad="1"/>
<connect gate="G$1" pin="VCC" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="GSM-MODEM-SIM900A">
<description>&lt;b&gt;GSM Mini Module&lt;/b&gt; based on &lt;b&gt;SIM900A&lt;/b&gt;
&lt;p&gt;Schematic available here:&lt;br /&gt;&lt;a href="http://www.electrodragon.com/w/SIM900_(SIM900A)_Mini_DEV_Board"&gt;http://www.electrodragon.com/w/SIM900_(SIM900A)_Mini_DEV_Board&lt;/a&gt;&lt;/p&gt;
&lt;p&gt;&lt;img alt="photo" src="http://www.diymodules.org/img/device-photo.php?name=GSM-MODEM-SIM900"&gt;&lt;/p&gt;</description>
<gates>
<gate name="G$1" symbol="GSM-MODEM-SIM900A"/>
</gates>
<devices>
<device name="" package="GSM-MODEM-SIM900A">
<connects>
<connect gate="G$1" pin="GND.1" pad="J1.2"/>
<connect gate="G$1" pin="GND.2" pad="J1.7"/>
<connect gate="G$1" pin="RST" pad="J1.8"/>
<connect gate="G$1" pin="SIMR" pad="J1.5"/>
<connect gate="G$1" pin="SIMT" pad="J1.6"/>
<connect gate="G$1" pin="VCC4" pad="J1.3"/>
<connect gate="G$1" pin="VCC5" pad="J1.1"/>
<connect gate="G$1" pin="VCCMCU" pad="J1.4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LED-24XRGB-RING">
<description>&lt;b&gt;24 LEDs RGB Ring&lt;/b&gt; based on &lt;b&gt;WS2812B&lt;/b&gt;
&lt;p&gt;&lt;img alt="photo" src="http://www.diymodules.org/img/device-photo.php?name=LED-24XRGB-RING"&gt;&lt;/p&gt;</description>
<gates>
<gate name="G$1" symbol="LED-24XRGB-RING"/>
</gates>
<devices>
<device name="" package="LED-24XRGB-RING">
<connects>
<connect gate="G$1" pin="GND.1" pad="1"/>
<connect gate="G$1" pin="GND.2" pad="6"/>
<connect gate="G$1" pin="IN" pad="3"/>
<connect gate="G$1" pin="OUT" pad="4"/>
<connect gate="G$1" pin="VCC.1" pad="2"/>
<connect gate="G$1" pin="VCC.2" pad="5"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="N-MOSFET-SWITCH">
<description>&lt;b&gt;Low Side N-MOSFET Switch&lt;/b&gt; with &lt;b&gt;Optocoupler&lt;/b&gt;
&lt;p&gt;&lt;img alt="photo" src="http://www.diymodules.org/img/device-photo.php?name=N-MOSFET-SWITCH"&gt;&lt;/p&gt;</description>
<gates>
<gate name="G$1" symbol="N-MOSFET-SWITCH"/>
</gates>
<devices>
<device name="" package="N-MOSFET-SWITCH">
<connects>
<connect gate="G$1" pin="CTRL" pad="J1.3"/>
<connect gate="G$1" pin="GND" pad="J1.1"/>
<connect gate="G$1" pin="VCC" pad="J1.2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="N-MOSFET-SWITCH#IC">
<description>&lt;b&gt;Low Side N-MOSFET Switch&lt;/b&gt; with &lt;b&gt;Optocoupler&lt;/b&gt;&lt;br /&gt;
Device with connector pins
&lt;p&gt;&lt;img alt="photo" src="http://www.diymodules.org/img/device-photo.php?name=N-MOSFET-SWITCH"&gt;&lt;/p&gt;</description>
<gates>
<gate name="G$1" symbol="N-MOSFET-SWITCH#IC"/>
</gates>
<devices>
<device name="" package="N-MOSFET-SWITCH#IC">
<connects>
<connect gate="G$1" pin="CTRL" pad="J1.3"/>
<connect gate="G$1" pin="GND" pad="J1.1"/>
<connect gate="G$1" pin="IN.COM" pad="P1.2"/>
<connect gate="G$1" pin="IN.V+" pad="P1.1"/>
<connect gate="G$1" pin="OUT.SW" pad="P2.2"/>
<connect gate="G$1" pin="OUT.V+" pad="P2.1"/>
<connect gate="G$1" pin="VCC" pad="J1.2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="BREADBOARD-POWER-V2">
<description>&lt;b&gt;Breadboard Power Adapter&lt;/b&gt; with onboard 3.3V and 5V regulators
&lt;p&gt;&lt;img alt="photo" src="http://www.diymodules.org/img/device-photo.php?name=BREADBOARD-POWER-V2"&gt;&lt;/p&gt;</description>
<gates>
<gate name="G$1" symbol="BREADBOARD-POWER-V2"/>
<gate name="G$2" symbol="BREADBOARD-POWER-V2"/>
</gates>
<devices>
<device name="" package="BREADBOARD-POWER-V2">
<connects>
<connect gate="G$1" pin="M.1" pad="A.M.1"/>
<connect gate="G$1" pin="M.2" pad="A.M.2"/>
<connect gate="G$1" pin="P.1" pad="A.P.1"/>
<connect gate="G$1" pin="P.2" pad="A.P.2"/>
<connect gate="G$2" pin="M.1" pad="B.M.1"/>
<connect gate="G$2" pin="M.2" pad="B.M.2"/>
<connect gate="G$2" pin="P.1" pad="B.P.1"/>
<connect gate="G$2" pin="P.2" pad="B.P.2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="SPARKFUN-AD-MUX-16X1">
<description>&lt;b&gt;SparkFun Analog/Digital MUX Breakout&lt;/b&gt; based on &lt;b&gt;CD74HC4067&lt;/b&gt; chip&lt;br /&gt;&lt;br /&gt;
Source: &lt;a href="https://www.sparkfun.com/products/9056"&gt;https://www.sparkfun.com/products/9056&lt;/a&gt;&lt;/p&gt;&lt;br /&gt;
&lt;p&gt;&lt;img alt="photo" src="http://www.diymodules.org/img/device-photo.php?name=SPARKFUN-AD-MUX-16X1"&gt;&lt;/p&gt;</description>
<gates>
<gate name="G$1" symbol="SPARKFUN-AD-MUX-16X1"/>
</gates>
<devices>
<device name="" package="SPARKFUN-AD-MUX-16X1">
<connects>
<connect gate="G$1" pin="C0" pad="J1.1"/>
<connect gate="G$1" pin="C1" pad="J1.2"/>
<connect gate="G$1" pin="C10" pad="J1.11"/>
<connect gate="G$1" pin="C11" pad="J1.12"/>
<connect gate="G$1" pin="C12" pad="J1.13"/>
<connect gate="G$1" pin="C13" pad="J1.14"/>
<connect gate="G$1" pin="C14" pad="J1.15"/>
<connect gate="G$1" pin="C15" pad="J1.16"/>
<connect gate="G$1" pin="C2" pad="J1.3"/>
<connect gate="G$1" pin="C3" pad="J1.4"/>
<connect gate="G$1" pin="C4" pad="J1.5"/>
<connect gate="G$1" pin="C5" pad="J1.6"/>
<connect gate="G$1" pin="C6" pad="J1.7"/>
<connect gate="G$1" pin="C7" pad="J1.8"/>
<connect gate="G$1" pin="C8" pad="J1.9"/>
<connect gate="G$1" pin="C9" pad="J1.10"/>
<connect gate="G$1" pin="EN" pad="J2.3"/>
<connect gate="G$1" pin="GND" pad="J2.1"/>
<connect gate="G$1" pin="S0" pad="J2.4"/>
<connect gate="G$1" pin="S1" pad="J2.5"/>
<connect gate="G$1" pin="S2" pad="J2.6"/>
<connect gate="G$1" pin="S3" pad="J2.7"/>
<connect gate="G$1" pin="SIG" pad="J2.8"/>
<connect gate="G$1" pin="VCC" pad="J2.2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
</devicesets>
</library>
</drawing>
</eagle>
