<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="7.6.0">
<drawing>
<library>
<packages>
<package name="HC-12_FOOTPRINT">
</package>
</packages>
<symbols>
<symbol name="HC-12_FOOTPRINT">
<pin name="VCC"/>
<pin name="GND"/>
<pin name="RX"/>
<pin name="TX"/>
<pin name="SET"/>
<pin name="ANT"/>
</symbol>
</symbols>
<devicesets>
<deviceset name="HC-12_FOOTPRINT">
<description>&lt;b&gt;HC-12 433MHz module footprint&lt;/b&gt;
&lt;p&gt;MCHFIX is for mechanical fix pin which is NC but on this file connected to GND&lt;/p&gt;

&lt;p&gt;https://github.com/meendiz/hc-12_si4463/&lt;/p&gt;</description>
<gates>
<gate name="G$1" symbol="HC-12_FOOTPRINT"/>
</gates>
<devices>
<device name="" package="HC-12_FOOTPRINT">
<connects>
<connect gate="G$1" pin="ANT" pad="ANT"/>
<connect gate="G$1" pin="GND" pad="GND GND1 GND2 MCHFIX"/>
<connect gate="G$1" pin="RX" pad="RXD"/>
<connect gate="G$1" pin="SET" pad="SET"/>
<connect gate="G$1" pin="TX" pad="TXD"/>
<connect gate="G$1" pin="VCC" pad="VCC"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
</devicesets>
</library>
</drawing>
</eagle>
