{"text_format":"3","workbook":"xls","n_sheets":1,"sheets":["3heats correct cal"],"not_rendered":{"charts":1,"external_links":1,"defined_names":10},"read":"whole","date_system":"1904","formulas":"cached_only"}

{"sheet":"3heats correct cal","index":0,"n_rows":111,"n_cols":4,"rows_kept":111,"flags":["formulas_cached_only"]}
["energy in pos and neg half-cycles with 3 different heater settings  (sketch = Mk2a_PV_Router, duration = 30 seconds)"]
["tally Num","energy in pos HCs","energy in neg HCs","energy at mid range of tally"]
[0," <- min value of tally range (W)"]
[3000," <- max value of tally range (W)"]
[30," <- step value between tallies (W)"]
[100," <- number of tallies"]
[30," <- duration of recording (sec)"]
[3000," <- no of values tallied"]
[89," <- samples per mains cycle (average)"]
[101,0,0]
[100,0,0,2985]
[99,0,0,2955]
[98,0,0,2925]
[97,0,0,2895]
[96,0,0,2865]
[95,0,0,2835]
[94,0,0,2805]
[93,0,0,2775]
[92,0,0,2745]
[91,0,0,2715]
[90,0,0,2685]
[89,0,0,2655]
[88,0,0,2625]
[87,0,0,2595]
[86,0,0,2565]
[85,0,0,2535]
[84,0,0,2505]
[83,0,0,2475]
[82,0,0,2445]
[81,0,0,2415]
[80,0,0,2385]
[79,0,0,2355]
[78,0,0,2325]
[77,0,0,2295]
[76,0,0,2265]
[75,0,0,2235]
[74,0,0,2205]
[73,0,0,2175]
[72,0,0,2145]
[71,0,1,2115]
[70,3,2,2085]
[69,68,71,2055]
[68,136,115,2025]
[67,191,165,1995]
[66,11,56,1965]
[65,1,0,1935]
[64,0,0,1905]
[63,0,0,1875]
[62,0,0,1845]
[61,0,0,1815]
[60,0,0,1785]
[59,0,0,1755]
[58,0,0,1725]
[57,0,0,1695]
[56,0,0,1665]
[55,0,0,1635]
[54,0,0,1605]
[53,0,0,1575]
[52,0,0,1545]
[51,0,0,1515]
[50,1,0,1485]
[49,0,0,1455]
[48,1,0,1425]
[47,0,0,1395]
[46,0,0,1365]
[45,1,2,1335]
[44,3,3,1305]
[43,85,58,1275]
[42,252,191,1245]
[41,31,120,1215]
[40,4,2,1185]
[39,1,0,1155]
[38,0,1,1125]
[37,0,0,1095]
[36,0,0,1065]
[35,0,1,1035]
[34,0,0,1005]
[33,0,1,975]
[32,0,0,945]
[31,0,0,915]
[30,0,1,885]
[29,1,1,855]
[28,2,0,825]
[27,105,57,795]
[26,277,261,765]
[25,29,93,735]
[24,1,2,705]
[23,0,0,675]
[22,0,0,645]
[21,0,0,615]
[20,1,0,585]
[19,0,0,555]
[18,0,0,525]
[17,0,0,495]
[16,0,0,465]
[15,0,0,435]
[14,0,0,405]
[13,0,0,375]
[12,0,0,345]
[11,0,0,315]
[10,0,0,285]
[9,0,0,255]
[8,0,0,225]
[7,0,0,195]
[6,0,0,165]
[5,0,0,135]
[4,0,1,105]
[3,0,0,75]
[2,0,1,45]
[1,7,0,15]
[0,288,294]